(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "VMM5320BJG"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 46.99 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "VMM5320BJG"
				(at 46.99 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "VMM5320BJG"
				(at 46.99 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://uploadcdn.oneyac.com/upload/document/1641525833084_8966.pdf"
				(at 46.99 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1 In to 2 Out HDMI2.0 Repeater with Audio Extraction/Insertion"
				(at 46.99 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "VMM5320BJG"
				(at 46.99 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Synaptics"
				(at 46.99 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 46.99 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 46.99 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, VIDEO, HDMI, DISPLAYPORT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "VMM5320BJG_1_1"
				(text "RX0"
					(at 13.97 -15.24 900)
				)
				(text "TX0"
					(at 20.32 -15.24 900)
				)
				(text "TX1"
					(at 20.32 -50.8 900)
				)
				(text "TX2"
					(at 20.32 -91.44 900)
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "RxN3")
					(number "A1")
				)
				(pin output line
					(at 33.02 0 180)
					(length 3.81)
					(name "Tx0P0")
					(number "A4")
				)
				(pin output line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "Tx0N0")
					(number "A5")
				)
				(pin output line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "Tx0P1")
					(number "A6")
				)
				(pin output line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "Tx0N1")
					(number "A7")
				)
				(pin output line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "Tx0P2")
					(number "A8")
				)
				(pin output line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "Tx0N2")
					(number "A9")
				)
				(pin output line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "Tx0P3")
					(number "A10")
				)
				(pin output line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "Tx0N3")
					(number "A11")
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 3.81)
					(name "Tx0SDA")
					(number "A13")
				)
				(pin input line
					(at 33.02 -21.59 180)
					(length 3.81)
					(name "CAD0")
					(number "A14")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "RxP3")
					(number "B1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "RxSRCDET")
					(number "B2")
				)
				(pin input line
					(at 33.02 -30.48 180)
					(length 3.81)
					(name "Tx0HPD")
					(number "B11")
				)
				(pin output line
					(at 33.02 -25.4 180)
					(length 3.81)
					(name "Tx0SCL")
					(number "B13")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "RxN2")
					(number "C1")
				)
				(pin output line
					(at 33.02 -34.29 180)
					(length 3.81)
					(name "Tx1P0")
					(number "C14")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "RxP2")
					(number "D1")
				)
				(pin output line
					(at 33.02 -36.83 180)
					(length 3.81)
					(name "Tx1N0")
					(number "D14")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "RxN1")
					(number "E1")
				)
				(pin output line
					(at 33.02 -39.37 180)
					(length 3.81)
					(name "Tx1P1")
					(number "E14")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "RxP1")
					(number "F1")
				)
				(pin output line
					(at 33.02 -41.91 180)
					(length 3.81)
					(name "Tx1N1")
					(number "F14")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "RxN0")
					(number "G1")
				)
				(pin output line
					(at 33.02 -44.45 180)
					(length 3.81)
					(name "Tx1P2")
					(number "G14")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "RxP0")
					(number "H1")
				)
				(pin output line
					(at 33.02 -46.99 180)
					(length 3.81)
					(name "Tx1N2")
					(number "H14")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "RxHPD")
					(number "J1")
				)
				(pin output line
					(at 33.02 -49.53 180)
					(length 3.81)
					(name "Tx1P3")
					(number "J14")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "RxAUXP")
					(number "K1")
				)
				(pin input line
					(at 33.02 -55.88 180)
					(length 3.81)
					(name "CAD1")
					(number "K12")
				)
				(pin input line
					(at 33.02 -71.12 180)
					(length 3.81)
					(name "Tx1HPD")
					(number "K13")
				)
				(pin output line
					(at 33.02 -52.07 180)
					(length 3.81)
					(name "Tx1N3")
					(number "K14")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 3.81)
					(name "RxAUXN")
					(number "L1")
				)
				(pin input line
					(at 33.02 -96.52 180)
					(length 3.81)
					(name "CAD2")
					(number "L2")
				)
				(pin output line
					(at 33.02 -106.68 180)
					(length 3.81)
					(name "Tx2SCL")
					(number "L3")
				)
				(pin bidirectional line
					(at 33.02 -100.33 180)
					(length 3.81)
					(name "Tx2AUXP")
					(number "L4")
				)
				(pin input line
					(at 33.02 -111.76 180)
					(length 3.81)
					(name "Tx2HPD")
					(number "L5")
				)
				(pin bidirectional line
					(at 33.02 -59.69 180)
					(length 3.81)
					(name "Tx1AUXP")
					(number "L13")
				)
				(pin bidirectional line
					(at 33.02 -62.23 180)
					(length 3.81)
					(name "Tx1AUXN")
					(number "L14")
				)
				(pin bidirectional line
					(at 33.02 -109.22 180)
					(length 3.81)
					(name "Tx2SDA")
					(number "M3")
				)
				(pin bidirectional line
					(at 33.02 -102.87 180)
					(length 3.81)
					(name "Tx2AUXN")
					(number "M4")
				)
				(pin output line
					(at 33.02 -92.71 180)
					(length 3.81)
					(name "Tx2N3")
					(number "M5")
				)
				(pin output line
					(at 33.02 -90.17 180)
					(length 3.81)
					(name "Tx2P3")
					(number "M6")
				)
				(pin output line
					(at 33.02 -87.63 180)
					(length 3.81)
					(name "Tx2N2")
					(number "M7")
				)
				(pin output line
					(at 33.02 -85.09 180)
					(length 3.81)
					(name "Tx2P2")
					(number "M8")
				)
				(pin output line
					(at 33.02 -82.55 180)
					(length 3.81)
					(name "Tx2N1")
					(number "M9")
				)
				(pin output line
					(at 33.02 -80.01 180)
					(length 3.81)
					(name "Tx2P1")
					(number "M10")
				)
				(pin output line
					(at 33.02 -77.47 180)
					(length 3.81)
					(name "Tx2N0")
					(number "M11")
				)
				(pin output line
					(at 33.02 -74.93 180)
					(length 3.81)
					(name "Tx2P0")
					(number "M12")
				)
				(pin output line
					(at 33.02 -66.04 180)
					(length 3.81)
					(name "Tx1SCL")
					(number "M13")
				)
				(pin bidirectional line
					(at 33.02 -68.58 180)
					(length 3.81)
					(name "Tx1SDA")
					(number "M14")
				)
			)
			(symbol "VMM5320BJG_2_1"
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "RX_STS")
					(number "A2")
				)
				(pin bidirectional line
					(at 27.94 -5.08 180)
					(length 3.81)
					(name "GPIO2")
					(number "A3")
				)
				(pin bidirectional line
					(at 27.94 -7.62 180)
					(length 3.81)
					(name "GPIO3")
					(number "B3")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "RSTN_I")
					(number "B4")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "TX0_STS")
					(number "B5")
				)
				(pin output line
					(at 0 -16.51 0)
					(length 3.81)
					(name "SPICSN")
					(number "B7")
				)
				(pin output line
					(at 0 -19.05 0)
					(length 3.81)
					(name "SPICLK")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "SPIDIO0")
					(number "B14")
				)
				(pin bidirectional line
					(at 27.94 -10.16 180)
					(length 3.81)
					(name "GPIO4")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 3.81)
					(name "SPIDIO1")
					(number "C13")
				)
				(pin bidirectional line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GPIO5")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 3.81)
					(name "SPIDIO2")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SSDA")
					(number "G3")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 3.81)
					(name "SPIDIO3")
					(number "G13")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SSCL")
					(number "H3")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "LP_CTL")
					(number "J2")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 3.81)
					(name "TX1_STS")
					(number "J13")
				)
				(pin bidirectional line
					(at 27.94 -15.24 180)
					(length 3.81)
					(name "GPIO6")
					(number "K2")
				)
				(pin bidirectional line
					(at 27.94 -17.78 180)
					(length 3.81)
					(name "GPIO7")
					(number "K5")
				)
				(pin bidirectional line
					(at 27.94 -20.32 180)
					(length 3.81)
					(name "GPIO8")
					(number "K6")
				)
				(pin bidirectional line
					(at 27.94 -22.86 180)
					(length 3.81)
					(name "GPIO9")
					(number "K7")
				)
				(pin bidirectional line
					(at 27.94 0 180)
					(length 3.81)
					(name "GPIO0")
					(number "K8")
				)
				(pin bidirectional line
					(at 27.94 -2.54 180)
					(length 3.81)
					(name "GPIO1")
					(number "K11")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 3.81)
					(name "TX2_STS")
					(number "L6")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 3.81)
					(name "XIN")
					(number "M1")
				)
				(pin output line
					(at 0 -6.35 0)
					(length 3.81)
					(name "XOUT")
					(number "M2")
				)
			)
			(symbol "VMM5320BJG_3_1"
				(pin no_connect line
					(at 24.13 0 180)
					(length 3.81)
					(name "NC")
					(number "A12")
				)
				(pin power_in line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "B6")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "B8")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "B9")
				)
				(pin no_connect line
					(at 24.13 -1.27 180)
					(length 3.81)
					(name "NC")
					(number "B12")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "C2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "C4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "C5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD33A")
					(number "C6")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "C7")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "C8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "C9")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD33A")
					(number "C10")
				)
				(pin no_connect line
					(at 24.13 -3.81 180)
					(length 3.81)
					(name "NC")
					(number "C11")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "C12")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "D2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD33A")
					(number "D4")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "D5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "D6")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "D7")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "D8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "D9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "D10")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "D11")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "D12")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "E2")
				)
				(pin no_connect line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "NC")
					(number "E3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "E4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "E5")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "E6")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "E9")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "E10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "E11")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD33A")
					(number "E12")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "E13")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F2")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDRx")
					(number "F4")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F6")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F9")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F10")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "F12")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "F13")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "G2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDRx")
					(number "G4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "G5")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "G6")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "G7")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "G9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "G10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "G11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "G12")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "H2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDRx")
					(number "H4")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "H5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "H6")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "H7")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "H8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "H9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "H10")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "H11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "H12")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "H13")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "J3")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD33A")
					(number "J4")
				)
				(pin no_connect line
					(at 24.13 -6.35 180)
					(length 3.81)
					(name "NC")
					(number "J5")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "J6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "J7")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDTx")
					(number "J8")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD33A")
					(number "J9")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "J10")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "J11")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD33A")
					(number "J12")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "K3")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD33")
					(number "K4")
				)
				(pin no_connect line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "NC")
					(number "K9")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "K10")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "L7")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "L8")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "L9")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "L10")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "L12")
				)
			)
			(embedded_fonts no)
		)
)
