(footprint "QFN-68-1EP_8x8mm_P0.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-68-1EP_8x8mm_P0.4mm"
		(at 0 5.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4.425 7.2 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.425 8.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.425 9.6 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.7 -1.7)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.7 0)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.7 1.7)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.7)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.7)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.7 -1.7)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.7 0)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.7 1.7)
		(size 1.5 1.5)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -3.95 -3.202 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -3.95 -2.801 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -3.95 -2.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -3.95 -2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -3.95 -1.601 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -3.95 -1.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -3.95 -0.802 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -3.95 -0.402 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -3.95 0 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -3.95 0.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -3.95 0.8 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -3.95 1.199 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -3.95 1.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at -3.95 1.999 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -3.95 2.398 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -3.95 2.798 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at -3.95 3.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at -3.202 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at -2.801 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at -2.4 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at -2 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at -1.601 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at -1.2 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at -0.802 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at -0.402 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 0 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 0.4 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 0.8 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 1.199 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 1.6 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 1.999 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 2.398 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 2.798 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 3.2 3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 3.95 3.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 3.95 2.798 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 3.95 2.398 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 3.95 1.999 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 3.95 1.6 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 3.95 1.199 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 3.95 0.8 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 3.95 0.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at 3.95 0 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at 3.95 -0.402 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at 3.95 -0.802 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at 3.95 -1.2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at 3.95 -1.601 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at 3.95 -2 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd oval
		(at 3.95 -2.4 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd oval
		(at 3.95 -2.801 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd oval
		(at 3.95 -3.202 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd oval
		(at 3.2 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd oval
		(at 2.798 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd oval
		(at 2.398 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd oval
		(at 1.999 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd oval
		(at 1.6 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd oval
		(at 1.199 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd oval
		(at 0.8 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd oval
		(at 0.4 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd oval
		(at 0 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd oval
		(at -0.402 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd oval
		(at -0.802 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd oval
		(at -1.2 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd oval
		(at -1.601 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd oval
		(at -2 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd oval
		(at -2.4 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd oval
		(at -2.801 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd oval
		(at -3.202 -3.95)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 0 0)
		(size 5.2 5.2)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_vsc8541xmvrt_hp.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
