(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "VSC8662XIC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 68.58 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "VSC8662XIC"
				(at 68.58 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "VSC8662XIC"
				(at 68.58 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/MCHP_S_A0008366719_1-2513824.pdf"
				(at 68.58 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "VSC8662 Series 1.25 Gbps Dual Port 10/100/1000 BASE-T & 100/1000BX PHY - BGA-256"
				(at 68.58 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "VSC8662XIC"
				(at 68.58 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 68.58 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 68.58 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 68.58 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, PHY, ETHERNET"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "VSC8662XIC_1_1"
				(pin no_connect line
					(at 3.81 -114.3 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A1")
				)
				(pin no_connect line
					(at 3.81 -116.84 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin no_connect line
					(at 3.81 -119.38 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A3")
				)
				(pin no_connect line
					(at 3.81 -121.92 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A4")
				)
				(pin no_connect line
					(at 3.81 -124.46 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A5")
				)
				(pin no_connect line
					(at 3.81 -127 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A6")
				)
				(pin no_connect line
					(at 3.81 -129.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A7")
				)
				(pin no_connect line
					(at 3.81 -132.08 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A8")
				)
				(pin no_connect line
					(at 3.81 -134.62 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A9")
				)
				(pin bidirectional line
					(at 53.34 -88.9 180)
					(length 3.81)
					(name "TXVPA_1")
					(number "A10")
				)
				(pin bidirectional line
					(at 53.34 -99.06 180)
					(length 3.81)
					(name "TXVPB_1")
					(number "A11")
				)
				(pin bidirectional line
					(at 53.34 -109.22 180)
					(length 3.81)
					(name "TXVPC_1")
					(number "A12")
				)
				(pin bidirectional line
					(at 53.34 -119.38 180)
					(length 3.81)
					(name "TXVPD_1")
					(number "A13")
				)
				(pin bidirectional line
					(at 53.34 -91.44 180)
					(length 3.81)
					(name "TXVPA_0")
					(number "A14")
				)
				(pin bidirectional line
					(at 53.34 -101.6 180)
					(length 3.81)
					(name "TXVPB_0")
					(number "A15")
				)
				(pin no_connect line
					(at 3.81 -137.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A16")
				)
				(pin power_in line
					(at 0 -187.96 0)
					(length 3.81)
					(name "VSS")
					(number "B1")
				)
				(pin no_connect line
					(at 3.81 -144.78 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B2")
				)
				(pin no_connect line
					(at 3.81 -147.32 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B3")
				)
				(pin no_connect line
					(at 3.81 -149.86 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B4")
				)
				(pin no_connect line
					(at 3.81 -152.4 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B5")
				)
				(pin no_connect line
					(at 3.81 -154.94 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B6")
				)
				(pin no_connect line
					(at 3.81 -157.48 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B7")
				)
				(pin no_connect line
					(at 3.81 -160.02 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B8")
				)
				(pin no_connect line
					(at 3.81 -139.7 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B9")
				)
				(pin bidirectional line
					(at 53.34 -93.98 180)
					(length 3.81)
					(name "TXVNA_1")
					(number "B10")
				)
				(pin bidirectional line
					(at 53.34 -104.14 180)
					(length 3.81)
					(name "TXVNB_1")
					(number "B11")
				)
				(pin bidirectional line
					(at 53.34 -114.3 180)
					(length 3.81)
					(name "TXVNC_1")
					(number "B12")
				)
				(pin bidirectional line
					(at 53.34 -124.46 180)
					(length 3.81)
					(name "TXVND_1")
					(number "B13")
				)
				(pin bidirectional line
					(at 53.34 -96.52 180)
					(length 3.81)
					(name "TXVNA_0")
					(number "B14")
				)
				(pin bidirectional line
					(at 53.34 -106.68 180)
					(length 3.81)
					(name "TXVNB_0")
					(number "B15")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B16")
				)
				(pin output line
					(at 0 -93.98 0)
					(length 3.81)
					(name "XTAL2")
					(number "C1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "C2")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "C4")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "C6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "C7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "C8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "C9")
				)
				(pin no_connect line
					(at 3.81 -142.24 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD33")
					(number "C11")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD12A")
					(number "C13")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "C14")
				)
				(pin bidirectional line
					(at 53.34 -116.84 180)
					(length 3.81)
					(name "TXVNC_0")
					(number "C15")
				)
				(pin bidirectional line
					(at 53.34 -111.76 180)
					(length 3.81)
					(name "TXVPC_0")
					(number "C16")
				)
				(pin input line
					(at 0 -91.44 0)
					(length 3.81)
					(name "XTAL1/REFCLK")
					(number "D1")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 3.81)
					(name "OSCEN")
					(number "D2")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "REF_FILT")
					(number "D3")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "REF_REXT")
					(number "D4")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D11")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D12")
				)
				(pin no_connect line
					(at 3.81 -162.56 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D13")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "CMODE5")
					(number "D14")
				)
				(pin bidirectional line
					(at 53.34 -127 180)
					(length 3.81)
					(name "TXVND_0")
					(number "D15")
				)
				(pin bidirectional line
					(at 53.34 -121.92 180)
					(length 3.81)
					(name "TXVPD_0")
					(number "D16")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PLLMODE")
					(number "E1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "TMS")
					(number "E2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "NTRST")
					(number "E3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "E4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "E5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E11")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDD12")
					(number "E12")
				)
				(pin no_connect line
					(at 3.81 -165.1 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E13")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "CMODE4")
					(number "E14")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "CMODE6")
					(number "E15")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 3.81)
					(name "CMODE7")
					(number "E16")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TDO")
					(number "F1")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "TDI")
					(number "F2")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "TCK")
					(number "F3")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "F5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "F12")
				)
				(pin no_connect line
					(at 3.81 -167.64 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F13")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "CMODE2")
					(number "F14")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "CMODE3")
					(number "F15")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 3.81)
					(name "RCVRD_CLK1")
					(number "F16")
				)
				(pin output line
					(at 0 -68.58 0)
					(length 3.81)
					(name "LED0_0")
					(number "G1")
				)
				(pin output line
					(at 0 -66.04 0)
					(length 3.81)
					(name "LED1_0")
					(number "G2")
				)
				(pin output line
					(at 0 -63.5 0)
					(length 3.81)
					(name "LED2_0")
					(number "G3")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 3.81)
					(name "LED3_0")
					(number "G4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "G5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "G12")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "CMODE0")
					(number "G13")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "CMODE1")
					(number "G14")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "CLKOUT")
					(number "G15")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 3.81)
					(name "RCVRD_CLK2")
					(number "G16")
				)
				(pin output line
					(at 0 -58.42 0)
					(length 3.81)
					(name "LED0_1")
					(number "H1")
				)
				(pin output line
					(at 0 -55.88 0)
					(length 3.81)
					(name "LED1_1")
					(number "H2")
				)
				(pin output line
					(at 0 -53.34 0)
					(length 3.81)
					(name "LED2_1")
					(number "H3")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 3.81)
					(name "LED3_1")
					(number "H4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "H5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "H12")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "H13")
				)
				(pin bidirectional line
					(at 53.34 -33.02 180)
					(length 3.81)
					(name "GPIO13")
					(number "H14")
				)
				(pin input line
					(at 0 -88.9 0)
					(length 3.81)
					(name "THERMDC")
					(number "H15")
				)
				(pin input line
					(at 0 -86.36 0)
					(length 3.81)
					(name "THERMDA")
					(number "H16")
				)
				(pin no_connect line
					(at 49.53 -144.78 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J1")
				)
				(pin no_connect line
					(at 49.53 -147.32 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J2")
				)
				(pin no_connect line
					(at 49.53 -149.86 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J3")
				)
				(pin no_connect line
					(at 49.53 -152.4 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "J5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "J12")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J13")
				)
				(pin bidirectional line
					(at 53.34 -30.48 180)
					(length 3.81)
					(name "GPIO12")
					(number "J14")
				)
				(pin bidirectional line
					(at 53.34 -35.56 180)
					(length 3.81)
					(name "GPIO14")
					(number "J15")
				)
				(pin bidirectional line
					(at 53.34 -38.1 180)
					(length 3.81)
					(name "GPIO15")
					(number "J16")
				)
				(pin no_connect line
					(at 49.53 -129.54 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K1")
				)
				(pin no_connect line
					(at 49.53 -132.08 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K2")
				)
				(pin no_connect line
					(at 49.53 -134.62 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K3")
				)
				(pin no_connect line
					(at 49.53 -137.16 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "K5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "K12")
				)
				(pin bidirectional line
					(at 53.34 -20.32 180)
					(length 3.81)
					(name "GPIO8/I2C_SDA")
					(number "K13")
				)
				(pin bidirectional line
					(at 53.34 -22.86 180)
					(length 3.81)
					(name "GPIO9/FASTLINKFAIL")
					(number "K14")
				)
				(pin bidirectional line
					(at 53.34 -25.4 180)
					(length 3.81)
					(name "GPIO10")
					(number "K15")
				)
				(pin bidirectional line
					(at 53.34 -27.94 180)
					(length 3.81)
					(name "GPIO11")
					(number "K16")
				)
				(pin no_connect line
					(at 49.53 -139.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L1")
				)
				(pin no_connect line
					(at 49.53 -142.24 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L2")
				)
				(pin input line
					(at 0 -111.76 0)
					(length 3.81)
					(name "NSRESET")
					(number "L3")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "L5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "L12")
				)
				(pin bidirectional line
					(at 53.34 -10.16 180)
					(length 3.81)
					(name "GPIO4/I2C_SCL_0")
					(number "L13")
				)
				(pin bidirectional line
					(at 53.34 -12.7 180)
					(length 3.81)
					(name "GPIO5/I2C_SCL_1")
					(number "L14")
				)
				(pin bidirectional line
					(at 53.34 -15.24 180)
					(length 3.81)
					(name "GPIO6")
					(number "L15")
				)
				(pin bidirectional line
					(at 53.34 -17.78 180)
					(length 3.81)
					(name "GPIO7")
					(number "L16")
				)
				(pin no_connect line
					(at 49.53 -160.02 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M1")
				)
				(pin output line
					(at 0 -106.68 0)
					(length 3.81)
					(name "MDINT0")
					(number "M2")
				)
				(pin input line
					(at 0 -109.22 0)
					(length 3.81)
					(name "NRESET")
					(number "M3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDIO")
					(number "M4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "M5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "M12")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "M13")
				)
				(pin bidirectional line
					(at 53.34 -2.54 180)
					(length 3.81)
					(name "GPIO1/SIGDET1")
					(number "M14")
				)
				(pin bidirectional line
					(at 53.34 -5.08 180)
					(length 3.81)
					(name "GPIO2")
					(number "M15")
				)
				(pin bidirectional line
					(at 53.34 -7.62 180)
					(length 3.81)
					(name "GPIO3")
					(number "M16")
				)
				(pin no_connect line
					(at 49.53 -154.94 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N1")
				)
				(pin output line
					(at 0 -101.6 0)
					(length 3.81)
					(name "MDIO")
					(number "N2")
				)
				(pin output line
					(at 0 -104.14 0)
					(length 3.81)
					(name "MDINT1")
					(number "N3")
				)
				(pin no_connect line
					(at 49.53 -157.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "N5")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N6")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N7")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N9")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N10")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD12")
					(number "N12")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N13")
				)
				(pin bidirectional line
					(at 53.34 0 180)
					(length 3.81)
					(name "GPIO0/SIGDET0")
					(number "N14")
				)
				(pin output line
					(at 53.34 -55.88 180)
					(length 3.81)
					(name "TDP_0")
					(number "N15")
				)
				(pin output line
					(at 53.34 -60.96 180)
					(length 3.81)
					(name "TDN_0")
					(number "N16")
				)
				(pin no_connect line
					(at 3.81 -182.88 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P1")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 3.81)
					(name "MDC")
					(number "P2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "P3")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "P4")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "P5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "P6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "P7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "P8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "P9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "P10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD12A")
					(number "P11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "P12")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "P13")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "P14")
				)
				(pin input line
					(at 53.34 -45.72 180)
					(length 3.81)
					(name "RDP_0")
					(number "P15")
				)
				(pin input line
					(at 53.34 -50.8 180)
					(length 3.81)
					(name "RDN_0")
					(number "P16")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "R1")
				)
				(pin no_connect line
					(at 49.53 -162.56 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R2")
				)
				(pin no_connect line
					(at 49.53 -165.1 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R3")
				)
				(pin no_connect line
					(at 49.53 -167.64 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R4")
				)
				(pin no_connect line
					(at 49.53 -170.18 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R5")
				)
				(pin no_connect line
					(at 49.53 -172.72 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R6")
				)
				(pin no_connect line
					(at 49.53 -175.26 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R7")
				)
				(pin no_connect line
					(at 49.53 -177.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R8")
				)
				(pin no_connect line
					(at 49.53 -180.34 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R9")
				)
				(pin output line
					(at 53.34 -76.2 180)
					(length 3.81)
					(name "FIBR_DOP_1")
					(number "R10")
				)
				(pin input line
					(at 53.34 -66.04 180)
					(length 3.81)
					(name "FIBR_DIP_1")
					(number "R11")
				)
				(pin input line
					(at 53.34 -43.18 180)
					(length 3.81)
					(name "RDP_1")
					(number "R12")
				)
				(pin output line
					(at 53.34 -53.34 180)
					(length 3.81)
					(name "TDP_1")
					(number "R13")
				)
				(pin output line
					(at 53.34 -78.74 180)
					(length 3.81)
					(name "FIBR_DOP_0")
					(number "R14")
				)
				(pin input line
					(at 53.34 -68.58 180)
					(length 3.81)
					(name "FIBR_DIP_0")
					(number "R15")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "R16")
				)
				(pin no_connect line
					(at 49.53 -182.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T1")
				)
				(pin no_connect line
					(at 49.53 -185.42 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T2")
				)
				(pin no_connect line
					(at 49.53 -187.96 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T3")
				)
				(pin no_connect line
					(at 49.53 -190.5 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T4")
				)
				(pin no_connect line
					(at 3.81 -170.18 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T5")
				)
				(pin no_connect line
					(at 3.81 -172.72 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T6")
				)
				(pin no_connect line
					(at 3.81 -175.26 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T7")
				)
				(pin no_connect line
					(at 3.81 -177.8 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T8")
				)
				(pin no_connect line
					(at 3.81 -180.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T9")
				)
				(pin output line
					(at 53.34 -81.28 180)
					(length 3.81)
					(name "FIBR_DON_1")
					(number "T10")
				)
				(pin input line
					(at 53.34 -71.12 180)
					(length 3.81)
					(name "FIBR_DIN_1")
					(number "T11")
				)
				(pin input line
					(at 53.34 -48.26 180)
					(length 3.81)
					(name "RDN_1")
					(number "T12")
				)
				(pin output line
					(at 53.34 -58.42 180)
					(length 3.81)
					(name "TDN_1")
					(number "T13")
				)
				(pin output line
					(at 53.34 -83.82 180)
					(length 3.81)
					(name "FIBR_DON_0")
					(number "T14")
				)
				(pin input line
					(at 53.34 -73.66 180)
					(length 3.81)
					(name "FIBR_DIN_0")
					(number "T15")
				)
				(pin no_connect line
					(at 3.81 -185.42 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T16")
				)
			)
			(embedded_fonts no)
		)
)
