(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "W25Q128JWEIQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "W25Q128JWEIQ"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "W25Q128JWEIQ"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.winbond.com/resource-files/W25Q128JW_RevG_07292021%20Plus.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FLASH - NOR Memory IC 128Mbit SPI - Quad I/O, QPI 133 MHz 8-WSON (5x6)"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Winbond"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "W25Q128JWEIQ TR"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "W25Q128JWEIQ_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DO/IO1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{WP}/IO2")
					(number "3")
				)
				(pin power_in line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "V_{SS}")
					(number "4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "DI/IO0")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCK")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{HOLD}/IO3")
					(number "7")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "V_{CC}")
					(number "8")
				)
				(pin no_connect line
					(at 17.78 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
