(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "W25Q32JVXGIQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "W25Q32JVXGIQ"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "W25Q32JVXGIQ"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/949/w25q32jv_revg_03272018_plus-1489806.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Flash Memory, Serial NOR, 32 Mbit, 4M x 8bit, SPI, XSON, 8 Pins"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "W25Q32JVXGIQ"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Winbond"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "FLASH, SPI, MEMORY, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "W25Q32JVXGIQ_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SO")
					(number "2")
					(alternate "IO1" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{WP}")
					(number "3")
					(alternate "IO2" passive line)
				)
				(pin power_in line
					(at 19.05 -12.7 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "SI")
					(number "5")
					(alternate "IO0" passive line)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCLK")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{HOLD}")
					(number "7")
					(alternate "IO3" passive line)
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
