(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "W25Q80DV_USON"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "W25Q80DV_USON"
				(at 38.1 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "W25Q80DV_USON"
				(at 38.1 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/949/w25q80dv_dl_revh_10022015-1489677.pdf"
				(at 38.1 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FLASH - NOR Memory IC 8Mbit SPI - Quad I/O 104 MHz 8-USON (2x3)"
				(at 38.1 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "W25Q80DVUXIE TR"
				(at 38.1 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Winbond"
				(at 38.1 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, FLASH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "W25Q80DV_USON_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SO/IO1")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{WP}/IO2")
					(number "3")
				)
				(pin power_in line
					(at 19.05 -12.7 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "SI/IO0")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCLK")
					(number "6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{HOLD}/IO3")
					(number "7")
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 19.05 -10.16 180)
					(length 2.54)
					(name "EP")
					(number "EP")
				)
			)
			(embedded_fonts no)
		)
)
