(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "XC7K160T-FBG676"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 86.36 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "XC7K160T-FBG676"
				(at 86.36 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "XC7K160T-FBG676"
				(at 86.36 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.xilinx.com/v/u/en-US/ds180_7Series_Overview"
				(at 86.36 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Kintex®-7 Field Programmable Gate Array (FPGA) IC 300 4976640 65600 676-BBGA, FCBGA"
				(at 86.36 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "XC7K160T-FBG676"
				(at 86.36 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "AMD-Xilinx"
				(at 86.36 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 86.36 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 86.36 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, IC, FPGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "XC7K160T-FBG676_1_1"
				(text "BANK 12"
					(at 11.43 2.54 0)
				)
				(text "BANK 13"
					(at 33.02 2.54 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_12")
					(number "AA21")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_12")
					(number "AA22")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_12")
					(number "AA23")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_12")
					(number "AA24")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7P_T1_12")
					(number "AA25")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L18P_T2_12")
					(number "AB21")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L17P_T2_12")
					(number "AB22")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_12")
					(number "AB24")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7N_T1_12")
					(number "AB25")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9P_T1_DQS_12")
					(number "AB26")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L18N_T2_12")
					(number "AC21")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L17N_T2_12")
					(number "AC22")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_12")
					(number "AC23")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_12")
					(number "AC24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_12")
					(number "AC25")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9N_T1_DQS_12")
					(number "AC26")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L19P_T3_12")
					(number "AD21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_12")
					(number "AD22")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L16P_T2_12")
					(number "AD23")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L16N_T2_12")
					(number "AD24")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L23P_T3_12")
					(number "AD25")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L21P_T3_DQS_12")
					(number "AD26")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L19N_T3_VREF_12")
					(number "AE21")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L24P_T3_12")
					(number "AE22")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L22P_T3_12")
					(number "AE23")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L23N_T3_12")
					(number "AE25")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L21N_T3_DQS_12")
					(number "AE26")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L24N_T3_12")
					(number "AF22")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L22N_T3_12")
					(number "AF23")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L20P_T3_12")
					(number "AF24")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L20N_T3_12")
					(number "AF25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_12")
					(number "AF26")
				)
				(pin power_in line
					(at 54.61 0 180)
					(length 5.08)
					(name "VCCO_13")
					(number "K24")
				)
				(pin bidirectional line
					(at 54.61 -6.35 180)
					(length 5.08)
					(name "IO_L1P_T0_13")
					(number "K25")
				)
				(pin bidirectional line
					(at 54.61 -8.89 180)
					(length 5.08)
					(name "IO_L1N_T0_13")
					(number "K26")
				)
				(pin bidirectional line
					(at 54.61 -44.45 180)
					(length 5.08)
					(name "IO_L8N_T1_13")
					(number "L24")
				)
				(pin bidirectional line
					(at 54.61 -19.05 180)
					(length 5.08)
					(name "IO_L3N_T0_DQS_13")
					(number "L25")
				)
				(pin bidirectional line
					(at 54.61 -115.57 180)
					(length 5.08)
					(name "IO_L22N_T3_13")
					(number "M19")
				)
				(pin bidirectional line
					(at 54.61 -39.37 180)
					(length 5.08)
					(name "IO_L7N_T1_13")
					(number "M20")
				)
				(pin bidirectional line
					(at 54.61 -52.07 180)
					(length 5.08)
					(name "IO_L10P_T1_13")
					(number "M21")
				)
				(pin bidirectional line
					(at 54.61 -54.61 180)
					(length 5.08)
					(name "IO_L10N_T1_13")
					(number "M22")
				)
				(pin bidirectional line
					(at 54.61 -41.91 180)
					(length 5.08)
					(name "IO_L8P_T1_13")
					(number "M24")
				)
				(pin bidirectional line
					(at 54.61 -16.51 180)
					(length 5.08)
					(name "IO_L3P_T0_DQS_13")
					(number "M25")
				)
				(pin bidirectional line
					(at 54.61 -29.21 180)
					(length 5.08)
					(name "IO_L5N_T0_13")
					(number "M26")
				)
				(pin bidirectional line
					(at 54.61 -3.81 180)
					(length 5.08)
					(name "IO_0_13")
					(number "N16")
				)
				(pin bidirectional line
					(at 54.61 -105.41 180)
					(length 5.08)
					(name "IO_L20N_T3_13")
					(number "N17")
				)
				(pin bidirectional line
					(at 54.61 -113.03 180)
					(length 5.08)
					(name "IO_L22P_T3_13")
					(number "N18")
				)
				(pin bidirectional line
					(at 54.61 -36.83 180)
					(length 5.08)
					(name "IO_L7P_T1_13")
					(number "N19")
				)
				(pin bidirectional line
					(at 54.61 -62.23 180)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_13")
					(number "N21")
				)
				(pin bidirectional line
					(at 54.61 -64.77 180)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_13")
					(number "N22")
				)
				(pin bidirectional line
					(at 54.61 -59.69 180)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_13")
					(number "N23")
				)
				(pin bidirectional line
					(at 54.61 -24.13 180)
					(length 5.08)
					(name "IO_L4N_T0_13")
					(number "N24")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_13")
					(number "N25")
				)
				(pin bidirectional line
					(at 54.61 -26.67 180)
					(length 5.08)
					(name "IO_L5P_T0_13")
					(number "N26")
				)
				(pin bidirectional line
					(at 54.61 -102.87 180)
					(length 5.08)
					(name "IO_L20P_T3_13")
					(number "P16")
				)
				(pin bidirectional line
					(at 54.61 -125.73 180)
					(length 5.08)
					(name "IO_L24N_T3_13")
					(number "P18")
				)
				(pin bidirectional line
					(at 54.61 -46.99 180)
					(length 5.08)
					(name "IO_L9P_T1_DQS_13")
					(number "P19")
				)
				(pin bidirectional line
					(at 54.61 -49.53 180)
					(length 5.08)
					(name "IO_L9N_T1_DQS_13")
					(number "P20")
				)
				(pin bidirectional line
					(at 54.61 -69.85 180)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_13")
					(number "P21")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_13")
					(number "P22")
				)
				(pin bidirectional line
					(at 54.61 -57.15 180)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_13")
					(number "P23")
				)
				(pin bidirectional line
					(at 54.61 -21.59 180)
					(length 5.08)
					(name "IO_L4P_T0_13")
					(number "P24")
				)
				(pin bidirectional line
					(at 54.61 -34.29 180)
					(length 5.08)
					(name "IO_L6N_T0_VREF_13")
					(number "P25")
				)
				(pin bidirectional line
					(at 54.61 -13.97 180)
					(length 5.08)
					(name "IO_L2N_T0_13")
					(number "P26")
				)
				(pin bidirectional line
					(at 54.61 -107.95 180)
					(length 5.08)
					(name "IO_L21P_T3_DQS_13")
					(number "R16")
				)
				(pin bidirectional line
					(at 54.61 -110.49 180)
					(length 5.08)
					(name "IO_L21N_T3_DQS_13")
					(number "R17")
				)
				(pin bidirectional line
					(at 54.61 -123.19 180)
					(length 5.08)
					(name "IO_L24P_T3_13")
					(number "R18")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_13")
					(number "R19")
				)
				(pin bidirectional line
					(at 54.61 -85.09 180)
					(length 5.08)
					(name "IO_L16N_T2_13")
					(number "R20")
				)
				(pin bidirectional line
					(at 54.61 -67.31 180)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_13")
					(number "R21")
				)
				(pin bidirectional line
					(at 54.61 -72.39 180)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_13")
					(number "R22")
				)
				(pin bidirectional line
					(at 54.61 -74.93 180)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_13")
					(number "R23")
				)
				(pin bidirectional line
					(at 54.61 -31.75 180)
					(length 5.08)
					(name "IO_L6P_T0_13")
					(number "R25")
				)
				(pin bidirectional line
					(at 54.61 -11.43 180)
					(length 5.08)
					(name "IO_L2P_T0_13")
					(number "R26")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_13")
					(number "T16")
				)
				(pin bidirectional line
					(at 54.61 -120.65 180)
					(length 5.08)
					(name "IO_L23N_T3_13")
					(number "T17")
				)
				(pin bidirectional line
					(at 54.61 -97.79 180)
					(length 5.08)
					(name "IO_L19P_T3_13")
					(number "T18")
				)
				(pin bidirectional line
					(at 54.61 -100.33 180)
					(length 5.08)
					(name "IO_L19N_T3_VREF_13")
					(number "T19")
				)
				(pin bidirectional line
					(at 54.61 -82.55 180)
					(length 5.08)
					(name "IO_L16P_T2_13")
					(number "T20")
				)
				(pin bidirectional line
					(at 54.61 -87.63 180)
					(length 5.08)
					(name "IO_L17P_T2_13")
					(number "T22")
				)
				(pin bidirectional line
					(at 54.61 -90.17 180)
					(length 5.08)
					(name "IO_L17N_T2_13")
					(number "T23")
				)
				(pin bidirectional line
					(at 54.61 -77.47 180)
					(length 5.08)
					(name "IO_L15P_T2_DQS_13")
					(number "T24")
				)
				(pin bidirectional line
					(at 54.61 -80.01 180)
					(length 5.08)
					(name "IO_L15N_T2_DQS_13")
					(number "T25")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_13")
					(number "T26")
				)
				(pin bidirectional line
					(at 54.61 -128.27 180)
					(length 5.08)
					(name "IO_25_13")
					(number "U16")
				)
				(pin bidirectional line
					(at 54.61 -118.11 180)
					(length 5.08)
					(name "IO_L23P_T3_13")
					(number "U17")
				)
				(pin bidirectional line
					(at 54.61 -92.71 180)
					(length 5.08)
					(name "IO_L18P_T2_13")
					(number "U19")
				)
				(pin bidirectional line
					(at 54.61 -95.25 180)
					(length 5.08)
					(name "IO_L18N_T2_13")
					(number "U20")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_0_12")
					(number "U21")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1P_T0_12")
					(number "U22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_12")
					(number "U23")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2P_T0_12")
					(number "U24")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2N_T0_12")
					(number "U25")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4P_T0_12")
					(number "U26")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_12")
					(number "V20")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6P_T0_12")
					(number "V21")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1N_T0_12")
					(number "V22")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3P_T0_DQS_12")
					(number "V23")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3N_T0_DQS_12")
					(number "V24")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4N_T0_12")
					(number "V26")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L15P_T2_DQS_12")
					(number "W20")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6N_T0_VREF_12")
					(number "W21")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8P_T1_12")
					(number "W23")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8N_T1_12")
					(number "W24")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5P_T0_12")
					(number "W25")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5N_T0_12")
					(number "W26")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_25_12")
					(number "Y20")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L15N_T2_DQS_12")
					(number "Y21")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_12")
					(number "Y22")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_12")
					(number "Y23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_12")
					(number "Y24")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10P_T1_12")
					(number "Y25")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10N_T1_12")
					(number "Y26")
				)
			)
			(symbol "XC7K160T-FBG676_2_1"
				(text "BANK 14"
					(at 11.43 2.54 0)
				)
				(text "BANK 15"
					(at 48.26 2.54 0)
				)
				(pin bidirectional line
					(at 71.12 -19.05 180)
					(length 5.08)
					(name "IO_L3N_T0_DQS_AD1N_15")
					(number "A17")
				)
				(pin bidirectional line
					(at 71.12 -11.43 180)
					(length 5.08)
					(name "IO_L2P_T0_AD8P_15")
					(number "A18")
				)
				(pin bidirectional line
					(at 71.12 -13.97 180)
					(length 5.08)
					(name "IO_L2N_T0_AD8N_15")
					(number "A19")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8N_T1_D12_14")
					(number "A20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_14")
					(number "A21")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2N_T0_D03_14")
					(number "A22")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4P_T0_D04_14")
					(number "A23")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4N_T0_D05_14")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1N_T0_D01_DIN_14")
					(number "A25")
				)
				(pin bidirectional line
					(at 71.12 -8.89 180)
					(length 5.08)
					(name "IO_L1N_T0_AD0N_15")
					(number "B16")
				)
				(pin bidirectional line
					(at 71.12 -16.51 180)
					(length 5.08)
					(name "IO_L3P_T0_DQS_AD1P_15")
					(number "B17")
				)
				(pin power_in line
					(at 71.12 0 180)
					(length 5.08)
					(name "VCCO_15")
					(number "B18")
				)
				(pin bidirectional line
					(at 71.12 -24.13 180)
					(length 5.08)
					(name "IO_L4N_T0_AD9N_15")
					(number "B19")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8P_T1_D11_14")
					(number "B20")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10N_T1_D15_14")
					(number "B21")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2P_T0_D02_14")
					(number "B22")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1P_T0_D00_MOSI_14")
					(number "B24")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3P_T0_DQS_PUDC_B_14")
					(number "B25")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3N_T0_DQS_EMCCLK_14")
					(number "B26")
				)
				(pin bidirectional line
					(at 71.12 -6.35 180)
					(length 5.08)
					(name "IO_L1P_T0_AD0P_15")
					(number "C16")
				)
				(pin bidirectional line
					(at 71.12 -26.67 180)
					(length 5.08)
					(name "IO_L5P_T0_AD2P_15")
					(number "C17")
				)
				(pin bidirectional line
					(at 71.12 -29.21 180)
					(length 5.08)
					(name "IO_L5N_T0_AD2N_15")
					(number "C18")
				)
				(pin bidirectional line
					(at 71.12 -21.59 180)
					(length 5.08)
					(name "IO_L4P_T0_AD9P_15")
					(number "C19")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10P_T1_D14_14")
					(number "C21")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7N_T1_D10_14")
					(number "C22")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6P_T0_FCS_B_14")
					(number "C23")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6N_T0_D08_VREF_14")
					(number "C24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_14")
					(number "C25")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5N_T0_D07_14")
					(number "C26")
				)
				(pin bidirectional line
					(at 71.12 -31.75 180)
					(length 5.08)
					(name "IO_L6P_T0_15")
					(number "D15")
				)
				(pin bidirectional line
					(at 71.12 -34.29 180)
					(length 5.08)
					(name "IO_L6N_T0_VREF_15")
					(number "D16")
				)
				(pin bidirectional line
					(at 71.12 -69.85 180)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_15")
					(number "D18")
				)
				(pin bidirectional line
					(at 71.12 -77.47 180)
					(length 5.08)
					(name "IO_L15P_T2_DQS_15")
					(number "D19")
				)
				(pin bidirectional line
					(at 71.12 -80.01 180)
					(length 5.08)
					(name "IO_L15N_T2_DQS_ADV_B_15")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7P_T1_D09_14")
					(number "D21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_14")
					(number "D22")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_14")
					(number "D23")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_14")
					(number "D24")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
					(number "D25")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5P_T0_D06_14")
					(number "D26")
				)
				(pin bidirectional line
					(at 71.12 -52.07 180)
					(length 5.08)
					(name "IO_L10P_T1_AD4P_15")
					(number "E15")
				)
				(pin bidirectional line
					(at 71.12 -54.61 180)
					(length 5.08)
					(name "IO_L10N_T1_AD4N_15")
					(number "E16")
				)
				(pin bidirectional line
					(at 71.12 -64.77 180)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_AD5N_15")
					(number "E17")
				)
				(pin bidirectional line
					(at 71.12 -67.31 180)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_15")
					(number "E18")
				)
				(pin passive line
					(at 71.12 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_15")
					(number "E19")
				)
				(pin bidirectional line
					(at 71.12 -90.17 180)
					(length 5.08)
					(name "IO_L17N_T2_A25_15")
					(number "E20")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9P_T1_DQS_14")
					(number "E21")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9N_T1_DQS_D13_14")
					(number "E22")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_14")
					(number "E23")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L15P_T2_DQS_RDWR_B_14")
					(number "E25")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L17N_T2_A13_D29_14")
					(number "E26")
				)
				(pin bidirectional line
					(at 71.12 -44.45 180)
					(length 5.08)
					(name "IO_L8N_T1_AD3N_15")
					(number "F15")
				)
				(pin passive line
					(at 71.12 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_15")
					(number "F16")
				)
				(pin bidirectional line
					(at 71.12 -62.23 180)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_AD5P_15")
					(number "F17")
				)
				(pin bidirectional line
					(at 71.12 -59.69 180)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_AD12N_15")
					(number "F18")
				)
				(pin bidirectional line
					(at 71.12 -87.63 180)
					(length 5.08)
					(name "IO_L17P_T2_A26_15")
					(number "F19")
				)
				(pin bidirectional line
					(at 71.12 -85.09 180)
					(length 5.08)
					(name "IO_L16N_T2_A27_15")
					(number "F20")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_14")
					(number "F22")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_14")
					(number "F23")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_14")
					(number "F24")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L17P_T2_A14_D30_14")
					(number "F25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_14")
					(number "F26")
				)
				(pin bidirectional line
					(at 71.12 -41.91 180)
					(length 5.08)
					(name "IO_L8P_T1_AD3P_15")
					(number "G15")
				)
				(pin bidirectional line
					(at 71.12 -39.37 180)
					(length 5.08)
					(name "IO_L7N_T1_AD10N_15")
					(number "G16")
				)
				(pin bidirectional line
					(at 71.12 -57.15 180)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_AD12P_15")
					(number "G17")
				)
				(pin bidirectional line
					(at 71.12 -82.55 180)
					(length 5.08)
					(name "IO_L16P_T2_A28_15")
					(number "G19")
				)
				(pin bidirectional line
					(at 71.12 -95.25 180)
					(length 5.08)
					(name "IO_L18N_T2_A23_15")
					(number "G20")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L19N_T3_A09_D25_VREF_14")
					(number "G21")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_14")
					(number "G22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_14")
					(number "G23")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_14")
					(number "G24")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L16P_T2_CSI_B_14")
					(number "G25")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L16N_T2_A15_D31_14")
					(number "G26")
				)
				(pin bidirectional line
					(at 71.12 -36.83 180)
					(length 5.08)
					(name "IO_L7P_T1_AD10P_15")
					(number "H16")
				)
				(pin bidirectional line
					(at 71.12 -72.39 180)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_15")
					(number "H17")
				)
				(pin bidirectional line
					(at 71.12 -74.93 180)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_15")
					(number "H18")
				)
				(pin bidirectional line
					(at 71.12 -92.71 180)
					(length 5.08)
					(name "IO_L18P_T2_A24_15")
					(number "H19")
				)
				(pin passive line
					(at 71.12 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_15")
					(number "H20")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L19P_T3_A10_D26_14")
					(number "H21")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L21N_T3_DQS_A06_D22_14")
					(number "H22")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L20P_T3_A08_D24_14")
					(number "H23")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L20N_T3_A07_D23_14")
					(number "H24")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L18N_T2_A11_D27_14")
					(number "H26")
				)
				(pin bidirectional line
					(at 71.12 -46.99 180)
					(length 5.08)
					(name "IO_L9P_T1_DQS_AD11P_15")
					(number "J15")
				)
				(pin bidirectional line
					(at 71.12 -49.53 180)
					(length 5.08)
					(name "IO_L9N_T1_DQS_AD11N_15")
					(number "J16")
				)
				(pin passive line
					(at 71.12 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_15")
					(number "J17")
				)
				(pin bidirectional line
					(at 71.12 -102.87 180)
					(length 5.08)
					(name "IO_L20P_T3_A20_15")
					(number "J18")
				)
				(pin bidirectional line
					(at 71.12 -105.41 180)
					(length 5.08)
					(name "IO_L20N_T3_A19_15")
					(number "J19")
				)
				(pin bidirectional line
					(at 71.12 -100.33 180)
					(length 5.08)
					(name "IO_L19N_T3_A21_VREF_15")
					(number "J20")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L21P_T3_DQS_14")
					(number "J21")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L24N_T3_A00_D16_14")
					(number "J23")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L22P_T3_A05_D21_14")
					(number "J24")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L22N_T3_A04_D20_14")
					(number "J25")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L18P_T2_A12_D28_14")
					(number "J26")
				)
				(pin bidirectional line
					(at 71.12 -3.81 180)
					(length 5.08)
					(name "IO_0_15")
					(number "K15")
				)
				(pin bidirectional line
					(at 71.12 -113.03 180)
					(length 5.08)
					(name "IO_L22P_T3_A17_15")
					(number "K16")
				)
				(pin bidirectional line
					(at 71.12 -115.57 180)
					(length 5.08)
					(name "IO_L22N_T3_A16_15")
					(number "K17")
				)
				(pin bidirectional line
					(at 71.12 -125.73 180)
					(length 5.08)
					(name "IO_L24N_T3_RS0_15")
					(number "K18")
				)
				(pin bidirectional line
					(at 71.12 -97.79 180)
					(length 5.08)
					(name "IO_L19P_T3_A22_15")
					(number "K20")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_0_14")
					(number "K21")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L23N_T3_A02_D18_14")
					(number "K22")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L24P_T3_A01_D17_14")
					(number "K23")
				)
				(pin bidirectional line
					(at 71.12 -123.19 180)
					(length 5.08)
					(name "IO_L24P_T3_RS1_15")
					(number "L17")
				)
				(pin bidirectional line
					(at 71.12 -120.65 180)
					(length 5.08)
					(name "IO_L23N_T3_FWE_B_15")
					(number "L18")
				)
				(pin bidirectional line
					(at 71.12 -107.95 180)
					(length 5.08)
					(name "IO_L21P_T3_DQS_15")
					(number "L19")
				)
				(pin bidirectional line
					(at 71.12 -110.49 180)
					(length 5.08)
					(name "IO_L21N_T3_DQS_A18_15")
					(number "L20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_14")
					(number "L21")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L23P_T3_A03_D19_14")
					(number "L22")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_25_14")
					(number "L23")
				)
				(pin bidirectional line
					(at 71.12 -128.27 180)
					(length 5.08)
					(name "IO_25_15")
					(number "M16")
				)
				(pin bidirectional line
					(at 71.12 -118.11 180)
					(length 5.08)
					(name "IO_L23P_T3_FOE_B_15")
					(number "M17")
				)
				(pin passive line
					(at 71.12 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_15")
					(number "M18")
				)
			)
			(symbol "XC7K160T-FBG676_3_1"
				(text "BANK 16"
					(at 11.43 2.54 0)
				)
				(text "BANK 32"
					(at 31.75 2.54 0)
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9N_T1_DQS_16")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9P_T1_DQS_16")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L22N_T3_16")
					(number "A10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_16")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L24N_T3_16")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L24P_T3_16")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L21N_T3_DQS_16")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L23N_T3_16")
					(number "A15")
				)
				(pin bidirectional line
					(at 54.61 -36.83 180)
					(length 5.08)
					(name "IO_L7P_T1_32")
					(number "AA14")
				)
				(pin bidirectional line
					(at 54.61 -39.37 180)
					(length 5.08)
					(name "IO_L7N_T1_32")
					(number "AA15")
				)
				(pin bidirectional line
					(at 54.61 -57.15 180)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_32")
					(number "AA17")
				)
				(pin bidirectional line
					(at 54.61 -59.69 180)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_32")
					(number "AA18")
				)
				(pin bidirectional line
					(at 54.61 -82.55 180)
					(length 5.08)
					(name "IO_L16P_T2_32")
					(number "AA19")
				)
				(pin bidirectional line
					(at 54.61 -85.09 180)
					(length 5.08)
					(name "IO_L16N_T2_32")
					(number "AA20")
				)
				(pin bidirectional line
					(at 54.61 -52.07 180)
					(length 5.08)
					(name "IO_L10P_T1_32")
					(number "AB14")
				)
				(pin bidirectional line
					(at 54.61 -54.61 180)
					(length 5.08)
					(name "IO_L10N_T1_32")
					(number "AB15")
				)
				(pin bidirectional line
					(at 54.61 -62.23 180)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_32")
					(number "AB16")
				)
				(pin bidirectional line
					(at 54.61 -72.39 180)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_32")
					(number "AB17")
				)
				(pin power_in line
					(at 54.61 0 180)
					(length 5.08)
					(name "VCCO_32")
					(number "AB18")
				)
				(pin bidirectional line
					(at 54.61 -92.71 180)
					(length 5.08)
					(name "IO_L18P_T2_32")
					(number "AB19")
				)
				(pin bidirectional line
					(at 54.61 -95.25 180)
					(length 5.08)
					(name "IO_L18N_T2_32")
					(number "AB20")
				)
				(pin bidirectional line
					(at 54.61 -41.91 180)
					(length 5.08)
					(name "IO_L8P_T1_32")
					(number "AC14")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_32")
					(number "AC15")
				)
				(pin bidirectional line
					(at 54.61 -64.77 180)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_32")
					(number "AC16")
				)
				(pin bidirectional line
					(at 54.61 -74.93 180)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_32")
					(number "AC17")
				)
				(pin bidirectional line
					(at 54.61 -67.31 180)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_32")
					(number "AC18")
				)
				(pin bidirectional line
					(at 54.61 -87.63 180)
					(length 5.08)
					(name "IO_L17P_T2_32")
					(number "AC19")
				)
				(pin bidirectional line
					(at 54.61 -44.45 180)
					(length 5.08)
					(name "IO_L8N_T1_32")
					(number "AD14")
				)
				(pin bidirectional line
					(at 54.61 -21.59 180)
					(length 5.08)
					(name "IO_L4P_T0_32")
					(number "AD15")
				)
				(pin bidirectional line
					(at 54.61 -31.75 180)
					(length 5.08)
					(name "IO_L6P_T0_32")
					(number "AD16")
				)
				(pin bidirectional line
					(at 54.61 -69.85 180)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_32")
					(number "AD18")
				)
				(pin bidirectional line
					(at 54.61 -90.17 180)
					(length 5.08)
					(name "IO_L17N_T2_32")
					(number "AD19")
				)
				(pin bidirectional line
					(at 54.61 -77.47 180)
					(length 5.08)
					(name "IO_L15P_T2_DQS_32")
					(number "AD20")
				)
				(pin bidirectional line
					(at 54.61 -24.13 180)
					(length 5.08)
					(name "IO_L4N_T0_32")
					(number "AE15")
				)
				(pin bidirectional line
					(at 54.61 -34.29 180)
					(length 5.08)
					(name "IO_L6N_T0_VREF_32")
					(number "AE16")
				)
				(pin bidirectional line
					(at 54.61 -6.35 180)
					(length 5.08)
					(name "IO_L1P_T0_32")
					(number "AE17")
				)
				(pin bidirectional line
					(at 54.61 -16.51 180)
					(length 5.08)
					(name "IO_L3P_T0_DQS_32")
					(number "AE18")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_32")
					(number "AE19")
				)
				(pin bidirectional line
					(at 54.61 -80.01 180)
					(length 5.08)
					(name "IO_L15N_T2_DQS_32")
					(number "AE20")
				)
				(pin bidirectional line
					(at 54.61 -11.43 180)
					(length 5.08)
					(name "IO_L2P_T0_32")
					(number "AF14")
				)
				(pin bidirectional line
					(at 54.61 -13.97 180)
					(length 5.08)
					(name "IO_L2N_T0_32")
					(number "AF15")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_32")
					(number "AF16")
				)
				(pin bidirectional line
					(at 54.61 -8.89 180)
					(length 5.08)
					(name "IO_L1N_T0_32")
					(number "AF17")
				)
				(pin bidirectional line
					(at 54.61 -19.05 180)
					(length 5.08)
					(name "IO_L3N_T0_DQS_32")
					(number "AF18")
				)
				(pin bidirectional line
					(at 54.61 -26.67 180)
					(length 5.08)
					(name "IO_L5P_T0_32")
					(number "AF19")
				)
				(pin bidirectional line
					(at 54.61 -29.21 180)
					(length 5.08)
					(name "IO_L5N_T0_32")
					(number "AF20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_16")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10N_T1_16")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L22P_T3_16")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L20N_T3_16")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L20P_T3_16")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L21P_T3_DQS_16")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L23P_T3_16")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10P_T1_16")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_16")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_16")
					(number "C12")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L19N_T3_VREF_16")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L19P_T3_16")
					(number "C14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_16")
					(number "C15")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8N_T1_16")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8P_T1_16")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_16")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_16")
					(number "D11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_16")
					(number "D12")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L17N_T2_16")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L17P_T2_16")
					(number "D14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_16")
					(number "E9")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_16")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_16")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L18N_T2_16")
					(number "E12")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L18P_T2_16")
					(number "E13")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7N_T1_16")
					(number "F8")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7P_T1_16")
					(number "F9")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_16")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L16N_T2_16")
					(number "F12")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L15N_T2_DQS_16")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L15P_T2_DQS_16")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2N_T0_16")
					(number "G9")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2P_T0_16")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_16")
					(number "G11")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L16P_T2_16")
					(number "G12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_16")
					(number "G13")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5N_T0_16")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1N_T0_16")
					(number "H8")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1P_T0_16")
					(number "H9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_16")
					(number "H10")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6N_T0_VREF_16")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6P_T0_16")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3N_T0_DQS_16")
					(number "H13")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5P_T0_16")
					(number "H14")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_0_16")
					(number "J8")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4N_T0_16")
					(number "J10")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4P_T0_16")
					(number "J11")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3P_T0_DQS_16")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_25_16")
					(number "J14")
				)
				(pin bidirectional line
					(at 54.61 -3.81 180)
					(length 5.08)
					(name "IO_0_VRN_32")
					(number "V13")
				)
				(pin bidirectional line
					(at 54.61 -123.19 180)
					(length 5.08)
					(name "IO_L24P_T3_32")
					(number "V14")
				)
				(pin bidirectional line
					(at 54.61 -102.87 180)
					(length 5.08)
					(name "IO_L20P_T3_32")
					(number "V16")
				)
				(pin bidirectional line
					(at 54.61 -105.41 180)
					(length 5.08)
					(name "IO_L20N_T3_32")
					(number "V17")
				)
				(pin bidirectional line
					(at 54.61 -118.11 180)
					(length 5.08)
					(name "IO_L23P_T3_32")
					(number "V18")
				)
				(pin bidirectional line
					(at 54.61 -120.65 180)
					(length 5.08)
					(name "IO_L23N_T3_32")
					(number "V19")
				)
				(pin bidirectional line
					(at 54.61 -128.27 180)
					(length 5.08)
					(name "IO_25_VRP_32")
					(number "W13")
				)
				(pin bidirectional line
					(at 54.61 -125.73 180)
					(length 5.08)
					(name "IO_L24N_T3_32")
					(number "W14")
				)
				(pin bidirectional line
					(at 54.61 -113.03 180)
					(length 5.08)
					(name "IO_L22P_T3_32")
					(number "W15")
				)
				(pin bidirectional line
					(at 54.61 -115.57 180)
					(length 5.08)
					(name "IO_L22N_T3_32")
					(number "W16")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_32")
					(number "W17")
				)
				(pin bidirectional line
					(at 54.61 -107.95 180)
					(length 5.08)
					(name "IO_L21P_T3_DQS_32")
					(number "W18")
				)
				(pin bidirectional line
					(at 54.61 -110.49 180)
					(length 5.08)
					(name "IO_L21N_T3_DQS_32")
					(number "W19")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_32")
					(number "Y14")
				)
				(pin bidirectional line
					(at 54.61 -46.99 180)
					(length 5.08)
					(name "IO_L9P_T1_DQS_32")
					(number "Y15")
				)
				(pin bidirectional line
					(at 54.61 -49.53 180)
					(length 5.08)
					(name "IO_L9N_T1_DQS_32")
					(number "Y16")
				)
				(pin bidirectional line
					(at 54.61 -97.79 180)
					(length 5.08)
					(name "IO_L19P_T3_32")
					(number "Y17")
				)
				(pin bidirectional line
					(at 54.61 -100.33 180)
					(length 5.08)
					(name "IO_L19N_T3_VREF_32")
					(number "Y18")
				)
			)
			(symbol "XC7K160T-FBG676_4_1"
				(text "BANK 33"
					(at 11.43 2.54 0)
				)
				(text "BANK 34"
					(at 31.75 2.54 0)
				)
				(pin power_in line
					(at 54.61 0 180)
					(length 5.08)
					(name "VCCO_34")
					(number "AA1")
				)
				(pin bidirectional line
					(at 54.61 -64.77 180)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_34")
					(number "AA2")
				)
				(pin bidirectional line
					(at 54.61 -62.23 180)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_34")
					(number "AA3")
				)
				(pin bidirectional line
					(at 54.61 -67.31 180)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_34")
					(number "AA4")
				)
				(pin bidirectional line
					(at 54.61 -77.47 180)
					(length 5.08)
					(name "IO_L15P_T2_DQS_34")
					(number "AA5")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8N_T1_33")
					(number "AA7")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8P_T1_33")
					(number "AA8")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_33")
					(number "AA9")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_33")
					(number "AA10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_33")
					(number "AA11")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L16N_T2_33")
					(number "AA12")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L16P_T2_33")
					(number "AA13")
				)
				(pin bidirectional line
					(at 54.61 -46.99 180)
					(length 5.08)
					(name "IO_L9P_T1_DQS_34")
					(number "AB1")
				)
				(pin bidirectional line
					(at 54.61 -57.15 180)
					(length 5.08)
					(name "IO_L11P_T1_SRCC_34")
					(number "AB2")
				)
				(pin bidirectional line
					(at 54.61 -69.85 180)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_34")
					(number "AB4")
				)
				(pin bidirectional line
					(at 54.61 -80.01 180)
					(length 5.08)
					(name "IO_L15N_T2_DQS_34")
					(number "AB5")
				)
				(pin bidirectional line
					(at 54.61 -82.55 180)
					(length 5.08)
					(name "IO_L16P_T2_34")
					(number "AB6")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10P_T1_33")
					(number "AB7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_33")
					(number "AB8")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_33")
					(number "AB9")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_33")
					(number "AB10")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13P_T2_MRCC_33")
					(number "AB11")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L15P_T2_DQS_33")
					(number "AB12")
				)
				(pin bidirectional line
					(at 54.61 -49.53 180)
					(length 5.08)
					(name "IO_L9N_T1_DQS_34")
					(number "AC1")
				)
				(pin bidirectional line
					(at 54.61 -59.69 180)
					(length 5.08)
					(name "IO_L11N_T1_SRCC_34")
					(number "AC2")
				)
				(pin bidirectional line
					(at 54.61 -74.93 180)
					(length 5.08)
					(name "IO_L14N_T2_SRCC_34")
					(number "AC3")
				)
				(pin bidirectional line
					(at 54.61 -72.39 180)
					(length 5.08)
					(name "IO_L14P_T2_SRCC_34")
					(number "AC4")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_34")
					(number "AC5")
				)
				(pin bidirectional line
					(at 54.61 -85.09 180)
					(length 5.08)
					(name "IO_L16N_T2_34")
					(number "AC6")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10N_T1_33")
					(number "AC7")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9P_T1_DQS_33")
					(number "AC8")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12P_T1_MRCC_33")
					(number "AC9")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13N_T2_MRCC_33")
					(number "AC11")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L15N_T2_DQS_33")
					(number "AC12")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L17P_T2_33")
					(number "AC13")
				)
				(pin bidirectional line
					(at 54.61 -102.87 180)
					(length 5.08)
					(name "IO_L20P_T3_34")
					(number "AD1")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_34")
					(number "AD2")
				)
				(pin bidirectional line
					(at 54.61 -100.33 180)
					(length 5.08)
					(name "IO_L19N_T3_VREF_34")
					(number "AD3")
				)
				(pin bidirectional line
					(at 54.61 -97.79 180)
					(length 5.08)
					(name "IO_L19P_T3_34")
					(number "AD4")
				)
				(pin bidirectional line
					(at 54.61 -95.25 180)
					(length 5.08)
					(name "IO_L18N_T2_34")
					(number "AD5")
				)
				(pin bidirectional line
					(at 54.61 -92.71 180)
					(length 5.08)
					(name "IO_L18P_T2_34")
					(number "AD6")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9N_T1_DQS_33")
					(number "AD8")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12N_T1_MRCC_33")
					(number "AD9")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L20P_T3_33")
					(number "AD10")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L19P_T3_33")
					(number "AD11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_33")
					(number "AD12")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L17N_T2_33")
					(number "AD13")
				)
				(pin bidirectional line
					(at 54.61 -105.41 180)
					(length 5.08)
					(name "IO_L20N_T3_34")
					(number "AE1")
				)
				(pin bidirectional line
					(at 54.61 -115.57 180)
					(length 5.08)
					(name "IO_L22N_T3_34")
					(number "AE2")
				)
				(pin bidirectional line
					(at 54.61 -113.03 180)
					(length 5.08)
					(name "IO_L22P_T3_34")
					(number "AE3")
				)
				(pin bidirectional line
					(at 54.61 -120.65 180)
					(length 5.08)
					(name "IO_L23N_T3_34")
					(number "AE5")
				)
				(pin bidirectional line
					(at 54.61 -118.11 180)
					(length 5.08)
					(name "IO_L23P_T3_34")
					(number "AE6")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7P_T1_33")
					(number "AE7")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L22P_T3_33")
					(number "AE8")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_33")
					(number "AE9")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L20N_T3_33")
					(number "AE10")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L19N_T3_VREF_33")
					(number "AE11")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L21P_T3_DQS_33")
					(number "AE12")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L23P_T3_33")
					(number "AE13")
				)
				(pin bidirectional line
					(at 54.61 -125.73 180)
					(length 5.08)
					(name "IO_L24N_T3_34")
					(number "AF2")
				)
				(pin bidirectional line
					(at 54.61 -123.19 180)
					(length 5.08)
					(name "IO_L24P_T3_34")
					(number "AF3")
				)
				(pin bidirectional line
					(at 54.61 -110.49 180)
					(length 5.08)
					(name "IO_L21N_T3_DQS_34")
					(number "AF4")
				)
				(pin bidirectional line
					(at 54.61 -107.95 180)
					(length 5.08)
					(name "IO_L21P_T3_DQS_34")
					(number "AF5")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_34")
					(number "AF6")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7N_T1_33")
					(number "AF7")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L22N_T3_33")
					(number "AF8")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L24N_T3_33")
					(number "AF9")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L24P_T3_33")
					(number "AF10")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L21N_T3_DQS_33")
					(number "AF12")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L23N_T3_33")
					(number "AF13")
				)
				(pin bidirectional line
					(at 54.61 -128.27 180)
					(length 5.08)
					(name "IO_25_VRP_34")
					(number "T7")
				)
				(pin bidirectional line
					(at 54.61 -13.97 180)
					(length 5.08)
					(name "IO_L2N_T0_34")
					(number "U1")
				)
				(pin bidirectional line
					(at 54.61 -11.43 180)
					(length 5.08)
					(name "IO_L2P_T0_34")
					(number "U2")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_34")
					(number "U3")
				)
				(pin bidirectional line
					(at 54.61 -3.81 180)
					(length 5.08)
					(name "IO_0_VRN_34")
					(number "U4")
				)
				(pin bidirectional line
					(at 54.61 -8.89 180)
					(length 5.08)
					(name "IO_L1N_T0_34")
					(number "U5")
				)
				(pin bidirectional line
					(at 54.61 -6.35 180)
					(length 5.08)
					(name "IO_L1P_T0_34")
					(number "U6")
				)
				(pin bidirectional line
					(at 54.61 -26.67 180)
					(length 5.08)
					(name "IO_L5P_T0_34")
					(number "U7")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_0_VRN_33")
					(number "U9")
				)
				(pin bidirectional line
					(at 54.61 -44.45 180)
					(length 5.08)
					(name "IO_L8N_T1_34")
					(number "V1")
				)
				(pin bidirectional line
					(at 54.61 -41.91 180)
					(length 5.08)
					(name "IO_L8P_T1_34")
					(number "V2")
				)
				(pin bidirectional line
					(at 54.61 -21.59 180)
					(length 5.08)
					(name "IO_L4P_T0_34")
					(number "V3")
				)
				(pin bidirectional line
					(at 54.61 -31.75 180)
					(length 5.08)
					(name "IO_L6P_T0_34")
					(number "V4")
				)
				(pin bidirectional line
					(at 54.61 -29.21 180)
					(length 5.08)
					(name "IO_L5N_T0_34")
					(number "V6")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2N_T0_33")
					(number "V7")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2P_T0_33")
					(number "V8")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6P_T0_33")
					(number "V9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_33")
					(number "V10")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1P_T0_33")
					(number "V11")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_25_VRP_33")
					(number "V12")
				)
				(pin bidirectional line
					(at 54.61 -52.07 180)
					(length 5.08)
					(name "IO_L10P_T1_34")
					(number "W1")
				)
				(pin bidirectional line
					(at 54.61 -24.13 180)
					(length 5.08)
					(name "IO_L4N_T0_34")
					(number "W3")
				)
				(pin bidirectional line
					(at 54.61 -34.29 180)
					(length 5.08)
					(name "IO_L6N_T0_VREF_34")
					(number "W4")
				)
				(pin bidirectional line
					(at 54.61 -19.05 180)
					(length 5.08)
					(name "IO_L3N_T0_DQS_34")
					(number "W5")
				)
				(pin bidirectional line
					(at 54.61 -16.51 180)
					(length 5.08)
					(name "IO_L3P_T0_DQS_34")
					(number "W6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_33")
					(number "W7")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6N_T0_VREF_33")
					(number "W8")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3N_T0_DQS_33")
					(number "W9")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3P_T0_DQS_33")
					(number "W10")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1N_T0_33")
					(number "W11")
				)
				(pin bidirectional line
					(at 54.61 -54.61 180)
					(length 5.08)
					(name "IO_L10N_T1_34")
					(number "Y1")
				)
				(pin bidirectional line
					(at 54.61 -39.37 180)
					(length 5.08)
					(name "IO_L7N_T1_34")
					(number "Y2")
				)
				(pin bidirectional line
					(at 54.61 -36.83 180)
					(length 5.08)
					(name "IO_L7P_T1_34")
					(number "Y3")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCO_34")
					(number "Y4")
				)
				(pin bidirectional line
					(at 54.61 -90.17 180)
					(length 5.08)
					(name "IO_L17N_T2_34")
					(number "Y5")
				)
				(pin bidirectional line
					(at 54.61 -87.63 180)
					(length 5.08)
					(name "IO_L17P_T2_34")
					(number "Y6")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4N_T0_33")
					(number "Y7")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4P_T0_33")
					(number "Y8")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5N_T0_33")
					(number "Y10")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5P_T0_33")
					(number "Y11")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L18N_T2_33")
					(number "Y12")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L18P_T2_33")
					(number "Y13")
				)
			)
			(symbol "XC7K160T-FBG676_5_1"
				(text "GTX 115"
					(at 11.43 2.54 0)
				)
				(text "GTX 116"
					(at 31.75 2.54 0)
				)
				(pin bidirectional line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "MGTXTXN3_116")
					(number "A3")
				)
				(pin bidirectional line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "MGTXTXP3_116")
					(number "A4")
				)
				(pin bidirectional line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "MGTXTXN2_116")
					(number "B1")
				)
				(pin bidirectional line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "MGTXTXP2_116")
					(number "B2")
				)
				(pin bidirectional line
					(at 48.26 -39.37 180)
					(length 5.08)
					(name "MGTXRXN3_116")
					(number "B5")
				)
				(pin bidirectional line
					(at 48.26 -36.83 180)
					(length 5.08)
					(name "MGTXRXP3_116")
					(number "B6")
				)
				(pin bidirectional line
					(at 48.26 -34.29 180)
					(length 5.08)
					(name "MGTXRXN2_116")
					(number "C3")
				)
				(pin bidirectional line
					(at 48.26 -31.75 180)
					(length 5.08)
					(name "MGTXRXP2_116")
					(number "C4")
				)
				(pin bidirectional line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "MGTXTXN1_116")
					(number "D1")
				)
				(pin bidirectional line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "MGTXTXP1_116")
					(number "D2")
				)
				(pin bidirectional line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "MGTREFCLK0N_116")
					(number "D5")
				)
				(pin bidirectional line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "MGTREFCLK0P_116")
					(number "D6")
				)
				(pin bidirectional line
					(at 48.26 -29.21 180)
					(length 5.08)
					(name "MGTXRXN1_116")
					(number "E3")
				)
				(pin bidirectional line
					(at 48.26 -26.67 180)
					(length 5.08)
					(name "MGTXRXP1_116")
					(number "E4")
				)
				(pin bidirectional line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "MGTXTXN0_116")
					(number "F1")
				)
				(pin bidirectional line
					(at 48.26 0 180)
					(length 5.08)
					(name "MGTXTXP0_116")
					(number "F2")
				)
				(pin bidirectional line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "MGTREFCLK1N_116")
					(number "F5")
				)
				(pin bidirectional line
					(at 48.26 -48.26 180)
					(length 5.08)
					(name "MGTREFCLK1P_116")
					(number "F6")
				)
				(pin bidirectional line
					(at 48.26 -24.13 180)
					(length 5.08)
					(name "MGTXRXN0_116")
					(number "G3")
				)
				(pin bidirectional line
					(at 48.26 -21.59 180)
					(length 5.08)
					(name "MGTXRXP0_116")
					(number "G4")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTXTXN3_115")
					(number "H1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTXTXP3_115")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTREFCLK0N_115")
					(number "H5")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTREFCLK0P_115")
					(number "H6")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "MGTXRXN3_115")
					(number "J3")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "MGTXRXP3_115")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTXTXN2_115")
					(number "K1")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTXTXP2_115")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "MGTREFCLK1N_115")
					(number "K5")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTREFCLK1P_115")
					(number "K6")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "MGTXRXN2_115")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "MGTXRXP2_115")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTXTXN1_115")
					(number "M1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTXTXP1_115")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "MGTXRXN1_115")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "MGTXRXP1_115")
					(number "N4")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTXTXN0_115")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MGTXTXP0_115")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "MGTXRXN0_115")
					(number "R3")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "MGTXRXP0_115")
					(number "R4")
				)
			)
			(symbol "XC7K160T-FBG676_6_1"
				(pin power_in line
					(at 39.37 -16.51 180)
					(length 5.08)
					(name "GND")
					(number "A1")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A6")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A7")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A16")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A26")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA6")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA16")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA26")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB13")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB23")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC10")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC20")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD7")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD17")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE4")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE14")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE24")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF1")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF11")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF21")
				)
				(pin power_in line
					(at 39.37 -5.08 180)
					(length 5.08)
					(name "MGTAVTT")
					(number "B3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B23")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C1")
				)
				(pin passive line
					(at 39.37 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT")
					(number "C2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at 39.37 0 180)
					(length 5.08)
					(name "MGTAVCC")
					(number "C6")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C7")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C10")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C20")
				)
				(pin passive line
					(at 39.37 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT")
					(number "D3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D7")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D17")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 39.37 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC")
					(number "E6")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VCCBATT_0")
					(number "E8")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E14")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E24")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F21")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 39.37 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT")
					(number "G2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 39.37 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC")
					(number "G6")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G18")
				)
				(pin passive line
					(at 39.37 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT")
					(number "H3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H4")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H7")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H25")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J1")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 39.37 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC")
					(number "J6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCINT")
					(number "J9")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J12")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J22")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K4")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K8")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K10")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K12")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K14")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K19")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L1")
				)
				(pin passive line
					(at 39.37 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT")
					(number "L2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L5")
				)
				(pin passive line
					(at 39.37 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC")
					(number "L6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L9")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCCAUX")
					(number "L11")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L13")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L16")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L26")
				)
				(pin passive line
					(at 39.37 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT")
					(number "M3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at 39.37 -7.62 180)
					(length 5.08)
					(name "MGTAVTTRCAL_115")
					(number "M5")
				)
				(pin power_in line
					(at 39.37 -10.16 180)
					(length 5.08)
					(name "MGTRREF_115")
					(number "M6")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M8")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "M10")
				)
				(pin power_in line
					(at 39.37 -13.97 180)
					(length 5.08)
					(name "GNDADC_0")
					(number "M11")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VCCADC_0")
					(number "M12")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M14")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M23")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N1")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at 39.37 -2.54 180)
					(length 5.08)
					(name "MGTVCCAUX")
					(number "N6")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N9")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "VCCBRAM")
					(number "N13")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N20")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P4")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VCCAUX_IO_G0")
					(number "P8")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "P10")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P14")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P17")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R1")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R5")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO_G0")
					(number "R9")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "R13")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "R15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R24")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T1")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T3")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO_G0")
					(number "T8")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "T10")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T11")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "T12")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T14")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T21")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U8")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "U11")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U12")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "U13")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U18")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V15")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V25")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W2")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W12")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W22")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y9")
				)
				(pin passive line
					(at 39.37 -16.51 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y19")
				)
			)
			(symbol "XC7K160T-FBG676_7_1"
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "CCLK_0")
					(number "C8")
				)
				(pin bidirectional line
					(at 35.56 -21.59 180)
					(length 5.08)
					(name "INIT_B_0")
					(number "G7")
				)
				(pin bidirectional line
					(at 35.56 -19.05 180)
					(length 5.08)
					(name "DONE_0")
					(number "J7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_0")
					(number "L7")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "TCK_0")
					(number "L8")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "TMS_0")
					(number "N8")
				)
				(pin bidirectional line
					(at 35.56 -8.89 180)
					(length 5.08)
					(name "VREFN_0")
					(number "N11")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 5.08)
					(name "VP_0")
					(number "N12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "M2_0")
					(number "P5")
				)
				(pin bidirectional line
					(at 35.56 -24.13 180)
					(length 5.08)
					(name "PROGRAM_B_0")
					(number "P6")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "CFGBVS_0")
					(number "P7")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VN_0")
					(number "P11")
				)
				(pin bidirectional line
					(at 35.56 -6.35 180)
					(length 5.08)
					(name "VREFP_0")
					(number "P12")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "TDI_0")
					(number "R6")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "TDO_0")
					(number "R7")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "DXN_0")
					(number "R11")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXP_0")
					(number "R12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "M1_0")
					(number "T2")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "M0_0")
					(number "T5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_0")
					(number "T6")
				)
			)
			(embedded_fonts no)
		)
)
