(footprint "BGA-900_31x31mm_Layout30x30_P1x1mm_FFG900"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -16.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-900_31x31mm_Layout30x30_P1x1mm_FFG900"
		(at 0 17.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -16.5 19.635 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -16.5 20.835 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -16.5 22.035 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -14.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A2" smd circle
		(at -13.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A3" smd circle
		(at -12.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.432)
		(solder_mask_margin 0.02)
	)
	(pad "A4" smd circle
		(at -11.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.414)
		(solder_mask_margin 0.02)
	)
	(pad "A5" smd circle
		(at -10.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A6" smd circle
		(at -9.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A7" smd circle
		(at -8.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.951)
		(solder_mask_margin 0.02)
	)
	(pad "A8" smd circle
		(at -7.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.93)
		(solder_mask_margin 0.02)
	)
	(pad "A9" smd circle
		(at -6.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A10" smd circle
		(at -5.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 30.087)
		(solder_mask_margin 0.02)
	)
	(pad "A11" smd circle
		(at -4.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 26.57)
		(solder_mask_margin 0.02)
	)
	(pad "A12" smd circle
		(at -3.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.299)
		(solder_mask_margin 0.02)
	)
	(pad "A13" smd circle
		(at -2.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.219)
		(solder_mask_margin 0.02)
	)
	(pad "A14" smd circle
		(at -1.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A15" smd circle
		(at -0.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.216)
		(solder_mask_margin 0.02)
	)
	(pad "A16" smd circle
		(at 0.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 26.083)
		(solder_mask_margin 0.02)
	)
	(pad "A17" smd circle
		(at 1.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.395)
		(solder_mask_margin 0.02)
	)
	(pad "A18" smd circle
		(at 2.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.265)
		(solder_mask_margin 0.02)
	)
	(pad "A19" smd circle
		(at 3.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A20" smd circle
		(at 4.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.453)
		(solder_mask_margin 0.02)
	)
	(pad "A21" smd circle
		(at 5.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.28)
		(solder_mask_margin 0.02)
	)
	(pad "A22" smd circle
		(at 6.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.922)
		(solder_mask_margin 0.02)
	)
	(pad "A23" smd circle
		(at 7.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.02)
		(solder_mask_margin 0.02)
	)
	(pad "A24" smd circle
		(at 8.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A25" smd circle
		(at 9.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.09)
		(solder_mask_margin 0.02)
	)
	(pad "A26" smd circle
		(at 10.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.986)
		(solder_mask_margin 0.02)
	)
	(pad "A27" smd circle
		(at 11.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.513)
		(solder_mask_margin 0.02)
	)
	(pad "A28" smd circle
		(at 12.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.234)
		(solder_mask_margin 0.02)
	)
	(pad "A29" smd circle
		(at 13.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "A30" smd circle
		(at 14.5 -14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.871)
		(solder_mask_margin 0.02)
	)
	(pad "AA1" smd circle
		(at -14.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA2" smd circle
		(at -13.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA3" smd circle
		(at -12.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.779)
		(solder_mask_margin 0.02)
	)
	(pad "AA4" smd circle
		(at -11.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.802)
		(solder_mask_margin 0.02)
	)
	(pad "AA5" smd circle
		(at -10.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA6" smd circle
		(at -9.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA7" smd circle
		(at -8.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA8" smd circle
		(at -7.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.905)
		(solder_mask_margin 0.02)
	)
	(pad "AA9" smd circle
		(at -6.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA10" smd circle
		(at -5.5 5.5 90)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.194)
		(solder_mask_margin 0.02)
	)
	(pad "AA11" smd circle
		(at -4.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.33)
		(solder_mask_margin 0.02)
	)
	(pad "AA12" smd circle
		(at -3.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.782)
		(solder_mask_margin 0.02)
	)
	(pad "AA13" smd circle
		(at -2.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.996)
		(solder_mask_margin 0.02)
	)
	(pad "AA14" smd circle
		(at -1.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA15" smd circle
		(at -0.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.195)
		(solder_mask_margin 0.02)
	)
	(pad "AA16" smd circle
		(at 0.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.54)
		(solder_mask_margin 0.02)
	)
	(pad "AA17" smd circle
		(at 1.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.445)
		(solder_mask_margin 0.02)
	)
	(pad "AA18" smd circle
		(at 2.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.589)
		(solder_mask_margin 0.02)
	)
	(pad "AA19" smd circle
		(at 3.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA20" smd circle
		(at 4.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.201)
		(solder_mask_margin 0.02)
	)
	(pad "AA21" smd circle
		(at 5.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.235)
		(solder_mask_margin 0.02)
	)
	(pad "AA22" smd circle
		(at 6.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.789)
		(solder_mask_margin 0.02)
	)
	(pad "AA23" smd circle
		(at 7.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.88)
		(solder_mask_margin 0.02)
	)
	(pad "AA24" smd circle
		(at 8.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA25" smd circle
		(at 9.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.199)
		(solder_mask_margin 0.02)
	)
	(pad "AA26" smd circle
		(at 10.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.222)
		(solder_mask_margin 0.02)
	)
	(pad "AA27" smd circle
		(at 11.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.889)
		(solder_mask_margin 0.02)
	)
	(pad "AA28" smd circle
		(at 12.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.752)
		(solder_mask_margin 0.02)
	)
	(pad "AA29" smd circle
		(at 13.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AA30" smd circle
		(at 14.5 5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.273)
		(solder_mask_margin 0.02)
	)
	(pad "AB1" smd circle
		(at -14.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 28.796)
		(solder_mask_margin 0.02)
	)
	(pad "AB2" smd circle
		(at -13.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 27.299)
		(solder_mask_margin 0.02)
	)
	(pad "AB3" smd circle
		(at -12.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AB4" smd circle
		(at -11.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AB5" smd circle
		(at -10.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.349)
		(solder_mask_margin 0.02)
	)
	(pad "AB6" smd circle
		(at -9.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AB7" smd circle
		(at -8.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.149)
		(solder_mask_margin 0.02)
	)
	(pad "AB8" smd circle
		(at -7.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.354)
		(solder_mask_margin 0.02)
	)
	(pad "AB9" smd circle
		(at -6.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.874)
		(solder_mask_margin 0.02)
	)
	(pad "AB10" smd circle
		(at -5.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.514)
		(solder_mask_margin 0.02)
	)
	(pad "AB11" smd circle
		(at -4.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AB12" smd circle
		(at -3.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.344)
		(solder_mask_margin 0.02)
	)
	(pad "AB13" smd circle
		(at -2.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.095)
		(solder_mask_margin 0.02)
	)
	(pad "AB14" smd circle
		(at -1.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.456)
		(solder_mask_margin 0.02)
	)
	(pad "AB15" smd circle
		(at -0.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.928)
		(solder_mask_margin 0.02)
	)
	(pad "AB16" smd circle
		(at 0.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AB17" smd circle
		(at 1.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.845)
		(solder_mask_margin 0.02)
	)
	(pad "AB18" smd circle
		(at 2.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.634)
		(solder_mask_margin 0.02)
	)
	(pad "AB19" smd circle
		(at 3.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.895)
		(solder_mask_margin 0.02)
	)
	(pad "AB20" smd circle
		(at 4.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.931)
		(solder_mask_margin 0.02)
	)
	(pad "AB21" smd circle
		(at 5.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AB22" smd circle
		(at 6.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.838)
		(solder_mask_margin 0.02)
	)
	(pad "AB23" smd circle
		(at 7.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.178)
		(solder_mask_margin 0.02)
	)
	(pad "AB24" smd circle
		(at 8.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.112)
		(solder_mask_margin 0.02)
	)
	(pad "AB25" smd circle
		(at 9.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.623)
		(solder_mask_margin 0.02)
	)
	(pad "AB26" smd circle
		(at 10.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AB27" smd circle
		(at 11.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.547)
		(solder_mask_margin 0.02)
	)
	(pad "AB28" smd circle
		(at 12.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.753)
		(solder_mask_margin 0.02)
	)
	(pad "AB29" smd circle
		(at 13.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.569)
		(solder_mask_margin 0.02)
	)
	(pad "AB30" smd circle
		(at 14.5 6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.386)
		(solder_mask_margin 0.02)
	)
	(pad "AC1" smd circle
		(at -14.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.921)
		(solder_mask_margin 0.02)
	)
	(pad "AC2" smd circle
		(at -13.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.032)
		(solder_mask_margin 0.02)
	)
	(pad "AC3" smd circle
		(at -12.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AC4" smd circle
		(at -11.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.452)
		(solder_mask_margin 0.02)
	)
	(pad "AC5" smd circle
		(at -10.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.757)
		(solder_mask_margin 0.02)
	)
	(pad "AC6" smd circle
		(at -9.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.428)
		(solder_mask_margin 0.02)
	)
	(pad "AC7" smd circle
		(at -8.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.548)
		(solder_mask_margin 0.02)
	)
	(pad "AC8" smd circle
		(at -7.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AC9" smd circle
		(at -6.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.56)
		(solder_mask_margin 0.02)
	)
	(pad "AC10" smd circle
		(at -5.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.11)
		(solder_mask_margin 0.02)
	)
	(pad "AC11" smd circle
		(at -4.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.841)
		(solder_mask_margin 0.02)
	)
	(pad "AC12" smd circle
		(at -3.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.948)
		(solder_mask_margin 0.02)
	)
	(pad "AC13" smd circle
		(at -2.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AC14" smd circle
		(at -1.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.461)
		(solder_mask_margin 0.02)
	)
	(pad "AC15" smd circle
		(at -0.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.881)
		(solder_mask_margin 0.02)
	)
	(pad "AC16" smd circle
		(at 0.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.421)
		(solder_mask_margin 0.02)
	)
	(pad "AC17" smd circle
		(at 1.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.722)
		(solder_mask_margin 0.02)
	)
	(pad "AC18" smd circle
		(at 2.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AC19" smd circle
		(at 3.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.941)
		(solder_mask_margin 0.02)
	)
	(pad "AC20" smd circle
		(at 4.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.323)
		(solder_mask_margin 0.02)
	)
	(pad "AC21" smd circle
		(at 5.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.293)
		(solder_mask_margin 0.02)
	)
	(pad "AC22" smd circle
		(at 6.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.349)
		(solder_mask_margin 0.02)
	)
	(pad "AC23" smd circle
		(at 7.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AC24" smd circle
		(at 8.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.538)
		(solder_mask_margin 0.02)
	)
	(pad "AC25" smd circle
		(at 9.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.609)
		(solder_mask_margin 0.02)
	)
	(pad "AC26" smd circle
		(at 10.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.896)
		(solder_mask_margin 0.02)
	)
	(pad "AC27" smd circle
		(at 11.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.768)
		(solder_mask_margin 0.02)
	)
	(pad "AC28" smd circle
		(at 12.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AC29" smd circle
		(at 13.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.896)
		(solder_mask_margin 0.02)
	)
	(pad "AC30" smd circle
		(at 14.5 7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.582)
		(solder_mask_margin 0.02)
	)
	(pad "AD1" smd circle
		(at -14.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.294)
		(solder_mask_margin 0.02)
	)
	(pad "AD2" smd circle
		(at -13.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.014)
		(solder_mask_margin 0.02)
	)
	(pad "AD3" smd circle
		(at -12.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.656)
		(solder_mask_margin 0.02)
	)
	(pad "AD4" smd circle
		(at -11.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.951)
		(solder_mask_margin 0.02)
	)
	(pad "AD5" smd circle
		(at -10.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AD6" smd circle
		(at -9.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.148)
		(solder_mask_margin 0.02)
	)
	(pad "AD7" smd circle
		(at -8.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.552)
		(solder_mask_margin 0.02)
	)
	(pad "AD8" smd circle
		(at -7.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.02)
		(solder_mask_margin 0.02)
	)
	(pad "AD9" smd circle
		(at -6.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.484)
		(solder_mask_margin 0.02)
	)
	(pad "AD10" smd circle
		(at -5.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AD11" smd circle
		(at -4.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.198)
		(solder_mask_margin 0.02)
	)
	(pad "AD12" smd circle
		(at -3.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.066)
		(solder_mask_margin 0.02)
	)
	(pad "AD13" smd circle
		(at -2.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.655)
		(solder_mask_margin 0.02)
	)
	(pad "AD14" smd circle
		(at -1.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.008)
		(solder_mask_margin 0.02)
	)
	(pad "AD15" smd circle
		(at -0.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AD16" smd circle
		(at 0.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.892)
		(solder_mask_margin 0.02)
	)
	(pad "AD17" smd circle
		(at 1.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.478)
		(solder_mask_margin 0.02)
	)
	(pad "AD18" smd circle
		(at 2.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.172)
		(solder_mask_margin 0.02)
	)
	(pad "AD19" smd circle
		(at 3.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.412)
		(solder_mask_margin 0.02)
	)
	(pad "AD20" smd circle
		(at 4.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AD21" smd circle
		(at 5.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.418)
		(solder_mask_margin 0.02)
	)
	(pad "AD22" smd circle
		(at 6.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.457)
		(solder_mask_margin 0.02)
	)
	(pad "AD23" smd circle
		(at 7.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.583)
		(solder_mask_margin 0.02)
	)
	(pad "AD24" smd circle
		(at 8.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.257)
		(solder_mask_margin 0.02)
	)
	(pad "AD25" smd circle
		(at 9.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AD26" smd circle
		(at 10.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.018)
		(solder_mask_margin 0.02)
	)
	(pad "AD27" smd circle
		(at 11.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.78)
		(solder_mask_margin 0.02)
	)
	(pad "AD28" smd circle
		(at 12.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.608)
		(solder_mask_margin 0.02)
	)
	(pad "AD29" smd circle
		(at 13.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.051)
		(solder_mask_margin 0.02)
	)
	(pad "AD30" smd circle
		(at 14.5 8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AE1" smd circle
		(at -14.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.484)
		(solder_mask_margin 0.02)
	)
	(pad "AE2" smd circle
		(at -13.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AE3" smd circle
		(at -12.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.774)
		(solder_mask_margin 0.02)
	)
	(pad "AE4" smd circle
		(at -11.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.074)
		(solder_mask_margin 0.02)
	)
	(pad "AE5" smd circle
		(at -10.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.14)
		(solder_mask_margin 0.02)
	)
	(pad "AE6" smd circle
		(at -9.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.788)
		(solder_mask_margin 0.02)
	)
	(pad "AE7" smd circle
		(at -8.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AE8" smd circle
		(at -7.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.592)
		(solder_mask_margin 0.02)
	)
	(pad "AE9" smd circle
		(at -6.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.427)
		(solder_mask_margin 0.02)
	)
	(pad "AE10" smd circle
		(at -5.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.465)
		(solder_mask_margin 0.02)
	)
	(pad "AE11" smd circle
		(at -4.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.396)
		(solder_mask_margin 0.02)
	)
	(pad "AE12" smd circle
		(at -3.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AE13" smd circle
		(at -2.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.974)
		(solder_mask_margin 0.02)
	)
	(pad "AE14" smd circle
		(at -1.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.352)
		(solder_mask_margin 0.02)
	)
	(pad "AE15" smd circle
		(at -0.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.144)
		(solder_mask_margin 0.02)
	)
	(pad "AE16" smd circle
		(at 0.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.283)
		(solder_mask_margin 0.02)
	)
	(pad "AE17" smd circle
		(at 1.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AE18" smd circle
		(at 2.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.208)
		(solder_mask_margin 0.02)
	)
	(pad "AE19" smd circle
		(at 3.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.544)
		(solder_mask_margin 0.02)
	)
	(pad "AE20" smd circle
		(at 4.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.449)
		(solder_mask_margin 0.02)
	)
	(pad "AE21" smd circle
		(at 5.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.51)
		(solder_mask_margin 0.02)
	)
	(pad "AE22" smd circle
		(at 6.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AE23" smd circle
		(at 7.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.622)
		(solder_mask_margin 0.02)
	)
	(pad "AE24" smd circle
		(at 8.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.679)
		(solder_mask_margin 0.02)
	)
	(pad "AE25" smd circle
		(at 9.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.226)
		(solder_mask_margin 0.02)
	)
	(pad "AE26" smd circle
		(at 10.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.263)
		(solder_mask_margin 0.02)
	)
	(pad "AE27" smd circle
		(at 11.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AE28" smd circle
		(at 12.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.231)
		(solder_mask_margin 0.02)
	)
	(pad "AE29" smd circle
		(at 13.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.383)
		(solder_mask_margin 0.02)
	)
	(pad "AE30" smd circle
		(at 14.5 9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.537)
		(solder_mask_margin 0.02)
	)
	(pad "AF1" smd circle
		(at -14.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.617)
		(solder_mask_margin 0.02)
	)
	(pad "AF2" smd circle
		(at -13.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.199)
		(solder_mask_margin 0.02)
	)
	(pad "AF3" smd circle
		(at -12.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.914)
		(solder_mask_margin 0.02)
	)
	(pad "AF4" smd circle
		(at -11.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AF5" smd circle
		(at -10.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.528)
		(solder_mask_margin 0.02)
	)
	(pad "AF6" smd circle
		(at -9.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.428)
		(solder_mask_margin 0.02)
	)
	(pad "AF7" smd circle
		(at -8.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.476)
		(solder_mask_margin 0.02)
	)
	(pad "AF8" smd circle
		(at -7.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.874)
		(solder_mask_margin 0.02)
	)
	(pad "AF9" smd circle
		(at -6.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AF10" smd circle
		(at -5.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.658)
		(solder_mask_margin 0.02)
	)
	(pad "AF11" smd circle
		(at -4.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.351)
		(solder_mask_margin 0.02)
	)
	(pad "AF12" smd circle
		(at -3.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.111)
		(solder_mask_margin 0.02)
	)
	(pad "AF13" smd circle
		(at -2.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.268)
		(solder_mask_margin 0.02)
	)
	(pad "AF14" smd circle
		(at -1.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AF15" smd circle
		(at -0.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.766)
		(solder_mask_margin 0.02)
	)
	(pad "AF16" smd circle
		(at 0.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.245)
		(solder_mask_margin 0.02)
	)
	(pad "AF17" smd circle
		(at 1.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.799)
		(solder_mask_margin 0.02)
	)
	(pad "AF18" smd circle
		(at 2.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.405)
		(solder_mask_margin 0.02)
	)
	(pad "AF19" smd circle
		(at 3.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AF20" smd circle
		(at 4.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.781)
		(solder_mask_margin 0.02)
	)
	(pad "AF21" smd circle
		(at 5.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.006)
		(solder_mask_margin 0.02)
	)
	(pad "AF22" smd circle
		(at 6.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.098)
		(solder_mask_margin 0.02)
	)
	(pad "AF23" smd circle
		(at 7.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.641)
		(solder_mask_margin 0.02)
	)
	(pad "AF24" smd circle
		(at 8.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AF25" smd circle
		(at 9.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.464)
		(solder_mask_margin 0.02)
	)
	(pad "AF26" smd circle
		(at 10.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.71)
		(solder_mask_margin 0.02)
	)
	(pad "AF27" smd circle
		(at 11.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.589)
		(solder_mask_margin 0.02)
	)
	(pad "AF28" smd circle
		(at 12.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.857)
		(solder_mask_margin 0.02)
	)
	(pad "AF29" smd circle
		(at 13.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AF30" smd circle
		(at 14.5 10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.947)
		(solder_mask_margin 0.02)
	)
	(pad "AG1" smd circle
		(at -14.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AG2" smd circle
		(at -13.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.704)
		(solder_mask_margin 0.02)
	)
	(pad "AG3" smd circle
		(at -12.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.545)
		(solder_mask_margin 0.02)
	)
	(pad "AG4" smd circle
		(at -11.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.769)
		(solder_mask_margin 0.02)
	)
	(pad "AG5" smd circle
		(at -10.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.454)
		(solder_mask_margin 0.02)
	)
	(pad "AG6" smd circle
		(at -9.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AG7" smd circle
		(at -8.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.497)
		(solder_mask_margin 0.02)
	)
	(pad "AG8" smd circle
		(at -7.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.362)
		(solder_mask_margin 0.02)
	)
	(pad "AG9" smd circle
		(at -6.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.472)
		(solder_mask_margin 0.02)
	)
	(pad "AG10" smd circle
		(at -5.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.427)
		(solder_mask_margin 0.02)
	)
	(pad "AG11" smd circle
		(at -4.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AG12" smd circle
		(at -3.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.042)
		(solder_mask_margin 0.02)
	)
	(pad "AG13" smd circle
		(at -2.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.152)
		(solder_mask_margin 0.02)
	)
	(pad "AG14" smd circle
		(at -1.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.861)
		(solder_mask_margin 0.02)
	)
	(pad "AG15" smd circle
		(at -0.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.43)
		(solder_mask_margin 0.02)
	)
	(pad "AG16" smd circle
		(at 0.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AG17" smd circle
		(at 1.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.963)
		(solder_mask_margin 0.02)
	)
	(pad "AG18" smd circle
		(at 2.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.178)
		(solder_mask_margin 0.02)
	)
	(pad "AG19" smd circle
		(at 3.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.281)
		(solder_mask_margin 0.02)
	)
	(pad "AG20" smd circle
		(at 4.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.048)
		(solder_mask_margin 0.02)
	)
	(pad "AG21" smd circle
		(at 5.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AG22" smd circle
		(at 6.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.529)
		(solder_mask_margin 0.02)
	)
	(pad "AG23" smd circle
		(at 7.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.265)
		(solder_mask_margin 0.02)
	)
	(pad "AG24" smd circle
		(at 8.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.801)
		(solder_mask_margin 0.02)
	)
	(pad "AG25" smd circle
		(at 9.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.835)
		(solder_mask_margin 0.02)
	)
	(pad "AG26" smd circle
		(at 10.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AG27" smd circle
		(at 11.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.137)
		(solder_mask_margin 0.02)
	)
	(pad "AG28" smd circle
		(at 12.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.984)
		(solder_mask_margin 0.02)
	)
	(pad "AG29" smd circle
		(at 13.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.893)
		(solder_mask_margin 0.02)
	)
	(pad "AG30" smd circle
		(at 14.5 11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.457)
		(solder_mask_margin 0.02)
	)
	(pad "AH1" smd circle
		(at -14.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.335)
		(solder_mask_margin 0.02)
	)
	(pad "AH2" smd circle
		(at -13.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.594)
		(solder_mask_margin 0.02)
	)
	(pad "AH3" smd circle
		(at -12.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AH4" smd circle
		(at -11.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.051)
		(solder_mask_margin 0.02)
	)
	(pad "AH5" smd circle
		(at -10.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.368)
		(solder_mask_margin 0.02)
	)
	(pad "AH6" smd circle
		(at -9.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.691)
		(solder_mask_margin 0.02)
	)
	(pad "AH7" smd circle
		(at -8.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.353)
		(solder_mask_margin 0.02)
	)
	(pad "AH8" smd circle
		(at -7.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AH9" smd circle
		(at -6.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.598)
		(solder_mask_margin 0.02)
	)
	(pad "AH10" smd circle
		(at -5.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.153)
		(solder_mask_margin 0.02)
	)
	(pad "AH11" smd circle
		(at -4.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.477)
		(solder_mask_margin 0.02)
	)
	(pad "AH12" smd circle
		(at -3.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.902)
		(solder_mask_margin 0.02)
	)
	(pad "AH13" smd circle
		(at -2.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AH14" smd circle
		(at -1.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.831)
		(solder_mask_margin 0.02)
	)
	(pad "AH15" smd circle
		(at -0.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.849)
		(solder_mask_margin 0.02)
	)
	(pad "AH16" smd circle
		(at 0.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.668)
		(solder_mask_margin 0.02)
	)
	(pad "AH17" smd circle
		(at 1.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.893)
		(solder_mask_margin 0.02)
	)
	(pad "AH18" smd circle
		(at 2.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AH19" smd circle
		(at 3.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.8)
		(solder_mask_margin 0.02)
	)
	(pad "AH20" smd circle
		(at 4.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.515)
		(solder_mask_margin 0.02)
	)
	(pad "AH21" smd circle
		(at 5.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.587)
		(solder_mask_margin 0.02)
	)
	(pad "AH22" smd circle
		(at 6.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.887)
		(solder_mask_margin 0.02)
	)
	(pad "AH23" smd circle
		(at 7.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AH24" smd circle
		(at 8.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.774)
		(solder_mask_margin 0.02)
	)
	(pad "AH25" smd circle
		(at 9.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.379)
		(solder_mask_margin 0.02)
	)
	(pad "AH26" smd circle
		(at 10.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.804)
		(solder_mask_margin 0.02)
	)
	(pad "AH27" smd circle
		(at 11.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.115)
		(solder_mask_margin 0.02)
	)
	(pad "AH28" smd circle
		(at 12.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AH29" smd circle
		(at 13.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.428)
		(solder_mask_margin 0.02)
	)
	(pad "AH30" smd circle
		(at 14.5 12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.408)
		(solder_mask_margin 0.02)
	)
	(pad "AJ1" smd circle
		(at -14.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.396)
		(solder_mask_margin 0.02)
	)
	(pad "AJ2" smd circle
		(at -13.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.465)
		(solder_mask_margin 0.02)
	)
	(pad "AJ3" smd circle
		(at -12.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.099)
		(solder_mask_margin 0.02)
	)
	(pad "AJ4" smd circle
		(at -11.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.012)
		(solder_mask_margin 0.02)
	)
	(pad "AJ5" smd circle
		(at -10.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AJ6" smd circle
		(at -9.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.732)
		(solder_mask_margin 0.02)
	)
	(pad "AJ7" smd circle
		(at -8.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.068)
		(solder_mask_margin 0.02)
	)
	(pad "AJ8" smd circle
		(at -7.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.132)
		(solder_mask_margin 0.02)
	)
	(pad "AJ9" smd circle
		(at -6.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.988)
		(solder_mask_margin 0.02)
	)
	(pad "AJ10" smd circle
		(at -5.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AJ11" smd circle
		(at -4.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.518)
		(solder_mask_margin 0.02)
	)
	(pad "AJ12" smd circle
		(at -3.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.055)
		(solder_mask_margin 0.02)
	)
	(pad "AJ13" smd circle
		(at -2.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.602)
		(solder_mask_margin 0.02)
	)
	(pad "AJ14" smd circle
		(at -1.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.179)
		(solder_mask_margin 0.02)
	)
	(pad "AJ15" smd circle
		(at -0.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AJ16" smd circle
		(at 0.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.232)
		(solder_mask_margin 0.02)
	)
	(pad "AJ17" smd circle
		(at 1.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.569)
		(solder_mask_margin 0.02)
	)
	(pad "AJ18" smd circle
		(at 2.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.796)
		(solder_mask_margin 0.02)
	)
	(pad "AJ19" smd circle
		(at 3.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.335)
		(solder_mask_margin 0.02)
	)
	(pad "AJ20" smd circle
		(at 4.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AJ21" smd circle
		(at 5.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.355)
		(solder_mask_margin 0.02)
	)
	(pad "AJ22" smd circle
		(at 6.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.698)
		(solder_mask_margin 0.02)
	)
	(pad "AJ23" smd circle
		(at 7.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.727)
		(solder_mask_margin 0.02)
	)
	(pad "AJ24" smd circle
		(at 8.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.604)
		(solder_mask_margin 0.02)
	)
	(pad "AJ25" smd circle
		(at 9.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AJ26" smd circle
		(at 10.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.345)
		(solder_mask_margin 0.02)
	)
	(pad "AJ27" smd circle
		(at 11.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.574)
		(solder_mask_margin 0.02)
	)
	(pad "AJ28" smd circle
		(at 12.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.784)
		(solder_mask_margin 0.02)
	)
	(pad "AJ29" smd circle
		(at 13.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.876)
		(solder_mask_margin 0.02)
	)
	(pad "AJ30" smd circle
		(at 14.5 13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AK1" smd circle
		(at -14.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.656)
		(solder_mask_margin 0.02)
	)
	(pad "AK2" smd circle
		(at -13.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AK3" smd circle
		(at -12.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.037)
		(solder_mask_margin 0.02)
	)
	(pad "AK4" smd circle
		(at -11.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.568)
		(solder_mask_margin 0.02)
	)
	(pad "AK5" smd circle
		(at -10.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.516)
		(solder_mask_margin 0.02)
	)
	(pad "AK6" smd circle
		(at -9.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.012)
		(solder_mask_margin 0.02)
	)
	(pad "AK7" smd circle
		(at -8.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AK8" smd circle
		(at -7.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.371)
		(solder_mask_margin 0.02)
	)
	(pad "AK9" smd circle
		(at -6.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.854)
		(solder_mask_margin 0.02)
	)
	(pad "AK10" smd circle
		(at -5.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.289)
		(solder_mask_margin 0.02)
	)
	(pad "AK11" smd circle
		(at -4.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.52)
		(solder_mask_margin 0.02)
	)
	(pad "AK12" smd circle
		(at -3.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AK13" smd circle
		(at -2.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.609)
		(solder_mask_margin 0.02)
	)
	(pad "AK14" smd circle
		(at -1.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.027)
		(solder_mask_margin 0.02)
	)
	(pad "AK15" smd circle
		(at -0.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.665)
		(solder_mask_margin 0.02)
	)
	(pad "AK16" smd circle
		(at 0.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.612)
		(solder_mask_margin 0.02)
	)
	(pad "AK17" smd circle
		(at 1.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AK18" smd circle
		(at 2.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.005)
		(solder_mask_margin 0.02)
	)
	(pad "AK19" smd circle
		(at 3.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.523)
		(solder_mask_margin 0.02)
	)
	(pad "AK20" smd circle
		(at 4.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.709)
		(solder_mask_margin 0.02)
	)
	(pad "AK21" smd circle
		(at 5.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.051)
		(solder_mask_margin 0.02)
	)
	(pad "AK22" smd circle
		(at 6.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AK23" smd circle
		(at 7.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.198)
		(solder_mask_margin 0.02)
	)
	(pad "AK24" smd circle
		(at 8.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.315)
		(solder_mask_margin 0.02)
	)
	(pad "AK25" smd circle
		(at 9.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.925)
		(solder_mask_margin 0.02)
	)
	(pad "AK26" smd circle
		(at 10.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.616)
		(solder_mask_margin 0.02)
	)
	(pad "AK27" smd circle
		(at 11.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "AK28" smd circle
		(at 12.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.362)
		(solder_mask_margin 0.02)
	)
	(pad "AK29" smd circle
		(at 13.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.007)
		(solder_mask_margin 0.02)
	)
	(pad "AK30" smd circle
		(at 14.5 14.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.946)
		(solder_mask_margin 0.02)
	)
	(pad "B1" smd circle
		(at -14.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.521)
		(solder_mask_margin 0.02)
	)
	(pad "B2" smd circle
		(at -13.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.53)
		(solder_mask_margin 0.02)
	)
	(pad "B3" smd circle
		(at -12.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B4" smd circle
		(at -11.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B5" smd circle
		(at -10.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.709)
		(solder_mask_margin 0.02)
	)
	(pad "B6" smd circle
		(at -9.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.944)
		(solder_mask_margin 0.02)
	)
	(pad "B7" smd circle
		(at -8.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B8" smd circle
		(at -7.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B9" smd circle
		(at -6.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B10" smd circle
		(at -5.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 29.155)
		(solder_mask_margin 0.02)
	)
	(pad "B11" smd circle
		(at -4.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B12" smd circle
		(at -3.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.173)
		(solder_mask_margin 0.02)
	)
	(pad "B13" smd circle
		(at -2.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.88)
		(solder_mask_margin 0.02)
	)
	(pad "B14" smd circle
		(at -1.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.532)
		(solder_mask_margin 0.02)
	)
	(pad "B15" smd circle
		(at -0.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.701)
		(solder_mask_margin 0.02)
	)
	(pad "B16" smd circle
		(at 0.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B17" smd circle
		(at 1.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.879)
		(solder_mask_margin 0.02)
	)
	(pad "B18" smd circle
		(at 2.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.881)
		(solder_mask_margin 0.02)
	)
	(pad "B19" smd circle
		(at 3.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.226)
		(solder_mask_margin 0.02)
	)
	(pad "B20" smd circle
		(at 4.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.681)
		(solder_mask_margin 0.02)
	)
	(pad "B21" smd circle
		(at 5.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B22" smd circle
		(at 6.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.288)
		(solder_mask_margin 0.02)
	)
	(pad "B23" smd circle
		(at 7.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.406)
		(solder_mask_margin 0.02)
	)
	(pad "B24" smd circle
		(at 8.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.133)
		(solder_mask_margin 0.02)
	)
	(pad "B25" smd circle
		(at 9.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.219)
		(solder_mask_margin 0.02)
	)
	(pad "B26" smd circle
		(at 10.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "B27" smd circle
		(at 11.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.903)
		(solder_mask_margin 0.02)
	)
	(pad "B28" smd circle
		(at 12.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.114)
		(solder_mask_margin 0.02)
	)
	(pad "B29" smd circle
		(at 13.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.831)
		(solder_mask_margin 0.02)
	)
	(pad "B30" smd circle
		(at 14.5 -13.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 24.67)
		(solder_mask_margin 0.02)
	)
	(pad "C1" smd circle
		(at -14.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C2" smd circle
		(at -13.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C3" smd circle
		(at -12.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.029)
		(solder_mask_margin 0.02)
	)
	(pad "C4" smd circle
		(at -11.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.008)
		(solder_mask_margin 0.02)
	)
	(pad "C5" smd circle
		(at -10.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C6" smd circle
		(at -9.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C7" smd circle
		(at -8.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.106)
		(solder_mask_margin 0.02)
	)
	(pad "C8" smd circle
		(at -7.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.647)
		(solder_mask_margin 0.02)
	)
	(pad "C9" smd circle
		(at -6.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C10" smd circle
		(at -5.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 28.237)
		(solder_mask_margin 0.02)
	)
	(pad "C11" smd circle
		(at -4.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.774)
		(solder_mask_margin 0.02)
	)
	(pad "C12" smd circle
		(at -3.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.474)
		(solder_mask_margin 0.02)
	)
	(pad "C13" smd circle
		(at -2.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C14" smd circle
		(at -1.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.366)
		(solder_mask_margin 0.02)
	)
	(pad "C15" smd circle
		(at -0.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.399)
		(solder_mask_margin 0.02)
	)
	(pad "C16" smd circle
		(at 0.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.846)
		(solder_mask_margin 0.02)
	)
	(pad "C17" smd circle
		(at 1.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.901)
		(solder_mask_margin 0.02)
	)
	(pad "C18" smd circle
		(at 2.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C19" smd circle
		(at 3.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 25.069)
		(solder_mask_margin 0.02)
	)
	(pad "C20" smd circle
		(at 4.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.681)
		(solder_mask_margin 0.02)
	)
	(pad "C21" smd circle
		(at 5.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.277)
		(solder_mask_margin 0.02)
	)
	(pad "C22" smd circle
		(at 6.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.905)
		(solder_mask_margin 0.02)
	)
	(pad "C23" smd circle
		(at 7.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C24" smd circle
		(at 8.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.699)
		(solder_mask_margin 0.02)
	)
	(pad "C25" smd circle
		(at 9.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.617)
		(solder_mask_margin 0.02)
	)
	(pad "C26" smd circle
		(at 10.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.862)
		(solder_mask_margin 0.02)
	)
	(pad "C27" smd circle
		(at 11.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.889)
		(solder_mask_margin 0.02)
	)
	(pad "C28" smd circle
		(at 12.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "C29" smd circle
		(at 13.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.768)
		(solder_mask_margin 0.02)
	)
	(pad "C30" smd circle
		(at 14.5 -12.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.33)
		(solder_mask_margin 0.02)
	)
	(pad "D1" smd circle
		(at -14.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.063)
		(solder_mask_margin 0.02)
	)
	(pad "D2" smd circle
		(at -13.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.112)
		(solder_mask_margin 0.02)
	)
	(pad "D3" smd circle
		(at -12.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D4" smd circle
		(at -11.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D5" smd circle
		(at -10.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.844)
		(solder_mask_margin 0.02)
	)
	(pad "D6" smd circle
		(at -9.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12)
		(solder_mask_margin 0.02)
	)
	(pad "D7" smd circle
		(at -8.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D8" smd circle
		(at -7.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D9" smd circle
		(at -6.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D10" smd circle
		(at -5.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D11" smd circle
		(at -4.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.711)
		(solder_mask_margin 0.02)
	)
	(pad "D12" smd circle
		(at -3.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.434)
		(solder_mask_margin 0.02)
	)
	(pad "D13" smd circle
		(at -2.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.524)
		(solder_mask_margin 0.02)
	)
	(pad "D14" smd circle
		(at -1.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.264)
		(solder_mask_margin 0.02)
	)
	(pad "D15" smd circle
		(at -0.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D16" smd circle
		(at 0.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.582)
		(solder_mask_margin 0.02)
	)
	(pad "D17" smd circle
		(at 1.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.562)
		(solder_mask_margin 0.02)
	)
	(pad "D18" smd circle
		(at 2.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.659)
		(solder_mask_margin 0.02)
	)
	(pad "D19" smd circle
		(at 3.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.704)
		(solder_mask_margin 0.02)
	)
	(pad "D20" smd circle
		(at 4.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D21" smd circle
		(at 5.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.622)
		(solder_mask_margin 0.02)
	)
	(pad "D22" smd circle
		(at 6.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.866)
		(solder_mask_margin 0.02)
	)
	(pad "D23" smd circle
		(at 7.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.449)
		(solder_mask_margin 0.02)
	)
	(pad "D24" smd circle
		(at 8.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.101)
		(solder_mask_margin 0.02)
	)
	(pad "D25" smd circle
		(at 9.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "D26" smd circle
		(at 10.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.509)
		(solder_mask_margin 0.02)
	)
	(pad "D27" smd circle
		(at 11.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.812)
		(solder_mask_margin 0.02)
	)
	(pad "D28" smd circle
		(at 12.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.301)
		(solder_mask_margin 0.02)
	)
	(pad "D29" smd circle
		(at 13.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.353)
		(solder_mask_margin 0.02)
	)
	(pad "D30" smd circle
		(at 14.5 -11.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E1" smd circle
		(at -14.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E2" smd circle
		(at -13.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E3" smd circle
		(at -12.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.064)
		(solder_mask_margin 0.02)
	)
	(pad "E4" smd circle
		(at -11.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.131)
		(solder_mask_margin 0.02)
	)
	(pad "E5" smd circle
		(at -10.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E6" smd circle
		(at -9.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E7" smd circle
		(at -8.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.062)
		(solder_mask_margin 0.02)
	)
	(pad "E8" smd circle
		(at -7.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.842)
		(solder_mask_margin 0.02)
	)
	(pad "E9" smd circle
		(at -6.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E10" smd circle
		(at -5.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 26.06)
		(solder_mask_margin 0.02)
	)
	(pad "E11" smd circle
		(at -4.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.276)
		(solder_mask_margin 0.02)
	)
	(pad "E12" smd circle
		(at -3.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E13" smd circle
		(at -2.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.055)
		(solder_mask_margin 0.02)
	)
	(pad "E14" smd circle
		(at -1.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.074)
		(solder_mask_margin 0.02)
	)
	(pad "E15" smd circle
		(at -0.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.086)
		(solder_mask_margin 0.02)
	)
	(pad "E16" smd circle
		(at 0.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.757)
		(solder_mask_margin 0.02)
	)
	(pad "E17" smd circle
		(at 1.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E18" smd circle
		(at 2.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.737)
		(solder_mask_margin 0.02)
	)
	(pad "E19" smd circle
		(at 3.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.56)
		(solder_mask_margin 0.02)
	)
	(pad "E20" smd circle
		(at 4.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.829)
		(solder_mask_margin 0.02)
	)
	(pad "E21" smd circle
		(at 5.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.731)
		(solder_mask_margin 0.02)
	)
	(pad "E22" smd circle
		(at 6.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E23" smd circle
		(at 7.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.705)
		(solder_mask_margin 0.02)
	)
	(pad "E24" smd circle
		(at 8.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.397)
		(solder_mask_margin 0.02)
	)
	(pad "E25" smd circle
		(at 9.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.213)
		(solder_mask_margin 0.02)
	)
	(pad "E26" smd circle
		(at 10.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.221)
		(solder_mask_margin 0.02)
	)
	(pad "E27" smd circle
		(at 11.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "E28" smd circle
		(at 12.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.92)
		(solder_mask_margin 0.02)
	)
	(pad "E29" smd circle
		(at 13.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.495)
		(solder_mask_margin 0.02)
	)
	(pad "E30" smd circle
		(at 14.5 -10.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.444)
		(solder_mask_margin 0.02)
	)
	(pad "F1" smd circle
		(at -14.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.68)
		(solder_mask_margin 0.02)
	)
	(pad "F2" smd circle
		(at -13.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.728)
		(solder_mask_margin 0.02)
	)
	(pad "F3" smd circle
		(at -12.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F4" smd circle
		(at -11.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F5" smd circle
		(at -10.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.765)
		(solder_mask_margin 0.02)
	)
	(pad "F6" smd circle
		(at -9.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.959)
		(solder_mask_margin 0.02)
	)
	(pad "F7" smd circle
		(at -8.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F8" smd circle
		(at -7.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F9" smd circle
		(at -6.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F10" smd circle
		(at -5.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 26.323)
		(solder_mask_margin 0.02)
	)
	(pad "F11" smd circle
		(at -4.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.906)
		(solder_mask_margin 0.02)
	)
	(pad "F12" smd circle
		(at -3.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 22.763)
		(solder_mask_margin 0.02)
	)
	(pad "F13" smd circle
		(at -2.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.979)
		(solder_mask_margin 0.02)
	)
	(pad "F14" smd circle
		(at -1.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F15" smd circle
		(at -0.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.661)
		(solder_mask_margin 0.02)
	)
	(pad "F16" smd circle
		(at 0.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.14)
		(solder_mask_margin 0.02)
	)
	(pad "F17" smd circle
		(at 1.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.72)
		(solder_mask_margin 0.02)
	)
	(pad "F18" smd circle
		(at 2.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.739)
		(solder_mask_margin 0.02)
	)
	(pad "F19" smd circle
		(at 3.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F20" smd circle
		(at 4.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.91)
		(solder_mask_margin 0.02)
	)
	(pad "F21" smd circle
		(at 5.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.319)
		(solder_mask_margin 0.02)
	)
	(pad "F22" smd circle
		(at 6.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.808)
		(solder_mask_margin 0.02)
	)
	(pad "F23" smd circle
		(at 7.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.681)
		(solder_mask_margin 0.02)
	)
	(pad "F24" smd circle
		(at 8.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F25" smd circle
		(at 9.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.196)
		(solder_mask_margin 0.02)
	)
	(pad "F26" smd circle
		(at 10.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.252)
		(solder_mask_margin 0.02)
	)
	(pad "F27" smd circle
		(at 11.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.729)
		(solder_mask_margin 0.02)
	)
	(pad "F28" smd circle
		(at 12.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.204)
		(solder_mask_margin 0.02)
	)
	(pad "F29" smd circle
		(at 13.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "F30" smd circle
		(at 14.5 -9.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.812)
		(solder_mask_margin 0.02)
	)
	(pad "G1" smd circle
		(at -14.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G2" smd circle
		(at -13.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G3" smd circle
		(at -12.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.896)
		(solder_mask_margin 0.02)
	)
	(pad "G4" smd circle
		(at -11.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.853)
		(solder_mask_margin 0.02)
	)
	(pad "G5" smd circle
		(at -10.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G6" smd circle
		(at -9.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G7" smd circle
		(at -8.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.176)
		(solder_mask_margin 0.02)
	)
	(pad "G8" smd circle
		(at -7.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.73)
		(solder_mask_margin 0.02)
	)
	(pad "G9" smd circle
		(at -6.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G10" smd circle
		(at -5.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.572)
		(solder_mask_margin 0.02)
	)
	(pad "G11" smd circle
		(at -4.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G12" smd circle
		(at -3.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.365)
		(solder_mask_margin 0.02)
	)
	(pad "G13" smd circle
		(at -2.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.803)
		(solder_mask_margin 0.02)
	)
	(pad "G14" smd circle
		(at -1.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.243)
		(solder_mask_margin 0.02)
	)
	(pad "G15" smd circle
		(at -0.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.863)
		(solder_mask_margin 0.02)
	)
	(pad "G16" smd circle
		(at 0.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G17" smd circle
		(at 1.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.206)
		(solder_mask_margin 0.02)
	)
	(pad "G18" smd circle
		(at 2.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.974)
		(solder_mask_margin 0.02)
	)
	(pad "G19" smd circle
		(at 3.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.384)
		(solder_mask_margin 0.02)
	)
	(pad "G20" smd circle
		(at 4.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.241)
		(solder_mask_margin 0.02)
	)
	(pad "G21" smd circle
		(at 5.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G22" smd circle
		(at 6.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.687)
		(solder_mask_margin 0.02)
	)
	(pad "G23" smd circle
		(at 7.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.196)
		(solder_mask_margin 0.02)
	)
	(pad "G24" smd circle
		(at 8.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.995)
		(solder_mask_margin 0.02)
	)
	(pad "G25" smd circle
		(at 9.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.465)
		(solder_mask_margin 0.02)
	)
	(pad "G26" smd circle
		(at 10.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "G27" smd circle
		(at 11.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.597)
		(solder_mask_margin 0.02)
	)
	(pad "G28" smd circle
		(at 12.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.625)
		(solder_mask_margin 0.02)
	)
	(pad "G29" smd circle
		(at 13.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.638)
		(solder_mask_margin 0.02)
	)
	(pad "G30" smd circle
		(at 14.5 -8.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.043)
		(solder_mask_margin 0.02)
	)
	(pad "H1" smd circle
		(at -14.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.476)
		(solder_mask_margin 0.02)
	)
	(pad "H2" smd circle
		(at -13.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.439)
		(solder_mask_margin 0.02)
	)
	(pad "H3" smd circle
		(at -12.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H4" smd circle
		(at -11.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H5" smd circle
		(at -10.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.235)
		(solder_mask_margin 0.02)
	)
	(pad "H6" smd circle
		(at -9.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.4)
		(solder_mask_margin 0.02)
	)
	(pad "H7" smd circle
		(at -8.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H8" smd circle
		(at -7.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H9" smd circle
		(at -6.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H10" smd circle
		(at -5.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.171)
		(solder_mask_margin 0.02)
	)
	(pad "H11" smd circle
		(at -4.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.026)
		(solder_mask_margin 0.02)
	)
	(pad "H12" smd circle
		(at -3.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.278)
		(solder_mask_margin 0.02)
	)
	(pad "H13" smd circle
		(at -2.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H14" smd circle
		(at -1.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.828)
		(solder_mask_margin 0.02)
	)
	(pad "H15" smd circle
		(at -0.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.975)
		(solder_mask_margin 0.02)
	)
	(pad "H16" smd circle
		(at 0.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.63)
		(solder_mask_margin 0.02)
	)
	(pad "H17" smd circle
		(at 1.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.161)
		(solder_mask_margin 0.02)
	)
	(pad "H18" smd circle
		(at 2.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H19" smd circle
		(at 3.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.623)
		(solder_mask_margin 0.02)
	)
	(pad "H20" smd circle
		(at 4.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.042)
		(solder_mask_margin 0.02)
	)
	(pad "H21" smd circle
		(at 5.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.269)
		(solder_mask_margin 0.02)
	)
	(pad "H22" smd circle
		(at 6.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.039)
		(solder_mask_margin 0.02)
	)
	(pad "H23" smd circle
		(at 7.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H24" smd circle
		(at 8.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.78)
		(solder_mask_margin 0.02)
	)
	(pad "H25" smd circle
		(at 9.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.174)
		(solder_mask_margin 0.02)
	)
	(pad "H26" smd circle
		(at 10.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.226)
		(solder_mask_margin 0.02)
	)
	(pad "H27" smd circle
		(at 11.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.224)
		(solder_mask_margin 0.02)
	)
	(pad "H28" smd circle
		(at 12.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "H29" smd circle
		(at 13.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.337)
		(solder_mask_margin 0.02)
	)
	(pad "H30" smd circle
		(at 14.5 -7.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.292)
		(solder_mask_margin 0.02)
	)
	(pad "J1" smd circle
		(at -14.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J2" smd circle
		(at -13.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J3" smd circle
		(at -12.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.925)
		(solder_mask_margin 0.02)
	)
	(pad "J4" smd circle
		(at -11.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.887)
		(solder_mask_margin 0.02)
	)
	(pad "J5" smd circle
		(at -10.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J6" smd circle
		(at -9.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J7" smd circle
		(at -8.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.91)
		(solder_mask_margin 0.02)
	)
	(pad "J8" smd circle
		(at -7.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.161)
		(solder_mask_margin 0.02)
	)
	(pad "J9" smd circle
		(at -6.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J10" smd circle
		(at -5.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J11" smd circle
		(at -4.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.323)
		(solder_mask_margin 0.02)
	)
	(pad "J12" smd circle
		(at -3.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.125)
		(solder_mask_margin 0.02)
	)
	(pad "J13" smd circle
		(at -2.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.187)
		(solder_mask_margin 0.02)
	)
	(pad "J14" smd circle
		(at -1.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.741)
		(solder_mask_margin 0.02)
	)
	(pad "J15" smd circle
		(at -0.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J16" smd circle
		(at 0.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.593)
		(solder_mask_margin 0.02)
	)
	(pad "J17" smd circle
		(at 1.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.515)
		(solder_mask_margin 0.02)
	)
	(pad "J18" smd circle
		(at 2.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.317)
		(solder_mask_margin 0.02)
	)
	(pad "J19" smd circle
		(at 3.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.052)
		(solder_mask_margin 0.02)
	)
	(pad "J20" smd circle
		(at 4.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J21" smd circle
		(at 5.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.084)
		(solder_mask_margin 0.02)
	)
	(pad "J22" smd circle
		(at 6.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.925)
		(solder_mask_margin 0.02)
	)
	(pad "J23" smd circle
		(at 7.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.063)
		(solder_mask_margin 0.02)
	)
	(pad "J24" smd circle
		(at 8.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.83)
		(solder_mask_margin 0.02)
	)
	(pad "J25" smd circle
		(at 9.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "J26" smd circle
		(at 10.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.197)
		(solder_mask_margin 0.02)
	)
	(pad "J27" smd circle
		(at 11.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.459)
		(solder_mask_margin 0.02)
	)
	(pad "J28" smd circle
		(at 12.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.849)
		(solder_mask_margin 0.02)
	)
	(pad "J29" smd circle
		(at 13.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.885)
		(solder_mask_margin 0.02)
	)
	(pad "J30" smd circle
		(at 14.5 -6.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K1" smd circle
		(at -14.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.162)
		(solder_mask_margin 0.02)
	)
	(pad "K2" smd circle
		(at -13.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.111)
		(solder_mask_margin 0.02)
	)
	(pad "K3" smd circle
		(at -12.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K4" smd circle
		(at -11.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K5" smd circle
		(at -10.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.726)
		(solder_mask_margin 0.02)
	)
	(pad "K6" smd circle
		(at -9.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.905)
		(solder_mask_margin 0.02)
	)
	(pad "K7" smd circle
		(at -8.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K8" smd circle
		(at -7.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K9" smd circle
		(at -6.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K10" smd circle
		(at -5.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.153)
		(solder_mask_margin 0.02)
	)
	(pad "K11" smd circle
		(at -4.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 21.727)
		(solder_mask_margin 0.02)
	)
	(pad "K12" smd circle
		(at -3.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K13" smd circle
		(at -2.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.821)
		(solder_mask_margin 0.02)
	)
	(pad "K14" smd circle
		(at -1.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.482)
		(solder_mask_margin 0.02)
	)
	(pad "K15" smd circle
		(at -0.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.67)
		(solder_mask_margin 0.02)
	)
	(pad "K16" smd circle
		(at 0.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.367)
		(solder_mask_margin 0.02)
	)
	(pad "K17" smd circle
		(at 1.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K18" smd circle
		(at 2.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.927)
		(solder_mask_margin 0.02)
	)
	(pad "K19" smd circle
		(at 3.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.177)
		(solder_mask_margin 0.02)
	)
	(pad "K20" smd circle
		(at 4.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.379)
		(solder_mask_margin 0.02)
	)
	(pad "K21" smd circle
		(at 5.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.872)
		(solder_mask_margin 0.02)
	)
	(pad "K22" smd circle
		(at 6.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K23" smd circle
		(at 7.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.884)
		(solder_mask_margin 0.02)
	)
	(pad "K24" smd circle
		(at 8.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.276)
		(solder_mask_margin 0.02)
	)
	(pad "K25" smd circle
		(at 9.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.47)
		(solder_mask_margin 0.02)
	)
	(pad "K26" smd circle
		(at 10.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.347)
		(solder_mask_margin 0.02)
	)
	(pad "K27" smd circle
		(at 11.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "K28" smd circle
		(at 12.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.837)
		(solder_mask_margin 0.02)
	)
	(pad "K29" smd circle
		(at 13.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.782)
		(solder_mask_margin 0.02)
	)
	(pad "K30" smd circle
		(at 14.5 -5.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.721)
		(solder_mask_margin 0.02)
	)
	(pad "L1" smd circle
		(at -14.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L2" smd circle
		(at -13.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L3" smd circle
		(at -12.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.585)
		(solder_mask_margin 0.02)
	)
	(pad "L4" smd circle
		(at -11.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.561)
		(solder_mask_margin 0.02)
	)
	(pad "L5" smd circle
		(at -10.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L6" smd circle
		(at -9.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L7" smd circle
		(at -8.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.449)
		(solder_mask_margin 0.02)
	)
	(pad "L8" smd circle
		(at -7.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.298)
		(solder_mask_margin 0.02)
	)
	(pad "L9" smd circle
		(at -6.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L10" smd circle
		(at -5.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.652)
		(solder_mask_margin 0.02)
	)
	(pad "L11" smd circle
		(at -4.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 20.929)
		(solder_mask_margin 0.02)
	)
	(pad "L12" smd circle
		(at -3.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.179)
		(solder_mask_margin 0.02)
	)
	(pad "L13" smd circle
		(at -2.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.134)
		(solder_mask_margin 0.02)
	)
	(pad "L14" smd circle
		(at -1.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L15" smd circle
		(at -0.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.689)
		(solder_mask_margin 0.02)
	)
	(pad "L16" smd circle
		(at 0.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.303)
		(solder_mask_margin 0.02)
	)
	(pad "L17" smd circle
		(at 1.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.576)
		(solder_mask_margin 0.02)
	)
	(pad "L18" smd circle
		(at 2.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.081)
		(solder_mask_margin 0.02)
	)
	(pad "L19" smd circle
		(at 3.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L20" smd circle
		(at 4.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.878)
		(solder_mask_margin 0.02)
	)
	(pad "L21" smd circle
		(at 5.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.376)
		(solder_mask_margin 0.02)
	)
	(pad "L22" smd circle
		(at 6.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.134)
		(solder_mask_margin 0.02)
	)
	(pad "L23" smd circle
		(at 7.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.328)
		(solder_mask_margin 0.02)
	)
	(pad "L24" smd circle
		(at 8.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L25" smd circle
		(at 9.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.993)
		(solder_mask_margin 0.02)
	)
	(pad "L26" smd circle
		(at 10.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.575)
		(solder_mask_margin 0.02)
	)
	(pad "L27" smd circle
		(at 11.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.25)
		(solder_mask_margin 0.02)
	)
	(pad "L28" smd circle
		(at 12.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.833)
		(solder_mask_margin 0.02)
	)
	(pad "L29" smd circle
		(at 13.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "L30" smd circle
		(at 14.5 -4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.142)
		(solder_mask_margin 0.02)
	)
	(pad "M1" smd circle
		(at -14.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.468)
		(solder_mask_margin 0.02)
	)
	(pad "M2" smd circle
		(at -13.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.415)
		(solder_mask_margin 0.02)
	)
	(pad "M3" smd circle
		(at -12.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M4" smd circle
		(at -11.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M5" smd circle
		(at -10.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.574)
		(solder_mask_margin 0.02)
	)
	(pad "M6" smd circle
		(at -9.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.789)
		(solder_mask_margin 0.02)
	)
	(pad "M7" smd circle
		(at -8.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M8" smd circle
		(at -7.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M9" smd circle
		(at -6.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M10" smd circle
		(at -5.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 19.51)
		(solder_mask_margin 0.02)
	)
	(pad "M11" smd circle
		(at -4.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M12" smd circle
		(at -3.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M13" smd circle
		(at -2.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M14" smd circle
		(at -1.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M15" smd circle
		(at -0.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M16" smd circle
		(at 0.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M17" smd circle
		(at 1.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M18" smd circle
		(at 2.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M19" smd circle
		(at 3.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.051)
		(solder_mask_margin 0.02)
	)
	(pad "M20" smd circle
		(at 4.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.146)
		(solder_mask_margin 0.02)
	)
	(pad "M21" smd circle
		(at 5.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M22" smd circle
		(at 6.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.019)
		(solder_mask_margin 0.02)
	)
	(pad "M23" smd circle
		(at 7.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.184)
		(solder_mask_margin 0.02)
	)
	(pad "M24" smd circle
		(at 8.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.067)
		(solder_mask_margin 0.02)
	)
	(pad "M25" smd circle
		(at 9.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.167)
		(solder_mask_margin 0.02)
	)
	(pad "M26" smd circle
		(at 10.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "M27" smd circle
		(at 11.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.949)
		(solder_mask_margin 0.02)
	)
	(pad "M28" smd circle
		(at 12.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.521)
		(solder_mask_margin 0.02)
	)
	(pad "M29" smd circle
		(at 13.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.261)
		(solder_mask_margin 0.02)
	)
	(pad "M30" smd circle
		(at 14.5 -3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.654)
		(solder_mask_margin 0.02)
	)
	(pad "N1" smd circle
		(at -14.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N2" smd circle
		(at -13.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N3" smd circle
		(at -12.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.433)
		(solder_mask_margin 0.02)
	)
	(pad "N4" smd circle
		(at -11.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.366)
		(solder_mask_margin 0.02)
	)
	(pad "N5" smd circle
		(at -10.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N6" smd circle
		(at -9.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N7" smd circle
		(at -8.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.657)
		(solder_mask_margin 0.02)
	)
	(pad "N8" smd circle
		(at -7.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.202)
		(solder_mask_margin 0.02)
	)
	(pad "N9" smd circle
		(at -6.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N10" smd circle
		(at -5.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N11" smd circle
		(at -4.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N12" smd circle
		(at -3.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N13" smd circle
		(at -2.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N14" smd circle
		(at -1.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N15" smd circle
		(at -0.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N16" smd circle
		(at 0.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N17" smd circle
		(at 1.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N18" smd circle
		(at 2.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N19" smd circle
		(at 3.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.222)
		(solder_mask_margin 0.02)
	)
	(pad "N20" smd circle
		(at 4.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.626)
		(solder_mask_margin 0.02)
	)
	(pad "N21" smd circle
		(at 5.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.801)
		(solder_mask_margin 0.02)
	)
	(pad "N22" smd circle
		(at 6.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.991)
		(solder_mask_margin 0.02)
	)
	(pad "N23" smd circle
		(at 7.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N24" smd circle
		(at 8.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.575)
		(solder_mask_margin 0.02)
	)
	(pad "N25" smd circle
		(at 9.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.113)
		(solder_mask_margin 0.02)
	)
	(pad "N26" smd circle
		(at 10.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.64)
		(solder_mask_margin 0.02)
	)
	(pad "N27" smd circle
		(at 11.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.775)
		(solder_mask_margin 0.02)
	)
	(pad "N28" smd circle
		(at 12.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "N29" smd circle
		(at 13.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.115)
		(solder_mask_margin 0.02)
	)
	(pad "N30" smd circle
		(at 14.5 -2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.693)
		(solder_mask_margin 0.02)
	)
	(pad "P1" smd circle
		(at -14.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.527)
		(solder_mask_margin 0.02)
	)
	(pad "P2" smd circle
		(at -13.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.639)
		(solder_mask_margin 0.02)
	)
	(pad "P3" smd circle
		(at -12.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P4" smd circle
		(at -11.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P5" smd circle
		(at -10.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.032)
		(solder_mask_margin 0.02)
	)
	(pad "P6" smd circle
		(at -9.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.187)
		(solder_mask_margin 0.02)
	)
	(pad "P7" smd circle
		(at -8.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P8" smd circle
		(at -7.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P9" smd circle
		(at -6.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P10" smd circle
		(at -5.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P11" smd circle
		(at -4.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P12" smd circle
		(at -3.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P13" smd circle
		(at -2.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P14" smd circle
		(at -1.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P15" smd circle
		(at -0.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P16" smd circle
		(at 0.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P17" smd circle
		(at 1.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P18" smd circle
		(at 2.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P19" smd circle
		(at 3.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.83)
		(solder_mask_margin 0.02)
	)
	(pad "P20" smd circle
		(at 4.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P21" smd circle
		(at 5.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.84)
		(solder_mask_margin 0.02)
	)
	(pad "P22" smd circle
		(at 6.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.806)
		(solder_mask_margin 0.02)
	)
	(pad "P23" smd circle
		(at 7.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.753)
		(solder_mask_margin 0.02)
	)
	(pad "P24" smd circle
		(at 8.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.124)
		(solder_mask_margin 0.02)
	)
	(pad "P25" smd circle
		(at 9.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "P26" smd circle
		(at 10.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.193)
		(solder_mask_margin 0.02)
	)
	(pad "P27" smd circle
		(at 11.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.077)
		(solder_mask_margin 0.02)
	)
	(pad "P28" smd circle
		(at 12.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.693)
		(solder_mask_margin 0.02)
	)
	(pad "P29" smd circle
		(at 13.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.815)
		(solder_mask_margin 0.02)
	)
	(pad "P30" smd circle
		(at 14.5 -1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R1" smd circle
		(at -14.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R2" smd circle
		(at -13.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R3" smd circle
		(at -12.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.761)
		(solder_mask_margin 0.02)
	)
	(pad "R4" smd circle
		(at -11.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.836)
		(solder_mask_margin 0.02)
	)
	(pad "R5" smd circle
		(at -10.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R6" smd circle
		(at -9.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R7" smd circle
		(at -8.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.794)
		(solder_mask_margin 0.02)
	)
	(pad "R8" smd circle
		(at -7.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.477)
		(solder_mask_margin 0.02)
	)
	(pad "R9" smd circle
		(at -6.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R10" smd circle
		(at -5.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R11" smd circle
		(at -4.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R12" smd circle
		(at -3.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R13" smd circle
		(at -2.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R14" smd circle
		(at -1.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.643)
		(solder_mask_margin 0.02)
	)
	(pad "R15" smd circle
		(at -0.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.522)
		(solder_mask_margin 0.02)
	)
	(pad "R16" smd circle
		(at 0.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R17" smd circle
		(at 1.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R18" smd circle
		(at 2.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R19" smd circle
		(at 3.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.988)
		(solder_mask_margin 0.02)
	)
	(pad "R20" smd circle
		(at 4.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.33)
		(solder_mask_margin 0.02)
	)
	(pad "R21" smd circle
		(at 5.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.937)
		(solder_mask_margin 0.02)
	)
	(pad "R22" smd circle
		(at 6.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R23" smd circle
		(at 7.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.245)
		(solder_mask_margin 0.02)
	)
	(pad "R24" smd circle
		(at 8.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.11)
		(solder_mask_margin 0.02)
	)
	(pad "R25" smd circle
		(at 9.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.823)
		(solder_mask_margin 0.02)
	)
	(pad "R26" smd circle
		(at 10.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.845)
		(solder_mask_margin 0.02)
	)
	(pad "R27" smd circle
		(at 11.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "R28" smd circle
		(at 12.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.17)
		(solder_mask_margin 0.02)
	)
	(pad "R29" smd circle
		(at 13.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.165)
		(solder_mask_margin 0.02)
	)
	(pad "R30" smd circle
		(at 14.5 -0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 16.981)
		(solder_mask_margin 0.02)
	)
	(pad "T1" smd circle
		(at -14.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.793)
		(solder_mask_margin 0.02)
	)
	(pad "T2" smd circle
		(at -13.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.764)
		(solder_mask_margin 0.02)
	)
	(pad "T3" smd circle
		(at -12.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T4" smd circle
		(at -11.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T5" smd circle
		(at -10.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.339)
		(solder_mask_margin 0.02)
	)
	(pad "T6" smd circle
		(at -9.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.521)
		(solder_mask_margin 0.02)
	)
	(pad "T7" smd circle
		(at -8.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T8" smd circle
		(at -7.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T9" smd circle
		(at -6.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T10" smd circle
		(at -5.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T11" smd circle
		(at -4.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T12" smd circle
		(at -3.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T13" smd circle
		(at -2.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T14" smd circle
		(at -1.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.582)
		(solder_mask_margin 0.02)
	)
	(pad "T15" smd circle
		(at -0.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.695)
		(solder_mask_margin 0.02)
	)
	(pad "T16" smd circle
		(at 0.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T17" smd circle
		(at 1.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T18" smd circle
		(at 2.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T19" smd circle
		(at 3.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T20" smd circle
		(at 4.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.515)
		(solder_mask_margin 0.02)
	)
	(pad "T21" smd circle
		(at 5.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.352)
		(solder_mask_margin 0.02)
	)
	(pad "T22" smd circle
		(at 6.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.945)
		(solder_mask_margin 0.02)
	)
	(pad "T23" smd circle
		(at 7.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.494)
		(solder_mask_margin 0.02)
	)
	(pad "T24" smd circle
		(at 8.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T25" smd circle
		(at 9.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.691)
		(solder_mask_margin 0.02)
	)
	(pad "T26" smd circle
		(at 10.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.679)
		(solder_mask_margin 0.02)
	)
	(pad "T27" smd circle
		(at 11.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.259)
		(solder_mask_margin 0.02)
	)
	(pad "T28" smd circle
		(at 12.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.716)
		(solder_mask_margin 0.02)
	)
	(pad "T29" smd circle
		(at 13.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "T30" smd circle
		(at 14.5 0.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 17.602)
		(solder_mask_margin 0.02)
	)
	(pad "U1" smd circle
		(at -14.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U2" smd circle
		(at -13.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U3" smd circle
		(at -12.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.101)
		(solder_mask_margin 0.02)
	)
	(pad "U4" smd circle
		(at -11.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.157)
		(solder_mask_margin 0.02)
	)
	(pad "U5" smd circle
		(at -10.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U6" smd circle
		(at -9.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U7" smd circle
		(at -8.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.79)
		(solder_mask_margin 0.02)
	)
	(pad "U8" smd circle
		(at -7.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.447)
		(solder_mask_margin 0.02)
	)
	(pad "U9" smd circle
		(at -6.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U10" smd circle
		(at -5.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U11" smd circle
		(at -4.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U12" smd circle
		(at -3.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U13" smd circle
		(at -2.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U14" smd circle
		(at -1.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.927)
		(solder_mask_margin 0.02)
	)
	(pad "U15" smd circle
		(at -0.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.856)
		(solder_mask_margin 0.02)
	)
	(pad "U16" smd circle
		(at 0.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U17" smd circle
		(at 1.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U18" smd circle
		(at 2.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U19" smd circle
		(at 3.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.184)
		(solder_mask_margin 0.02)
	)
	(pad "U20" smd circle
		(at 4.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.954)
		(solder_mask_margin 0.02)
	)
	(pad "U21" smd circle
		(at 5.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U22" smd circle
		(at 6.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.116)
		(solder_mask_margin 0.02)
	)
	(pad "U23" smd circle
		(at 7.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.023)
		(solder_mask_margin 0.02)
	)
	(pad "U24" smd circle
		(at 8.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.857)
		(solder_mask_margin 0.02)
	)
	(pad "U25" smd circle
		(at 9.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.788)
		(solder_mask_margin 0.02)
	)
	(pad "U26" smd circle
		(at 10.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "U27" smd circle
		(at 11.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.108)
		(solder_mask_margin 0.02)
	)
	(pad "U28" smd circle
		(at 12.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.478)
		(solder_mask_margin 0.02)
	)
	(pad "U29" smd circle
		(at 13.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.917)
		(solder_mask_margin 0.02)
	)
	(pad "U30" smd circle
		(at 14.5 1.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.496)
		(solder_mask_margin 0.02)
	)
	(pad "V1" smd circle
		(at -14.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.451)
		(solder_mask_margin 0.02)
	)
	(pad "V2" smd circle
		(at -13.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.516)
		(solder_mask_margin 0.02)
	)
	(pad "V3" smd circle
		(at -12.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V4" smd circle
		(at -11.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V5" smd circle
		(at -10.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.463)
		(solder_mask_margin 0.02)
	)
	(pad "V6" smd circle
		(at -9.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.634)
		(solder_mask_margin 0.02)
	)
	(pad "V7" smd circle
		(at -8.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V8" smd circle
		(at -7.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V9" smd circle
		(at -6.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V10" smd circle
		(at -5.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V11" smd circle
		(at -4.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V12" smd circle
		(at -3.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V13" smd circle
		(at -2.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V14" smd circle
		(at -1.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V15" smd circle
		(at -0.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V16" smd circle
		(at 0.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V17" smd circle
		(at 1.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V18" smd circle
		(at 2.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V19" smd circle
		(at 3.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.087)
		(solder_mask_margin 0.02)
	)
	(pad "V20" smd circle
		(at 4.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.502)
		(solder_mask_margin 0.02)
	)
	(pad "V21" smd circle
		(at 5.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.935)
		(solder_mask_margin 0.02)
	)
	(pad "V22" smd circle
		(at 6.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.194)
		(solder_mask_margin 0.02)
	)
	(pad "V23" smd circle
		(at 7.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V24" smd circle
		(at 8.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.102)
		(solder_mask_margin 0.02)
	)
	(pad "V25" smd circle
		(at 9.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.952)
		(solder_mask_margin 0.02)
	)
	(pad "V26" smd circle
		(at 10.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.076)
		(solder_mask_margin 0.02)
	)
	(pad "V27" smd circle
		(at 11.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.112)
		(solder_mask_margin 0.02)
	)
	(pad "V28" smd circle
		(at 12.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "V29" smd circle
		(at 13.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.653)
		(solder_mask_margin 0.02)
	)
	(pad "V30" smd circle
		(at 14.5 2.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.213)
		(solder_mask_margin 0.02)
	)
	(pad "W1" smd circle
		(at -14.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W2" smd circle
		(at -13.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W3" smd circle
		(at -12.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.13)
		(solder_mask_margin 0.02)
	)
	(pad "W4" smd circle
		(at -11.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.15)
		(solder_mask_margin 0.02)
	)
	(pad "W5" smd circle
		(at -10.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W6" smd circle
		(at -9.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W7" smd circle
		(at -8.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.818)
		(solder_mask_margin 0.02)
	)
	(pad "W8" smd circle
		(at -7.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.623)
		(solder_mask_margin 0.02)
	)
	(pad "W9" smd circle
		(at -6.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W10" smd circle
		(at -5.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W11" smd circle
		(at -4.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W12" smd circle
		(at -3.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W13" smd circle
		(at -2.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W14" smd circle
		(at -1.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W15" smd circle
		(at -0.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W16" smd circle
		(at 0.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W17" smd circle
		(at 1.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W18" smd circle
		(at 2.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W19" smd circle
		(at 3.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.678)
		(solder_mask_margin 0.02)
	)
	(pad "W20" smd circle
		(at 4.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W21" smd circle
		(at 5.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.855)
		(solder_mask_margin 0.02)
	)
	(pad "W22" smd circle
		(at 6.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.287)
		(solder_mask_margin 0.02)
	)
	(pad "W23" smd circle
		(at 7.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.317)
		(solder_mask_margin 0.02)
	)
	(pad "W24" smd circle
		(at 8.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.141)
		(solder_mask_margin 0.02)
	)
	(pad "W25" smd circle
		(at 9.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "W26" smd circle
		(at 10.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.963)
		(solder_mask_margin 0.02)
	)
	(pad "W27" smd circle
		(at 11.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.615)
		(solder_mask_margin 0.02)
	)
	(pad "W28" smd circle
		(at 12.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.971)
		(solder_mask_margin 0.02)
	)
	(pad "W29" smd circle
		(at 13.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.012)
		(solder_mask_margin 0.02)
	)
	(pad "W30" smd circle
		(at 14.5 3.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y1" smd circle
		(at -14.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.513)
		(solder_mask_margin 0.02)
	)
	(pad "Y2" smd circle
		(at -13.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.611)
		(solder_mask_margin 0.02)
	)
	(pad "Y3" smd circle
		(at -12.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y4" smd circle
		(at -11.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y5" smd circle
		(at -10.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.381)
		(solder_mask_margin 0.02)
	)
	(pad "Y6" smd circle
		(at -9.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.366)
		(solder_mask_margin 0.02)
	)
	(pad "Y7" smd circle
		(at -8.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y8" smd circle
		(at -7.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y9" smd circle
		(at -6.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y10" smd circle
		(at -5.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.48)
		(solder_mask_margin 0.02)
	)
	(pad "Y11" smd circle
		(at -4.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.911)
		(solder_mask_margin 0.02)
	)
	(pad "Y12" smd circle
		(at -3.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y13" smd circle
		(at -2.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.67)
		(solder_mask_margin 0.02)
	)
	(pad "Y14" smd circle
		(at -1.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.537)
		(solder_mask_margin 0.02)
	)
	(pad "Y15" smd circle
		(at -0.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 15.861)
		(solder_mask_margin 0.02)
	)
	(pad "Y16" smd circle
		(at 0.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.497)
		(solder_mask_margin 0.02)
	)
	(pad "Y17" smd circle
		(at 1.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y18" smd circle
		(at 2.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.661)
		(solder_mask_margin 0.02)
	)
	(pad "Y19" smd circle
		(at 3.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 23.666)
		(solder_mask_margin 0.02)
	)
	(pad "Y20" smd circle
		(at 4.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.993)
		(solder_mask_margin 0.02)
	)
	(pad "Y21" smd circle
		(at 5.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.039)
		(solder_mask_margin 0.02)
	)
	(pad "Y22" smd circle
		(at 6.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y23" smd circle
		(at 7.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.411)
		(solder_mask_margin 0.02)
	)
	(pad "Y24" smd circle
		(at 8.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.014)
		(solder_mask_margin 0.02)
	)
	(pad "Y25" smd circle
		(at 9.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.219)
		(solder_mask_margin 0.02)
	)
	(pad "Y26" smd circle
		(at 10.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.658)
		(solder_mask_margin 0.02)
	)
	(pad "Y27" smd circle
		(at 11.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.02)
	)
	(pad "Y28" smd circle
		(at 12.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.559)
		(solder_mask_margin 0.02)
	)
	(pad "Y29" smd circle
		(at 13.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 14.587)
		(solder_mask_margin 0.02)
	)
	(pad "Y30" smd circle
		(at 14.5 4.5)
		(size 0.5 0.5)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 18.627)
		(solder_mask_margin 0.02)
	)
	(embedded_fonts no)
	(model "antmicro_xc7k410t_2ffg900i.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
