(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "XCAU25P-2FFVB676I"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 63.5 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "XCAU25P-2FFVB676I"
				(at 63.5 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "XCAU25P-2FFVB676I"
				(at 63.5 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.xilinx.com/viewer/book-attachment/2PXOpPtpaABIt0fkzeBLnw/hvbsEUaOT0OxFhln7VEVyA"
				(at 63.5 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Artix UltraScale+ Field Programmable Gate Array"
				(at 63.5 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "XCAU25P-2FFVB676I"
				(at 63.5 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "AMD-Xilinx"
				(at 63.5 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 63.5 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 63.5 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "FPGA, LVDS, MIPI, CMOS, BGA, ETHERNET, VIDEO, DSP, BRIDGE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "XCAU25P-2FFVB676I_1_1"
				(text "CFG"
					(at 15.24 -3.81 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "M1_0")
					(number "AA9")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "M0_0")
					(number "AA10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_0")
					(number "AA11")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "RDWR_FCS_B_0")
					(number "AA12")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PROGRAM_B_0")
					(number "AB9")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "TMS_0")
					(number "AB10")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "DONE_0")
					(number "AB11")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "TDI_0")
					(number "AB12")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "D02_0")
					(number "AC11")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "D01_DIN_0")
					(number "AC12")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "D00_MOSI_0")
					(number "AD11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_0")
					(number "AD12")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "D03_0")
					(number "AE11")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "TCK_0")
					(number "AE12")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "M2_0")
					(number "AF12")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 5.08)
					(name "VREFN")
					(number "P13")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "VP")
					(number "P14")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 5.08)
					(name "VN")
					(number "R13")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 5.08)
					(name "VREFP")
					(number "R14")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "DXN")
					(number "T13")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "DXP")
					(number "T14")
				)
				(pin input line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PUDC_B_0")
					(number "W9")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "INIT_B_0")
					(number "W10")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 5.08)
					(name "TDO_0")
					(number "Y10")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "CCLK_0")
					(number "Y11")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "Y12")
				)
			)
			(symbol "XCAU25P-2FFVB676I_2_1"
				(text "BANK 64"
					(at 30.48 -5.08 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AA17")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AA18")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AA19")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AA20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_64")
					(number "AA21")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AA22")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AB17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "AB18")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AB19")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AB20")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AB21")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AB22")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB24")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AB25")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AB26")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AC16")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AC17")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AC18")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC19")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AC21")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AC22")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AC23")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC24")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AC26")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AD16")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD18")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AD19")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD20")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AD21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "AD22")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AD23")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AD24")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AD25")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AD26")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AE16")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AE17")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AE18")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AE20")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AE21")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AE22")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AE23")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AE25")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AE26")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AF17")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AF18")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AF19")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AF20")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AF22")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AF23")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AF24")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AF25")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_64")
					(number "W18")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "Y17")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "Y18")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "Y20")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "Y21")
				)
			)
			(symbol "XCAU25P-2FFVB676I_3_1"
				(text "BANK 65"
					(at 36.83 -3.81 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_T1U_N12_SMBALERT_65")
					(number "AA23")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_A14_D30_65")
					(number "AA24")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_A15_D31_65")
					(number "AA25")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "N19")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_EMCCLK_65")
					(number "N21")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_DOUT_CSO_B_65")
					(number "N22")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_D04_65")
					(number "N23")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_A02_D18_65")
					(number "N24")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_T2U_N12_CSI_ADV_B_65")
					(number "N26")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_PERSTN1_I2C_SDA_65")
					(number "P19")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_D08_65")
					(number "P20")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_D09_65")
					(number "P21")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_65")
					(number "P22")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_D05_65")
					(number "P23")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_A03_D19_65")
					(number "P24")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_D14_65")
					(number "P25")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_D15_65")
					(number "P26")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_D06_65")
					(number "R20")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_D07_65")
					(number "R21")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_D10_65")
					(number "R22")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_D11_65")
					(number "R23")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_D12_65")
					(number "R25")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_D13_65")
					(number "R26")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_T3U_N12_PERSTN0_65")
					(number "T19")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_A26_65")
					(number "T20")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_A22_65")
					(number "T22")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_A23_65")
					(number "T23")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_A06_D22_65")
					(number "T24")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_A04_D20_65")
					(number "T25")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_RS0_65")
					(number "U19")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_A27_65")
					(number "U20")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_FOE_B_65")
					(number "U21")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_FWE_FCS2_B_65")
					(number "U22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "U23")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_A07_D23_65")
					(number "U24")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_A05_D21_65")
					(number "U25")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_A00_D16_65")
					(number "U26")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_65")
					(number "V18")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_RS1_65")
					(number "V19")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_A24_65")
					(number "V21")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_A25_65")
					(number "V22")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_A10_D26_65")
					(number "V23")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_A08_D24_65")
					(number "V24")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_A01_D17_65")
					(number "V26")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_A20_65")
					(number "W19")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_A21_65")
					(number "W20")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_A28_65")
					(number "W21")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_A11_D27_65")
					(number "W23")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_A09_D25_65")
					(number "W24")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_A12_D28_65")
					(number "W25")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_A13_D29_65")
					(number "W26")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_A18_65")
					(number "Y22")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_A19_65")
					(number "Y23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "Y24")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_A16_65")
					(number "Y25")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_A17_65")
					(number "Y26")
				)
			)
			(symbol "XCAU25P-2FFVB676I_4_1"
				(text "BANK 66"
					(at 30.48 -5.08 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "B25")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B26")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "C24")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "C26")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "D23")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "D24")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "D25")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "D26")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "E23")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_66")
					(number "E24")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "E25")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "E26")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "F22")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "F23")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "F24")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F25")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "G22")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "G24")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "G25")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "G26")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "H21")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "H22")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "H23")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "H24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "H25")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "H26")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_66")
					(number "J18")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "J19")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "J20")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "J21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "J22")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "J23")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "J24")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "J25")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "J26")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "K18")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "K20")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "K21")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "K22")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "K23")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "K25")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "K26")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "L18")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "L19")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "L20")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "L22")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "L23")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "L24")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "L25")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "M19")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "M20")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "M21")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "M22")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "M24")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "M25")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "M26")
				)
			)
			(symbol "XCAU25P-2FFVB676I_5_1"
				(text "BANK 67"
					(at 30.48 -5.08 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_67")
					(number "A15")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_67")
					(number "A17")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_67")
					(number "A18")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_67")
					(number "A19")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_67")
					(number "A20")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_67")
					(number "A22")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_67")
					(number "A23")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_67")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_67")
					(number "A25")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_67")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_T2U_N12_67")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_67")
					(number "B17")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_67")
					(number "B19")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_67")
					(number "B20")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_67")
					(number "B21")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_67")
					(number "B22")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_67")
					(number "B24")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_67")
					(number "C16")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_67")
					(number "C17")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_67")
					(number "C18")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_67")
					(number "C19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_67")
					(number "C20")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_67")
					(number "C21")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_67")
					(number "C22")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_67")
					(number "C23")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_67")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_67")
					(number "D16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_67")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_67")
					(number "D19")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_67")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_67")
					(number "D21")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_67")
					(number "E15")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_67")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_67")
					(number "E17")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_67")
					(number "E18")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_67")
					(number "E20")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_67")
					(number "E21")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_T3U_N12_67")
					(number "E22")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_67")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_67")
					(number "F17")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_67")
					(number "F18")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_67")
					(number "F19")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_67")
					(number "F20")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_67")
					(number "G15")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_67")
					(number "G16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_67")
					(number "G17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "G18")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_T1U_N12_67")
					(number "G19")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_67")
					(number "G20")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_67")
					(number "G21")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_67")
					(number "H16")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_67")
					(number "H17")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_67")
					(number "H18")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_67")
					(number "H19")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_67")
					(number "J16")
				)
			)
			(symbol "XCAU25P-2FFVB676I_6_1"
				(text "BANK 84"
					(at 22.86 -2.54 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L11N_AD1N_84")
					(number "AA13")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_84")
					(number "AA14")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_84")
					(number "AA15")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_84")
					(number "AB14")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_84")
					(number "AB15")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_84")
					(number "AB16")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_84")
					(number "AC13")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_84")
					(number "AC14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_84")
					(number "AC15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4P_AD8P_84")
					(number "AD13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L4N_AD8N_84")
					(number "AD14")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3P_AD9P_84")
					(number "AD15")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2P_AD10P_84")
					(number "AE13")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L3N_AD9N_84")
					(number "AE15")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L2N_AD10N_84")
					(number "AF13")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1P_AD11P_84")
					(number "AF14")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L1N_AD11N_84")
					(number "AF15")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12P_AD0P_84")
					(number "W12")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L12N_AD0N_84")
					(number "W13")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10P_AD2P_84")
					(number "W14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L10N_AD2N_84")
					(number "W15")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9P_AD3P_84")
					(number "W16")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11P_AD1P_84")
					(number "Y13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_84")
					(number "Y14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_84")
					(number "Y15")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L9N_AD3N_84")
					(number "Y16")
				)
			)
			(symbol "XCAU25P-2FFVB676I_7_1"
				(text "BANK 86"
					(at 22.86 -2.54 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L10N_AD2N_86")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L11N_AD1N_86")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10P_AD2P_86")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11P_AD1P_86")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L12N_AD0N_86")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L9N_AD3N_86")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12P_AD0P_86")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9P_AD3P_86")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_86")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_86")
					(number "D11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_86")
					(number "E9")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_86")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_86")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_86")
					(number "F9")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_86")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_86")
					(number "G9")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_86")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L4N_AD8N_86")
					(number "G11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L3N_AD9N_86")
					(number "H9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_86")
					(number "H10")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4P_AD8P_86")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3P_AD9P_86")
					(number "J9")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L2N_AD10N_86")
					(number "J10")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2P_AD10P_86")
					(number "J11")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L1N_AD11N_86")
					(number "K9")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1P_AD11P_86")
					(number "K10")
				)
			)
			(symbol "XCAU25P-2FFVB676I_8_1"
				(text "BANK 87"
					(at 22.86 -2.54 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L11N_AD9N_87")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11P_AD9P_87")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L12N_AD8N_87")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L10N_AD10N_87")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12P_AD8P_87")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10P_AD10P_87")
					(number "C12")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L9N_AD11N_87")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9P_AD11P_87")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L8N_HDGC_87")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8P_HDGC_87")
					(number "D14")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L7N_HDGC_87")
					(number "E12")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7P_HDGC_87")
					(number "E13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_87")
					(number "E14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L5N_HDGC_87")
					(number "F12")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L6N_HDGC_87")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6P_HDGC_87")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5P_HDGC_87")
					(number "G12")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L3N_AD13N_87")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L1N_AD15N_87")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L2N_AD14N_87")
					(number "H13")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3P_AD13P_87")
					(number "H14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_87")
					(number "H15")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1P_AD15P_87")
					(number "J12")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2P_AD14P_87")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L4N_AD12N_87")
					(number "J14")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4P_AD12P_87")
					(number "J15")
				)
			)
			(symbol "XCAU25P-2FFVB676I_9_1"
				(text "GTX 224"
					(at 6.35 2.54 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXN3_224")
					(number "AB1")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYRXP3_224")
					(number "AB2")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "AB6")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "AB7")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYTXN3_224")
					(number "AC4")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYTXP3_224")
					(number "AC5")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYRXN2_224")
					(number "AD1")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXP2_224")
					(number "AD2")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTYTXN2_224")
					(number "AD6")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTYTXP2_224")
					(number "AD7")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXN1_224")
					(number "AE3")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTYRXP1_224")
					(number "AE4")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN1_224")
					(number "AE8")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP1_224")
					(number "AE9")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTYRXN0_224")
					(number "AF1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYRXP0_224")
					(number "AF2")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYTXN0_224")
					(number "AF6")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYTXP0_224")
					(number "AF7")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "Y6")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "Y7")
				)
			)
			(symbol "XCAU25P-2FFVB676I_10_1"
				(text "GTX 225"
					(at 6.35 2.54 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYTXN0_225")
					(number "AA4")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYTXP0_225")
					(number "AA5")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXN3_225")
					(number "P1")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYRXP3_225")
					(number "P2")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYTXN3_225")
					(number "R4")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYTXP3_225")
					(number "R5")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYRXN2_225")
					(number "T1")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXP2_225")
					(number "T2")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTREFCLK1N_225")
					(number "T6")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "MGTREFCLK1P_225")
					(number "T7")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTYTXN2_225")
					(number "U4")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTYTXP2_225")
					(number "U5")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXN1_225")
					(number "V1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTYRXP1_225")
					(number "V2")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTREFCLK0N_225")
					(number "V6")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTREFCLK0P_225")
					(number "V7")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN1_225")
					(number "W4")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP1_225")
					(number "W5")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTYRXN0_225")
					(number "Y1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYRXP0_225")
					(number "Y2")
				)
			)
			(symbol "XCAU25P-2FFVB676I_11_1"
				(text "GTX 226"
					(at 6.35 2.54 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(text ""
					(at 50.8 -31.75 0)
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXN3_226")
					(number "F1")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYRXP3_226")
					(number "F2")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYTXN3_226")
					(number "G4")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYTXP3_226")
					(number "G5")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYRXN2_226")
					(number "H1")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXP2_226")
					(number "H2")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTYTXN2_226")
					(number "J4")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTYTXP2_226")
					(number "J5")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXN1_226")
					(number "K1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTYRXP1_226")
					(number "K2")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN1_226")
					(number "L4")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP1_226")
					(number "L5")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTYRXN0_226")
					(number "M1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYRXP0_226")
					(number "M2")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTREFCLK1N_226")
					(number "M6")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "MGTREFCLK1P_226")
					(number "M7")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYTXN0_226")
					(number "N4")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYTXP0_226")
					(number "N5")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTREFCLK0N_226")
					(number "P6")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTREFCLK0P_226")
					(number "P7")
				)
			)
			(symbol "XCAU25P-2FFVB676I_12_1"
				(text ""
					(at 21.59 -3.175 900)
				)
				(text ""
					(at 21.59 -3.175 900)
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "A1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A2")
				)
				(pin no_connect line
					(at 15.24 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A3")
				)
				(pin no_connect line
					(at 10.16 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A6")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "A7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "AA7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AB5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "AC7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "AD8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTRREF_R")
					(number "AD9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AE7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE24")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF26")
				)
				(pin no_connect line
					(at 17.78 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B1")
				)
				(pin no_connect line
					(at 7.62 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin no_connect line
					(at 20.32 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B6")
				)
				(pin no_connect line
					(at 30.48 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C2")
				)
				(pin no_connect line
					(at 20.32 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C3")
				)
				(pin no_connect line
					(at 10.16 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "C7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C25")
				)
				(pin no_connect line
					(at 22.86 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D1")
				)
				(pin no_connect line
					(at 12.7 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D5")
				)
				(pin no_connect line
					(at 17.78 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D6")
				)
				(pin no_connect line
					(at 27.94 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E3")
				)
				(pin no_connect line
					(at 15.24 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E4")
				)
				(pin no_connect line
					(at 25.4 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "E7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "F5")
				)
				(pin no_connect line
					(at 12.7 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F6")
				)
				(pin no_connect line
					(at 22.86 -27.94 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "G7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "H5")
				)
				(pin no_connect line
					(at 27.94 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H6")
				)
				(pin no_connect line
					(at 25.4 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "J7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "K5")
				)
				(pin no_connect line
					(at 33.02 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K6")
				)
				(pin no_connect line
					(at 30.48 2.54 270)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K8")
				)
				(pin power_in line
					(at 40.64 0 180)
					(length 5.08)
					(name "VCCINT")
					(number "K11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K12")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K14")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K16")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K24")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "L7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L8")
				)
				(pin power_in line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L9")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L13")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L15")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "M5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M8")
				)
				(pin passive line
					(at 40.64 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M10")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M12")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M14")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M16")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M17")
				)
				(pin power_in line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "N7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N8")
				)
				(pin passive line
					(at 40.64 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "N9")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N11")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N12")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GNDADC")
					(number "N13")
				)
				(pin power_in line
					(at 40.64 -20.32 180)
					(length 5.08)
					(name "VCCADC")
					(number "N14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N15")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N17")
				)
				(pin passive line
					(at 40.64 -7.62 180)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "N18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "P5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P8")
				)
				(pin passive line
					(at 40.64 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "P9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P10")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P12")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P16")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P17")
				)
				(pin power_in line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "P18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R6")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "R7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R8")
				)
				(pin power_in line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "R9")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "R10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R11")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "R12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R15")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "R16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R17")
				)
				(pin passive line
					(at 40.64 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "R18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R24")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "T5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T8")
				)
				(pin passive line
					(at 40.64 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "T9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T10")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T12")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T16")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T17")
				)
				(pin passive line
					(at 40.64 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "T18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTVCCAUX_R")
					(number "U7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U8")
				)
				(pin passive line
					(at 40.64 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "U9")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U11")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U13")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U15")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "V5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V8")
				)
				(pin passive line
					(at 40.64 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "V9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V10")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V12")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V14")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V16")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "W7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "RSVDGND")
					(number "W11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "Y5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y8")
				)
				(pin power_in line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "VBATT")
					(number "Y9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y19")
				)
			)
			(embedded_fonts no)
		)
)
