(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "XCVM2202-NSVH1369"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 58.42 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "XCVM2202-NSVH1369"
				(at 58.42 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "XCVM2202-NSVH1369"
				(at 58.42 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.xilinx.com/v/u/en-US/ds950-versal-overview"
				(at 58.42 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FPGA, AMD-Xilinx Versal Adaptive SoC, Prime series, XCVM2202, NSVH1369"
				(at 58.42 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "XCVM2202-1MLINSVH1369"
				(at 58.42 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "AMD-Xilinx"
				(at 58.42 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 58.42 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, IC, FPGA, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "XCVM2202-NSVH1369_1_1"
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_102")
					(number "AA8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_102")
					(number "AA9")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_102")
					(number "AB1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_102")
					(number "AB2")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_102")
					(number "AC4")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_102")
					(number "AC5")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_102")
					(number "AD1")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_102")
					(number "AD2")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_102")
					(number "AE4")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_102")
					(number "AE5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_102")
					(number "AF1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_102")
					(number "AF2")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_102")
					(number "AG4")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_102")
					(number "AG5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_102")
					(number "AH1")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_102")
					(number "AH2")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_102")
					(number "AJ4")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_102")
					(number "AJ5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_102")
					(number "V6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_102")
					(number "V7")
				)
			)
			(symbol "XCVM2202-NSVH1369_2_1"
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_103")
					(number "AA3")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_103")
					(number "AA4")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_103")
					(number "AB6")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_103")
					(number "AB7")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_103")
					(number "P6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_103")
					(number "P7")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_103")
					(number "T1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_103")
					(number "T2")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_103")
					(number "U4")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_103")
					(number "U5")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_103")
					(number "U8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_103")
					(number "U9")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_103")
					(number "V1")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_103")
					(number "V2")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_103")
					(number "W4")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_103")
					(number "W5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_103")
					(number "Y1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_103")
					(number "Y2")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_103")
					(number "Y6")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_103")
					(number "Y7")
				)
			)
			(symbol "XCVM2202-NSVH1369_3_1"
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_104")
					(number "H1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_104")
					(number "H2")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_104")
					(number "J4")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_104")
					(number "J5")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_104")
					(number "K1")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_104")
					(number "K2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_104")
					(number "K6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_104")
					(number "K7")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_104")
					(number "L4")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_104")
					(number "L5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_104")
					(number "M1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_104")
					(number "M2")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_104")
					(number "M6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_104")
					(number "M7")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_104")
					(number "N4")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_104")
					(number "N5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_104")
					(number "P1")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_104")
					(number "P2")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_104")
					(number "R4")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_104")
					(number "R5")
				)
			)
			(symbol "XCVM2202-NSVH1369_4_1"
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_105")
					(number "C8")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_105")
					(number "C9")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_105")
					(number "D1")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_105")
					(number "D2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_105")
					(number "D5")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_105")
					(number "D6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_105")
					(number "E3")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_105")
					(number "E4")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_105")
					(number "E8")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_105")
					(number "E9")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_105")
					(number "F1")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_105")
					(number "F2")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_105")
					(number "F6")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_105")
					(number "F7")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_105")
					(number "G4")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_105")
					(number "G5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_105")
					(number "G8")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_105")
					(number "G9")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_105")
					(number "H6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_105")
					(number "H7")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_AVTTRCAL_RS")
					(number "W8")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_LPD_RREF_RS")
					(number "W9")
				)
			)
			(symbol "XCVM2202-NSVH1369_5_1"
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_RXN3_106")
					(number "A3")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_RXP3_106")
					(number "A4")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_TXN2_106")
					(number "A8")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "GTYP_TXP2_106")
					(number "A9")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_TXN3_106")
					(number "A12")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "GTYP_TXP3_106")
					(number "A13")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_RXN1_106")
					(number "B1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_RXP1_106")
					(number "B2")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_RXN2_106")
					(number "B5")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_RXP2_106")
					(number "B6")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_TXN1_106")
					(number "B10")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_TXP1_106")
					(number "B11")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_RXN0_106")
					(number "C3")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_RXP0_106")
					(number "C4")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_TXN0_106")
					(number "C12")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_TXP0_106")
					(number "C13")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_REFCLKN1_106")
					(number "D10")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_REFCLKP1_106")
					(number "D11")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_REFCLKN0_106")
					(number "F10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_REFCLKP0_106")
					(number "F11")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_AVTTRCAL_RN")
					(number "T6")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_RREF_RN")
					(number "T7")
				)
			)
			(symbol "XCVM2202-NSVH1369_6_1"
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_TXP3_204")
					(number "L33")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_TXN3_204")
					(number "L34")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_RXP3_204")
					(number "M36")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_RXN3_204")
					(number "M37")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_TXP2_204")
					(number "N33")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_TXN2_204")
					(number "N34")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_RXP2_204")
					(number "P36")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_RXN2_204")
					(number "P37")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_TXP1_204")
					(number "R33")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_TXN1_204")
					(number "R34")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_REFCLKP1_204")
					(number "T31")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_REFCLKN1_204")
					(number "T32")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_RXP1_204")
					(number "T36")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_RXN1_204")
					(number "T37")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_TXP0_204")
					(number "U33")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_TXN0_204")
					(number "U34")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_REFCLKP0_204")
					(number "V31")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_REFCLKN0_204")
					(number "V32")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_RXP0_204")
					(number "V36")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_RXN0_204")
					(number "V37")
				)
			)
			(symbol "XCVM2202-NSVH1369_7_1"
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "GTYP_TXP3_205")
					(number "E29")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_TXN3_205")
					(number "E30")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_RXP3_205")
					(number "E34")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_RXN3_205")
					(number "E35")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "GTYP_TXP2_205")
					(number "F31")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_TXN2_205")
					(number "F32")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_RXP2_205")
					(number "F36")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_RXN2_205")
					(number "F37")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_TXP1_205")
					(number "G33")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_TXN1_205")
					(number "G34")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_RXP1_205")
					(number "H36")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_RXN1_205")
					(number "H37")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_TXP0_205")
					(number "J33")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_TXN0_205")
					(number "J34")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_REFCLKP1_205")
					(number "K31")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_REFCLKN1_205")
					(number "K32")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_RXP0_205")
					(number "K36")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_RXN0_205")
					(number "K37")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_REFCLKP0_205")
					(number "M31")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_REFCLKN0_205")
					(number "M32")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_RREF_L")
					(number "P31")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_AVTTRCAL_L")
					(number "P32")
				)
			)
			(symbol "XCVM2202-NSVH1369_8_1"
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_TXP3_206")
					(number "A29")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_TXN3_206")
					(number "A30")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_RXP3_206")
					(number "A34")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_RXN3_206")
					(number "A35")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_TXP2_206")
					(number "B31")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_TXN2_206")
					(number "B32")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_RXP2_206")
					(number "B36")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_RXN2_206")
					(number "B37")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_TXP1_206")
					(number "C29")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_TXN1_206")
					(number "C30")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_RXP1_206")
					(number "C34")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_RXN1_206")
					(number "C35")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_TXP0_206")
					(number "D31")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_TXN0_206")
					(number "D32")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_RXP0_206")
					(number "D36")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_RXN0_206")
					(number "D37")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_REFCLKP1_206")
					(number "G29")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_REFCLKN1_206")
					(number "G30")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_REFCLKP0_206")
					(number "H31")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_REFCLKN0_206")
					(number "H32")
				)
			)
			(symbol "XCVM2202-NSVH1369_9_1"
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_400")
					(number "AB27")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L9P_400")
					(number "AB28")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L8P_400")
					(number "AB29")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L7P_400")
					(number "AB30")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_400")
					(number "AC26")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L9N_400")
					(number "AC27")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L8N_400")
					(number "AC29")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L7N_400")
					(number "AC30")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L4P_400")
					(number "AD26")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L4N_400")
					(number "AD27")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L5P_HDGC_400")
					(number "AD28")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L6P_HDGC_400")
					(number "AD29")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L3P_400")
					(number "AE26")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L5N_HDGC_400")
					(number "AE28")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L6N_HDGC_400")
					(number "AE29")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_400")
					(number "AE30")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L3N_400")
					(number "AF26")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L2P_400")
					(number "AF27")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L1P_400")
					(number "AF28")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 5.08)
					(name "VCCO_400")
					(number "AF29")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_400")
					(number "AF30")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_400")
					(number "AG26")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L2N_400")
					(number "AG27")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L1N_400")
					(number "AG28")
				)
			)
			(symbol "XCVM2202-NSVH1369_10_1"
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L3N_401")
					(number "AA26")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L2P_401")
					(number "AA27")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L2N_401")
					(number "AA28")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 5.08)
					(name "VCCO_401")
					(number "AA29")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_401")
					(number "AA30")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_401")
					(number "AB26")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_401")
					(number "T26")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_401")
					(number "T27")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L8P_401")
					(number "T28")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L7P_401")
					(number "T29")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L9P_401")
					(number "U27")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L8N_401")
					(number "U28")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L7N_401")
					(number "U29")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L4P_401")
					(number "V26")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L9N_401")
					(number "V27")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L6P_HDGC_401")
					(number "V29")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L4N_401")
					(number "W26")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L5P_HDGC_401")
					(number "W27")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L5N_HDGC_401")
					(number "W28")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L6N_HDGC_401")
					(number "W29")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L3P_401")
					(number "Y26")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L1P_401")
					(number "Y28")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L1N_401")
					(number "Y29")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_401")
					(number "Y30")
				)
			)
			(symbol "XCVM2202-NSVH1369_11_1"
				(pin power_in line
					(at 0 -66.04 0)
					(length 5.08)
					(name "VCCO_500")
					(number "AF10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_500")
					(number "AF11")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PMC_MIO25_500")
					(number "E13")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PMC_MIO20_500")
					(number "E14")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PMC_MIO19_500")
					(number "E15")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PMC_MIO13_500")
					(number "E16")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PMC_MIO7_500")
					(number "E18")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PMC_MIO6_500")
					(number "E19")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "PMC_MIO0_500")
					(number "E20")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PMC_MIO24_500")
					(number "F13")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PMC_MIO18_500")
					(number "F15")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PMC_MIO14_500")
					(number "F16")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PMC_MIO12_500")
					(number "F17")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PMC_MIO8_500")
					(number "F18")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PMC_MIO1_500")
					(number "F20")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PMC_MIO23_500")
					(number "G13")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PMC_MIO21_500")
					(number "G14")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PMC_MIO17_500")
					(number "G15")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PMC_MIO11_500")
					(number "G17")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PMC_MIO9_500")
					(number "G18")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PMC_MIO5_500")
					(number "G19")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PMC_MIO2_500")
					(number "G20")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PMC_MIO22_500")
					(number "H14")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PMC_MIO16_500")
					(number "H15")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PMC_MIO15_500")
					(number "H16")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PMC_MIO10_500")
					(number "H17")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PMC_MIO4_500")
					(number "H19")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PMC_MIO3_500")
					(number "H20")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 5.08)
					(name "VP_500")
					(number "V14")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 5.08)
					(name "VREFN_500")
					(number "V15")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 5.08)
					(name "VREFP_500")
					(number "W14")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 5.08)
					(name "VN_500")
					(number "W15")
				)
			)
			(symbol "XCVM2202-NSVH1369_12_1"
				(pin power_in line
					(at 0 -66.04 0)
					(length 5.08)
					(name "VCCO_501")
					(number "AF13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_501")
					(number "AF14")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PMC_MIO48_501")
					(number "D22")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PMC_MIO41_501")
					(number "D23")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PMC_MIO40_501")
					(number "D24")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PMC_MIO32_501")
					(number "D26")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PMC_MIO49_501")
					(number "E21")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PMC_MIO42_501")
					(number "E23")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PMC_MIO39_501")
					(number "E24")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PMC_MIO33_501")
					(number "E25")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PMC_MIO31_501")
					(number "E26")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PMC_MIO50_501")
					(number "F21")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PMC_MIO47_501")
					(number "F22")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PMC_MIO43_501")
					(number "F23")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PMC_MIO34_501")
					(number "F25")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PMC_MIO30_501")
					(number "F26")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "PMC_MIO26_501")
					(number "F27")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PMC_MIO46_501")
					(number "G22")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PMC_MIO44_501")
					(number "G23")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PMC_MIO38_501")
					(number "G24")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PMC_MIO35_501")
					(number "G25")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PMC_MIO27_501")
					(number "G27")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PMC_MIO51_501")
					(number "H21")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PMC_MIO45_501")
					(number "H22")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PMC_MIO37_501")
					(number "H24")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PMC_MIO36_501")
					(number "H25")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PMC_MIO29_501")
					(number "H26")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PMC_MIO28_501")
					(number "H27")
				)
			)
			(symbol "XCVM2202-NSVH1369_13_1"
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "LPD_MIO25_502")
					(number "A15")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "LPD_MIO19_502")
					(number "A16")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "LPD_MIO18_502")
					(number "A17")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "LPD_MIO12_502")
					(number "A18")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "LPD_MIO6_502")
					(number "A20")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "LPD_MIO5_502")
					(number "A21")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "LPD_MIO0_502")
					(number "A22")
				)
				(pin power_in line
					(at 0 -66.04 0)
					(length 5.08)
					(name "VCCO_502")
					(number "AD12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_502")
					(number "AD13")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "LPD_MIO24_502")
					(number "B15")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "LPD_MIO17_502")
					(number "B17")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "LPD_MIO13_502")
					(number "B18")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "LPD_MIO11_502")
					(number "B19")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 5.08)
					(name "LPD_MIO7_502")
					(number "B20")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "LPD_MIO1_502")
					(number "B22")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "LPD_MIO23_502")
					(number "C15")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "LPD_MIO20_502")
					(number "C16")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "LPD_MIO16_502")
					(number "C17")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "LPD_MIO10_502")
					(number "C19")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 5.08)
					(name "LPD_MIO8_502")
					(number "C20")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "LPD_MIO4_502")
					(number "C21")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "LPD_MIO2_502")
					(number "C22")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "LPD_MIO22_502")
					(number "D15")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "LPD_MIO21_502")
					(number "D16")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "LPD_MIO15_502")
					(number "D17")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "LPD_MIO14_502")
					(number "D18")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 5.08)
					(name "LPD_MIO9_502")
					(number "D19")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "LPD_MIO3_502")
					(number "D21")
				)
			)
			(symbol "XCVM2202-NSVH1369_14_1"
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "TDI_503")
					(number "A23")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "RTC_PADI_503")
					(number "A25")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "RTC_PADO_503")
					(number "A26")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "DONE_503")
					(number "A27")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "POR_B_503")
					(number "AC13")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "REF_CLK_503")
					(number "AC14")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VCCO_503")
					(number "AE14")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_503")
					(number "AE15")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "TDO_503")
					(number "B23")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MODE1_503")
					(number "B24")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MODE0_503")
					(number "B25")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "ERROR_OUT_503")
					(number "B27")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MODE2_503")
					(number "C24")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MODE3_503")
					(number "C25")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PUDC_B_503")
					(number "C26")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "TCK_503")
					(number "C27")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "TMS_503")
					(number "D27")
				)
			)
			(symbol "XCVM2202-NSVH1369_15_1"
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_VR_700")
					(number "AF7")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M0P36_700")
					(number "AG7")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M0P37_700")
					(number "AH8")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M0P40_700")
					(number "AJ7")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M0P38_700")
					(number "AJ8")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M0P42_700")
					(number "AK1")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M0P44_700")
					(number "AK2")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M0P41_700")
					(number "AK7")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M0P39_700")
					(number "AK8")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M0P43_700")
					(number "AL1")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M0P45_700")
					(number "AL2")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M0P46_700")
					(number "AL3")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M0P47_700")
					(number "AL4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M0P28_700")
					(number "AL5")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M0P30_700")
					(number "AL6")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M0P32_700")
					(number "AL7")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M0P34_700")
					(number "AL8")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M0P24_700")
					(number "AM2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M0P26_700")
					(number "AM3")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M0P48_700")
					(number "AM4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M0P29_700")
					(number "AM5")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M0P31_700")
					(number "AM7")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M0P33_700")
					(number "AM8")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M0P35_700")
					(number "AM9")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M0P25_700")
					(number "AN1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M0P27_700")
					(number "AN2")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M0P49_700")
					(number "AN4")
				)
				(pin power_in line
					(at 0 -139.7 0)
					(length 5.08)
					(name "VCCO_700")
					(number "AN5")
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_700")
					(number "AN6")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M0P52_700")
					(number "AN7")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M0P12_700")
					(number "AP1")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M0P14_700")
					(number "AP2")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M0P50_700")
					(number "AP3")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M0P51_700")
					(number "AP4")
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_700")
					(number "AP6")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M0P53_700")
					(number "AP7")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M0P20_700")
					(number "AP8")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M0P13_700")
					(number "AR1")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M0P15_700")
					(number "AR3")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M0P16_700")
					(number "AR4")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M0P18_700")
					(number "AR5")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M0P19_700")
					(number "AR6")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M0P21_700")
					(number "AR8")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M0P22_700")
					(number "AR9")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M0P0_700")
					(number "AT1")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M0P2_700")
					(number "AT2")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M0P4_700")
					(number "AT3")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M0P17_700")
					(number "AT5")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M0P6_700")
					(number "AT6")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M0P8_700")
					(number "AT7")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M0P23_700")
					(number "AT8")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M0P1_700")
					(number "AU2")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M0P3_700")
					(number "AU3")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M0P5_700")
					(number "AU4")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M0P7_700")
					(number "AU5")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M0P9_700")
					(number "AU7")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M0P10_700")
					(number "AU8")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M0P11_700")
					(number "AU9")
				)
			)
			(symbol "XCVM2202-NSVH1369_16_1"
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M0P78_701")
					(number "AG9")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M0P80_701")
					(number "AG10")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M0P90_701")
					(number "AG12")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M0P91_701")
					(number "AG13")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M0P92_701")
					(number "AG15")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M0P79_701")
					(number "AH9")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M0P81_701")
					(number "AH11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M0P82_701")
					(number "AH12")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M0P94_701")
					(number "AH14")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M0P93_701")
					(number "AH15")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M0P84_701")
					(number "AJ10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M0P83_701")
					(number "AJ11")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M0P96_701")
					(number "AJ13")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M0P95_701")
					(number "AJ14")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M0P85_701")
					(number "AK9")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M0P86_701")
					(number "AK10")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M0P88_701")
					(number "AK11")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M0P97_701")
					(number "AK13")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M0P98_701")
					(number "AK14")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M0P100_701")
					(number "AK15")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M0P87_701")
					(number "AL10")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M0P89_701")
					(number "AL11")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M0P104_701")
					(number "AL12")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M0P99_701")
					(number "AL13")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M0P101_701")
					(number "AL15")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M0P54_701")
					(number "AM10")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M0P105_701")
					(number "AM12")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M0P102_701")
					(number "AM13")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M0P103_701")
					(number "AM14")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M0P66_701")
					(number "AM15")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_701")
					(number "AN9")
				)
				(pin power_in line
					(at 0 -137.16 0)
					(length 5.08)
					(name "VCCO_701")
					(number "AN10")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M0P55_701")
					(number "AN11")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M0P106_701")
					(number "AN12")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M0P67_701")
					(number "AN15")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M0P68_701")
					(number "AN16")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_701")
					(number "AP9")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M0P56_701")
					(number "AP11")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M0P107_701")
					(number "AP12")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M0P69_701")
					(number "AP16")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M0P57_701")
					(number "AR10")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M0P58_701")
					(number "AR11")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M0P72_701")
					(number "AR13")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M0P73_701")
					(number "AR14")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M0P74_701")
					(number "AR15")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M0P70_701")
					(number "AR16")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M0P60_701")
					(number "AT10")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M0P59_701")
					(number "AT11")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M0P62_701")
					(number "AT12")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M0P64_701")
					(number "AT13")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M0P75_701")
					(number "AT15")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M0P71_701")
					(number "AT16")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M0P61_701")
					(number "AU10")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M0P63_701")
					(number "AU12")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M0P65_701")
					(number "AU13")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M0P76_701")
					(number "AU14")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M0P77_701")
					(number "AU15")
				)
			)
			(symbol "XCVM2202-NSVH1369_17_1"
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M0P144_702")
					(number "AG16")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M0P146_702")
					(number "AG18")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M0P148_702")
					(number "AG19")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M0P150_702")
					(number "AG21")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M0P151_702")
					(number "AG22")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M0P145_702")
					(number "AH17")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M0P147_702")
					(number "AH18")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M0P149_702")
					(number "AH20")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M0P152_702")
					(number "AH21")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M0P132_702")
					(number "AJ16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M0P133_702")
					(number "AJ17")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M0P134_702")
					(number "AJ19")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M0P136_702")
					(number "AJ20")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M0P153_702")
					(number "AJ22")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M0P142_702")
					(number "AK16")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M0P135_702")
					(number "AK18")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M0P137_702")
					(number "AK19")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M0P154_702")
					(number "AK20")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M0P155_702")
					(number "AK21")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M0P143_702")
					(number "AL16")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M0P140_702")
					(number "AL17")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M0P156_702")
					(number "AL18")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M0P158_702")
					(number "AL20")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M0P160_702")
					(number "AL21")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M0P138_702")
					(number "AL22")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M0P139_702")
					(number "AL23")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M0P141_702")
					(number "AM17")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M0P157_702")
					(number "AM18")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M0P159_702")
					(number "AM19")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M0P161_702")
					(number "AM20")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M0P126_702")
					(number "AM22")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M0P127_702")
					(number "AM23")
				)
				(pin power_in line
					(at 0 -137.16 0)
					(length 5.08)
					(name "VCCO_702")
					(number "AN14")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M0P120_702")
					(number "AN19")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M0P121_702")
					(number "AN20")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M0P128_702")
					(number "AN22")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_702")
					(number "AP13")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_702")
					(number "AP14")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M0P122_702")
					(number "AP19")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M0P129_702")
					(number "AP23")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M0P110_702")
					(number "AR18")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M0P123_702")
					(number "AR19")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M0P124_702")
					(number "AR20")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M0P125_702")
					(number "AR21")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M0P130_702")
					(number "AR23")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M0P108_702")
					(number "AT17")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M0P111_702")
					(number "AT18")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M0P114_702")
					(number "AT20")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M0P116_702")
					(number "AT21")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M0P118_702")
					(number "AT22")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M0P131_702")
					(number "AT23")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M0P109_702")
					(number "AU17")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M0P112_702")
					(number "AU18")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M0P113_702")
					(number "AU19")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M0P115_702")
					(number "AU20")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M0P117_702")
					(number "AU22")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M0P119_702")
					(number "AU23")
				)
			)
			(symbol "XCVM2202-NSVH1369_18_1"
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M1P36_703")
					(number "AG24")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M1P37_703")
					(number "AG25")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M1P46_703")
					(number "AG29")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M1P38_703")
					(number "AH23")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M1P40_703")
					(number "AH24")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M1P42_703")
					(number "AH26")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M1P44_703")
					(number "AH27")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M1P32_703")
					(number "AH29")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M1P47_703")
					(number "AH30")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M1P39_703")
					(number "AJ23")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M1P41_703")
					(number "AJ25")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M1P43_703")
					(number "AJ26")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M1P45_703")
					(number "AJ27")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M1P30_703")
					(number "AJ28")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M1P33_703")
					(number "AJ29")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M1P24_703")
					(number "AK23")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M1P25_703")
					(number "AK24")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M1P26_703")
					(number "AK25")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M1P28_703")
					(number "AK26")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M1P50_703")
					(number "AK28")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M1P31_703")
					(number "AK29")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M1P34_703")
					(number "AK30")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M1P48_703")
					(number "AL25")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M1P27_703")
					(number "AL26")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M1P29_703")
					(number "AL27")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M1P51_703")
					(number "AL28")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M1P35_703")
					(number "AL30")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M1P12_703")
					(number "AM24")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M1P49_703")
					(number "AM25")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M1P52_703")
					(number "AM27")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M1P53_703")
					(number "AM28")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M1P18_703")
					(number "AM29")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M1P19_703")
					(number "AM30")
				)
				(pin power_in line
					(at 0 -137.16 0)
					(length 5.08)
					(name "VCCO_703")
					(number "AN17")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M1P13_703")
					(number "AN24")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M1P16_703")
					(number "AN27")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M1P20_703")
					(number "AN29")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_703")
					(number "AP17")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_703")
					(number "AP18")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M1P14_703")
					(number "AP24")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M1P17_703")
					(number "AP27")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M1P22_703")
					(number "AP28")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M1P21_703")
					(number "AP29")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M1P15_703")
					(number "AR24")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M1P2_703")
					(number "AR25")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M1P4_703")
					(number "AR26")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M1P8_703")
					(number "AR28")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M1P23_703")
					(number "AR29")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M1P3_703")
					(number "AT25")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M1P5_703")
					(number "AT26")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M1P6_703")
					(number "AT27")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M1P9_703")
					(number "AT28")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M1P0_703")
					(number "AU24")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M1P1_703")
					(number "AU25")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M1P7_703")
					(number "AU27")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M1P10_703")
					(number "AU28")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M1P11_703")
					(number "AU29")
				)
			)
			(symbol "XCVM2202-NSVH1369_19_1"
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M1P78_704")
					(number "AJ31")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M1P79_704")
					(number "AJ32")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M1P82_704")
					(number "AJ33")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M1P90_704")
					(number "AJ34")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M1P92_704")
					(number "AJ36")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M1P93_704")
					(number "AJ37")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M1P80_704")
					(number "AK31")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M1P83_704")
					(number "AK33")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M1P91_704")
					(number "AK34")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M1P94_704")
					(number "AK35")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M1P96_704")
					(number "AK36")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M1P81_704")
					(number "AL31")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M1P84_704")
					(number "AL32")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M1P85_704")
					(number "AL33")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M1P95_704")
					(number "AL35")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M1P97_704")
					(number "AL36")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M1P98_704")
					(number "AL37")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M1P86_704")
					(number "AM32")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M1P102_704")
					(number "AM33")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M1P103_704")
					(number "AM34")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M1P100_704")
					(number "AM35")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M1P99_704")
					(number "AM37")
				)
				(pin power_in line
					(at 0 -137.16 0)
					(length 5.08)
					(name "VCCO_704")
					(number "AN21")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M1P88_704")
					(number "AN30")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M1P89_704")
					(number "AN31")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M1P87_704")
					(number "AN32")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M1P104_704")
					(number "AN34")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M1P66_704")
					(number "AN35")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M1P101_704")
					(number "AN36")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M1P68_704")
					(number "AN37")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_704")
					(number "AP21")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_704")
					(number "AP22")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M1P54_704")
					(number "AP31")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M1P106_704")
					(number "AP32")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M1P107_704")
					(number "AP33")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M1P105_704")
					(number "AP34")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M1P67_704")
					(number "AP36")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M1P69_704")
					(number "AP37")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M1P55_704")
					(number "AR30")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M1P58_704")
					(number "AR31")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M1P60_704")
					(number "AR33")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M1P72_704")
					(number "AR34")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M1P73_704")
					(number "AR35")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M1P70_704")
					(number "AR36")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M1P56_704")
					(number "AT30")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M1P59_704")
					(number "AT31")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M1P62_704")
					(number "AT32")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M1P61_704")
					(number "AT33")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M1P74_704")
					(number "AT35")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M1P71_704")
					(number "AT36")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M1P76_704")
					(number "AT37")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M1P57_704")
					(number "AU30")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M1P63_704")
					(number "AU32")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M1P64_704")
					(number "AU33")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M1P65_704")
					(number "AU34")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M1P75_704")
					(number "AU35")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M1P77_704")
					(number "AU36")
				)
			)
			(symbol "XCVM2202-NSVH1369_20_1"
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M1P152_705")
					(number "AA31")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M1P153_705")
					(number "AA32")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M1P140_705")
					(number "AA33")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M1P128_705")
					(number "AA35")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M1P129_705")
					(number "AA36")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M1P118_705")
					(number "AA37")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M1P138_705")
					(number "AB32")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M1P139_705")
					(number "AB33")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M1P160_705")
					(number "AB34")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M1P161_705")
					(number "AB35")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M1P117_705")
					(number "AB37")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M1P150_705")
					(number "AC31")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M1P151_705")
					(number "AC32")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M1P158_705")
					(number "AC34")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M1P159_705")
					(number "AC35")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M1P116_705")
					(number "AC36")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M1P115_705")
					(number "AC37")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M1P149_705")
					(number "AD31")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M1P136_705")
					(number "AD32")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M1P137_705")
					(number "AD33")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M1P157_705")
					(number "AD34")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M1P114_705")
					(number "AD36")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M1P113_705")
					(number "AD37")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M1P148_705")
					(number "AE31")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M1P156_705")
					(number "AE33")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M1P126_705")
					(number "AE34")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M1P127_705")
					(number "AE35")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M1P112_705")
					(number "AE36")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M1P146_705")
					(number "AF31")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M1P147_705")
					(number "AF32")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M1P135_705")
					(number "AF33")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M1P124_705")
					(number "AF35")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M1P125_705")
					(number "AF36")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M1P111_705")
					(number "AF37")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M1P144_705")
					(number "AG30")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M1P133_705")
					(number "AG32")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M1P134_705")
					(number "AG33")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M1P122_705")
					(number "AG34")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M1P123_705")
					(number "AG35")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M1P110_705")
					(number "AG37")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M1P145_705")
					(number "AH31")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M1P132_705")
					(number "AH32")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M1P120_705")
					(number "AH34")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M1P121_705")
					(number "AH35")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M1P108_705")
					(number "AH36")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M1P109_705")
					(number "AH37")
				)
				(pin power_in line
					(at 0 -137.16 0)
					(length 5.08)
					(name "VCCO_705")
					(number "AN25")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_705")
					(number "AN26")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_705")
					(number "AP26")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M1P143_705")
					(number "W34")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M1P154_705")
					(number "Y31")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M1P155_705")
					(number "Y32")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M1P142_705")
					(number "Y33")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M1P141_705")
					(number "Y34")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M1P130_705")
					(number "Y35")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M1P131_705")
					(number "Y36")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M1P119_705")
					(number "Y37")
				)
			)
			(symbol "XCVM2202-NSVH1369_21_1"
				(pin power_in line
					(at 0 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "A1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_AVCC_RS")
					(number "AA7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA10")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "VCC_CPM5")
					(number "AA11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA12")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 5.08)
					(name "VCCINT")
					(number "AA13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA14")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA16")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VCCAUX")
					(number "AA17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA18")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AA19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA20")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AA21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA22")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 5.08)
					(name "VCC_RAM")
					(number "AA23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA24")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 5.08)
					(name "VCC_SOC")
					(number "AA25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB10")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 5.08)
					(name "VCCAUX_PMC")
					(number "AB11")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "VCC_BATT")
					(number "AB12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB13")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCC_RS")
					(number "AC7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC8")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 5.08)
					(name "VCC_PSFP")
					(number "AC9")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_PMC")
					(number "AC10")
				)
				(pin power_in line
					(at 0 -58.42 0)
					(length 5.08)
					(name "VCC_PSLP")
					(number "AC11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC22")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC24")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AC25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD4")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_AVTT_RS")
					(number "AD5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD8")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSLP")
					(number "AD9")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSFP")
					(number "AD10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD14")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "VCC_FUSE")
					(number "AD15")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD17")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD18")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD20")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD21")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD23")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD24")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE6")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "VCC_PMC")
					(number "AE7")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PMC")
					(number "AE8")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSLP")
					(number "AE9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE10")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSFP")
					(number "AE11")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSFP")
					(number "AE12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE16")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AE17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE22")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RS")
					(number "AF5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF6")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PMC")
					(number "AF8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF15")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "VCC_IO")
					(number "AF16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF17")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AF18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF19")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AF20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF21")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AF22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF23")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AF24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RS")
					(number "AH5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G28")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_AVCCAUX_L")
					(number "G31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_AVTT_RN")
					(number "H5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H10")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "RSVD_GND_SENSE")
					(number "H11")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "RSVD_VCCINT_SENSE")
					(number "H12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H30")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_AVTT_L")
					(number "H33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_AVCCAUX_RN")
					(number "J7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J8")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J14")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J22")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J26")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J28")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "J29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J30")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCCAUX_L")
					(number "J31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_RN")
					(number "K5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K9")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K13")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K25")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K27")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "K28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K30")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_L")
					(number "K33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCCAUX_RN")
					(number "L7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L8")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L14")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L22")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L26")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L28")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "L29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L30")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_AVCC_L")
					(number "L31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_RN")
					(number "M5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M9")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M11")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M13")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M25")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M27")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M30")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_L")
					(number "M33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_AVCC_RN")
					(number "N7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N8")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N14")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N22")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N26")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N28")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N30")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCC_L")
					(number "N31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_RN")
					(number "P5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P9")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P11")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P13")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P25")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P27")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P30")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_L")
					(number "P33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCC_RN")
					(number "R7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R8")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R10")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R12")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R14")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R16")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R18")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R20")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R22")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R24")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R26")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R28")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "R29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R30")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCC_L")
					(number "R31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RS")
					(number "T5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T8")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T11")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T13")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T30")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_L")
					(number "T33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCC_RS")
					(number "U7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U13")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VCCAUX_SMON")
					(number "U14")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GND_SMON")
					(number "U15")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VCC_RAM")
					(number "U23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U30")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCC_L")
					(number "U31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RS")
					(number "V5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V8")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_AVCCAUX_RS")
					(number "V9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "V12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V13")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W1")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCC_RS")
					(number "W7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W10")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "W11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VCC_RAM")
					(number "W23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W33")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCCAUX_RS")
					(number "Y9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y11")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "Y12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y13")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "RSVDGND")
					(number "Y14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(hide yes)
					(name "RSVDGND")
					(number "Y15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y18")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y27")
				)
			)
			(embedded_fonts no)
		)
)
