(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "XCVP1202-2MSEVSVA2785"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 68.58 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "XCVP1202-2MSEVSVA2785"
				(at 68.58 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "XCVP1202-2MSEVSVA2785"
				(at 68.58 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.xilinx.com/r/en-US/ug1568-vpk120-eval-bd/Introduction"
				(at 68.58 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FPGA Xilinx Versal, 1969240 logic cells, BGA2809"
				(at 68.58 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "AMD-Xilinx"
				(at 68.58 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "XCVP1202-2MSEVSVA2785"
				(at 68.58 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 68.58 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 68.58 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, IC, FPGA, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "XCVP1202-2MSEVSVA2785_1_1"
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A10")
				)
				(pin power_in line
					(at 0 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "A11")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A13")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A34")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A36")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA11")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_AVTT_RUC")
					(number "AA12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA17")
				)
				(pin power_in line
					(at 0 -36.83 0)
					(length 5.08)
					(name "VCCINT")
					(number "AA18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA23")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA25")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA27")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA29")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA31")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA37")
				)
				(pin power_in line
					(at 0 -39.37 0)
					(length 5.08)
					(name "VCCINT_GT")
					(number "AA38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA42")
				)
				(pin power_in line
					(at 52.07 -13.97 180)
					(length 5.08)
					(name "GTM_AVTT_LC")
					(number "AA45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_AVCC_RUC")
					(number "AB11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB16")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB22")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB24")
				)
				(pin power_in line
					(at 0 -72.39 0)
					(length 5.08)
					(name "VCC_SOC")
					(number "AB25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB26")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AB27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB28")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AB29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB30")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB36")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "AB37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB42")
				)
				(pin passive line
					(at 52.07 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LC")
					(number "AB43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_AVCCAUX_RUC")
					(number "AC12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC14")
				)
				(pin power_in line
					(at 0 -67.31 0)
					(length 5.08)
					(name "VCC_PSLP")
					(number "AC16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC17")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC23")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AC24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC25")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AC26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC27")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AC28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC29")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AC30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC31")
				)
				(pin power_in line
					(at 0 -69.85 0)
					(length 5.08)
					(name "VCC_RAM")
					(number "AC32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC37")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 5.08)
					(name "VCCAUX")
					(number "AC38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC42")
				)
				(pin passive line
					(at 52.07 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LC")
					(number "AC45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCCAUX_RUC")
					(number "AD11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD13")
				)
				(pin power_in line
					(at 0 -57.15 0)
					(length 5.08)
					(name "VCC_FUSE")
					(number "AD14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD15")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSLP")
					(number "AD16")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD20")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD22")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD23")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AD31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD36")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "AD37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD43")
				)
				(pin passive line
					(at 52.07 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LC")
					(number "AD44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE9")
				)
				(pin power_in line
					(at 52.07 -77.47 180)
					(length 5.08)
					(name "GTYP_LPD_AVTT_RLC")
					(number "AE12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSLP")
					(number "AE15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE17")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE31")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 5.08)
					(hide yes)
					(name "VCC_RAM")
					(number "AE32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE37")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AE38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE44")
				)
				(pin passive line
					(at 52.07 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LC")
					(number "AE45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF10")
				)
				(pin passive line
					(at 52.07 -77.47 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RLC")
					(number "AF11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 0 -64.77 0)
					(length 5.08)
					(name "VCC_PSFP")
					(number "AF15")
				)
				(pin power_in line
					(at 0 -52.07 0)
					(length 5.08)
					(name "VCC_BATT")
					(number "AF16")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF20")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF22")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AF23")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AF31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF36")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "AF37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF43")
				)
				(pin power_in line
					(at 52.07 -8.89 180)
					(length 5.08)
					(name "GTM_AVCC_LC")
					(number "AF44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG9")
				)
				(pin passive line
					(at 52.07 -77.47 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RLC")
					(number "AG12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG13")
				)
				(pin power_in line
					(at 0 -62.23 0)
					(length 5.08)
					(name "VCC_PMC")
					(number "AG14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG15")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSFP")
					(number "AG16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG17")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 5.08)
					(name "VCCAUX_PMC")
					(number "AG18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG31")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 5.08)
					(hide yes)
					(name "VCC_RAM")
					(number "AG32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG37")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AG38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG45")
				)
				(pin passive line
					(at 52.07 -8.89 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCC_LC")
					(number "AG46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH7")
				)
				(pin power_in line
					(at 52.07 -58.42 180)
					(length 5.08)
					(name "GTYP_LPD_AVCCAUX_RLC")
					(number "AH10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH13")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PMC")
					(number "AH14")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PMC")
					(number "AH15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH16")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSFP")
					(number "AH17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH20")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH22")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AH23")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AH31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH36")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "AH37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH46")
				)
				(pin passive line
					(at 52.07 -8.89 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCC_LC")
					(number "AH47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ8")
				)
				(pin power_in line
					(at 52.07 -68.58 180)
					(length 5.08)
					(name "GTYP_LPD_AVCC_RLC")
					(number "AJ9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ14")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSFP")
					(number "AJ16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ17")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_PMC")
					(number "AJ18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ31")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 5.08)
					(hide yes)
					(name "VCC_RAM")
					(number "AJ32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ37")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AJ38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ45")
				)
				(pin power_in line
					(at 52.07 -6.35 180)
					(length 5.08)
					(name "GTM_AVCCAUX_LC")
					(number "AJ46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK7")
				)
				(pin passive line
					(at 52.07 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCCAUX_RLC")
					(number "AK10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK16")
				)
				(pin power_in line
					(at 0 -54.61 0)
					(length 5.08)
					(name "VCC_CPM5")
					(number "AK17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK20")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK22")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AK23")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AK31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK36")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "AK37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK46")
				)
				(pin passive line
					(at 52.07 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCCAUX_LC")
					(number "AK47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL8")
				)
				(pin passive line
					(at 52.07 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCC_RLC")
					(number "AL9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL13")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "AL16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL17")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "AL18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AL20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AL22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL23")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AL24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL25")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AL26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL27")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AL28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL29")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AL30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL31")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 5.08)
					(hide yes)
					(name "VCC_RAM")
					(number "AL32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AL34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AL36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL37")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AL38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL45")
				)
				(pin power_in line
					(at 52.07 -50.8 180)
					(length 5.08)
					(name "GTYP_AVTT_LS")
					(number "AL46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM7")
				)
				(pin power_in line
					(at 52.07 -71.12 180)
					(length 5.08)
					(name "GTYP_LPD_AVCC_RS")
					(number "AM10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM16")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "AM17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM20")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM22")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM24")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM26")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM28")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM30")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AM35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM36")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "AM37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM46")
				)
				(pin power_in line
					(at 52.07 -45.72 180)
					(length 5.08)
					(name "GTYP_AVCC_LS")
					(number "AM47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN8")
				)
				(pin passive line
					(at 52.07 -71.12 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCC_RS")
					(number "AN9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN15")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "AN16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN17")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "AN18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN20")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN23")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN24")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN26")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN27")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN29")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN30")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AN36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN37")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AN38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN45")
				)
				(pin passive line
					(at 52.07 -50.8 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_LS")
					(number "AN46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP16")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(hide yes)
					(name "VCC_CPM5")
					(number "AP17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP22")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP24")
				)
				(pin power_in line
					(at 0 -59.69 0)
					(length 5.08)
					(name "VCC_IO")
					(number "AP25")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AP26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP27")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AP28")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AP29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP30")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP31")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AP35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP36")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "AP37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP46")
				)
				(pin passive line
					(at 52.07 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCC_LS")
					(number "AP47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR14")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR17")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR19")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR20")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR22")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR23")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR25")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AR26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR28")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(hide yes)
					(name "VCC_IO")
					(number "AR29")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR31")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR32")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR34")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR35")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR37")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 5.08)
					(hide yes)
					(name "VCC_SOC")
					(number "AR38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR45")
				)
				(pin passive line
					(at 52.07 -50.8 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_LS")
					(number "AR46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT46")
				)
				(pin power_in line
					(at 52.07 -40.64 180)
					(length 5.08)
					(name "GTYP_AVCCAUX_LS")
					(number "AT47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV6")
				)
				(pin power_in line
					(at 52.07 -80.01 180)
					(length 5.08)
					(name "GTYP_LPD_AVTT_RS")
					(number "AV7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV46")
				)
				(pin passive line
					(at 52.07 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCCAUX_LS")
					(number "AV47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY6")
				)
				(pin passive line
					(at 52.07 -80.01 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RS")
					(number "AY7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B34")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B36")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB6")
				)
				(pin passive line
					(at 52.07 -80.01 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVTT_RS")
					(number "BB7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD6")
				)
				(pin power_in line
					(at 52.07 -60.96 180)
					(length 5.08)
					(name "GTYP_LPD_AVCCAUX_RS")
					(number "BD7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF6")
				)
				(pin passive line
					(at 52.07 -60.96 180)
					(length 5.08)
					(hide yes)
					(name "GTYP_LPD_AVCCAUX_RS")
					(number "BF7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BG51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BH53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BJ51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BK53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BL52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BM51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BN50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C2")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C4")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C35")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C41")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D2")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D12")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D14")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D35")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D37")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D41")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D43")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D45")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D53")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E1")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E12")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E14")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E37")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E43")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E45")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E51")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E52")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F2")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F3")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F13")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F34")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F36")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "F50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F53")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G1")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G13")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G34")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G36")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G51")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G52")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H2")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H3")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H10")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H35")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H53")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J1")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J36")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J41")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J44")
				)
				(pin power_in line
					(at 52.07 -11.43 180)
					(length 5.08)
					(name "GTM_AVCC_LN")
					(number "J45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J51")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J52")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K4")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K41")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K45")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K46")
				)
				(pin passive line
					(at 52.07 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCC_LN")
					(number "K47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K53")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L1")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L37")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L44")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 5.08)
					(name "GTM_AVTT_LN")
					(number "L45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L51")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L52")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M2")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M3")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M35")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M42")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M45")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M46")
				)
				(pin passive line
					(at 52.07 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCC_LN")
					(number "M47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "M50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M53")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N1")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N43")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N44")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LN")
					(number "N45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N51")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N52")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P3")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P4")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P26")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P36")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P42")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LN")
					(number "P43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P45")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P46")
				)
				(pin passive line
					(at 52.07 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCC_LN")
					(number "P47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P50")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P53")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R1")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R29")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R34")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R38")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R43")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R44")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LN")
					(number "R45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R51")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R52")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T2")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T3")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T32")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T37")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T42")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LN")
					(number "T43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T44")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T45")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T46")
				)
				(pin passive line
					(at 52.07 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCC_LN")
					(number "T47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "T50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T53")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U1")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U9")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U10")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U35")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U42")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U43")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U44")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LN")
					(number "U45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U46")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U51")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U52")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "U53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V7")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_RUC")
					(number "V11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V18")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V42")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 5.08)
					(name "GTM_AVCCAUX_LN")
					(number "V43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V48")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V49")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V53")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W4")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W5")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W6")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W8")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVTT_RUC")
					(number "W12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W16")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W19")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W20")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W22")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W23")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W25")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W26")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W28")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W29")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W31")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W33")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W34")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W36")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W37")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_GT")
					(number "W38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W40")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W42")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "GTM_AVTT_LN")
					(number "W45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W46")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W47")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W50")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W51")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y1")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y3")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "Y4")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "Y5")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y6")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y7")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GTYP_AVCC_RUC")
					(number "Y11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y12")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y13")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y14")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y17")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y18")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y19")
				)
				(pin power_in line
					(at 0 -26.67 0)
					(length 5.08)
					(name "VCCAUX_SMON")
					(number "Y20")
				)
				(pin power_in line
					(at 52.07 0 180)
					(length 5.08)
					(name "GND_SMON")
					(number "Y21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y22")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y23")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y24")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y26")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y27")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y28")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y29")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y30")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y33")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y35")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y36")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y37")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y38")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "Y39")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "Y40")
				)
				(pin no_connect line
					(at 5.08 -82.55 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "Y41")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y42")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "GTM_AVCCAUX_LN")
					(number "Y43")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y44")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y48")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y49")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y52")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y53")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_2_1"
				(text "BANK 102"
					(at 30.48 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_102")
					(number "AP8")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_102")
					(number "AP9")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_102")
					(number "AU6")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_102")
					(number "AU7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_102")
					(number "BB3")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_102")
					(number "BB4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_102")
					(number "BC1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_102")
					(number "BC2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_102")
					(number "BD4")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_102")
					(number "BD5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_102")
					(number "BE1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_102")
					(number "BE2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_102")
					(number "BE6")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_102")
					(number "BE7")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_102")
					(number "BF4")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_102")
					(number "BF5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_102")
					(number "BG1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_102")
					(number "BG2")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_102")
					(number "BG6")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_102")
					(number "BG7")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_3_1"
				(text "BANK 103"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_103")
					(number "AH8")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_103")
					(number "AH9")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_103")
					(number "AK8")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_103")
					(number "AK9")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_103")
					(number "AU1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_103")
					(number "AU2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_103")
					(number "AV4")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_103")
					(number "AV5")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_103")
					(number "AW1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_103")
					(number "AW2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_103")
					(number "AW6")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_103")
					(number "AW7")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_103")
					(number "AY3")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_103")
					(number "AY4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_103")
					(number "BA1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_103")
					(number "BA2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_103")
					(number "BA6")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_103")
					(number "BA7")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_103")
					(number "BC6")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_103")
					(number "BC7")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_4_1"
				(text "BANK 104"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_104")
					(number "AE10")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_104")
					(number "AE11")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_104")
					(number "AF8")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_104")
					(number "AF9")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_104")
					(number "AJ1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_104")
					(number "AJ2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_104")
					(number "AL1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_104")
					(number "AL2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_104")
					(number "AN1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_104")
					(number "AN2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_104")
					(number "AN6")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_104")
					(number "AN7")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_104")
					(number "AP4")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_104")
					(number "AP5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_104")
					(number "AR1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_104")
					(number "AR2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_104")
					(number "AR6")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_104")
					(number "AR7")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_104")
					(number "AT4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_104")
					(number "AT5")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_5_1"
				(text "BANK 105"
					(at 31.75 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "GTYP_LPD_RXN3_105")
					(number "AC1")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "GTYP_LPD_RXP3_105")
					(number "AC2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN1_105")
					(number "AC10")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP1_105")
					(number "AC11")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "GTYP_LPD_RXN2_105")
					(number "AD3")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "GTYP_LPD_RXP2_105")
					(number "AD4")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKN0_105")
					(number "AD8")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "GTYP_LPD_REFCLKP0_105")
					(number "AD9")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "GTYP_LPD_RXN1_105")
					(number "AE1")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "GTYP_LPD_RXP1_105")
					(number "AE2")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "GTYP_LPD_RXN0_105")
					(number "AG1")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "GTYP_LPD_RXP0_105")
					(number "AG2")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "GTYP_LPD_TXN3_105")
					(number "AJ6")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "GTYP_LPD_TXP3_105")
					(number "AJ7")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "GTYP_LPD_TXN2_105")
					(number "AK4")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "GTYP_LPD_TXP2_105")
					(number "AK5")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "GTYP_LPD_TXN1_105")
					(number "AL6")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "GTYP_LPD_TXP1_105")
					(number "AL7")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "GTYP_LPD_TXN0_105")
					(number "AM4")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "GTYP_LPD_TXP0_105")
					(number "AM5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_LPD_AVTTRCAL_RLC")
					(number "AM8")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "GTYP_LPD_RREF_RLC")
					(number "AM9")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_6_1"
				(text "BANK 106"
					(at 31.75 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "GTYP_RXN1_106")
					(number "AA1")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "GTYP_RXP1_106")
					(number "AA2")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "GTYP_RXN0_106")
					(number "AB3")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "GTYP_RXP0_106")
					(number "AB4")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "GTYP_TXN3_106")
					(number "AE6")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "GTYP_TXP3_106")
					(number "AE7")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "GTYP_TXN2_106")
					(number "AF4")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "GTYP_TXP2_106")
					(number "AF5")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "GTYP_TXN1_106")
					(number "AG6")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "GTYP_TXP1_106")
					(number "AG7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_AVTTRCAL_RUC")
					(number "AG10")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "GTYP_RREF_RUC")
					(number "AG11")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "GTYP_TXN0_106")
					(number "AH4")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "GTYP_TXP0_106")
					(number "AH5")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "GTYP_RXN3_106")
					(number "V3")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "GTYP_RXP3_106")
					(number "V4")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "GTYP_RXN2_106")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "GTYP_RXP2_106")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "GTYP_REFCLKN1_106")
					(number "W10")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "GTYP_REFCLKP1_106")
					(number "W11")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "GTYP_REFCLKN0_106")
					(number "Y8")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "GTYP_REFCLKP0_106")
					(number "Y9")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_7_1"
				(text "BANK 200"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_REFCLKP1_200")
					(number "AU47")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_REFCLKN1_200")
					(number "AU48")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_REFCLKP0_200")
					(number "AW47")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_REFCLKN0_200")
					(number "AW48")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_TXP1_200")
					(number "BG37")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_TXP3_200")
					(number "BG39")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_TXN1_200")
					(number "BH37")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_TXN3_200")
					(number "BH39")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_TXP0_200")
					(number "BJ36")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_TXP2_200")
					(number "BJ38")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_TXN0_200")
					(number "BK36")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_TXN2_200")
					(number "BK38")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_RXP0_200")
					(number "BM37")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_RXP1_200")
					(number "BM39")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_RXP2_200")
					(number "BM41")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_RXP3_200")
					(number "BM43")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_RXN0_200")
					(number "BN37")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_RXN1_200")
					(number "BN39")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_RXN2_200")
					(number "BN41")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_RXN3_200")
					(number "BN43")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_8_1"
				(text "BANK 201"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTYP_RREF_LS")
					(number "AL47")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "GTYP_AVTTRCAL_LS")
					(number "AL48")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTYP_REFCLKP1_201")
					(number "AN47")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTYP_REFCLKN1_201")
					(number "AN48")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTYP_REFCLKP0_201")
					(number "AR47")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTYP_REFCLKN0_201")
					(number "AR48")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTYP_TXP1_201")
					(number "BG41")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "GTYP_TXP3_201")
					(number "BG43")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTYP_TXN1_201")
					(number "BH41")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTYP_TXN3_201")
					(number "BH43")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTYP_TXP0_201")
					(number "BJ40")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "GTYP_TXP2_201")
					(number "BJ42")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTYP_TXN0_201")
					(number "BK40")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTYP_TXN2_201")
					(number "BK42")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTYP_RXP0_201")
					(number "BK44")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTYP_RXP2_201")
					(number "BK46")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTYP_RXN0_201")
					(number "BL44")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTYP_RXN2_201")
					(number "BL46")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTYP_RXP1_201")
					(number "BM45")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTYP_RXP3_201")
					(number "BM47")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTYP_RXN1_201")
					(number "BN45")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTYP_RXN3_201")
					(number "BN47")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_9_1"
				(text "BANK 202"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTM_REFCLKP1_202")
					(number "AG47")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTM_REFCLKN1_202")
					(number "AG48")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTM_REFCLKP0_202")
					(number "AJ47")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTM_REFCLKN0_202")
					(number "AJ48")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTM_TXP3_202")
					(number "BF49")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTM_TXN3_202")
					(number "BF50")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTM_TXP0_202")
					(number "BG45")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTM_TXP1_202")
					(number "BG47")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTM_TXN0_202")
					(number "BH45")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTM_TXN1_202")
					(number "BH47")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTM_RXP3_202")
					(number "BH50")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTM_RXN3_202")
					(number "BH51")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTM_TXP2_202")
					(number "BJ48")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTM_RXP2_202")
					(number "BJ52")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTM_RXN2_202")
					(number "BJ53")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTM_TXN2_202")
					(number "BK48")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTM_RXP1_202")
					(number "BK50")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTM_RXN1_202")
					(number "BK51")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTM_RXP0_202")
					(number "BM49")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTM_RXN0_202")
					(number "BN49")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_10_1"
				(text "BANK 203"
					(at 31.75 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "GTM_RREF_LC")
					(number "AC43")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "GTM_AVTTRCAL_LC")
					(number "AC44")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "GTM_REFCLKP1_203")
					(number "AD45")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "GTM_REFCLKN1_203")
					(number "AD46")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "GTM_REFCLKP0_203")
					(number "AF45")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "GTM_REFCLKN0_203")
					(number "AF46")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "GTM_RXP3_203")
					(number "BA52")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "GTM_RXN3_203")
					(number "BA53")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "GTM_TXP3_203")
					(number "BB49")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "GTM_TXN3_203")
					(number "BB50")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "GTM_TXP2_203")
					(number "BC47")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "GTM_TXN2_203")
					(number "BC48")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "GTM_RXP2_203")
					(number "BC52")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "GTM_RXN2_203")
					(number "BC53")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "GTM_TXP1_203")
					(number "BD49")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "GTM_TXN1_203")
					(number "BD50")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "GTM_TXP0_203")
					(number "BE47")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "GTM_TXN0_203")
					(number "BE48")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "GTM_RXP1_203")
					(number "BE52")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "GTM_RXN1_203")
					(number "BE53")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "GTM_RXP0_203")
					(number "BG52")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "GTM_RXN0_203")
					(number "BG53")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_11_1"
				(text "BANK 204"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTM_REFCLKP1_204")
					(number "AA43")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTM_REFCLKN1_204")
					(number "AA44")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTM_REFCLKP0_204")
					(number "AB45")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTM_REFCLKN0_204")
					(number "AB46")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTM_RXP3_204")
					(number "AN52")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTM_RXN3_204")
					(number "AN53")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTM_RXP2_204")
					(number "AR52")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTM_RXN2_204")
					(number "AR53")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTM_TXP3_204")
					(number "AT49")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTM_TXN3_204")
					(number "AT50")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTM_RXP1_204")
					(number "AU52")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTM_RXN1_204")
					(number "AU53")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTM_TXP2_204")
					(number "AV49")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTM_TXN2_204")
					(number "AV50")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTM_RXP0_204")
					(number "AW52")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTM_RXN0_204")
					(number "AW53")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTM_TXP1_204")
					(number "AY49")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTM_TXN1_204")
					(number "AY50")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTM_TXP0_204")
					(number "BA47")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTM_TXN0_204")
					(number "BA48")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_12_1"
				(text "BANK 205"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTM_RXP3_205")
					(number "AE52")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTM_RXN3_205")
					(number "AE53")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTM_RXP2_205")
					(number "AG52")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTM_RXN2_205")
					(number "AG53")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTM_TXP3_205")
					(number "AH49")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTM_TXN3_205")
					(number "AH50")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTM_RXP1_205")
					(number "AJ52")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTM_RXN1_205")
					(number "AJ53")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTM_TXP2_205")
					(number "AK49")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTM_TXN2_205")
					(number "AK50")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTM_RXP0_205")
					(number "AL52")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTM_RXN0_205")
					(number "AL53")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTM_TXP1_205")
					(number "AM49")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTM_TXN1_205")
					(number "AM50")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTM_TXP0_205")
					(number "AP49")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTM_TXN0_205")
					(number "AP50")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTM_REFCLKP1_205")
					(number "W43")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTM_REFCLKN1_205")
					(number "W44")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTM_REFCLKP0_205")
					(number "Y45")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTM_REFCLKN0_205")
					(number "Y46")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_13_1"
				(text "BANK 206"
					(at 31.75 2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GTM_RXP1_206")
					(number "AA52")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GTM_RXN1_206")
					(number "AA53")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GTM_TXP3_206")
					(number "AC47")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GTM_TXN3_206")
					(number "AC48")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GTM_RXP0_206")
					(number "AC52")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GTM_RXN0_206")
					(number "AC53")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GTM_TXP2_206")
					(number "AD49")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GTM_TXN2_206")
					(number "AD50")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GTM_TXP1_206")
					(number "AE47")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GTM_TXN1_206")
					(number "AE48")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GTM_TXP0_206")
					(number "AF49")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GTM_TXN0_206")
					(number "AF50")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GTM_REFCLKP1_206")
					(number "U47")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GTM_REFCLKN1_206")
					(number "U48")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GTM_REFCLKP0_206")
					(number "V45")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GTM_REFCLKN0_206")
					(number "V46")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GTM_RXP3_206")
					(number "W52")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GTM_RXN3_206")
					(number "W53")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GTM_RXP2_206")
					(number "Y50")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GTM_RXN2_206")
					(number "Y51")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_14_1"
				(text "BANK 500"
					(at 30.48 -13.97 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VP_500")
					(number "AA20")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VREFN_500")
					(number "AA21")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "VREFP_500")
					(number "AB20")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VN_500")
					(number "AB21")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "RSVDGND")
					(number "AC20")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "RSVDGND")
					(number "AC21")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PMC_MIO0_500")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PMC_MIO15_500")
					(number "J14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PMC_MIO16_500")
					(number "J15")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PMC_MIO1_500")
					(number "K13")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PMC_MIO17_500")
					(number "K15")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PMC_MIO2_500")
					(number "L13")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PMC_MIO14_500")
					(number "L14")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PMC_MIO18_500")
					(number "L15")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PMC_MIO3_500")
					(number "M13")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PMC_MIO13_500")
					(number "M14")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PMC_MIO12_500")
					(number "N14")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PMC_MIO19_500")
					(number "N15")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PMC_MIO4_500")
					(number "P13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PMC_MIO11_500")
					(number "P14")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PMC_MIO20_500")
					(number "P15")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PMC_MIO5_500")
					(number "R13")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PMC_MIO21_500")
					(number "R15")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PMC_MIO6_500")
					(number "T13")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PMC_MIO10_500")
					(number "T14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PMC_MIO22_500")
					(number "T15")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PMC_MIO7_500")
					(number "U13")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PMC_MIO9_500")
					(number "U14")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PMC_MIO25_500")
					(number "U16")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PMC_MIO8_500")
					(number "V14")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PMC_MIO23_500")
					(number "V15")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PMC_MIO24_500")
					(number "V16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_500")
					(number "W14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_500")
					(number "W15")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_15_1"
				(text "BANK 501"
					(at 30.48 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_501")
					(number "AA14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_501")
					(number "AB14")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "PMC_MIO31_501")
					(number "K16")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PMC_MIO30_501")
					(number "L16")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PMC_MIO29_501")
					(number "M16")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PMC_MIO32_501")
					(number "M17")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "PMC_MIO44_501")
					(number "M18")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "PMC_MIO45_501")
					(number "M19")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "PMC_MIO28_501")
					(number "N16")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PMC_MIO33_501")
					(number "N17")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "PMC_MIO46_501")
					(number "N19")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "PMC_MIO51_501")
					(number "N20")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "PMC_MIO34_501")
					(number "P17")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "PMC_MIO43_501")
					(number "P18")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "PMC_MIO47_501")
					(number "P19")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "PMC_MIO27_501")
					(number "R16")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "PMC_MIO35_501")
					(number "R17")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "PMC_MIO42_501")
					(number "R18")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "PMC_MIO26_501")
					(number "T16")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "PMC_MIO41_501")
					(number "T18")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "PMC_MIO48_501")
					(number "T19")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "PMC_MIO36_501")
					(number "U17")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "PMC_MIO40_501")
					(number "U18")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "PMC_MIO49_501")
					(number "U19")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "PMC_MIO37_501")
					(number "V17")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "PMC_MIO50_501")
					(number "V19")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "PMC_MIO38_501")
					(number "W17")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "PMC_MIO39_501")
					(number "W18")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_16_1"
				(text "BANK 502"
					(at 30.48 0 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "LPD_MIO7_502")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "LPD_MIO8_502")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "LPD_MIO6_502")
					(number "E17")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "LPD_MIO9_502")
					(number "E18")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "LPD_MIO20_502")
					(number "E20")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "LPD_MIO10_502")
					(number "F18")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "LPD_MIO19_502")
					(number "F19")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "LPD_MIO21_502")
					(number "F20")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "LPD_MIO0_502")
					(number "G16")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "LPD_MIO5_502")
					(number "G17")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "LPD_MIO11_502")
					(number "G18")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "LPD_MIO18_502")
					(number "G19")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "LPD_MIO1_502")
					(number "H16")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "LPD_MIO4_502")
					(number "H17")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "LPD_MIO17_502")
					(number "H19")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "LPD_MIO22_502")
					(number "H20")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "LPD_MIO3_502")
					(number "J17")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "LPD_MIO12_502")
					(number "J18")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "LPD_MIO16_502")
					(number "J19")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "LPD_MIO23_502")
					(number "J20")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "LPD_MIO2_502")
					(number "K17")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "LPD_MIO13_502")
					(number "K18")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "LPD_MIO24_502")
					(number "K20")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "LPD_MIO14_502")
					(number "L18")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "LPD_MIO15_502")
					(number "L19")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "LPD_MIO25_502")
					(number "L20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_502")
					(number "Y15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_502")
					(number "Y16")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_17_1"
				(text "BANK 503"
					(at 30.48 -2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "DONE_503")
					(number "A16")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "ERROR_OUT_503")
					(number "A18")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "RTC_PADO_503")
					(number "A19")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "RTC_PADI_503")
					(number "A20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_503")
					(number "AA16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_503")
					(number "AB15")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "REF_CLK_503")
					(number "AC15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "POR_B_503")
					(number "AE14")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "TMS_503")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "TDO_503")
					(number "B17")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "TDI_503")
					(number "B18")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "TCK_503")
					(number "B19")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PUDC_B_503")
					(number "C17")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MODE2_503")
					(number "C19")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MODE3_503")
					(number "C20")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MODE1_503")
					(number "D19")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MODE0_503")
					(number "D20")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_18_1"
				(text "BANK 700"
					(at 31.75 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M0P38_700")
					(number "AJ12")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M0P39_700")
					(number "AJ13")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M0P36_700")
					(number "AJ15")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M0P42_700")
					(number "AK13")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M0P37_700")
					(number "AK14")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M0P43_700")
					(number "AL12")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M0P44_700")
					(number "AL14")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M0P40_700")
					(number "AL15")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M0P46_700")
					(number "AM12")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M0P45_700")
					(number "AM13")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M0P41_700")
					(number "AM15")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M0P47_700")
					(number "AN13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M0P24_700")
					(number "AN14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M0P26_700")
					(number "AP11")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M0P28_700")
					(number "AP12")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M0P30_700")
					(number "AP14")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M0P25_700")
					(number "AP15")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M0P27_700")
					(number "AR12")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M0P29_700")
					(number "AR13")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M0P31_700")
					(number "AR15")
				)
				(pin bidirectional line
					(at 0 -142.24 0)
					(length 5.08)
					(name "IO_VR_700")
					(number "AR27")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M0P50_700")
					(number "AT10")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M0P48_700")
					(number "AT11")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M0P32_700")
					(number "AT13")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M0P33_700")
					(number "AT14")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M0P51_700")
					(number "AU9")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M0P52_700")
					(number "AU11")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M0P49_700")
					(number "AU12")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M0P34_700")
					(number "AU14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_700")
					(number "AV9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_700")
					(number "AV10")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M0P53_700")
					(number "AV12")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M0P35_700")
					(number "AV13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_700")
					(number "AW10")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M0P14_700")
					(number "AW11")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M0P16_700")
					(number "AW13")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M0P12_700")
					(number "AW14")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M0P18_700")
					(number "AY9")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M0P15_700")
					(number "AY11")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M0P17_700")
					(number "AY12")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M0P13_700")
					(number "AY14")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M0P19_700")
					(number "BA9")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M0P2_700")
					(number "BA10")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M0P22_700")
					(number "BA12")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M0P20_700")
					(number "BA13")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M0P3_700")
					(number "BB10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M0P23_700")
					(number "BB11")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M0P21_700")
					(number "BB12")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M0P6_700")
					(number "BC9")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M0P7_700")
					(number "BC10")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M0P4_700")
					(number "BC12")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M0P0_700")
					(number "BC13")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M0P8_700")
					(number "BD10")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M0P5_700")
					(number "BD11")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M0P1_700")
					(number "BD12")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M0P10_700")
					(number "BE9")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M0P9_700")
					(number "BE10")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M0P11_700")
					(number "BF10")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_19_1"
				(text "BANK 701"
					(at 33.02 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M0P80_701")
					(number "BE12")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M0P78_701")
					(number "BE13")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M0P81_701")
					(number "BF11")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M0P79_701")
					(number "BF12")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M0P84_701")
					(number "BG9")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M0P88_701")
					(number "BG10")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M0P86_701")
					(number "BG12")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M0P82_701")
					(number "BG13")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M0P60_701")
					(number "BH4")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M0P85_701")
					(number "BH9")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M0P89_701")
					(number "BH10")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M0P87_701")
					(number "BH11")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M0P83_701")
					(number "BH12")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M0P64_701")
					(number "BJ2")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M0P62_701")
					(number "BJ3")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M0P61_701")
					(number "BJ4")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M0P56_701")
					(number "BJ5")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M0P54_701")
					(number "BJ7")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M0P107_701")
					(number "BJ8")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M0P106_701")
					(number "BJ9")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M0P100_701")
					(number "BJ10")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M0P92_701")
					(number "BJ12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_701")
					(number "BJ13")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M0P65_701")
					(number "BK2")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M0P63_701")
					(number "BK3")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M0P57_701")
					(number "BK5")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M0P55_701")
					(number "BK6")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M0P69_701")
					(number "BK7")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M0P103_701")
					(number "BK8")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M0P101_701")
					(number "BK10")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M0P93_701")
					(number "BK11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_701")
					(number "BK12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_701")
					(number "BK13")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M0P59_701")
					(number "BL3")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M0P58_701")
					(number "BL4")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M0P77_701")
					(number "BL5")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M0P76_701")
					(number "BL6")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M0P68_701")
					(number "BL8")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M0P102_701")
					(number "BL9")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M0P99_701")
					(number "BL10")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M0P98_701")
					(number "BL11")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M0P90_701")
					(number "BL13")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M0P75_701")
					(number "BM4")
				)
				(pin bidirectional line
					(at 0 -138.43 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M0P72_701")
					(number "BM6")
				)
				(pin bidirectional line
					(at 0 -133.35 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M0P70_701")
					(number "BM7")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M0P67_701")
					(number "BM8")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M0P105_701")
					(number "BM9")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M0P96_701")
					(number "BM11")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M0P94_701")
					(number "BM12")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M0P91_701")
					(number "BM13")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M0P74_701")
					(number "BN5")
				)
				(pin bidirectional line
					(at 0 -135.89 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M0P73_701")
					(number "BN6")
				)
				(pin bidirectional line
					(at 0 -130.81 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M0P71_701")
					(number "BN7")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M0P66_701")
					(number "BN9")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M0P104_701")
					(number "BN10")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M0P97_701")
					(number "BN11")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M0P95_701")
					(number "BN12")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_20_1"
				(text "BANK 702"
					(at 31.75 -2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M0P146_702")
					(number "AT16")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M0P144_702")
					(number "AT17")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M0P147_702")
					(number "AU15")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M0P145_702")
					(number "AU17")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M0P150_702")
					(number "AV15")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M0P148_702")
					(number "AV16")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M0P151_702")
					(number "AW16")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M0P149_702")
					(number "AW17")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M0P154_702")
					(number "AY15")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M0P152_702")
					(number "AY17")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M0P155_702")
					(number "BA15")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M0P153_702")
					(number "BA16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M0P134_702")
					(number "BB14")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M0P135_702")
					(number "BB15")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M0P132_702")
					(number "BB16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_702")
					(number "BC14")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M0P136_702")
					(number "BC16")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M0P133_702")
					(number "BC17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_702")
					(number "BD14")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M0P138_702")
					(number "BD15")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M0P137_702")
					(number "BD16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_702")
					(number "BE14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M0P139_702")
					(number "BE16")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M0P142_702")
					(number "BE17")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M0P140_702")
					(number "BE18")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M0P158_702")
					(number "BF14")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M0P160_702")
					(number "BF15")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M0P143_702")
					(number "BF16")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M0P141_702")
					(number "BF18")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M0P159_702")
					(number "BG14")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M0P161_702")
					(number "BG16")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M0P156_702")
					(number "BG17")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M0P157_702")
					(number "BG18")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M0P122_702")
					(number "BH14")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M0P126_702")
					(number "BH15")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M0P124_702")
					(number "BH16")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M0P120_702")
					(number "BH17")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M0P123_702")
					(number "BJ14")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M0P127_702")
					(number "BJ15")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M0P125_702")
					(number "BJ17")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M0P121_702")
					(number "BJ18")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M0P130_702")
					(number "BK15")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M0P110_702")
					(number "BK16")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M0P108_702")
					(number "BK17")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M0P128_702")
					(number "BK18")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M0P131_702")
					(number "BL14")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M0P111_702")
					(number "BL15")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M0P109_702")
					(number "BL16")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M0P129_702")
					(number "BL18")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M0P114_702")
					(number "BM14")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M0P118_702")
					(number "BM16")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M0P116_702")
					(number "BM17")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M0P112_702")
					(number "BM18")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M0P115_702")
					(number "BN14")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M0P119_702")
					(number "BN15")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M0P117_702")
					(number "BN16")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M0P113_702")
					(number "BN17")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_21_1"
				(text "BANK 703"
					(at 31.75 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M1P38_703")
					(number "AT19")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M1P36_703")
					(number "AT20")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M1P39_703")
					(number "AU18")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M1P40_703")
					(number "AU20")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M1P37_703")
					(number "AU21")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M1P42_703")
					(number "AV18")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M1P46_703")
					(number "AV19")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M1P41_703")
					(number "AV21")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M1P44_703")
					(number "AV22")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M1P43_703")
					(number "AW19")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M1P47_703")
					(number "AW20")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M1P45_703")
					(number "AW22")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M1P26_703")
					(number "AY18")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M1P28_703")
					(number "AY20")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M1P24_703")
					(number "AY21")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M1P27_703")
					(number "BA18")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M1P30_703")
					(number "BA19")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M1P29_703")
					(number "BA21")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M1P25_703")
					(number "BA22")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M1P31_703")
					(number "BB18")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M1P34_703")
					(number "BB19")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M1P35_703")
					(number "BB20")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M1P32_703")
					(number "BB22")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_703")
					(number "BC18")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M1P48_703")
					(number "BC20")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M1P33_703")
					(number "BC21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_703")
					(number "BD18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_703")
					(number "BD19")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M1P49_703")
					(number "BD20")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M1P50_703")
					(number "BE20")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M1P52_703")
					(number "BE21")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M1P51_703")
					(number "BF19")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M1P53_703")
					(number "BF20")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M1P12_703")
					(number "BF22")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M1P14_703")
					(number "BG20")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M1P16_703")
					(number "BG21")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M1P13_703")
					(number "BG22")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M1P15_703")
					(number "BH19")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M1P18_703")
					(number "BH20")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M1P20_703")
					(number "BH21")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M1P17_703")
					(number "BH22")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M1P19_703")
					(number "BJ19")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M1P22_703")
					(number "BJ20")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M1P21_703")
					(number "BJ22")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M1P23_703")
					(number "BK20")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M1P2_703")
					(number "BK21")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M1P0_703")
					(number "BK22")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M1P4_703")
					(number "BL19")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M1P3_703")
					(number "BL20")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M1P1_703")
					(number "BL21")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M1P5_703")
					(number "BM19")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M1P10_703")
					(number "BM21")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M1P8_703")
					(number "BM22")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M1P6_703")
					(number "BN19")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M1P7_703")
					(number "BN20")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M1P11_703")
					(number "BN21")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M1P9_703")
					(number "BN22")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_22_1"
				(text "BANK 704"
					(at 33.02 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M1P78_704")
					(number "AT22")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M1P79_704")
					(number "AT23")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M1P82_704")
					(number "AT25")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M1P90_704")
					(number "AT26")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M1P80_704")
					(number "AU23")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M1P83_704")
					(number "AU24")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M1P91_704")
					(number "AU26")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M1P81_704")
					(number "AV24")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M1P92_704")
					(number "AV25")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M1P84_704")
					(number "AW23")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M1P97_704")
					(number "AW25")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M1P93_704")
					(number "AW26")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M1P85_704")
					(number "AY23")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M1P96_704")
					(number "AY24")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M1P94_704")
					(number "AY26")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M1P86_704")
					(number "BA24")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M1P95_704")
					(number "BA25")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M1P87_704")
					(number "BB23")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M1P88_704")
					(number "BB24")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M1P98_704")
					(number "BB26")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_704")
					(number "BC22")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M1P89_704")
					(number "BC24")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M1P99_704")
					(number "BC25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_704")
					(number "BD22")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M1P104_704")
					(number "BD23")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M1P100_704")
					(number "BD24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_704")
					(number "BE22")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M1P105_704")
					(number "BE24")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M1P101_704")
					(number "BE25")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M1P102_704")
					(number "BE26")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M1P106_704")
					(number "BF23")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M1P107_704")
					(number "BF24")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M1P103_704")
					(number "BF26")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M1P54_704")
					(number "BG24")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M1P66_704")
					(number "BG26")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M1P55_704")
					(number "BH24")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M1P68_704")
					(number "BH25")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M1P67_704")
					(number "BH26")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M1P56_704")
					(number "BJ23")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M1P58_704")
					(number "BJ24")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M1P69_704")
					(number "BJ25")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M1P57_704")
					(number "BK23")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M1P59_704")
					(number "BK25")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M1P72_704")
					(number "BK26")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M1P70_704")
					(number "BK27")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M1P60_704")
					(number "BL23")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M1P62_704")
					(number "BL24")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M1P73_704")
					(number "BL25")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M1P71_704")
					(number "BL26")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M1P61_704")
					(number "BM23")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M1P63_704")
					(number "BM24")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M1P76_704")
					(number "BM26")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M1P74_704")
					(number "BM27")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M1P64_704")
					(number "BN24")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M1P65_704")
					(number "BN25")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M1P77_704")
					(number "BN26")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M1P75_704")
					(number "BN27")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_23_1"
				(text "BANK 705"
					(at 33.02 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M1P146_705")
					(number "AT28")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M1P144_705")
					(number "AT29")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M1P147_705")
					(number "AU27")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M1P148_705")
					(number "AU29")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M1P145_705")
					(number "AU30")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M1P150_705")
					(number "AV27")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M1P149_705")
					(number "AV28")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M1P152_705")
					(number "AV30")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M1P151_705")
					(number "AW28")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M1P153_705")
					(number "AW29")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M1P154_705")
					(number "AY27")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M1P134_705")
					(number "AY29")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M1P132_705")
					(number "AY30")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M1P155_705")
					(number "BA27")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M1P135_705")
					(number "BA28")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M1P133_705")
					(number "BA30")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M1P138_705")
					(number "BB27")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M1P140_705")
					(number "BB28")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M1P136_705")
					(number "BB30")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_705")
					(number "BC26")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M1P139_705")
					(number "BC28")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M1P141_705")
					(number "BC29")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M1P137_705")
					(number "BC30")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_705")
					(number "BD26")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_705")
					(number "BD27")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M1P142_705")
					(number "BD28")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M1P156_705")
					(number "BD30")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M1P143_705")
					(number "BE28")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M1P158_705")
					(number "BE29")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M1P157_705")
					(number "BE30")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M1P122_705")
					(number "BF27")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M1P159_705")
					(number "BF28")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M1P160_705")
					(number "BF30")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M1P123_705")
					(number "BG28")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M1P161_705")
					(number "BG29")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M1P120_705")
					(number "BG30")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M1P126_705")
					(number "BH27")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M1P128_705")
					(number "BH29")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M1P124_705")
					(number "BH30")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M1P121_705")
					(number "BH31")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M1P127_705")
					(number "BJ27")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M1P130_705")
					(number "BJ28")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M1P129_705")
					(number "BJ29")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M1P125_705")
					(number "BJ30")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M1P131_705")
					(number "BK28")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M1P112_705")
					(number "BK30")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M1P108_705")
					(number "BK31")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M1P110_705")
					(number "BL28")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M1P113_705")
					(number "BL29")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M1P114_705")
					(number "BL30")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M1P109_705")
					(number "BL31")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M1P111_705")
					(number "BM28")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M1P115_705")
					(number "BM29")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M1P116_705")
					(number "BM31")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M1P118_705")
					(number "BN29")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M1P119_705")
					(number "BN30")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M1P117_705")
					(number "BN31")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_24_1"
				(text "BANK 706"
					(at 31.75 0 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M2P38_706")
					(number "AT31")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M2P40_706")
					(number "AT32")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M2P36_706")
					(number "AT34")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M2P37_706")
					(number "AT35")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M2P39_706")
					(number "AU32")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M2P41_706")
					(number "AU33")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M2P44_706")
					(number "AU35")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M2P42_706")
					(number "AV31")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M2P46_706")
					(number "AV33")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M2P45_706")
					(number "AV34")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M2P43_706")
					(number "AW31")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M2P47_706")
					(number "AW32")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M2P24_706")
					(number "AW34")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M2P28_706")
					(number "AW35")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M2P26_706")
					(number "AY32")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M2P25_706")
					(number "AY33")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M2P29_706")
					(number "AY35")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M2P27_706")
					(number "BA31")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M2P32_706")
					(number "BA33")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M2P33_706")
					(number "BA34")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M2P30_706")
					(number "BB31")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M2P31_706")
					(number "BB32")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M2P34_706")
					(number "BB34")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_706")
					(number "BC32")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M2P52_706")
					(number "BC33")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M2P35_706")
					(number "BC34")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_706")
					(number "BD31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_706")
					(number "BD32")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M2P53_706")
					(number "BD34")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M2P50_706")
					(number "BD35")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M2P48_706")
					(number "BE32")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M2P49_706")
					(number "BE33")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M2P51_706")
					(number "BE34")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M2P14_706")
					(number "BF31")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M2P15_706")
					(number "BF32")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M2P12_706")
					(number "BF34")
				)
				(pin bidirectional line
					(at 0 -133.35 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M2P16_706")
					(number "BF35")
				)
				(pin bidirectional line
					(at 0 -138.43 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M2P18_706")
					(number "BG32")
				)
				(pin bidirectional line
					(at 0 -135.89 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M2P19_706")
					(number "BG33")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M2P13_706")
					(number "BG34")
				)
				(pin bidirectional line
					(at 0 -130.81 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M2P17_706")
					(number "BG35")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M2P22_706")
					(number "BH32")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M2P20_706")
					(number "BH34")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M2P23_706")
					(number "BJ32")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M2P4_706")
					(number "BJ33")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M2P21_706")
					(number "BJ34")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M2P2_706")
					(number "BK32")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M2P5_706")
					(number "BK33")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M2P3_706")
					(number "BL33")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M2P0_706")
					(number "BL34")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M2P10_706")
					(number "BM32")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M2P6_706")
					(number "BM33")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M2P8_706")
					(number "BM34")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M2P1_706")
					(number "BM35")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M2P11_706")
					(number "BN32")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M2P7_706")
					(number "BN34")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M2P9_706")
					(number "BN35")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_25_1"
				(text "BANK 707"
					(at 33.02 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M2P94_707")
					(number "AT37")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M2P95_707")
					(number "AT38")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M2P92_707")
					(number "AU36")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M2P90_707")
					(number "AU38")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M2P100_707")
					(number "AV36")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M2P93_707")
					(number "AV37")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M2P91_707")
					(number "AV39")
				)
				(pin bidirectional line
					(at 0 -133.35 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M2P70_707")
					(number "AV40")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M2P101_707")
					(number "AW37")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M2P98_707")
					(number "AW38")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M2P68_707")
					(number "AW40")
				)
				(pin bidirectional line
					(at 0 -130.81 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M2P71_707")
					(number "AW41")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M2P82_707")
					(number "AY36")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M2P96_707")
					(number "AY38")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M2P99_707")
					(number "AY39")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M2P69_707")
					(number "AY41")
				)
				(pin bidirectional line
					(at 0 -135.89 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M2P73_707")
					(number "AY42")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M2P77_707")
					(number "AY45")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M2P81_707")
					(number "BA36")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M2P83_707")
					(number "BA37")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M2P97_707")
					(number "BA39")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M2P67_707")
					(number "BA40")
				)
				(pin bidirectional line
					(at 0 -138.43 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M2P72_707")
					(number "BA42")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M2P74_707")
					(number "BA43")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M2P75_707")
					(number "BA44")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M2P76_707")
					(number "BA45")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M2P80_707")
					(number "BB35")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M2P78_707")
					(number "BB36")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M2P86_707")
					(number "BB38")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M2P87_707")
					(number "BB39")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M2P66_707")
					(number "BB40")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M2P59_707")
					(number "BB42")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M2P54_707")
					(number "BB43")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M2P55_707")
					(number "BB44")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_707")
					(number "BC36")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M2P79_707")
					(number "BC37")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M2P85_707")
					(number "BC38")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M2P106_707")
					(number "BC40")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M2P107_707")
					(number "BC41")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M2P58_707")
					(number "BC42")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M2P60_707")
					(number "BC44")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M2P61_707")
					(number "BC45")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_707")
					(number "BD36")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M2P84_707")
					(number "BD38")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M2P104_707")
					(number "BD39")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M2P105_707")
					(number "BD40")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M2P57_707")
					(number "BD42")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M2P62_707")
					(number "BD43")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M2P63_707")
					(number "BD44")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_707")
					(number "BE36")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M2P88_707")
					(number "BE37")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M2P89_707")
					(number "BE38")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M2P102_707")
					(number "BE40")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M2P103_707")
					(number "BE41")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M2P56_707")
					(number "BE42")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M2P64_707")
					(number "BE44")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M2P65_707")
					(number "BE45")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_26_1"
				(text "BANK 708"
					(at 33.02 -2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M2P146_708")
					(number "AD40")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M2P144_708")
					(number "AD41")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M2P147_708")
					(number "AE39")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M2P148_708")
					(number "AE41")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M2P145_708")
					(number "AE42")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M2P150_708")
					(number "AF39")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M2P152_708")
					(number "AF40")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M2P149_708")
					(number "AF42")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M2P151_708")
					(number "AG40")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M2P153_708")
					(number "AG41")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M2P154_708")
					(number "AH39")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M2P134_708")
					(number "AH41")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M2P136_708")
					(number "AH42")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M2P132_708")
					(number "AH44")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M2P155_708")
					(number "AJ39")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M2P135_708")
					(number "AJ40")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M2P137_708")
					(number "AJ42")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M2P133_708")
					(number "AJ43")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M2P138_708")
					(number "AK40")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M2P142_708")
					(number "AK41")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M2P156_708")
					(number "AK43")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M2P140_708")
					(number "AK44")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M2P139_708")
					(number "AL39")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M2P143_708")
					(number "AL41")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M2P157_708")
					(number "AL42")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M2P141_708")
					(number "AL44")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M2P122_708")
					(number "AM39")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M2P123_708")
					(number "AM40")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M2P120_708")
					(number "AM42")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M2P158_708")
					(number "AM43")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M2P126_708")
					(number "AN40")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M2P121_708")
					(number "AN41")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M2P159_708")
					(number "AN43")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M2P160_708")
					(number "AN44")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M2P127_708")
					(number "AP39")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M2P124_708")
					(number "AP41")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M2P125_708")
					(number "AP42")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M2P161_708")
					(number "AP44")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M2P130_708")
					(number "AR39")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M2P131_708")
					(number "AR40")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_708")
					(number "AR42")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_708")
					(number "AR43")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_708")
					(number "AR44")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M2P110_708")
					(number "AT40")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M2P128_708")
					(number "AT41")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M2P108_708")
					(number "AT43")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M2P111_708")
					(number "AU39")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M2P129_708")
					(number "AU41")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M2P109_708")
					(number "AU42")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M2P112_708")
					(number "AU44")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M2P113_708")
					(number "AU45")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M2P114_708")
					(number "AV42")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M2P118_708")
					(number "AV43")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M2P116_708")
					(number "AV44")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M2P115_708")
					(number "AW43")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M2P119_708")
					(number "AW44")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M2P117_708")
					(number "AW45")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_27_1"
				(text "BANK 709"
					(at 31.75 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M3P7_709")
					(number "A21")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M3P9_709")
					(number "A23")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M3P11_709")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M3P6_709")
					(number "B21")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M3P5_709")
					(number "B22")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M3P8_709")
					(number "B23")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M3P10_709")
					(number "B24")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M3P1_709")
					(number "C21")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M3P4_709")
					(number "C22")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M3P3_709")
					(number "C24")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M3P0_709")
					(number "D22")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M3P23_709")
					(number "D23")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M3P2_709")
					(number "D24")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M3P21_709")
					(number "E21")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M3P20_709")
					(number "E22")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M3P22_709")
					(number "E23")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_709")
					(number "F21")
				)
				(pin bidirectional line
					(at 0 -135.89 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M3P19_709")
					(number "F23")
				)
				(pin bidirectional line
					(at 0 -138.43 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M3P18_709")
					(number "F24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_709")
					(number "G21")
				)
				(pin bidirectional line
					(at 0 -130.81 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M3P17_709")
					(number "G22")
				)
				(pin bidirectional line
					(at 0 -133.35 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M3P16_709")
					(number "G23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_709")
					(number "H21")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M3P15_709")
					(number "H22")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M3P14_709")
					(number "J22")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M3P13_709")
					(number "J23")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M3P53_709")
					(number "K21")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M3P51_709")
					(number "K22")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M3P12_709")
					(number "K23")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M3P52_709")
					(number "L21")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M3P50_709")
					(number "L23")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M3P49_709")
					(number "L24")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M3P35_709")
					(number "M21")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M3P31_709")
					(number "M22")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M3P33_709")
					(number "M23")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M3P48_709")
					(number "M24")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M3P34_709")
					(number "N21")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M3P30_709")
					(number "N22")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M3P32_709")
					(number "N24")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M3P47_709")
					(number "P20")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M3P25_709")
					(number "P22")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M3P27_709")
					(number "P23")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M3P29_709")
					(number "P24")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M3P46_709")
					(number "R20")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M3P24_709")
					(number "R21")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M3P26_709")
					(number "R22")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M3P28_709")
					(number "R23")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M3P43_709")
					(number "T20")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M3P41_709")
					(number "T21")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M3P45_709")
					(number "T23")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M3P44_709")
					(number "T24")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M3P42_709")
					(number "U21")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M3P40_709")
					(number "U22")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M3P39_709")
					(number "U23")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M3P37_709")
					(number "V20")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M3P36_709")
					(number "V21")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M3P38_709")
					(number "V22")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_28_1"
				(text "BANK 709"
					(at 33.02 -2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M3P77_710")
					(number "A25")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M3P75_710")
					(number "A26")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M3P65_710")
					(number "A28")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M3P76_710")
					(number "B26")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M3P74_710")
					(number "B27")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M3P64_710")
					(number "B28")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M3P73_710")
					(number "C25")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M3P61_710")
					(number "C26")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M3P63_710")
					(number "C27")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M3P72_710")
					(number "D25")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M3P60_710")
					(number "D27")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M3P62_710")
					(number "D28")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M3P71_710")
					(number "E25")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M3P69_710")
					(number "E26")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M3P68_710")
					(number "E27")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M3P59_710")
					(number "E28")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M3P70_710")
					(number "F25")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M3P67_710")
					(number "F26")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M3P58_710")
					(number "F28")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_710")
					(number "G24")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M3P66_710")
					(number "G26")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M3P55_710")
					(number "G27")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M3P57_710")
					(number "G28")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_710")
					(number "H24")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M3P107_710")
					(number "H25")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M3P54_710")
					(number "H26")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M3P56_710")
					(number "H27")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_710")
					(number "J24")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M3P106_710")
					(number "J25")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M3P105_710")
					(number "J27")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M3P103_710")
					(number "K25")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M3P102_710")
					(number "K26")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M3P104_710")
					(number "K27")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M3P101_710")
					(number "L25")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M3P99_710")
					(number "L26")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M3P100_710")
					(number "M26")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M3P98_710")
					(number "M27")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M3P89_710")
					(number "M28")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M3P97_710")
					(number "N25")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M3P96_710")
					(number "N26")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M3P88_710")
					(number "N27")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M3P95_710")
					(number "P25")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M3P85_710")
					(number "P27")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M3P87_710")
					(number "P28")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M3P94_710")
					(number "R25")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M3P83_710")
					(number "R26")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M3P84_710")
					(number "R27")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M3P86_710")
					(number "R28")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M3P93_710")
					(number "T25")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M3P82_710")
					(number "T26")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M3P92_710")
					(number "U24")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M3P81_710")
					(number "U26")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M3P79_710")
					(number "U27")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M3P91_710")
					(number "V24")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M3P90_710")
					(number "V25")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M3P80_710")
					(number "V26")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M3P78_710")
					(number "V27")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_29_1"
				(text "BANK 711"
					(at 33.02 -2.54 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L4N_N1P3_M3P117_711")
					(number "A29")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L5N_N1P5_M3P119_711")
					(number "A30")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L5P_N1P4_M3P118_711")
					(number "A31")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_M3P115_711")
					(number "A33")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L4P_N1P2_M3P116_711")
					(number "B29")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L1N_N0P3_M3P111_711")
					(number "B31")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_M3P109_711")
					(number "B32")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_M3P114_711")
					(number "B33")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L2N_N0P5_M3P113_711")
					(number "C29")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_M3P127_711")
					(number "C30")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L1P_N0P2_M3P110_711")
					(number "C31")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_M3P108_711")
					(number "C32")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L2P_N0P4_M3P112_711")
					(number "D29")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_M3P126_711")
					(number "D30")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_L8N_N2P5_M3P125_711")
					(number "D32")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L11N_N3P5_M3P131_711")
					(number "D33")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L10N_N3P3_M3P129_711")
					(number "D34")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_L7N_N2P3_M3P123_711")
					(number "E30")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "IO_L8P_N2P4_M3P124_711")
					(number "E31")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L11P_N3P4_M3P130_711")
					(number "E32")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L10P_N3P2_M3P128_711")
					(number "E33")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L26N_N8P5_M3P161_711")
					(number "F29")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_L7P_N2P2_M3P122_711")
					(number "F30")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_M3P157_711")
					(number "F31")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_M3P121_711")
					(number "F33")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L26P_N8P4_M3P160_711")
					(number "G29")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_M3P156_711")
					(number "G31")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L25N_N8P3_M3P159_711")
					(number "G32")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_M3P120_711")
					(number "G33")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L16N_N5P3_M3P141_711")
					(number "H29")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L17N_N5P5_M3P143_711")
					(number "H30")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L25P_N8P2_M3P158_711")
					(number "H31")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_711")
					(number "J28")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L16P_N5P2_M3P140_711")
					(number "J29")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L17P_N5P4_M3P142_711")
					(number "J30")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_711")
					(number "K28")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L14N_N4P5_M3P137_711")
					(number "K30")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_M3P139_711")
					(number "K31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_711")
					(number "L28")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L13N_N4P3_M3P135_711")
					(number "L29")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L14P_N4P4_M3P136_711")
					(number "L30")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_M3P138_711")
					(number "L31")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L13P_N4P2_M3P134_711")
					(number "M29")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_M3P133_711")
					(number "M31")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L23N_N7P5_M3P155_711")
					(number "N29")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L22N_N7P3_M3P153_711")
					(number "N30")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_M3P132_711")
					(number "N31")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L23P_N7P4_M3P154_711")
					(number "P29")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L22P_N7P2_M3P152_711")
					(number "P30")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_M3P151_711")
					(number "R30")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L20N_N6P5_M3P149_711")
					(number "T28")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L19N_N6P3_M3P147_711")
					(number "T29")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_M3P150_711")
					(number "T30")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L20P_N6P4_M3P148_711")
					(number "U28")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L19P_N6P2_M3P146_711")
					(number "U29")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_M3P145_711")
					(number "V29")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_M3P144_711")
					(number "V30")
				)
			)
			(symbol "XCVP1202-2MSEVSVA2785_30_1"
				(text "BANK 712"
					(at 27.94 -1.27 0)
				)
				(text ""
					(at 52.07 -26.67 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_712")
					(number "H32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_712")
					(number "J32")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "IO_L5N_N1P5_712")
					(number "J33")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "IO_L3N_XCC_N1P1_712")
					(number "J34")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "IO_L3P_XCC_N1P0_712")
					(number "J35")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "IO_L4N_N1P3_712")
					(number "J37")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "IO_L4P_N1P2_712")
					(number "J38")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_712")
					(number "K32")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 5.08)
					(name "IO_L5P_N1P4_712")
					(number "K33")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_L0N_XCC_N0P1_712")
					(number "K35")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L0P_XCC_N0P0_712")
					(number "K36")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L1N_N0P3_712")
					(number "K37")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "IO_L2N_N0P5_712")
					(number "K38")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L11N_N3P5_712")
					(number "L33")
				)
				(pin bidirectional line
					(at 0 -135.89 0)
					(length 5.08)
					(name "IO_L9N_GC_XCC_N3P1_712")
					(number "L34")
				)
				(pin bidirectional line
					(at 0 -130.81 0)
					(length 5.08)
					(name "IO_L8N_N2P5_712")
					(number "L35")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L1P_N0P2_712")
					(number "L36")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "IO_L2P_N0P4_712")
					(number "L38")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 5.08)
					(name "IO_L7N_N2P3_712")
					(number "M32")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L11P_N3P4_712")
					(number "M33")
				)
				(pin bidirectional line
					(at 0 -138.43 0)
					(length 5.08)
					(name "IO_L9P_GC_XCC_N3P0_712")
					(number "M34")
				)
				(pin bidirectional line
					(at 0 -133.35 0)
					(length 5.08)
					(name "IO_L8P_N2P4_712")
					(number "M36")
				)
				(pin bidirectional line
					(at 0 -120.65 0)
					(length 5.08)
					(name "IO_L6N_GC_XCC_N2P1_712")
					(number "M37")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L10N_N3P3_712")
					(number "M38")
				)
				(pin bidirectional line
					(at 0 -128.27 0)
					(length 5.08)
					(name "IO_L7P_N2P2_712")
					(number "N32")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "IO_L25N_N8P3_712")
					(number "N34")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "IO_L26N_N8P5_712")
					(number "N35")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 5.08)
					(name "IO_L6P_GC_XCC_N2P0_712")
					(number "N36")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L10P_N3P2_712")
					(number "N37")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "IO_L24N_GC_XCC_N8P1_712")
					(number "P32")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L15N_XCC_N5P1_712")
					(number "P33")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "IO_L25P_N8P2_712")
					(number "P34")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "IO_L26P_N8P4_712")
					(number "P35")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L16N_N5P3_712")
					(number "P37")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L17N_N5P5_712")
					(number "R31")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "IO_L24P_GC_XCC_N8P0_712")
					(number "R32")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L15P_XCC_N5P0_712")
					(number "R33")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L12N_GC_XCC_N4P1_712")
					(number "R35")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L14N_N4P5_712")
					(number "R36")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L16P_N5P2_712")
					(number "R37")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L17P_N5P4_712")
					(number "T31")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "IO_L23N_N7P5_712")
					(number "T33")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L13N_N4P3_712")
					(number "T34")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L12P_GC_XCC_N4P0_712")
					(number "T35")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L14P_N4P4_712")
					(number "T36")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L21N_XCC_N7P1_712")
					(number "U31")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L19N_N6P3_712")
					(number "U32")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "IO_L23P_N7P4_712")
					(number "U33")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L13P_N4P2_712")
					(number "U34")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L20N_N6P5_712")
					(number "U36")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "IO_L22N_N7P3_712")
					(number "U37")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "IO_L21P_XCC_N7P0_712")
					(number "V31")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L19P_N6P2_712")
					(number "V32")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L18N_XCC_N6P1_712")
					(number "V34")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L18P_XCC_N6P0_712")
					(number "V35")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L20P_N6P4_712")
					(number "V36")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "IO_L22P_N7P2_712")
					(number "V37")
				)
			)
			(embedded_fonts no)
		)
)
