(footprint "BGA-2116-2104_52.5x52.5mm_Layout46x46_P1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -27.4 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-2116-2104_52.5x52.5mm_Layout46x46_P1mm"
		(at 0 28.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -27.25 30.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -27.25 31.8 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -27.25 33 0)
		(layer "F.Fab")
	)
	(pad "A3" smd circle
		(at -20.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A4" smd circle
		(at -19.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A5" smd circle
		(at -18.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "A6" smd circle
		(at -17.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A7" smd circle
		(at -16.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A8" smd circle
		(at -15.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A9" smd circle
		(at -14.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A10" smd circle
		(at -13.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A11" smd circle
		(at -12.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A12" smd circle
		(at -11.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A13" smd circle
		(at -10.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A14" smd circle
		(at -9.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A15" smd circle
		(at -8.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A16" smd circle
		(at -7.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A17" smd circle
		(at -6.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A18" smd circle
		(at -5.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A19" smd circle
		(at -4.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A20" smd circle
		(at -3.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A21" smd circle
		(at -2.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A22" smd circle
		(at -1.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A23" smd circle
		(at -0.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A24" smd circle
		(at 0.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A25" smd circle
		(at 1.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A26" smd circle
		(at 2.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A27" smd circle
		(at 3.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A28" smd circle
		(at 4.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A29" smd circle
		(at 5.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A30" smd circle
		(at 6.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A31" smd circle
		(at 7.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A32" smd circle
		(at 8.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A33" smd circle
		(at 9.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A34" smd circle
		(at 10.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A35" smd circle
		(at 11.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A36" smd circle
		(at 12.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A37" smd circle
		(at 13.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A38" smd circle
		(at 14.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A39" smd circle
		(at 15.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A40" smd circle
		(at 16.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A41" smd circle
		(at 17.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A42" smd circle
		(at 18.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "A43" smd circle
		(at 19.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "A44" smd circle
		(at 20.5 -22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA1" smd circle
		(at -22.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA2" smd circle
		(at -21.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA3" smd circle
		(at -20.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA4" smd circle
		(at -19.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA5" smd circle
		(at -18.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA6" smd circle
		(at -17.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AA7" smd circle
		(at -16.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA8" smd circle
		(at -15.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA9" smd circle
		(at -14.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA10" smd circle
		(at -13.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AA11" smd circle
		(at -12.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA12" smd circle
		(at -11.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA13" smd circle
		(at -10.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA14" smd circle
		(at -9.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA15" smd circle
		(at -8.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA16" smd circle
		(at -7.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA17" smd circle
		(at -6.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA18" smd circle
		(at -5.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA19" smd circle
		(at -4.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA20" smd circle
		(at -3.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA21" smd circle
		(at -2.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA22" smd circle
		(at -1.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA23" smd circle
		(at -0.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA24" smd circle
		(at 0.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA25" smd circle
		(at 1.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA26" smd circle
		(at 2.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA27" smd circle
		(at 3.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA28" smd circle
		(at 4.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA29" smd circle
		(at 5.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA30" smd circle
		(at 6.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA31" smd circle
		(at 7.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA32" smd circle
		(at 8.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA33" smd circle
		(at 9.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA34" smd circle
		(at 10.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA35" smd circle
		(at 11.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA36" smd circle
		(at 12.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AA37" smd circle
		(at 13.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA38" smd circle
		(at 14.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA39" smd circle
		(at 15.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA40" smd circle
		(at 16.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA41" smd circle
		(at 17.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA42" smd circle
		(at 18.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA43" smd circle
		(at 19.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA44" smd circle
		(at 20.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA45" smd circle
		(at 21.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AA46" smd circle
		(at 22.5 -2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB1" smd circle
		(at -22.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB2" smd circle
		(at -21.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB3" smd circle
		(at -20.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB4" smd circle
		(at -19.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB5" smd circle
		(at -18.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB6" smd circle
		(at -17.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB7" smd circle
		(at -16.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB8" smd circle
		(at -15.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB9" smd circle
		(at -14.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AB10" smd circle
		(at -13.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB11" smd circle
		(at -12.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB12" smd circle
		(at -11.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB13" smd circle
		(at -10.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB14" smd circle
		(at -9.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB15" smd circle
		(at -8.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB16" smd circle
		(at -7.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB17" smd circle
		(at -6.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB18" smd circle
		(at -5.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB19" smd circle
		(at -4.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB20" smd circle
		(at -3.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB21" smd circle
		(at -2.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB22" smd circle
		(at -1.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB23" smd circle
		(at -0.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB24" smd circle
		(at 0.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB25" smd circle
		(at 1.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB26" smd circle
		(at 2.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB27" smd circle
		(at 3.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB28" smd circle
		(at 4.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB29" smd circle
		(at 5.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB30" smd circle
		(at 6.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB31" smd circle
		(at 7.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB32" smd circle
		(at 8.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB33" smd circle
		(at 9.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB34" smd circle
		(at 10.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB35" smd circle
		(at 11.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB36" smd circle
		(at 12.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB37" smd circle
		(at 13.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AB38" smd circle
		(at 14.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB39" smd circle
		(at 15.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB40" smd circle
		(at 16.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AB41" smd circle
		(at 17.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB42" smd circle
		(at 18.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB43" smd circle
		(at 19.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB44" smd circle
		(at 20.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB45" smd circle
		(at 21.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AB46" smd circle
		(at 22.5 -1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC1" smd circle
		(at -22.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC2" smd circle
		(at -21.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC3" smd circle
		(at -20.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC4" smd circle
		(at -19.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC5" smd circle
		(at -18.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC6" smd circle
		(at -17.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC7" smd circle
		(at -16.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AC8" smd circle
		(at -15.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC9" smd circle
		(at -14.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC10" smd circle
		(at -13.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AC11" smd circle
		(at -12.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC12" smd circle
		(at -11.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC13" smd circle
		(at -10.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC14" smd circle
		(at -9.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC15" smd circle
		(at -8.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC16" smd circle
		(at -7.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC17" smd circle
		(at -6.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC18" smd circle
		(at -5.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC19" smd circle
		(at -4.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC20" smd circle
		(at -3.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC21" smd circle
		(at -2.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC22" smd circle
		(at -1.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC23" smd circle
		(at -0.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC24" smd circle
		(at 0.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC25" smd circle
		(at 1.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC26" smd circle
		(at 2.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC27" smd circle
		(at 3.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC28" smd circle
		(at 4.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC29" smd circle
		(at 5.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC30" smd circle
		(at 6.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC31" smd circle
		(at 7.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC32" smd circle
		(at 8.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC33" smd circle
		(at 9.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC34" smd circle
		(at 10.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC35" smd circle
		(at 11.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC36" smd circle
		(at 12.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AC37" smd circle
		(at 13.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC38" smd circle
		(at 14.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC39" smd circle
		(at 15.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AC40" smd circle
		(at 16.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC41" smd circle
		(at 17.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC42" smd circle
		(at 18.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC43" smd circle
		(at 19.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC44" smd circle
		(at 20.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC45" smd circle
		(at 21.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AC46" smd circle
		(at 22.5 -0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD1" smd circle
		(at -22.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD2" smd circle
		(at -21.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD3" smd circle
		(at -20.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD4" smd circle
		(at -19.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD5" smd circle
		(at -18.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD6" smd circle
		(at -17.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD7" smd circle
		(at -16.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD8" smd circle
		(at -15.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD9" smd circle
		(at -14.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD10" smd circle
		(at -13.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD11" smd circle
		(at -12.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AD12" smd circle
		(at -11.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD13" smd circle
		(at -10.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD14" smd circle
		(at -9.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD15" smd circle
		(at -8.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD16" smd circle
		(at -7.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD17" smd circle
		(at -6.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD18" smd circle
		(at -5.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD19" smd circle
		(at -4.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD20" smd circle
		(at -3.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD21" smd circle
		(at -2.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD22" smd circle
		(at -1.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD23" smd circle
		(at -0.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD24" smd circle
		(at 0.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD25" smd circle
		(at 1.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD26" smd circle
		(at 2.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD27" smd circle
		(at 3.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD28" smd circle
		(at 4.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD29" smd circle
		(at 5.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD30" smd circle
		(at 6.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD31" smd circle
		(at 7.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD32" smd circle
		(at 8.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD33" smd circle
		(at 9.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD34" smd circle
		(at 10.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD35" smd circle
		(at 11.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD36" smd circle
		(at 12.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD37" smd circle
		(at 13.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AD38" smd circle
		(at 14.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD39" smd circle
		(at 15.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD40" smd circle
		(at 16.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD41" smd circle
		(at 17.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AD42" smd circle
		(at 18.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD43" smd circle
		(at 19.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD44" smd circle
		(at 20.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD45" smd circle
		(at 21.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AD46" smd circle
		(at 22.5 0.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE1" smd circle
		(at -22.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE2" smd circle
		(at -21.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE3" smd circle
		(at -20.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE4" smd circle
		(at -19.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE5" smd circle
		(at -18.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE6" smd circle
		(at -17.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AE7" smd circle
		(at -16.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE8" smd circle
		(at -15.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE9" smd circle
		(at -14.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE10" smd circle
		(at -13.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AE11" smd circle
		(at -12.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE12" smd circle
		(at -11.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE13" smd circle
		(at -10.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE14" smd circle
		(at -9.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE15" smd circle
		(at -8.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE16" smd circle
		(at -7.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE17" smd circle
		(at -6.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE18" smd circle
		(at -5.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE19" smd circle
		(at -4.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE20" smd circle
		(at -3.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE21" smd circle
		(at -2.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE22" smd circle
		(at -1.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE23" smd circle
		(at -0.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE24" smd circle
		(at 0.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE25" smd circle
		(at 1.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE26" smd circle
		(at 2.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE27" smd circle
		(at 3.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE28" smd circle
		(at 4.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE29" smd circle
		(at 5.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE30" smd circle
		(at 6.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE31" smd circle
		(at 7.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE32" smd circle
		(at 8.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE33" smd circle
		(at 9.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE34" smd circle
		(at 10.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE35" smd circle
		(at 11.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE36" smd circle
		(at 12.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AE37" smd circle
		(at 13.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE38" smd circle
		(at 14.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE39" smd circle
		(at 15.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE40" smd circle
		(at 16.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE41" smd circle
		(at 17.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE42" smd circle
		(at 18.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE43" smd circle
		(at 19.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE44" smd circle
		(at 20.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE45" smd circle
		(at 21.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AE46" smd circle
		(at 22.5 1.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF1" smd circle
		(at -22.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF2" smd circle
		(at -21.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF3" smd circle
		(at -20.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF4" smd circle
		(at -19.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF5" smd circle
		(at -18.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF6" smd circle
		(at -17.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF7" smd circle
		(at -16.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF8" smd circle
		(at -15.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF9" smd circle
		(at -14.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF10" smd circle
		(at -13.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF11" smd circle
		(at -12.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AF12" smd circle
		(at -11.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF13" smd circle
		(at -10.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF14" smd circle
		(at -9.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF15" smd circle
		(at -8.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF16" smd circle
		(at -7.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF17" smd circle
		(at -6.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF18" smd circle
		(at -5.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF19" smd circle
		(at -4.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF20" smd circle
		(at -3.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF21" smd circle
		(at -2.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF22" smd circle
		(at -1.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF23" smd circle
		(at -0.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF24" smd circle
		(at 0.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF25" smd circle
		(at 1.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF26" smd circle
		(at 2.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF27" smd circle
		(at 3.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF28" smd circle
		(at 4.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF29" smd circle
		(at 5.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF30" smd circle
		(at 6.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF31" smd circle
		(at 7.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF32" smd circle
		(at 8.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF33" smd circle
		(at 9.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF34" smd circle
		(at 10.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF35" smd circle
		(at 11.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF36" smd circle
		(at 12.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF37" smd circle
		(at 13.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AF38" smd circle
		(at 14.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF39" smd circle
		(at 15.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF40" smd circle
		(at 16.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AF41" smd circle
		(at 17.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF42" smd circle
		(at 18.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF43" smd circle
		(at 19.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF44" smd circle
		(at 20.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF45" smd circle
		(at 21.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AF46" smd circle
		(at 22.5 2.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG1" smd circle
		(at -22.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG2" smd circle
		(at -21.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG3" smd circle
		(at -20.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG4" smd circle
		(at -19.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG5" smd circle
		(at -18.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG6" smd circle
		(at -17.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG7" smd circle
		(at -16.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AG8" smd circle
		(at -15.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG9" smd circle
		(at -14.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG10" smd circle
		(at -13.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AG11" smd circle
		(at -12.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG12" smd circle
		(at -11.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG13" smd circle
		(at -10.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG14" smd circle
		(at -9.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG15" smd circle
		(at -8.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG16" smd circle
		(at -7.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG17" smd circle
		(at -6.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG18" smd circle
		(at -5.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG19" smd circle
		(at -4.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG20" smd circle
		(at -3.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG21" smd circle
		(at -2.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG22" smd circle
		(at -1.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG23" smd circle
		(at -0.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG24" smd circle
		(at 0.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG25" smd circle
		(at 1.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG26" smd circle
		(at 2.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG27" smd circle
		(at 3.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG28" smd circle
		(at 4.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG29" smd circle
		(at 5.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG30" smd circle
		(at 6.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG31" smd circle
		(at 7.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG32" smd circle
		(at 8.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG33" smd circle
		(at 9.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG34" smd circle
		(at 10.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG35" smd circle
		(at 11.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG36" smd circle
		(at 12.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG37" smd circle
		(at 13.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AG38" smd circle
		(at 14.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG39" smd circle
		(at 15.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG40" smd circle
		(at 16.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG41" smd circle
		(at 17.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG42" smd circle
		(at 18.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG43" smd circle
		(at 19.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG44" smd circle
		(at 20.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG45" smd circle
		(at 21.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AG46" smd circle
		(at 22.5 3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH1" smd circle
		(at -22.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH2" smd circle
		(at -21.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH3" smd circle
		(at -20.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH4" smd circle
		(at -19.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH5" smd circle
		(at -18.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH6" smd circle
		(at -17.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH7" smd circle
		(at -16.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH8" smd circle
		(at -15.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AH9" smd circle
		(at -14.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH10" smd circle
		(at -13.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH11" smd circle
		(at -12.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH12" smd circle
		(at -11.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH13" smd circle
		(at -10.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH14" smd circle
		(at -9.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH15" smd circle
		(at -8.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH16" smd circle
		(at -7.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH17" smd circle
		(at -6.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH18" smd circle
		(at -5.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH19" smd circle
		(at -4.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH20" smd circle
		(at -3.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH21" smd circle
		(at -2.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH22" smd circle
		(at -1.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH23" smd circle
		(at -0.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH24" smd circle
		(at 0.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH25" smd circle
		(at 1.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH26" smd circle
		(at 2.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH27" smd circle
		(at 3.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH28" smd circle
		(at 4.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH29" smd circle
		(at 5.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH30" smd circle
		(at 6.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH31" smd circle
		(at 7.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH32" smd circle
		(at 8.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH33" smd circle
		(at 9.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH34" smd circle
		(at 10.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH35" smd circle
		(at 11.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH36" smd circle
		(at 12.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH37" smd circle
		(at 13.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH38" smd circle
		(at 14.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH39" smd circle
		(at 15.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH40" smd circle
		(at 16.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH41" smd circle
		(at 17.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AH42" smd circle
		(at 18.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH43" smd circle
		(at 19.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AH44" smd circle
		(at 20.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH45" smd circle
		(at 21.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AH46" smd circle
		(at 22.5 4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ1" smd circle
		(at -22.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AJ2" smd circle
		(at -21.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AJ3" smd circle
		(at -20.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ4" smd circle
		(at -19.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ5" smd circle
		(at -18.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ6" smd circle
		(at -17.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AJ7" smd circle
		(at -16.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ8" smd circle
		(at -15.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ9" smd circle
		(at -14.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ10" smd circle
		(at -13.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AJ11" smd circle
		(at -12.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ12" smd circle
		(at -11.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ13" smd circle
		(at -10.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ14" smd circle
		(at -9.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ15" smd circle
		(at -8.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ16" smd circle
		(at -7.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ17" smd circle
		(at -6.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ18" smd circle
		(at -5.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ19" smd circle
		(at -4.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ20" smd circle
		(at -3.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ21" smd circle
		(at -2.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ22" smd circle
		(at -1.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ23" smd circle
		(at -0.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ24" smd circle
		(at 0.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ25" smd circle
		(at 1.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ26" smd circle
		(at 2.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ27" smd circle
		(at 3.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ28" smd circle
		(at 4.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ29" smd circle
		(at 5.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ30" smd circle
		(at 6.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ31" smd circle
		(at 7.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ32" smd circle
		(at 8.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ33" smd circle
		(at 9.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ34" smd circle
		(at 10.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ35" smd circle
		(at 11.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ36" smd circle
		(at 12.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ37" smd circle
		(at 13.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ38" smd circle
		(at 14.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AJ39" smd circle
		(at 15.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ40" smd circle
		(at 16.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ41" smd circle
		(at 17.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ42" smd circle
		(at 18.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AJ43" smd circle
		(at 19.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ44" smd circle
		(at 20.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ45" smd circle
		(at 21.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AJ46" smd circle
		(at 22.5 5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK1" smd circle
		(at -22.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AK2" smd circle
		(at -21.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AK3" smd circle
		(at -20.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AK4" smd circle
		(at -19.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK5" smd circle
		(at -18.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK6" smd circle
		(at -17.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK7" smd circle
		(at -16.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK8" smd circle
		(at -15.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK9" smd circle
		(at -14.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AK10" smd circle
		(at -13.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK11" smd circle
		(at -12.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK12" smd circle
		(at -11.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK13" smd circle
		(at -10.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK14" smd circle
		(at -9.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK15" smd circle
		(at -8.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK16" smd circle
		(at -7.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK17" smd circle
		(at -6.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK18" smd circle
		(at -5.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK19" smd circle
		(at -4.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK20" smd circle
		(at -3.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK21" smd circle
		(at -2.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK22" smd circle
		(at -1.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK23" smd circle
		(at -0.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK24" smd circle
		(at 0.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK25" smd circle
		(at 1.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK26" smd circle
		(at 2.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK27" smd circle
		(at 3.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK28" smd circle
		(at 4.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK29" smd circle
		(at 5.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK30" smd circle
		(at 6.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK31" smd circle
		(at 7.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK32" smd circle
		(at 8.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK33" smd circle
		(at 9.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK34" smd circle
		(at 10.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK35" smd circle
		(at 11.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK36" smd circle
		(at 12.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK37" smd circle
		(at 13.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK38" smd circle
		(at 14.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK39" smd circle
		(at 15.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK40" smd circle
		(at 16.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AK41" smd circle
		(at 17.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK42" smd circle
		(at 18.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK43" smd circle
		(at 19.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK44" smd circle
		(at 20.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK45" smd circle
		(at 21.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AK46" smd circle
		(at 22.5 6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL1" smd circle
		(at -22.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL2" smd circle
		(at -21.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL3" smd circle
		(at -20.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL4" smd circle
		(at -19.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AL5" smd circle
		(at -18.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL6" smd circle
		(at -17.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL7" smd circle
		(at -16.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AL8" smd circle
		(at -15.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL9" smd circle
		(at -14.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL10" smd circle
		(at -13.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AL11" smd circle
		(at -12.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL12" smd circle
		(at -11.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL13" smd circle
		(at -10.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL14" smd circle
		(at -9.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL15" smd circle
		(at -8.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL16" smd circle
		(at -7.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL17" smd circle
		(at -6.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL18" smd circle
		(at -5.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL19" smd circle
		(at -4.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL20" smd circle
		(at -3.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL21" smd circle
		(at -2.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL22" smd circle
		(at -1.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL23" smd circle
		(at -0.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL24" smd circle
		(at 0.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL25" smd circle
		(at 1.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL26" smd circle
		(at 2.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL27" smd circle
		(at 3.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL28" smd circle
		(at 4.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL29" smd circle
		(at 5.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL30" smd circle
		(at 6.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL31" smd circle
		(at 7.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL32" smd circle
		(at 8.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL33" smd circle
		(at 9.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL34" smd circle
		(at 10.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL35" smd circle
		(at 11.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL36" smd circle
		(at 12.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL37" smd circle
		(at 13.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL38" smd circle
		(at 14.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL39" smd circle
		(at 15.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AL40" smd circle
		(at 16.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AL41" smd circle
		(at 17.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL42" smd circle
		(at 18.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL43" smd circle
		(at 19.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AL44" smd circle
		(at 20.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL45" smd circle
		(at 21.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AL46" smd circle
		(at 22.5 7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM1" smd circle
		(at -22.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM2" smd circle
		(at -21.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM3" smd circle
		(at -20.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM4" smd circle
		(at -19.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM5" smd circle
		(at -18.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AM6" smd circle
		(at -17.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM7" smd circle
		(at -16.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM8" smd circle
		(at -15.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AM9" smd circle
		(at -14.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM10" smd circle
		(at -13.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM11" smd circle
		(at -12.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM12" smd circle
		(at -11.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM13" smd circle
		(at -10.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM14" smd circle
		(at -9.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM15" smd circle
		(at -8.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM16" smd circle
		(at -7.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM17" smd circle
		(at -6.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM18" smd circle
		(at -5.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM19" smd circle
		(at -4.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM20" smd circle
		(at -3.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM21" smd circle
		(at -2.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM22" smd circle
		(at -1.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM23" smd circle
		(at -0.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM24" smd circle
		(at 0.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM25" smd circle
		(at 1.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM26" smd circle
		(at 2.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM27" smd circle
		(at 3.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM28" smd circle
		(at 4.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM29" smd circle
		(at 5.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM30" smd circle
		(at 6.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM31" smd circle
		(at 7.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM32" smd circle
		(at 8.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM33" smd circle
		(at 9.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM34" smd circle
		(at 10.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM35" smd circle
		(at 11.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM36" smd circle
		(at 12.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM37" smd circle
		(at 13.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM38" smd circle
		(at 14.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM39" smd circle
		(at 15.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM40" smd circle
		(at 16.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AM41" smd circle
		(at 17.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AM42" smd circle
		(at 18.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM43" smd circle
		(at 19.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM44" smd circle
		(at 20.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM45" smd circle
		(at 21.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AM46" smd circle
		(at 22.5 8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN1" smd circle
		(at -22.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN2" smd circle
		(at -21.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN3" smd circle
		(at -20.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN4" smd circle
		(at -19.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN5" smd circle
		(at -18.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN6" smd circle
		(at -17.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AN7" smd circle
		(at -16.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN8" smd circle
		(at -15.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN9" smd circle
		(at -14.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN10" smd circle
		(at -13.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AN11" smd circle
		(at -12.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN12" smd circle
		(at -11.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN13" smd circle
		(at -10.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN14" smd circle
		(at -9.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN15" smd circle
		(at -8.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN16" smd circle
		(at -7.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN17" smd circle
		(at -6.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN18" smd circle
		(at -5.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN19" smd circle
		(at -4.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN20" smd circle
		(at -3.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN21" smd circle
		(at -2.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN22" smd circle
		(at -1.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN23" smd circle
		(at -0.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN24" smd circle
		(at 0.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN25" smd circle
		(at 1.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN26" smd circle
		(at 2.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN27" smd circle
		(at 3.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN28" smd circle
		(at 4.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN29" smd circle
		(at 5.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN30" smd circle
		(at 6.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN31" smd circle
		(at 7.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN32" smd circle
		(at 8.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN33" smd circle
		(at 9.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN34" smd circle
		(at 10.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN35" smd circle
		(at 11.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN36" smd circle
		(at 12.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN37" smd circle
		(at 13.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN38" smd circle
		(at 14.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN39" smd circle
		(at 15.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN40" smd circle
		(at 16.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "AN41" smd circle
		(at 17.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN42" smd circle
		(at 18.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AN43" smd circle
		(at 19.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN44" smd circle
		(at 20.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN45" smd circle
		(at 21.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AN46" smd circle
		(at 22.5 9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP1" smd circle
		(at -22.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP2" smd circle
		(at -21.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP3" smd circle
		(at -20.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP4" smd circle
		(at -19.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AP5" smd circle
		(at -18.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP6" smd circle
		(at -17.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP7" smd circle
		(at -16.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP8" smd circle
		(at -15.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP9" smd circle
		(at -14.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AP10" smd circle
		(at -13.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP11" smd circle
		(at -12.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP12" smd circle
		(at -11.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP13" smd circle
		(at -10.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP14" smd circle
		(at -9.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP15" smd circle
		(at -8.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP16" smd circle
		(at -7.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP17" smd circle
		(at -6.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP18" smd circle
		(at -5.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP19" smd circle
		(at -4.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP20" smd circle
		(at -3.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP21" smd circle
		(at -2.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP22" smd circle
		(at -1.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP23" smd circle
		(at -0.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP24" smd circle
		(at 0.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP25" smd circle
		(at 1.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP26" smd circle
		(at 2.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP27" smd circle
		(at 3.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP28" smd circle
		(at 4.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP29" smd circle
		(at 5.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP30" smd circle
		(at 6.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP31" smd circle
		(at 7.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP32" smd circle
		(at 8.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP33" smd circle
		(at 9.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP34" smd circle
		(at 10.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP35" smd circle
		(at 11.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP36" smd circle
		(at 12.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP37" smd circle
		(at 13.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP38" smd circle
		(at 14.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP39" smd circle
		(at 15.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP40" smd circle
		(at 16.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AP41" smd circle
		(at 17.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP42" smd circle
		(at 18.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP43" smd circle
		(at 19.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP44" smd circle
		(at 20.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP45" smd circle
		(at 21.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AP46" smd circle
		(at 22.5 10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR1" smd circle
		(at -22.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR2" smd circle
		(at -21.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR3" smd circle
		(at -20.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR4" smd circle
		(at -19.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR5" smd circle
		(at -18.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR6" smd circle
		(at -17.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR7" smd circle
		(at -16.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AR8" smd circle
		(at -15.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR9" smd circle
		(at -14.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR10" smd circle
		(at -13.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AR11" smd circle
		(at -12.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR12" smd circle
		(at -11.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR13" smd circle
		(at -10.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR14" smd circle
		(at -9.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR15" smd circle
		(at -8.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR16" smd circle
		(at -7.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR17" smd circle
		(at -6.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR18" smd circle
		(at -5.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR19" smd circle
		(at -4.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR20" smd circle
		(at -3.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR21" smd circle
		(at -2.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR22" smd circle
		(at -1.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR23" smd circle
		(at -0.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR24" smd circle
		(at 0.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR25" smd circle
		(at 1.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR26" smd circle
		(at 2.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR27" smd circle
		(at 3.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR28" smd circle
		(at 4.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR29" smd circle
		(at 5.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR30" smd circle
		(at 6.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR31" smd circle
		(at 7.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR32" smd circle
		(at 8.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR33" smd circle
		(at 9.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR34" smd circle
		(at 10.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR35" smd circle
		(at 11.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR36" smd circle
		(at 12.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR37" smd circle
		(at 13.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR38" smd circle
		(at 14.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR39" smd circle
		(at 15.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR40" smd circle
		(at 16.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR41" smd circle
		(at 17.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR42" smd circle
		(at 18.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR43" smd circle
		(at 19.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AR44" smd circle
		(at 20.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR45" smd circle
		(at 21.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AR46" smd circle
		(at 22.5 11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT1" smd circle
		(at -22.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT2" smd circle
		(at -21.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT3" smd circle
		(at -20.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT4" smd circle
		(at -19.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT5" smd circle
		(at -18.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AT6" smd circle
		(at -17.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT7" smd circle
		(at -16.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT8" smd circle
		(at -15.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AT9" smd circle
		(at -14.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT10" smd circle
		(at -13.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT11" smd circle
		(at -12.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT12" smd circle
		(at -11.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT13" smd circle
		(at -10.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT14" smd circle
		(at -9.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT15" smd circle
		(at -8.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT16" smd circle
		(at -7.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT17" smd circle
		(at -6.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT18" smd circle
		(at -5.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT19" smd circle
		(at -4.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT20" smd circle
		(at -3.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT21" smd circle
		(at -2.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT22" smd circle
		(at -1.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT23" smd circle
		(at -0.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT24" smd circle
		(at 0.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT25" smd circle
		(at 1.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT26" smd circle
		(at 2.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT27" smd circle
		(at 3.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT28" smd circle
		(at 4.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT29" smd circle
		(at 5.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT30" smd circle
		(at 6.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT31" smd circle
		(at 7.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT32" smd circle
		(at 8.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT33" smd circle
		(at 9.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT34" smd circle
		(at 10.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT35" smd circle
		(at 11.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT36" smd circle
		(at 12.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT37" smd circle
		(at 13.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT38" smd circle
		(at 14.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT39" smd circle
		(at 15.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT40" smd circle
		(at 16.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT41" smd circle
		(at 17.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT42" smd circle
		(at 18.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT43" smd circle
		(at 19.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT44" smd circle
		(at 20.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT45" smd circle
		(at 21.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AT46" smd circle
		(at 22.5 12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU1" smd circle
		(at -22.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU2" smd circle
		(at -21.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU3" smd circle
		(at -20.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU4" smd circle
		(at -19.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU5" smd circle
		(at -18.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU6" smd circle
		(at -17.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AU7" smd circle
		(at -16.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU8" smd circle
		(at -15.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU9" smd circle
		(at -14.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU10" smd circle
		(at -13.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU11" smd circle
		(at -12.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU12" smd circle
		(at -11.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU13" smd circle
		(at -10.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU14" smd circle
		(at -9.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU15" smd circle
		(at -8.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU16" smd circle
		(at -7.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU17" smd circle
		(at -6.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU18" smd circle
		(at -5.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU19" smd circle
		(at -4.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU20" smd circle
		(at -3.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU21" smd circle
		(at -2.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU22" smd circle
		(at -1.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU23" smd circle
		(at -0.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU24" smd circle
		(at 0.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU25" smd circle
		(at 1.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU26" smd circle
		(at 2.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU27" smd circle
		(at 3.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU28" smd circle
		(at 4.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU29" smd circle
		(at 5.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU30" smd circle
		(at 6.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU31" smd circle
		(at 7.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU32" smd circle
		(at 8.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU33" smd circle
		(at 9.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU34" smd circle
		(at 10.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU35" smd circle
		(at 11.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU36" smd circle
		(at 12.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU37" smd circle
		(at 13.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU38" smd circle
		(at 14.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU39" smd circle
		(at 15.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU40" smd circle
		(at 16.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU41" smd circle
		(at 17.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU42" smd circle
		(at 18.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AU43" smd circle
		(at 19.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU44" smd circle
		(at 20.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU45" smd circle
		(at 21.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AU46" smd circle
		(at 22.5 13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV1" smd circle
		(at -22.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV2" smd circle
		(at -21.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV3" smd circle
		(at -20.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV4" smd circle
		(at -19.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AV5" smd circle
		(at -18.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV6" smd circle
		(at -17.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV7" smd circle
		(at -16.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV8" smd circle
		(at -15.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV9" smd circle
		(at -14.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV10" smd circle
		(at -13.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV11" smd circle
		(at -12.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV12" smd circle
		(at -11.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV13" smd circle
		(at -10.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV14" smd circle
		(at -9.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV15" smd circle
		(at -8.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV16" smd circle
		(at -7.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV17" smd circle
		(at -6.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV18" smd circle
		(at -5.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV19" smd circle
		(at -4.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV20" smd circle
		(at -3.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV21" smd circle
		(at -2.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV22" smd circle
		(at -1.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV23" smd circle
		(at -0.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV24" smd circle
		(at 0.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV25" smd circle
		(at 1.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV26" smd circle
		(at 2.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV27" smd circle
		(at 3.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV28" smd circle
		(at 4.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV29" smd circle
		(at 5.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV30" smd circle
		(at 6.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV31" smd circle
		(at 7.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV32" smd circle
		(at 8.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV33" smd circle
		(at 9.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV34" smd circle
		(at 10.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV35" smd circle
		(at 11.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV36" smd circle
		(at 12.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV37" smd circle
		(at 13.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV38" smd circle
		(at 14.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV39" smd circle
		(at 15.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV40" smd circle
		(at 16.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV41" smd circle
		(at 17.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV42" smd circle
		(at 18.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV43" smd circle
		(at 19.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV44" smd circle
		(at 20.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV45" smd circle
		(at 21.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AV46" smd circle
		(at 22.5 14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW1" smd circle
		(at -22.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW2" smd circle
		(at -21.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW3" smd circle
		(at -20.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW4" smd circle
		(at -19.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW5" smd circle
		(at -18.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW6" smd circle
		(at -17.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW7" smd circle
		(at -16.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW8" smd circle
		(at -15.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW9" smd circle
		(at -14.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW10" smd circle
		(at -13.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW11" smd circle
		(at -12.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW12" smd circle
		(at -11.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW13" smd circle
		(at -10.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW14" smd circle
		(at -9.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW15" smd circle
		(at -8.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW16" smd circle
		(at -7.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW17" smd circle
		(at -6.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW18" smd circle
		(at -5.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW19" smd circle
		(at -4.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW20" smd circle
		(at -3.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW21" smd circle
		(at -2.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW22" smd circle
		(at -1.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW23" smd circle
		(at -0.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW24" smd circle
		(at 0.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW25" smd circle
		(at 1.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW26" smd circle
		(at 2.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW27" smd circle
		(at 3.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW28" smd circle
		(at 4.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW29" smd circle
		(at 5.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW30" smd circle
		(at 6.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW31" smd circle
		(at 7.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW32" smd circle
		(at 8.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW33" smd circle
		(at 9.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW34" smd circle
		(at 10.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW35" smd circle
		(at 11.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW36" smd circle
		(at 12.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW37" smd circle
		(at 13.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW38" smd circle
		(at 14.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW39" smd circle
		(at 15.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW40" smd circle
		(at 16.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW41" smd circle
		(at 17.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW42" smd circle
		(at 18.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW43" smd circle
		(at 19.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "AW44" smd circle
		(at 20.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW45" smd circle
		(at 21.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AW46" smd circle
		(at 22.5 15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY1" smd circle
		(at -22.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY2" smd circle
		(at -21.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY3" smd circle
		(at -20.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY4" smd circle
		(at -19.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY5" smd circle
		(at -18.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "AY6" smd circle
		(at -17.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY7" smd circle
		(at -16.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY8" smd circle
		(at -15.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY9" smd circle
		(at -14.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY10" smd circle
		(at -13.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY11" smd circle
		(at -12.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY12" smd circle
		(at -11.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY13" smd circle
		(at -10.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY14" smd circle
		(at -9.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY15" smd circle
		(at -8.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY16" smd circle
		(at -7.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY17" smd circle
		(at -6.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY18" smd circle
		(at -5.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY19" smd circle
		(at -4.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY20" smd circle
		(at -3.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY21" smd circle
		(at -2.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY22" smd circle
		(at -1.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY23" smd circle
		(at -0.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY24" smd circle
		(at 0.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY25" smd circle
		(at 1.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY26" smd circle
		(at 2.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY27" smd circle
		(at 3.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY28" smd circle
		(at 4.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY29" smd circle
		(at 5.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY30" smd circle
		(at 6.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY31" smd circle
		(at 7.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY32" smd circle
		(at 8.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY33" smd circle
		(at 9.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY34" smd circle
		(at 10.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY35" smd circle
		(at 11.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY36" smd circle
		(at 12.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY37" smd circle
		(at 13.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY38" smd circle
		(at 14.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY39" smd circle
		(at 15.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY40" smd circle
		(at 16.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY41" smd circle
		(at 17.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY42" smd circle
		(at 18.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY43" smd circle
		(at 19.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY44" smd circle
		(at 20.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY45" smd circle
		(at 21.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "AY46" smd circle
		(at 22.5 16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B2" smd circle
		(at -21.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B3" smd circle
		(at -20.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "B4" smd circle
		(at -19.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B5" smd circle
		(at -18.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "B6" smd circle
		(at -17.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B7" smd circle
		(at -16.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B8" smd circle
		(at -15.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B9" smd circle
		(at -14.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B10" smd circle
		(at -13.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B11" smd circle
		(at -12.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B12" smd circle
		(at -11.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B13" smd circle
		(at -10.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B14" smd circle
		(at -9.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B15" smd circle
		(at -8.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B16" smd circle
		(at -7.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B17" smd circle
		(at -6.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B18" smd circle
		(at -5.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B19" smd circle
		(at -4.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B20" smd circle
		(at -3.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B21" smd circle
		(at -2.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B22" smd circle
		(at -1.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B23" smd circle
		(at -0.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B24" smd circle
		(at 0.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B25" smd circle
		(at 1.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B26" smd circle
		(at 2.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B27" smd circle
		(at 3.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B28" smd circle
		(at 4.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B29" smd circle
		(at 5.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B30" smd circle
		(at 6.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B31" smd circle
		(at 7.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B32" smd circle
		(at 8.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B33" smd circle
		(at 9.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B34" smd circle
		(at 10.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B35" smd circle
		(at 11.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B36" smd circle
		(at 12.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B37" smd circle
		(at 13.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B38" smd circle
		(at 14.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B39" smd circle
		(at 15.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B40" smd circle
		(at 16.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B41" smd circle
		(at 17.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B42" smd circle
		(at 18.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B43" smd circle
		(at 19.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "B44" smd circle
		(at 20.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "B45" smd circle
		(at 21.5 -21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA1" smd circle
		(at -22.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA2" smd circle
		(at -21.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA3" smd circle
		(at -20.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA4" smd circle
		(at -19.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA5" smd circle
		(at -18.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA6" smd circle
		(at -17.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA7" smd circle
		(at -16.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA8" smd circle
		(at -15.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA9" smd circle
		(at -14.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA10" smd circle
		(at -13.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA11" smd circle
		(at -12.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA12" smd circle
		(at -11.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA13" smd circle
		(at -10.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA14" smd circle
		(at -9.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA15" smd circle
		(at -8.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA16" smd circle
		(at -7.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA17" smd circle
		(at -6.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA18" smd circle
		(at -5.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA19" smd circle
		(at -4.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA20" smd circle
		(at -3.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA21" smd circle
		(at -2.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA22" smd circle
		(at -1.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA23" smd circle
		(at -0.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA24" smd circle
		(at 0.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA25" smd circle
		(at 1.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA26" smd circle
		(at 2.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA27" smd circle
		(at 3.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA28" smd circle
		(at 4.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA29" smd circle
		(at 5.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA30" smd circle
		(at 6.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA31" smd circle
		(at 7.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA32" smd circle
		(at 8.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA33" smd circle
		(at 9.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA34" smd circle
		(at 10.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA35" smd circle
		(at 11.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA36" smd circle
		(at 12.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA37" smd circle
		(at 13.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA38" smd circle
		(at 14.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA39" smd circle
		(at 15.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA40" smd circle
		(at 16.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA41" smd circle
		(at 17.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA42" smd circle
		(at 18.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "BA43" smd circle
		(at 19.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA44" smd circle
		(at 20.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA45" smd circle
		(at 21.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BA46" smd circle
		(at 22.5 17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB1" smd circle
		(at -22.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB2" smd circle
		(at -21.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB3" smd circle
		(at -20.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB4" smd circle
		(at -19.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "BB5" smd circle
		(at -18.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB6" smd circle
		(at -17.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB7" smd circle
		(at -16.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB8" smd circle
		(at -15.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB9" smd circle
		(at -14.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB10" smd circle
		(at -13.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB11" smd circle
		(at -12.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB12" smd circle
		(at -11.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB13" smd circle
		(at -10.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB14" smd circle
		(at -9.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB15" smd circle
		(at -8.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB16" smd circle
		(at -7.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB17" smd circle
		(at -6.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB18" smd circle
		(at -5.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB19" smd circle
		(at -4.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB20" smd circle
		(at -3.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB21" smd circle
		(at -2.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB22" smd circle
		(at -1.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB23" smd circle
		(at -0.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB24" smd circle
		(at 0.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB25" smd circle
		(at 1.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB26" smd circle
		(at 2.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB27" smd circle
		(at 3.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB28" smd circle
		(at 4.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB29" smd circle
		(at 5.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB30" smd circle
		(at 6.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB31" smd circle
		(at 7.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB32" smd circle
		(at 8.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB33" smd circle
		(at 9.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB34" smd circle
		(at 10.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB35" smd circle
		(at 11.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB36" smd circle
		(at 12.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB37" smd circle
		(at 13.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB38" smd circle
		(at 14.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB39" smd circle
		(at 15.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB40" smd circle
		(at 16.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB41" smd circle
		(at 17.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB42" smd circle
		(at 18.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB43" smd circle
		(at 19.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB44" smd circle
		(at 20.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB45" smd circle
		(at 21.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BB46" smd circle
		(at 22.5 18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC1" smd circle
		(at -22.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC2" smd circle
		(at -21.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC3" smd circle
		(at -20.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC4" smd circle
		(at -19.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC5" smd circle
		(at -18.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC6" smd circle
		(at -17.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC7" smd circle
		(at -16.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC8" smd circle
		(at -15.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC9" smd circle
		(at -14.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC10" smd circle
		(at -13.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC11" smd circle
		(at -12.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC12" smd circle
		(at -11.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC13" smd circle
		(at -10.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC14" smd circle
		(at -9.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC15" smd circle
		(at -8.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC16" smd circle
		(at -7.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC17" smd circle
		(at -6.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC18" smd circle
		(at -5.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC19" smd circle
		(at -4.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC20" smd circle
		(at -3.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC21" smd circle
		(at -2.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC22" smd circle
		(at -1.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC23" smd circle
		(at -0.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC24" smd circle
		(at 0.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC25" smd circle
		(at 1.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC26" smd circle
		(at 2.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC27" smd circle
		(at 3.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC28" smd circle
		(at 4.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC29" smd circle
		(at 5.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC30" smd circle
		(at 6.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC31" smd circle
		(at 7.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC32" smd circle
		(at 8.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC33" smd circle
		(at 9.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC34" smd circle
		(at 10.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC35" smd circle
		(at 11.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC36" smd circle
		(at 12.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC37" smd circle
		(at 13.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC38" smd circle
		(at 14.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC39" smd circle
		(at 15.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC40" smd circle
		(at 16.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC41" smd circle
		(at 17.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC42" smd circle
		(at 18.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC43" smd circle
		(at 19.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "BC44" smd circle
		(at 20.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC45" smd circle
		(at 21.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BC46" smd circle
		(at 22.5 19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD1" smd circle
		(at -22.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD2" smd circle
		(at -21.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD3" smd circle
		(at -20.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "BD4" smd circle
		(at -19.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD5" smd circle
		(at -18.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "BD6" smd circle
		(at -17.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD7" smd circle
		(at -16.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD8" smd circle
		(at -15.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD9" smd circle
		(at -14.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD10" smd circle
		(at -13.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD11" smd circle
		(at -12.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD12" smd circle
		(at -11.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD13" smd circle
		(at -10.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD14" smd circle
		(at -9.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD15" smd circle
		(at -8.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD16" smd circle
		(at -7.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD17" smd circle
		(at -6.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD18" smd circle
		(at -5.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD19" smd circle
		(at -4.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD20" smd circle
		(at -3.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD21" smd circle
		(at -2.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD22" smd circle
		(at -1.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD23" smd circle
		(at -0.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD24" smd circle
		(at 0.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD25" smd circle
		(at 1.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD26" smd circle
		(at 2.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD27" smd circle
		(at 3.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD28" smd circle
		(at 4.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD29" smd circle
		(at 5.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD30" smd circle
		(at 6.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD31" smd circle
		(at 7.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD32" smd circle
		(at 8.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD33" smd circle
		(at 9.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD34" smd circle
		(at 10.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD35" smd circle
		(at 11.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD36" smd circle
		(at 12.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD37" smd circle
		(at 13.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD38" smd circle
		(at 14.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD39" smd circle
		(at 15.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD40" smd circle
		(at 16.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD41" smd circle
		(at 17.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD42" smd circle
		(at 18.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD43" smd circle
		(at 19.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD44" smd circle
		(at 20.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD45" smd circle
		(at 21.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BD46" smd circle
		(at 22.5 20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE2" smd circle
		(at -21.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE3" smd circle
		(at -20.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "BE4" smd circle
		(at -19.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE5" smd circle
		(at -18.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE6" smd circle
		(at -17.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE7" smd circle
		(at -16.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE8" smd circle
		(at -15.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE9" smd circle
		(at -14.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE10" smd circle
		(at -13.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE11" smd circle
		(at -12.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE12" smd circle
		(at -11.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE13" smd circle
		(at -10.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE14" smd circle
		(at -9.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE15" smd circle
		(at -8.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE16" smd circle
		(at -7.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE17" smd circle
		(at -6.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE18" smd circle
		(at -5.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE19" smd circle
		(at -4.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE20" smd circle
		(at -3.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE21" smd circle
		(at -2.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE22" smd circle
		(at -1.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE23" smd circle
		(at -0.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE24" smd circle
		(at 0.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE25" smd circle
		(at 1.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE26" smd circle
		(at 2.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE27" smd circle
		(at 3.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE28" smd circle
		(at 4.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE29" smd circle
		(at 5.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE30" smd circle
		(at 6.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE31" smd circle
		(at 7.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE32" smd circle
		(at 8.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE33" smd circle
		(at 9.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE34" smd circle
		(at 10.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE35" smd circle
		(at 11.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE36" smd circle
		(at 12.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE37" smd circle
		(at 13.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE38" smd circle
		(at 14.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE39" smd circle
		(at 15.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE40" smd circle
		(at 16.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE41" smd circle
		(at 17.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BE42" smd circle
		(at 18.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "BE43" smd circle
		(at 19.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04572)
	)
	(pad "BE44" smd circle
		(at 20.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "BE45" smd circle
		(at 21.5 21.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF3" smd circle
		(at -20.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF4" smd circle
		(at -19.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "BF5" smd circle
		(at -18.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF6" smd circle
		(at -17.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF7" smd circle
		(at -16.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF8" smd circle
		(at -15.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF9" smd circle
		(at -14.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF10" smd circle
		(at -13.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF11" smd circle
		(at -12.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF12" smd circle
		(at -11.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF13" smd circle
		(at -10.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF14" smd circle
		(at -9.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF15" smd circle
		(at -8.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF16" smd circle
		(at -7.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF17" smd circle
		(at -6.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF18" smd circle
		(at -5.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF19" smd circle
		(at -4.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF20" smd circle
		(at -3.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF21" smd circle
		(at -2.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF22" smd circle
		(at -1.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF23" smd circle
		(at -0.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF24" smd circle
		(at 0.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF25" smd circle
		(at 1.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF26" smd circle
		(at 2.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF27" smd circle
		(at 3.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF28" smd circle
		(at 4.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF29" smd circle
		(at 5.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF30" smd circle
		(at 6.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF31" smd circle
		(at 7.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF32" smd circle
		(at 8.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF33" smd circle
		(at 9.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF34" smd circle
		(at 10.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF35" smd circle
		(at 11.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF36" smd circle
		(at 12.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF37" smd circle
		(at 13.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF38" smd circle
		(at 14.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF39" smd circle
		(at 15.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF40" smd circle
		(at 16.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF41" smd circle
		(at 17.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "BF42" smd circle
		(at 18.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "BF43" smd circle
		(at 19.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04572)
	)
	(pad "BF44" smd circle
		(at 20.5 22.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C1" smd circle
		(at -22.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C2" smd circle
		(at -21.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C3" smd circle
		(at -20.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C4" smd circle
		(at -19.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C5" smd circle
		(at -18.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C6" smd circle
		(at -17.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C7" smd circle
		(at -16.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C8" smd circle
		(at -15.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C9" smd circle
		(at -14.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C10" smd circle
		(at -13.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C11" smd circle
		(at -12.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C12" smd circle
		(at -11.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C13" smd circle
		(at -10.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C14" smd circle
		(at -9.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C15" smd circle
		(at -8.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C16" smd circle
		(at -7.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C17" smd circle
		(at -6.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C18" smd circle
		(at -5.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C19" smd circle
		(at -4.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C20" smd circle
		(at -3.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C21" smd circle
		(at -2.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C22" smd circle
		(at -1.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C23" smd circle
		(at -0.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C24" smd circle
		(at 0.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C25" smd circle
		(at 1.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C26" smd circle
		(at 2.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C27" smd circle
		(at 3.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C28" smd circle
		(at 4.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C29" smd circle
		(at 5.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C30" smd circle
		(at 6.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C31" smd circle
		(at 7.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C32" smd circle
		(at 8.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C33" smd circle
		(at 9.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C34" smd circle
		(at 10.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C35" smd circle
		(at 11.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C36" smd circle
		(at 12.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C37" smd circle
		(at 13.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C38" smd circle
		(at 14.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C39" smd circle
		(at 15.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C40" smd circle
		(at 16.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C41" smd circle
		(at 17.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C42" smd circle
		(at 18.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C43" smd circle
		(at 19.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "C44" smd circle
		(at 20.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "C45" smd circle
		(at 21.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "C46" smd circle
		(at 22.5 -20.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D1" smd circle
		(at -22.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D2" smd circle
		(at -21.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D3" smd circle
		(at -20.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D4" smd circle
		(at -19.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "D5" smd circle
		(at -18.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D6" smd circle
		(at -17.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D7" smd circle
		(at -16.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D8" smd circle
		(at -15.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D9" smd circle
		(at -14.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D10" smd circle
		(at -13.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D11" smd circle
		(at -12.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D12" smd circle
		(at -11.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D13" smd circle
		(at -10.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D14" smd circle
		(at -9.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D15" smd circle
		(at -8.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D16" smd circle
		(at -7.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D17" smd circle
		(at -6.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D18" smd circle
		(at -5.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D19" smd circle
		(at -4.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D20" smd circle
		(at -3.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D21" smd circle
		(at -2.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D22" smd circle
		(at -1.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D23" smd circle
		(at -0.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D24" smd circle
		(at 0.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D25" smd circle
		(at 1.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D26" smd circle
		(at 2.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D27" smd circle
		(at 3.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D28" smd circle
		(at 4.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D29" smd circle
		(at 5.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D30" smd circle
		(at 6.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D31" smd circle
		(at 7.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D32" smd circle
		(at 8.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D33" smd circle
		(at 9.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D34" smd circle
		(at 10.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D35" smd circle
		(at 11.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D36" smd circle
		(at 12.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D37" smd circle
		(at 13.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D38" smd circle
		(at 14.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D39" smd circle
		(at 15.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D40" smd circle
		(at 16.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D41" smd circle
		(at 17.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D42" smd circle
		(at 18.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D43" smd circle
		(at 19.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D44" smd circle
		(at 20.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D45" smd circle
		(at 21.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "D46" smd circle
		(at 22.5 -19.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E1" smd circle
		(at -22.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E2" smd circle
		(at -21.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E3" smd circle
		(at -20.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E4" smd circle
		(at -19.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E5" smd circle
		(at -18.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E6" smd circle
		(at -17.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E7" smd circle
		(at -16.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E8" smd circle
		(at -15.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E9" smd circle
		(at -14.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E10" smd circle
		(at -13.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E11" smd circle
		(at -12.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E12" smd circle
		(at -11.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E13" smd circle
		(at -10.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E14" smd circle
		(at -9.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E15" smd circle
		(at -8.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E16" smd circle
		(at -7.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E17" smd circle
		(at -6.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E18" smd circle
		(at -5.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E19" smd circle
		(at -4.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E20" smd circle
		(at -3.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E21" smd circle
		(at -2.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E22" smd circle
		(at -1.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E23" smd circle
		(at -0.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E24" smd circle
		(at 0.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E25" smd circle
		(at 1.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E26" smd circle
		(at 2.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E27" smd circle
		(at 3.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E28" smd circle
		(at 4.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E29" smd circle
		(at 5.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E30" smd circle
		(at 6.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E31" smd circle
		(at 7.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E32" smd circle
		(at 8.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E33" smd circle
		(at 9.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E34" smd circle
		(at 10.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E35" smd circle
		(at 11.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E36" smd circle
		(at 12.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E37" smd circle
		(at 13.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E38" smd circle
		(at 14.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E39" smd circle
		(at 15.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E40" smd circle
		(at 16.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E41" smd circle
		(at 17.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E42" smd circle
		(at 18.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "E43" smd circle
		(at 19.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E44" smd circle
		(at 20.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E45" smd circle
		(at 21.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "E46" smd circle
		(at 22.5 -18.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F1" smd circle
		(at -22.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F2" smd circle
		(at -21.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F3" smd circle
		(at -20.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F4" smd circle
		(at -19.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F5" smd circle
		(at -18.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "F6" smd circle
		(at -17.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F7" smd circle
		(at -16.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F8" smd circle
		(at -15.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F9" smd circle
		(at -14.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F10" smd circle
		(at -13.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F11" smd circle
		(at -12.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F12" smd circle
		(at -11.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F13" smd circle
		(at -10.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F14" smd circle
		(at -9.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F15" smd circle
		(at -8.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F16" smd circle
		(at -7.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F17" smd circle
		(at -6.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F18" smd circle
		(at -5.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F19" smd circle
		(at -4.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F20" smd circle
		(at -3.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F21" smd circle
		(at -2.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F22" smd circle
		(at -1.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F23" smd circle
		(at -0.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F24" smd circle
		(at 0.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F25" smd circle
		(at 1.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F26" smd circle
		(at 2.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F27" smd circle
		(at 3.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F28" smd circle
		(at 4.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F29" smd circle
		(at 5.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F30" smd circle
		(at 6.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F31" smd circle
		(at 7.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F32" smd circle
		(at 8.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F33" smd circle
		(at 9.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F34" smd circle
		(at 10.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F35" smd circle
		(at 11.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F36" smd circle
		(at 12.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F37" smd circle
		(at 13.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F38" smd circle
		(at 14.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F39" smd circle
		(at 15.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F40" smd circle
		(at 16.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F41" smd circle
		(at 17.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F42" smd circle
		(at 18.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F43" smd circle
		(at 19.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F44" smd circle
		(at 20.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F45" smd circle
		(at 21.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "F46" smd circle
		(at 22.5 -17.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G1" smd circle
		(at -22.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G2" smd circle
		(at -21.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G3" smd circle
		(at -20.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G4" smd circle
		(at -19.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G5" smd circle
		(at -18.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G6" smd circle
		(at -17.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G7" smd circle
		(at -16.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "G8" smd circle
		(at -15.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G9" smd circle
		(at -14.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G10" smd circle
		(at -13.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G11" smd circle
		(at -12.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G12" smd circle
		(at -11.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G13" smd circle
		(at -10.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G14" smd circle
		(at -9.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G15" smd circle
		(at -8.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G16" smd circle
		(at -7.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G17" smd circle
		(at -6.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G18" smd circle
		(at -5.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G19" smd circle
		(at -4.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G20" smd circle
		(at -3.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G21" smd circle
		(at -2.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G22" smd circle
		(at -1.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G23" smd circle
		(at -0.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G24" smd circle
		(at 0.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G25" smd circle
		(at 1.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G26" smd circle
		(at 2.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G27" smd circle
		(at 3.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G28" smd circle
		(at 4.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G29" smd circle
		(at 5.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G30" smd circle
		(at 6.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G31" smd circle
		(at 7.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G32" smd circle
		(at 8.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G33" smd circle
		(at 9.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G34" smd circle
		(at 10.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G35" smd circle
		(at 11.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G36" smd circle
		(at 12.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G37" smd circle
		(at 13.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G38" smd circle
		(at 14.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G39" smd circle
		(at 15.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G40" smd circle
		(at 16.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G41" smd circle
		(at 17.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G42" smd circle
		(at 18.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G43" smd circle
		(at 19.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "G44" smd circle
		(at 20.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G45" smd circle
		(at 21.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "G46" smd circle
		(at 22.5 -16.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H1" smd circle
		(at -22.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H2" smd circle
		(at -21.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H3" smd circle
		(at -20.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H4" smd circle
		(at -19.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "H5" smd circle
		(at -18.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H6" smd circle
		(at -17.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H7" smd circle
		(at -16.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H8" smd circle
		(at -15.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H9" smd circle
		(at -14.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H10" smd circle
		(at -13.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H11" smd circle
		(at -12.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H12" smd circle
		(at -11.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H13" smd circle
		(at -10.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H14" smd circle
		(at -9.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H15" smd circle
		(at -8.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H16" smd circle
		(at -7.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H17" smd circle
		(at -6.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H18" smd circle
		(at -5.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H19" smd circle
		(at -4.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H20" smd circle
		(at -3.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H21" smd circle
		(at -2.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H22" smd circle
		(at -1.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H23" smd circle
		(at -0.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H24" smd circle
		(at 0.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H25" smd circle
		(at 1.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H26" smd circle
		(at 2.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H27" smd circle
		(at 3.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H28" smd circle
		(at 4.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H29" smd circle
		(at 5.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H30" smd circle
		(at 6.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H31" smd circle
		(at 7.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H32" smd circle
		(at 8.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H33" smd circle
		(at 9.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H34" smd circle
		(at 10.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H35" smd circle
		(at 11.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H36" smd circle
		(at 12.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H37" smd circle
		(at 13.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H38" smd circle
		(at 14.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H39" smd circle
		(at 15.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H40" smd circle
		(at 16.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H41" smd circle
		(at 17.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H42" smd circle
		(at 18.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H43" smd circle
		(at 19.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H44" smd circle
		(at 20.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H45" smd circle
		(at 21.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "H46" smd circle
		(at 22.5 -15.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J1" smd circle
		(at -22.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J2" smd circle
		(at -21.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J3" smd circle
		(at -20.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J4" smd circle
		(at -19.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J5" smd circle
		(at -18.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J6" smd circle
		(at -17.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "J7" smd circle
		(at -16.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J8" smd circle
		(at -15.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J9" smd circle
		(at -14.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J10" smd circle
		(at -13.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J11" smd circle
		(at -12.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J12" smd circle
		(at -11.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J13" smd circle
		(at -10.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J14" smd circle
		(at -9.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J15" smd circle
		(at -8.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J16" smd circle
		(at -7.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J17" smd circle
		(at -6.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J18" smd circle
		(at -5.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J19" smd circle
		(at -4.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J20" smd circle
		(at -3.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J21" smd circle
		(at -2.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J22" smd circle
		(at -1.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J23" smd circle
		(at -0.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J24" smd circle
		(at 0.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J25" smd circle
		(at 1.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J26" smd circle
		(at 2.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J27" smd circle
		(at 3.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J28" smd circle
		(at 4.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J29" smd circle
		(at 5.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J30" smd circle
		(at 6.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J31" smd circle
		(at 7.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J32" smd circle
		(at 8.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J33" smd circle
		(at 9.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J34" smd circle
		(at 10.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J35" smd circle
		(at 11.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J36" smd circle
		(at 12.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J37" smd circle
		(at 13.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J38" smd circle
		(at 14.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J39" smd circle
		(at 15.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J40" smd circle
		(at 16.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J41" smd circle
		(at 17.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J42" smd circle
		(at 18.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "J43" smd circle
		(at 19.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J44" smd circle
		(at 20.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J45" smd circle
		(at 21.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "J46" smd circle
		(at 22.5 -14.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K1" smd circle
		(at -22.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K2" smd circle
		(at -21.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K3" smd circle
		(at -20.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K4" smd circle
		(at -19.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K5" smd circle
		(at -18.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "K6" smd circle
		(at -17.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K7" smd circle
		(at -16.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K8" smd circle
		(at -15.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K9" smd circle
		(at -14.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "K10" smd circle
		(at -13.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K11" smd circle
		(at -12.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K12" smd circle
		(at -11.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K13" smd circle
		(at -10.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K14" smd circle
		(at -9.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K15" smd circle
		(at -8.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K16" smd circle
		(at -7.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K17" smd circle
		(at -6.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K18" smd circle
		(at -5.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K19" smd circle
		(at -4.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K20" smd circle
		(at -3.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K21" smd circle
		(at -2.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K22" smd circle
		(at -1.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K23" smd circle
		(at -0.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K24" smd circle
		(at 0.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K25" smd circle
		(at 1.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K26" smd circle
		(at 2.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K27" smd circle
		(at 3.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K28" smd circle
		(at 4.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K29" smd circle
		(at 5.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K30" smd circle
		(at 6.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K31" smd circle
		(at 7.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K32" smd circle
		(at 8.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K33" smd circle
		(at 9.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K34" smd circle
		(at 10.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K35" smd circle
		(at 11.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K36" smd circle
		(at 12.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K37" smd circle
		(at 13.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K38" smd circle
		(at 14.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K39" smd circle
		(at 15.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K40" smd circle
		(at 16.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K41" smd circle
		(at 17.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K42" smd circle
		(at 18.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K43" smd circle
		(at 19.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K44" smd circle
		(at 20.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K45" smd circle
		(at 21.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "K46" smd circle
		(at 22.5 -13.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L1" smd circle
		(at -22.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L2" smd circle
		(at -21.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L3" smd circle
		(at -20.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L4" smd circle
		(at -19.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L5" smd circle
		(at -18.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L6" smd circle
		(at -17.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L7" smd circle
		(at -16.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "L8" smd circle
		(at -15.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L9" smd circle
		(at -14.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L10" smd circle
		(at -13.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L11" smd circle
		(at -12.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L12" smd circle
		(at -11.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L13" smd circle
		(at -10.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L14" smd circle
		(at -9.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L15" smd circle
		(at -8.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L16" smd circle
		(at -7.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L17" smd circle
		(at -6.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L18" smd circle
		(at -5.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L19" smd circle
		(at -4.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L20" smd circle
		(at -3.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L21" smd circle
		(at -2.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L22" smd circle
		(at -1.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L23" smd circle
		(at -0.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L24" smd circle
		(at 0.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L25" smd circle
		(at 1.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L26" smd circle
		(at 2.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L27" smd circle
		(at 3.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L28" smd circle
		(at 4.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L29" smd circle
		(at 5.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L30" smd circle
		(at 6.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L31" smd circle
		(at 7.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L32" smd circle
		(at 8.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L33" smd circle
		(at 9.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L34" smd circle
		(at 10.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L35" smd circle
		(at 11.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L36" smd circle
		(at 12.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L37" smd circle
		(at 13.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L38" smd circle
		(at 14.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L39" smd circle
		(at 15.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L40" smd circle
		(at 16.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "L41" smd circle
		(at 17.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L42" smd circle
		(at 18.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L43" smd circle
		(at 19.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "L44" smd circle
		(at 20.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L45" smd circle
		(at 21.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "L46" smd circle
		(at 22.5 -12.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M1" smd circle
		(at -22.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M2" smd circle
		(at -21.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M3" smd circle
		(at -20.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M4" smd circle
		(at -19.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "M5" smd circle
		(at -18.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M6" smd circle
		(at -17.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M7" smd circle
		(at -16.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M8" smd circle
		(at -15.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "M9" smd circle
		(at -14.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M10" smd circle
		(at -13.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M11" smd circle
		(at -12.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M12" smd circle
		(at -11.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M13" smd circle
		(at -10.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M14" smd circle
		(at -9.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M15" smd circle
		(at -8.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M16" smd circle
		(at -7.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M17" smd circle
		(at -6.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M18" smd circle
		(at -5.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M19" smd circle
		(at -4.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M20" smd circle
		(at -3.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M21" smd circle
		(at -2.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M22" smd circle
		(at -1.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M23" smd circle
		(at -0.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M24" smd circle
		(at 0.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M25" smd circle
		(at 1.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M26" smd circle
		(at 2.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M27" smd circle
		(at 3.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M28" smd circle
		(at 4.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M29" smd circle
		(at 5.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M30" smd circle
		(at 6.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M31" smd circle
		(at 7.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M32" smd circle
		(at 8.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M33" smd circle
		(at 9.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M34" smd circle
		(at 10.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M35" smd circle
		(at 11.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M36" smd circle
		(at 12.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M37" smd circle
		(at 13.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M38" smd circle
		(at 14.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M39" smd circle
		(at 15.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M40" smd circle
		(at 16.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M41" smd circle
		(at 17.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M42" smd circle
		(at 18.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M43" smd circle
		(at 19.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M44" smd circle
		(at 20.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M45" smd circle
		(at 21.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "M46" smd circle
		(at 22.5 -11.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N1" smd circle
		(at -22.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N2" smd circle
		(at -21.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N3" smd circle
		(at -20.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N4" smd circle
		(at -19.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N5" smd circle
		(at -18.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "N6" smd circle
		(at -17.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "N7" smd circle
		(at -16.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N8" smd circle
		(at -15.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N9" smd circle
		(at -14.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N10" smd circle
		(at -13.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N11" smd circle
		(at -12.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N12" smd circle
		(at -11.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N13" smd circle
		(at -10.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N14" smd circle
		(at -9.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N15" smd circle
		(at -8.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N16" smd circle
		(at -7.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N17" smd circle
		(at -6.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N18" smd circle
		(at -5.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N19" smd circle
		(at -4.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N20" smd circle
		(at -3.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N21" smd circle
		(at -2.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N22" smd circle
		(at -1.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N23" smd circle
		(at -0.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N24" smd circle
		(at 0.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N25" smd circle
		(at 1.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N26" smd circle
		(at 2.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N27" smd circle
		(at 3.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N28" smd circle
		(at 4.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N29" smd circle
		(at 5.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N30" smd circle
		(at 6.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N31" smd circle
		(at 7.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N32" smd circle
		(at 8.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N33" smd circle
		(at 9.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N34" smd circle
		(at 10.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N35" smd circle
		(at 11.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N36" smd circle
		(at 12.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N37" smd circle
		(at 13.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N38" smd circle
		(at 14.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N39" smd circle
		(at 15.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N40" smd circle
		(at 16.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N41" smd circle
		(at 17.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N42" smd circle
		(at 18.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "N43" smd circle
		(at 19.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N44" smd circle
		(at 20.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N45" smd circle
		(at 21.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "N46" smd circle
		(at 22.5 -10.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P1" smd circle
		(at -22.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P2" smd circle
		(at -21.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P3" smd circle
		(at -20.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P4" smd circle
		(at -19.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P5" smd circle
		(at -18.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P6" smd circle
		(at -17.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P7" smd circle
		(at -16.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P8" smd circle
		(at -15.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P9" smd circle
		(at -14.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "P10" smd circle
		(at -13.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P11" smd circle
		(at -12.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P12" smd circle
		(at -11.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P13" smd circle
		(at -10.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P14" smd circle
		(at -9.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P15" smd circle
		(at -8.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P16" smd circle
		(at -7.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P17" smd circle
		(at -6.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P18" smd circle
		(at -5.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P19" smd circle
		(at -4.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P20" smd circle
		(at -3.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P21" smd circle
		(at -2.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P22" smd circle
		(at -1.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P23" smd circle
		(at -0.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P24" smd circle
		(at 0.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P25" smd circle
		(at 1.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P26" smd circle
		(at 2.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P27" smd circle
		(at 3.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P28" smd circle
		(at 4.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P29" smd circle
		(at 5.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P30" smd circle
		(at 6.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P31" smd circle
		(at 7.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P32" smd circle
		(at 8.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P33" smd circle
		(at 9.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P34" smd circle
		(at 10.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P35" smd circle
		(at 11.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P36" smd circle
		(at 12.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P37" smd circle
		(at 13.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P38" smd circle
		(at 14.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P39" smd circle
		(at 15.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P40" smd circle
		(at 16.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "P41" smd circle
		(at 17.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P42" smd circle
		(at 18.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P43" smd circle
		(at 19.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P44" smd circle
		(at 20.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P45" smd circle
		(at 21.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "P46" smd circle
		(at 22.5 -9.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R1" smd circle
		(at -22.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04572)
	)
	(pad "R2" smd circle
		(at -21.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04572)
	)
	(pad "R3" smd circle
		(at -20.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R4" smd circle
		(at -19.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R5" smd circle
		(at -18.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R6" smd circle
		(at -17.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R7" smd circle
		(at -16.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "R8" smd circle
		(at -15.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R9" smd circle
		(at -14.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R10" smd circle
		(at -13.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R11" smd circle
		(at -12.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R12" smd circle
		(at -11.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R13" smd circle
		(at -10.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R14" smd circle
		(at -9.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R15" smd circle
		(at -8.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R16" smd circle
		(at -7.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R17" smd circle
		(at -6.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R18" smd circle
		(at -5.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R19" smd circle
		(at -4.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R20" smd circle
		(at -3.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R21" smd circle
		(at -2.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R22" smd circle
		(at -1.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R23" smd circle
		(at -0.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R24" smd circle
		(at 0.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R25" smd circle
		(at 1.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R26" smd circle
		(at 2.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R27" smd circle
		(at 3.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R28" smd circle
		(at 4.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R29" smd circle
		(at 5.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R30" smd circle
		(at 6.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R31" smd circle
		(at 7.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R32" smd circle
		(at 8.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R33" smd circle
		(at 9.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R34" smd circle
		(at 10.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R35" smd circle
		(at 11.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R36" smd circle
		(at 12.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R37" smd circle
		(at 13.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R38" smd circle
		(at 14.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R39" smd circle
		(at 15.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R40" smd circle
		(at 16.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R41" smd circle
		(at 17.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R42" smd circle
		(at 18.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R43" smd circle
		(at 19.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "R44" smd circle
		(at 20.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R45" smd circle
		(at 21.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "R46" smd circle
		(at 22.5 -8.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T1" smd circle
		(at -22.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04572)
	)
	(pad "T2" smd circle
		(at -21.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04572)
	)
	(pad "T3" smd circle
		(at -20.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "T4" smd circle
		(at -19.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T5" smd circle
		(at -18.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T6" smd circle
		(at -17.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T7" smd circle
		(at -16.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T8" smd circle
		(at -15.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T9" smd circle
		(at -14.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T10" smd circle
		(at -13.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T11" smd circle
		(at -12.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T12" smd circle
		(at -11.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T13" smd circle
		(at -10.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T14" smd circle
		(at -9.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T15" smd circle
		(at -8.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T16" smd circle
		(at -7.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T17" smd circle
		(at -6.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T18" smd circle
		(at -5.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T19" smd circle
		(at -4.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T20" smd circle
		(at -3.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T21" smd circle
		(at -2.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T22" smd circle
		(at -1.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T23" smd circle
		(at -0.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T24" smd circle
		(at 0.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T25" smd circle
		(at 1.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T26" smd circle
		(at 2.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T27" smd circle
		(at 3.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T28" smd circle
		(at 4.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T29" smd circle
		(at 5.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T30" smd circle
		(at 6.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T31" smd circle
		(at 7.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T32" smd circle
		(at 8.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T33" smd circle
		(at 9.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T34" smd circle
		(at 10.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T35" smd circle
		(at 11.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T36" smd circle
		(at 12.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T37" smd circle
		(at 13.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T38" smd circle
		(at 14.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T39" smd circle
		(at 15.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T40" smd circle
		(at 16.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T41" smd circle
		(at 17.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "T42" smd circle
		(at 18.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T43" smd circle
		(at 19.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T44" smd circle
		(at 20.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T45" smd circle
		(at 21.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "T46" smd circle
		(at 22.5 -7.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U1" smd circle
		(at -22.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U2" smd circle
		(at -21.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U3" smd circle
		(at -20.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U4" smd circle
		(at -19.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U5" smd circle
		(at -18.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U6" smd circle
		(at -17.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "U7" smd circle
		(at -16.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U8" smd circle
		(at -15.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U9" smd circle
		(at -14.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U10" smd circle
		(at -13.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U11" smd circle
		(at -12.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U12" smd circle
		(at -11.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U13" smd circle
		(at -10.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U14" smd circle
		(at -9.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U15" smd circle
		(at -8.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U16" smd circle
		(at -7.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U17" smd circle
		(at -6.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U18" smd circle
		(at -5.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U19" smd circle
		(at -4.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U20" smd circle
		(at -3.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U21" smd circle
		(at -2.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U22" smd circle
		(at -1.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U23" smd circle
		(at -0.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U24" smd circle
		(at 0.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U25" smd circle
		(at 1.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U26" smd circle
		(at 2.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U27" smd circle
		(at 3.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U28" smd circle
		(at 4.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U29" smd circle
		(at 5.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U30" smd circle
		(at 6.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U31" smd circle
		(at 7.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U32" smd circle
		(at 8.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U33" smd circle
		(at 9.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U34" smd circle
		(at 10.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U35" smd circle
		(at 11.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U36" smd circle
		(at 12.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U37" smd circle
		(at 13.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U38" smd circle
		(at 14.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "U39" smd circle
		(at 15.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U40" smd circle
		(at 16.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U41" smd circle
		(at 17.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U42" smd circle
		(at 18.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "U43" smd circle
		(at 19.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U44" smd circle
		(at 20.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U45" smd circle
		(at 21.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "U46" smd circle
		(at 22.5 -6.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V1" smd circle
		(at -22.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V2" smd circle
		(at -21.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V3" smd circle
		(at -20.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V4" smd circle
		(at -19.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V5" smd circle
		(at -18.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V6" smd circle
		(at -17.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V7" smd circle
		(at -16.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V8" smd circle
		(at -15.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V9" smd circle
		(at -14.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V10" smd circle
		(at -13.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V11" smd circle
		(at -12.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V12" smd circle
		(at -11.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V13" smd circle
		(at -10.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V14" smd circle
		(at -9.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V15" smd circle
		(at -8.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V16" smd circle
		(at -7.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V17" smd circle
		(at -6.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V18" smd circle
		(at -5.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V19" smd circle
		(at -4.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V20" smd circle
		(at -3.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V21" smd circle
		(at -2.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V22" smd circle
		(at -1.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V23" smd circle
		(at -0.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V24" smd circle
		(at 0.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V25" smd circle
		(at 1.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V26" smd circle
		(at 2.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V27" smd circle
		(at 3.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V28" smd circle
		(at 4.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V29" smd circle
		(at 5.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V30" smd circle
		(at 6.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V31" smd circle
		(at 7.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V32" smd circle
		(at 8.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V33" smd circle
		(at 9.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V34" smd circle
		(at 10.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V35" smd circle
		(at 11.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V36" smd circle
		(at 12.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V37" smd circle
		(at 13.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "V38" smd circle
		(at 14.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V39" smd circle
		(at 15.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V40" smd circle
		(at 16.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "V41" smd circle
		(at 17.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V42" smd circle
		(at 18.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V43" smd circle
		(at 19.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "V44" smd circle
		(at 20.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V45" smd circle
		(at 21.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "V46" smd circle
		(at 22.5 -5.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W1" smd circle
		(at -22.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W2" smd circle
		(at -21.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W3" smd circle
		(at -20.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W4" smd circle
		(at -19.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W5" smd circle
		(at -18.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W6" smd circle
		(at -17.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W7" smd circle
		(at -16.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "W8" smd circle
		(at -15.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W9" smd circle
		(at -14.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W10" smd circle
		(at -13.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "W11" smd circle
		(at -12.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W12" smd circle
		(at -11.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W13" smd circle
		(at -10.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W14" smd circle
		(at -9.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W15" smd circle
		(at -8.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W16" smd circle
		(at -7.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W17" smd circle
		(at -6.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W18" smd circle
		(at -5.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W19" smd circle
		(at -4.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W20" smd circle
		(at -3.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W21" smd circle
		(at -2.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W22" smd circle
		(at -1.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W23" smd circle
		(at -0.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W24" smd circle
		(at 0.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W25" smd circle
		(at 1.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W26" smd circle
		(at 2.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W27" smd circle
		(at 3.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W28" smd circle
		(at 4.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W29" smd circle
		(at 5.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W30" smd circle
		(at 6.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W31" smd circle
		(at 7.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W32" smd circle
		(at 8.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W33" smd circle
		(at 9.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W34" smd circle
		(at 10.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W35" smd circle
		(at 11.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W36" smd circle
		(at 12.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "W37" smd circle
		(at 13.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W38" smd circle
		(at 14.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W39" smd circle
		(at 15.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W40" smd circle
		(at 16.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W41" smd circle
		(at 17.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W42" smd circle
		(at 18.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W43" smd circle
		(at 19.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W44" smd circle
		(at 20.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W45" smd circle
		(at 21.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "W46" smd circle
		(at 22.5 -4.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y1" smd circle
		(at -22.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y2" smd circle
		(at -21.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y3" smd circle
		(at -20.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y4" smd circle
		(at -19.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y5" smd circle
		(at -18.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y6" smd circle
		(at -17.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y7" smd circle
		(at -16.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y8" smd circle
		(at -15.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "Y9" smd circle
		(at -14.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y10" smd circle
		(at -13.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y11" smd circle
		(at -12.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y12" smd circle
		(at -11.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y13" smd circle
		(at -10.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y14" smd circle
		(at -9.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y15" smd circle
		(at -8.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y16" smd circle
		(at -7.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y17" smd circle
		(at -6.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y18" smd circle
		(at -5.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y19" smd circle
		(at -4.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y20" smd circle
		(at -3.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y21" smd circle
		(at -2.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y22" smd circle
		(at -1.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y23" smd circle
		(at -0.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y24" smd circle
		(at 0.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y25" smd circle
		(at 1.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y26" smd circle
		(at 2.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y27" smd circle
		(at 3.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y28" smd circle
		(at 4.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y29" smd circle
		(at 5.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y30" smd circle
		(at 6.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y31" smd circle
		(at 7.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y32" smd circle
		(at 8.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y33" smd circle
		(at 9.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y34" smd circle
		(at 10.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y35" smd circle
		(at 11.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y36" smd circle
		(at 12.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y37" smd circle
		(at 13.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0127)
	)
	(pad "Y38" smd circle
		(at 14.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y39" smd circle
		(at 15.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y40" smd circle
		(at 16.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y41" smd circle
		(at 17.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0127)
		(solder_paste_margin -0.0127)
	)
	(pad "Y42" smd circle
		(at 18.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y43" smd circle
		(at 19.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y44" smd circle
		(at 20.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y45" smd circle
		(at 21.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(pad "Y46" smd circle
		(at 22.5 -3.5)
		(size 0.4826 0.4826)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07366)
	)
	(embedded_fonts no)
	(model "antmicro_xcvu13p_2fhga2104e.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
