(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "XCVU13P-2FHGA2104E"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 54.61 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "XCVU13P-2FHGA2104E"
				(at 54.61 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "XCVU13P-2FHGA2104E"
				(at 54.61 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/903/ds890_ultrascale_overview-1591529.pdf"
				(at 54.61 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Virtex® UltraScale+™ Field Programmable Gate Array (FPGA) IC 832 514867200 3780000 2104-BBGA, FCBGA"
				(at 54.61 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "XCVU13P-2FHGA2104E"
				(at 54.61 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "AMD-Xilinx"
				(at 54.61 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 54.61 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 54.61 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, IC, FPGA, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "XCVU13P-2FHGA2104E_1_1"
				(text "Bank 0"
					(at 11.43 2.54 0)
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 5.08)
					(name "RSVDGND")
					(number "AB11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_0")
					(number "AB12")
				)
				(pin power_in line
					(at 0 -73.66 0)
					(length 5.08)
					(name "GNDADC")
					(number "AB17")
				)
				(pin power_in line
					(at 0 -71.12 0)
					(length 5.08)
					(name "VCCADC")
					(number "AB18")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "INIT_B_0")
					(number "AC12")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "VREFN")
					(number "AC17")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "VP")
					(number "AC18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PUDC_B_0")
					(number "AD12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "TDO_0")
					(number "AD13")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "TDI_0")
					(number "AD15")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "VN")
					(number "AD17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "VREFP")
					(number "AD18")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DONE_0")
					(number "AE12")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "TCK_0")
					(number "AE13")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "DXN")
					(number "AE17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "DXP")
					(number "AE18")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "CCLK_0")
					(number "AF13")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "TMS_0")
					(number "AF15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "AG12")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PROGRAM_B_0")
					(number "AH11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_0")
					(number "AH12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "RDWR_FCS_B_0")
					(number "AJ11")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "D03_0")
					(number "AL11")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "D02_0")
					(number "AM11")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "D01_DIN_0")
					(number "AN11")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "D00_MOSI_0")
					(number "AP11")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VBATT")
					(number "AT11")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "M0_0")
					(number "U10")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "M2_0")
					(number "W11")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "M1_0")
					(number "Y11")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_2_1"
				(text "Bank 60"
					(at 11.43 2.54 0)
				)
				(text "Die 0"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_60")
					(number "AN29")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_60")
					(number "AN30")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_60")
					(number "AN31")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_60")
					(number "AP30")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_60")
					(number "AP31")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_60")
					(number "AP32")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_60")
					(number "AR29")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_60")
					(number "AR30")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_60")
					(number "AR31")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_60")
					(number "AR32")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_60")
					(number "AR33")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_60")
					(number "AT29")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_60")
					(number "AT30")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_60")
					(number "AT31")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_60")
					(number "AT32")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_60")
					(number "AT34")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_60")
					(number "AU29")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_60")
					(number "AU31")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_60")
					(number "AU32")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_60")
					(number "AU33")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_60")
					(number "AU34")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_60")
					(number "AV29")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_60")
					(number "AV30")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_60")
					(number "AV31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_60")
					(number "AV32")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_60")
					(number "AV33")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_60")
					(number "AV34")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_60")
					(number "AW29")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_60")
					(number "AW30")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_60")
					(number "AW31")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_60")
					(number "AW32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_60")
					(number "AW33")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_60")
					(number "AY30")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_60")
					(number "AY32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_60")
					(number "AY33")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_60")
					(number "AY34")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_60")
					(number "BA30")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_60")
					(number "BA31")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_60")
					(number "BA32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_60")
					(number "BA33")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_60")
					(number "BA34")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_60")
					(number "BB30")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_60")
					(number "BB31")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_60")
					(number "BB32")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_60")
					(number "BB33")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_60")
					(number "BC30")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_60")
					(number "BC31")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_60")
					(number "BC33")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_60")
					(number "BD30")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_60")
					(number "BD31")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_60")
					(number "BD32")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_60")
					(number "BD33")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_60")
					(number "BE30")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_60")
					(number "BE31")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_60")
					(number "BE32")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_60")
					(number "BE33")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_60")
					(number "BF30")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_60")
					(number "BF31")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_60")
					(number "BF32")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_3_1"
				(text "Bank 61"
					(at 11.43 2.54 0)
				)
				(text "Die 0"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_61")
					(number "AL26")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_61")
					(number "AL27")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_61")
					(number "AM26")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_61")
					(number "AM27")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_61")
					(number "AM28")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_61")
					(number "AN25")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_61")
					(number "AN26")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_61")
					(number "AN27")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_61")
					(number "AN28")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_61")
					(number "AP25")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_61")
					(number "AP26")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_61")
					(number "AP27")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_61")
					(number "AP28")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_61")
					(number "AR25")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_61")
					(number "AR27")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_61")
					(number "AR28")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_61")
					(number "AT25")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_61")
					(number "AT26")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_61")
					(number "AT27")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_61")
					(number "AT28")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_61")
					(number "AU25")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_61")
					(number "AU26")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_61")
					(number "AU27")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_61")
					(number "AU28")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_61")
					(number "AV25")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_61")
					(number "AV26")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_61")
					(number "AV28")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_61")
					(number "AW26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_61")
					(number "AW27")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_61")
					(number "AW28")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_61")
					(number "AY26")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_61")
					(number "AY27")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_61")
					(number "AY28")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_61")
					(number "AY29")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_61")
					(number "BA26")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_61")
					(number "BA27")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_61")
					(number "BA29")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_61")
					(number "BB26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_61")
					(number "BB27")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_61")
					(number "BB28")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_61")
					(number "BB29")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_61")
					(number "BC25")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_61")
					(number "BC26")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_61")
					(number "BC27")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_61")
					(number "BC28")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_61")
					(number "BC29")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_61")
					(number "BD25")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_61")
					(number "BD26")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_61")
					(number "BD27")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_61")
					(number "BD28")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_61")
					(number "BE25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_61")
					(number "BE27")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_61")
					(number "BE28")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_61")
					(number "BE29")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_61")
					(number "BF25")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_61")
					(number "BF26")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_61")
					(number "BF27")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_61")
					(number "BF28")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_61")
					(number "BF29")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_4_1"
				(text "Bank 62"
					(at 11.43 2.54 0)
				)
				(text "Die 0"
					(at 26.67 2.54 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_62")
					(number "AU35")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_62")
					(number "AU36")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_62")
					(number "AU37")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_62")
					(number "AU38")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_62")
					(number "AU39")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_62")
					(number "AU40")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_62")
					(number "AV35")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_62")
					(number "AV36")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_62")
					(number "AV38")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_62")
					(number "AV39")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_62")
					(number "AV40")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_62")
					(number "AW35")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_62")
					(number "AW36")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_62")
					(number "AW37")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_62")
					(number "AW38")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_62")
					(number "AW39")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_62")
					(number "AW40")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_62")
					(number "AY35")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_62")
					(number "AY36")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_62")
					(number "AY37")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_62")
					(number "AY38")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_62")
					(number "AY39")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_62")
					(number "AY40")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_62")
					(number "BA35")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_62")
					(number "BA36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_62")
					(number "BA37")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_62")
					(number "BA39")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_62")
					(number "BA40")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_62")
					(number "BB34")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_62")
					(number "BB36")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_62")
					(number "BB37")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_62")
					(number "BB38")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_62")
					(number "BB39")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_62")
					(number "BB40")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_62")
					(number "BC34")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_62")
					(number "BC35")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_62")
					(number "BC36")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_62")
					(number "BC37")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_62")
					(number "BC38")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_62")
					(number "BC39")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_62")
					(number "BC40")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_62")
					(number "BD34")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_62")
					(number "BD35")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_62")
					(number "BD36")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_62")
					(number "BD37")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_62")
					(number "BD38")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_62")
					(number "BD40")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_62")
					(number "BE34")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_62")
					(number "BE35")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_62")
					(number "BE37")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_62")
					(number "BE38")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_62")
					(number "BE39")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_62")
					(number "BE40")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_62")
					(number "BF34")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_62")
					(number "BF35")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_62")
					(number "BF36")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_62")
					(number "BF37")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_62")
					(number "BF38")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_62")
					(number "BF39")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_62")
					(number "BF40")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_5_1"
				(text "Bank 63"
					(at 11.43 2.54 0)
				)
				(text "Die 0"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_63")
					(number "AG31")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_63")
					(number "AG32")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_63")
					(number "AG33")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_63")
					(number "AG34")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_63")
					(number "AH30")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_63")
					(number "AH31")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_63")
					(number "AH32")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_63")
					(number "AH33")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_63")
					(number "AH34")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_63")
					(number "AH35")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_63")
					(number "AJ29")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_63")
					(number "AJ30")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_63")
					(number "AJ31")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_63")
					(number "AJ32")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_63")
					(number "AJ33")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_63")
					(number "AJ35")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_63")
					(number "AJ36")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_63")
					(number "AK29")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_63")
					(number "AK30")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_63")
					(number "AK32")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_63")
					(number "AK33")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_63")
					(number "AK34")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_63")
					(number "AK35")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_63")
					(number "AK36")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_63")
					(number "AL29")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_63")
					(number "AL30")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_63")
					(number "AL31")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_63")
					(number "AL32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_63")
					(number "AL33")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_63")
					(number "AL34")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_63")
					(number "AL35")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_63")
					(number "AL36")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_63")
					(number "AM29")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_63")
					(number "AM30")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_63")
					(number "AM31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_63")
					(number "AM32")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_63")
					(number "AM33")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_63")
					(number "AM34")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_63")
					(number "AM36")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_63")
					(number "AN33")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_63")
					(number "AN34")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_63")
					(number "AN35")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_63")
					(number "AN36")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_63")
					(number "AP33")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_63")
					(number "AP34")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_63")
					(number "AP35")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_63")
					(number "AP36")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_63")
					(number "AP37")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_63")
					(number "AP38")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_63")
					(number "AR34")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_63")
					(number "AR35")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_63")
					(number "AR37")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_63")
					(number "AR38")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_63")
					(number "AT35")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_63")
					(number "AT36")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_63")
					(number "AT37")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_63")
					(number "AT38")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_63")
					(number "AT39")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_63")
					(number "AT40")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_6_1"
				(text "Bank 64"
					(at 11.43 2.54 0)
				)
				(text "Die 1"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AL21")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_64")
					(number "AL22")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_64")
					(number "AL23")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AL24")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AL25")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AM21")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AM22")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AM23")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AM24")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AN21")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AN23")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AN24")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AP21")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AP22")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AP23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "AP24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "AR21")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AR22")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AR23")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AR24")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AT21")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AT22")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AT24")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AU21")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AU22")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AU23")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AU24")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AV21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "AV22")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AV23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AV24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AW22")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AW23")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AW25")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AY22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AY23")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AY24")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AY25")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "BA21")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "BA22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "BA23")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "BA24")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "BA25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "BB20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "BB21")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "BB22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "BB23")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "BB24")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "BC21")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "BC23")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "BC24")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "BD21")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "BD22")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "BD23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "BD24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "BE21")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "BE22")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "BE23")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "BE24")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "BF22")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "BF24")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_7_1"
				(text "Bank 65"
					(at 11.43 2.54 0)
				)
				(text "Die 1"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_65")
					(number "AL17")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_DOUT_CSO_B_65")
					(number "AL19")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_EMCCLK_65")
					(number "AL20")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_PERSTN0_65")
					(number "AM17")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_D05_65")
					(number "AM18")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_D04_65")
					(number "AM19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_65")
					(number "AM20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "AN17")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_D09_65")
					(number "AN18")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_D08_65")
					(number "AN19")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_D06_65")
					(number "AN20")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_PERSTN1_I2C_SDA_65")
					(number "AP17")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "AP18")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_D07_65")
					(number "AP20")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_D11_65")
					(number "AR17")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_D10_65")
					(number "AR18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_A01_D17_65")
					(number "AR19")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_A00_D16_65")
					(number "AR20")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_D14_65")
					(number "AT17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "AT18")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_D13_65")
					(number "AT19")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_D12_65")
					(number "AT20")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_D15_65")
					(number "AU17")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_A05_D21_65")
					(number "AU18")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_A04_D20_65")
					(number "AU19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_A07_D23_65")
					(number "AV18")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_A06_D22_65")
					(number "AV19")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_A02_D18_65")
					(number "AV20")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_CSI_ADV_B_65")
					(number "AW17")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_A08_D24_65")
					(number "AW18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "AW19")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_A03_D19_65")
					(number "AW20")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_SMBALERT_65")
					(number "AY17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_A09_D25_65")
					(number "AY18")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_A10_D26_65")
					(number "AY19")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_A18_65")
					(number "AY20")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_A12_D28_65")
					(number "BA17")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_A11_D27_65")
					(number "BA19")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_A19_65")
					(number "BA20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_A13_D29_65")
					(number "BB17")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_A16_65")
					(number "BB18")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_A14_D30_65")
					(number "BB19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "BC17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_A17_65")
					(number "BC18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_A15_D31_65")
					(number "BC19")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_A22_65")
					(number "BC20")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_A21_65")
					(number "BD17")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_A20_65")
					(number "BD18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_A23_65")
					(number "BD20")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_A25_65")
					(number "BE17")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_A24_65")
					(number "BE18")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_A26_65")
					(number "BE19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_RS0_65")
					(number "BE20")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_FWE_FCS2_B_65")
					(number "BF16")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_FOE_B_65")
					(number "BF17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "BF18")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_A27_65")
					(number "BF19")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_RS1_65")
					(number "BF20")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_A28_65")
					(number "BF21")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_8_1"
				(text "Bank 66"
					(at 11.43 2.54 0)
				)
				(text "Die 1"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "AV8")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "AV9")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "AW7")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "AW8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_66")
					(number "AW9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "AY7")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "AY8")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "AY9")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "BA7")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "BA9")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "BA10")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_66")
					(number "BA11")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "BA14")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "BA15")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "BA16")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "BB7")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "BB8")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "BB9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "BB10")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "BB11")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "BB12")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "BB13")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "BB14")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "BB16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "BC7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "BC8")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "BC9")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "BC10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "BC11")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "BC13")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "BC14")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "BC15")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "BC16")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "BD7")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "BD8")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "BD10")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "BD11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "BD12")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "BD13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "BD14")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "BD15")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "BD16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "BE7")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "BE8")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "BE9")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "BE10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "BE11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "BE12")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "BE13")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "BE14")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "BE15")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "BF7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "BF8")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "BF9")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "BF10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "BF11")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "BF12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "BF14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "BF15")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_9_1"
				(text "Bank 67"
					(at 11.43 2.54 0)
				)
				(text "Die 1"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_67")
					(number "AJ12")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_67")
					(number "AJ13")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_67")
					(number "AK12")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_67")
					(number "AK13")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_67")
					(number "AK14")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_67")
					(number "AK15")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_67")
					(number "AL12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_67")
					(number "AL13")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_67")
					(number "AL14")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_67")
					(number "AL15")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_67")
					(number "AL16")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_67")
					(number "AM12")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_67")
					(number "AM13")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_67")
					(number "AM14")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_67")
					(number "AM16")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_67")
					(number "AN13")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_67")
					(number "AN14")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_67")
					(number "AN15")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_67")
					(number "AN16")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_67")
					(number "AP12")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_67")
					(number "AP13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "AP14")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_67")
					(number "AP15")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_67")
					(number "AP16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_67")
					(number "AR12")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_67")
					(number "AR13")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_67")
					(number "AR14")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_67")
					(number "AR15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_67")
					(number "AT12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_67")
					(number "AT14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_67")
					(number "AT15")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_67")
					(number "AT16")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_67")
					(number "AU11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_67")
					(number "AU12")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_67")
					(number "AU13")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_67")
					(number "AU14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "AU15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_67")
					(number "AU16")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_67")
					(number "AV10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_67")
					(number "AV11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "AV12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_67")
					(number "AV13")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_67")
					(number "AV14")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_67")
					(number "AV15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_67")
					(number "AV16")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_67")
					(number "AW10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_67")
					(number "AW11")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_67")
					(number "AW12")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_67")
					(number "AW13")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_67")
					(number "AW15")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_67")
					(number "AW16")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_67")
					(number "AY10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_67")
					(number "AY12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_67")
					(number "AY13")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_67")
					(number "AY14")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_67")
					(number "AY15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "AY16")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_67")
					(number "BA12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "BA13")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_10_1"
				(text "Bank 68"
					(at 11.43 2.54 0)
				)
				(text "Die 2"
					(at 26.67 2.54 0)
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_68")
					(number "K33")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_68")
					(number "K34")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_68")
					(number "K36")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_68")
					(number "L33")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_68")
					(number "L34")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_68")
					(number "L35")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_68")
					(number "L36")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_68")
					(number "L37")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_68")
					(number "L38")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_68")
					(number "M32")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_68")
					(number "M33")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_68")
					(number "M34")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_68")
					(number "M35")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_68")
					(number "M36")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_68")
					(number "M37")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_68")
					(number "M38")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_68")
					(number "N32")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_68")
					(number "N33")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_68")
					(number "N34")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_68")
					(number "N35")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_68")
					(number "N37")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_68")
					(number "N38")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_68")
					(number "P31")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_68")
					(number "P32")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_68")
					(number "P34")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_68")
					(number "P35")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_68")
					(number "P36")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_68")
					(number "P37")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_68")
					(number "P38")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_68")
					(number "R31")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_68")
					(number "R32")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_68")
					(number "R33")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_68")
					(number "R34")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_68")
					(number "R35")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_68")
					(number "R36")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_68")
					(number "T30")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_68")
					(number "T31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_68")
					(number "T32")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_68")
					(number "T33")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_68")
					(number "T34")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_68")
					(number "T35")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_68")
					(number "T36")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_68")
					(number "U30")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_68")
					(number "U31")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_68")
					(number "U32")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_68")
					(number "U33")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_68")
					(number "U35")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_68")
					(number "V30")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_68")
					(number "V32")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_68")
					(number "V33")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_68")
					(number "V34")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_68")
					(number "W31")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_68")
					(number "W32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_68")
					(number "W33")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_68")
					(number "W34")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_68")
					(number "Y31")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_68")
					(number "Y32")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_68")
					(number "Y33")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_68")
					(number "Y34")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_11_1"
				(text "Bank 69"
					(at 11.43 2.54 0)
				)
				(text "Die 2"
					(at 26.67 2.54 0)
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_69")
					(number "A34")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_69")
					(number "A35")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_69")
					(number "A36")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_69")
					(number "A37")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_69")
					(number "A38")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_69")
					(number "A39")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_69")
					(number "A40")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_69")
					(number "B34")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_69")
					(number "B35")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_69")
					(number "B36")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_69")
					(number "B37")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_69")
					(number "B38")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_69")
					(number "B40")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_69")
					(number "C34")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_69")
					(number "C35")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_69")
					(number "C37")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_69")
					(number "C38")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_69")
					(number "C39")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_69")
					(number "C40")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_69")
					(number "D34")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_69")
					(number "D35")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_69")
					(number "D36")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_69")
					(number "D37")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_69")
					(number "D38")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_69")
					(number "D39")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_69")
					(number "D40")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_69")
					(number "E34")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_69")
					(number "E35")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_69")
					(number "E36")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_69")
					(number "E37")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_69")
					(number "E38")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_69")
					(number "E39")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_69")
					(number "F34")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_69")
					(number "F35")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_69")
					(number "F36")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_69")
					(number "F38")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_69")
					(number "F39")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_69")
					(number "F40")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_69")
					(number "G35")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_69")
					(number "G36")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_69")
					(number "G37")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_69")
					(number "G38")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_69")
					(number "G39")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_69")
					(number "G40")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_69")
					(number "H34")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_69")
					(number "H35")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_69")
					(number "H36")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_69")
					(number "H37")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_69")
					(number "H38")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_69")
					(number "H39")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_69")
					(number "H40")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_69")
					(number "J34")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_69")
					(number "J35")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_69")
					(number "J36")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_69")
					(number "J37")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_69")
					(number "J39")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_69")
					(number "J40")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_69")
					(number "K37")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_69")
					(number "K38")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_12_1"
				(text "Bank 70"
					(at 11.43 2.54 0)
				)
				(text "Die 2"
					(at 26.67 2.54 0)
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_70")
					(number "A29")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_70")
					(number "A30")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_70")
					(number "A31")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_70")
					(number "A33")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_70")
					(number "B30")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_70")
					(number "B31")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_70")
					(number "B32")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_70")
					(number "B33")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_70")
					(number "C29")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_70")
					(number "C30")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_70")
					(number "C31")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_70")
					(number "C32")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_70")
					(number "C33")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_70")
					(number "D29")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_70")
					(number "D30")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_70")
					(number "D31")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_70")
					(number "D32")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_70")
					(number "E29")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_70")
					(number "E31")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_70")
					(number "E32")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_70")
					(number "E33")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_70")
					(number "F29")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_70")
					(number "F30")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_70")
					(number "F31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_70")
					(number "F32")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_70")
					(number "F33")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_70")
					(number "G29")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_70")
					(number "G30")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_70")
					(number "G31")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_70")
					(number "G32")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_70")
					(number "G33")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_70")
					(number "H29")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_70")
					(number "H30")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_70")
					(number "H32")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_70")
					(number "H33")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_70")
					(number "J29")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_70")
					(number "J30")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_70")
					(number "J31")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_70")
					(number "J32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_70")
					(number "J33")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_70")
					(number "K29")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_70")
					(number "K30")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_70")
					(number "K31")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_70")
					(number "K32")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_70")
					(number "L29")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_70")
					(number "L30")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_70")
					(number "L31")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_70")
					(number "M30")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_70")
					(number "M31")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_70")
					(number "N28")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_70")
					(number "N29")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_70")
					(number "N30")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_70")
					(number "N31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_70")
					(number "P28")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_70")
					(number "P29")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_70")
					(number "P30")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_70")
					(number "R28")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_70")
					(number "R29")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_70")
					(number "T28")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_70")
					(number "T29")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_13_1"
				(text "Bank 71"
					(at 11.43 2.54 0)
				)
				(text "Die 2"
					(at 26.67 2.54 0)
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_71")
					(number "A25")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_71")
					(number "A26")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_71")
					(number "A27")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_71")
					(number "A28")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_71")
					(number "B25")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_71")
					(number "B26")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_71")
					(number "B27")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_71")
					(number "B28")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_71")
					(number "C25")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_71")
					(number "C27")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_71")
					(number "C28")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_71")
					(number "D25")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_71")
					(number "D26")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_71")
					(number "D27")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_71")
					(number "D28")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_71")
					(number "E25")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_71")
					(number "E26")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_71")
					(number "E27")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_71")
					(number "E28")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_71")
					(number "F25")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_71")
					(number "F26")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_71")
					(number "F28")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_71")
					(number "G25")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_71")
					(number "G26")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_71")
					(number "G27")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_71")
					(number "G28")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_71")
					(number "H25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_71")
					(number "H26")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_71")
					(number "H27")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_71")
					(number "H28")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_71")
					(number "J25")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_71")
					(number "J26")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_71")
					(number "J27")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_71")
					(number "K26")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_71")
					(number "K27")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_71")
					(number "K28")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_71")
					(number "L24")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_71")
					(number "L25")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_71")
					(number "L26")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_71")
					(number "L27")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_71")
					(number "L28")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_71")
					(number "M24")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_71")
					(number "M25")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_71")
					(number "M26")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_71")
					(number "M27")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_71")
					(number "M28")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_71")
					(number "N24")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_71")
					(number "N25")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_71")
					(number "N27")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_71")
					(number "P24")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_71")
					(number "P25")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_71")
					(number "P26")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_71")
					(number "P27")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_71")
					(number "R24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_71")
					(number "R25")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_71")
					(number "R26")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_71")
					(number "R27")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_71")
					(number "T24")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_71")
					(number "T25")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_71")
					(number "T26")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_14_1"
				(text "Bank 72"
					(at 11.43 2.54 0)
				)
				(text "Die 3"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_72")
					(number "AA12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_72")
					(number "AA13")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_72")
					(number "AA14")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_72")
					(number "AB13")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_72")
					(number "J11")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_72")
					(number "J12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_72")
					(number "J13")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_72")
					(number "J14")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_72")
					(number "K11")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_72")
					(number "K12")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_72")
					(number "K13")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_72")
					(number "K14")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_72")
					(number "L11")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_72")
					(number "L13")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_72")
					(number "L14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_72")
					(number "L15")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_72")
					(number "M11")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_72")
					(number "M12")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_72")
					(number "M13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_72")
					(number "M14")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_72")
					(number "M15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_72")
					(number "N11")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_72")
					(number "N12")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_72")
					(number "N13")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_72")
					(number "N14")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_72")
					(number "N15")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_72")
					(number "P11")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_72")
					(number "P12")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_72")
					(number "P14")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_72")
					(number "P15")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_72")
					(number "R11")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_72")
					(number "R12")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_72")
					(number "R13")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_72")
					(number "R14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_72")
					(number "R15")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_72")
					(number "R16")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_72")
					(number "T11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_72")
					(number "T12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_72")
					(number "T13")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_72")
					(number "T14")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_72")
					(number "T15")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_72")
					(number "T16")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_72")
					(number "U11")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_72")
					(number "U12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_72")
					(number "U13")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_72")
					(number "U15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_72")
					(number "U16")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_72")
					(number "V12")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_72")
					(number "V13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_72")
					(number "V14")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_72")
					(number "V15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_72")
					(number "V16")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_72")
					(number "W12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_72")
					(number "W13")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_72")
					(number "W14")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_72")
					(number "W15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_72")
					(number "Y12")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_72")
					(number "Y13")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_72")
					(number "Y14")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_15_1"
				(text "Bank 73"
					(at 11.43 2.54 0)
				)
				(text "Die 3"
					(at 26.67 2.54 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_73")
					(number "A7")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_73")
					(number "A8")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_73")
					(number "A9")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_73")
					(number "A10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_73")
					(number "A11")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_73")
					(number "A13")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_73")
					(number "A14")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_73")
					(number "A15")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_73")
					(number "A16")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_73")
					(number "B7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_73")
					(number "B8")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_73")
					(number "B10")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_73")
					(number "B11")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_73")
					(number "B12")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_73")
					(number "B13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_73")
					(number "B14")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_73")
					(number "B15")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_73")
					(number "B16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_73")
					(number "C7")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_73")
					(number "C8")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_73")
					(number "C9")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_73")
					(number "C10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_73")
					(number "C11")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_73")
					(number "C12")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_73")
					(number "C13")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_73")
					(number "C14")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_73")
					(number "C15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_73")
					(number "D7")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_73")
					(number "D8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_73")
					(number "D9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_73")
					(number "D10")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_73")
					(number "D11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_73")
					(number "D12")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_73")
					(number "D14")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_73")
					(number "D15")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_73")
					(number "E9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_73")
					(number "E11")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_73")
					(number "E12")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_73")
					(number "E13")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_73")
					(number "E14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_73")
					(number "E15")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_73")
					(number "F9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_73")
					(number "F10")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_73")
					(number "F11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_73")
					(number "F12")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_73")
					(number "F13")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_73")
					(number "F14")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_73")
					(number "F15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_73")
					(number "G9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_73")
					(number "G10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_73")
					(number "G11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_73")
					(number "G12")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_73")
					(number "G13")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_73")
					(number "G15")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_73")
					(number "H12")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_73")
					(number "H13")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_73")
					(number "H14")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_73")
					(number "H15")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_73")
					(number "J15")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_16_1"
				(text "Bank 74"
					(at 11.43 2.54 0)
				)
				(text "Die 3"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_74")
					(number "A21")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_74")
					(number "A23")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_74")
					(number "A24")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_74")
					(number "B21")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_74")
					(number "B22")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_74")
					(number "B23")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_74")
					(number "B24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_74")
					(number "C21")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_74")
					(number "C22")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_74")
					(number "C23")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_74")
					(number "C24")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_74")
					(number "D21")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_74")
					(number "D22")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_74")
					(number "D24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_74")
					(number "E21")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_74")
					(number "E22")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_74")
					(number "E23")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_74")
					(number "E24")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_74")
					(number "F21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_74")
					(number "F22")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_74")
					(number "F23")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_74")
					(number "F24")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_74")
					(number "G21")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_74")
					(number "G22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_74")
					(number "G23")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_74")
					(number "H20")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_74")
					(number "H22")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_74")
					(number "H23")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_74")
					(number "H24")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_74")
					(number "J20")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_74")
					(number "J21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_74")
					(number "J22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_74")
					(number "J23")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_74")
					(number "J24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_74")
					(number "K20")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_74")
					(number "K21")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_74")
					(number "K22")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_74")
					(number "K23")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_74")
					(number "K24")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_74")
					(number "L20")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_74")
					(number "L21")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_74")
					(number "L23")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_74")
					(number "M20")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_74")
					(number "M21")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_74")
					(number "M22")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_74")
					(number "M23")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_74")
					(number "N20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_74")
					(number "N21")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_74")
					(number "N22")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_74")
					(number "N23")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_74")
					(number "P20")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_74")
					(number "P21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_74")
					(number "P22")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_74")
					(number "R21")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_74")
					(number "R22")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_74")
					(number "R23")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_74")
					(number "T20")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_74")
					(number "T21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_74")
					(number "T22")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_74")
					(number "T23")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_17_1"
				(text "Bank 75"
					(at 11.43 2.54 0)
				)
				(text "Die 3"
					(at 26.67 2.54 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_75")
					(number "A17")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_75")
					(number "A18")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_75")
					(number "A19")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "IO_T3U_N12_75")
					(number "A20")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_75")
					(number "B17")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_75")
					(number "B18")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "IO_L24N_T3U_N11_75")
					(number "B20")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_75")
					(number "C17")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_75")
					(number "C18")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_75")
					(number "C19")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "IO_L24P_T3U_N10_75")
					(number "C20")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_75")
					(number "D16")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_75")
					(number "D17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_75")
					(number "D18")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "IO_L23N_T3U_N9_75")
					(number "D19")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "IO_L23P_T3U_N8_75")
					(number "D20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_75")
					(number "E16")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_75")
					(number "E17")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_75")
					(number "E18")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_75")
					(number "E19")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_75")
					(number "F16")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_75")
					(number "F18")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_75")
					(number "F19")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_75")
					(number "F20")
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "IO_T2U_N12_75")
					(number "G16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_75")
					(number "G17")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_75")
					(number "G18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_75")
					(number "G19")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_75")
					(number "G20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_75")
					(number "H16")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_75")
					(number "H17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_75")
					(number "H18")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_75")
					(number "H19")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_75")
					(number "J16")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_75")
					(number "J17")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_75")
					(number "J19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_75")
					(number "K16")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_75")
					(number "K17")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_75")
					(number "K18")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_75")
					(number "K19")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_75")
					(number "L16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_75")
					(number "L17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_75")
					(number "L18")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "IO_T1U_N12_75")
					(number "L19")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_75")
					(number "M16")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_75")
					(number "M17")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_75")
					(number "M18")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_75")
					(number "N17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_75")
					(number "N18")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_75")
					(number "N19")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_75")
					(number "P16")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_75")
					(number "P17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_75")
					(number "P18")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_75")
					(number "P19")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_75")
					(number "R17")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_75")
					(number "R18")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_75")
					(number "R19")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "IO_T0U_N12_VRP_75")
					(number "T18")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "VREF_75")
					(number "T19")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_18_1"
				(text "Quads 125, 126"
					(at 7.62 2.54 0)
				)
				(text "Die 1"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MGTREFCLK1P_126")
					(number "AH38")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MGTREFCLK1N_126")
					(number "AH39")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "MGTYRXP3_126")
					(number "AJ45")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "MGTYRXN3_126")
					(number "AJ46")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MGTREFCLK0P_126")
					(number "AK38")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MGTREFCLK0N_126")
					(number "AK39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "MGTYTXP3_126")
					(number "AL40")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "MGTYTXN3_126")
					(number "AL41")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "MGTYRXP2_126")
					(number "AL45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "MGTYRXN2_126")
					(number "AL46")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTREFCLK1P_125")
					(number "AM38")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTREFCLK1N_125")
					(number "AM39")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "MGTYTXP2_126")
					(number "AM42")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "MGTYTXN2_126")
					(number "AM43")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTREFCLK0P_125")
					(number "AN40")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTREFCLK0N_125")
					(number "AN41")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MGTYRXP1_126")
					(number "AN45")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MGTYRXN1_126")
					(number "AN46")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MGTYTXP1_126")
					(number "AP42")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MGTYTXN1_126")
					(number "AP43")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTYRXP0_126")
					(number "AR45")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MGTYRXN0_126")
					(number "AR46")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "MGTYTXP0_126")
					(number "AT42")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MGTYTXN0_126")
					(number "AT43")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXP3_125")
					(number "AU45")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTYRXN3_125")
					(number "AU46")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTYTXP3_125")
					(number "AV42")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTYTXN3_125")
					(number "AV43")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXP2_125")
					(number "AW45")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXN2_125")
					(number "AW46")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYTXP2_125")
					(number "AY42")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYTXN2_125")
					(number "AY43")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYRXP1_125")
					(number "BA45")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYRXN1_125")
					(number "BA46")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MGTYTXP1_125")
					(number "BB42")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYTXN1_125")
					(number "BB43")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYRXP0_125")
					(number "BC45")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYRXN0_125")
					(number "BC46")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP0_125")
					(number "BD42")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN0_125")
					(number "BD43")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_19_1"
				(text "Quads 127, 129"
					(at 7.62 2.54 0)
				)
				(text "Die 1, 2"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MGTYTXP1_129")
					(number "AA40")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MGTYTXN1_129")
					(number "AA41")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "MGTYRXP2_129")
					(number "AA45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "MGTYRXN2_129")
					(number "AA46")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MGTREFCLK0P_129")
					(number "AB38")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MGTREFCLK0N_129")
					(number "AB39")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MGTYRXP1_129")
					(number "AB43")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MGTYRXN1_129")
					(number "AB44")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "MGTYTXP0_129")
					(number "AC40")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MGTYTXN0_129")
					(number "AC41")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTYRXP0_129")
					(number "AC45")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MGTYRXN0_129")
					(number "AC46")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTREFCLK1P_127")
					(number "AD38")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTREFCLK1N_127")
					(number "AD39")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXP3_127")
					(number "AD43")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTYRXN3_127")
					(number "AD44")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTYTXP3_127")
					(number "AE40")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTYTXN3_127")
					(number "AE41")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXP2_127")
					(number "AE45")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXN2_127")
					(number "AE46")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTREFCLK0P_127")
					(number "AF38")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTREFCLK0N_127")
					(number "AF39")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYRXP1_127")
					(number "AF43")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYRXN1_127")
					(number "AF44")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYTXP2_127")
					(number "AG40")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYTXN2_127")
					(number "AG41")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYRXP0_127")
					(number "AG45")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYRXN0_127")
					(number "AG46")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MGTYTXP1_127")
					(number "AJ40")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYTXN1_127")
					(number "AJ41")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP0_127")
					(number "AK42")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN0_127")
					(number "AK43")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "MGTYTXP3_129")
					(number "U40")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "MGTYTXN3_129")
					(number "U41")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "MGTYTXP2_129")
					(number "W40")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "MGTYTXN2_129")
					(number "W41")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MGTREFCLK1P_129")
					(number "Y38")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MGTREFCLK1N_129")
					(number "Y39")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "MGTYRXP3_129")
					(number "Y43")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "MGTYRXN3_129")
					(number "Y44")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_20_1"
				(text "Quads 130, 131"
					(at 7.62 2.54 0)
				)
				(text "Die 2"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "MGTYTXP3_131")
					(number "B42")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "MGTYTXN3_131")
					(number "B43")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "MGTYTXP2_131")
					(number "D42")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "MGTYTXN2_131")
					(number "D43")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "MGTYRXP3_131")
					(number "E45")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "MGTYRXN3_131")
					(number "E46")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MGTYTXP1_131")
					(number "F42")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MGTYTXN1_131")
					(number "F43")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "MGTYRXP2_131")
					(number "G45")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "MGTYRXN2_131")
					(number "G46")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "MGTYTXP0_131")
					(number "H42")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MGTYTXN0_131")
					(number "H43")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MGTYRXP1_131")
					(number "J45")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MGTYRXN1_131")
					(number "J46")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTYTXP3_130")
					(number "K42")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTYTXN3_130")
					(number "K43")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTYRXP0_131")
					(number "L45")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MGTYRXN0_131")
					(number "L46")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYTXP2_130")
					(number "M42")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYTXN2_130")
					(number "M43")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MGTREFCLK1P_131")
					(number "N40")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MGTREFCLK1N_131")
					(number "N41")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXP3_130")
					(number "N45")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTYRXN3_130")
					(number "N46")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MGTYTXP1_130")
					(number "P42")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYTXN1_130")
					(number "P43")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MGTREFCLK0P_131")
					(number "R40")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MGTREFCLK0N_131")
					(number "R41")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXP2_130")
					(number "R45")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXN2_130")
					(number "R46")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTREFCLK1P_130")
					(number "T38")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTREFCLK1N_130")
					(number "T39")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP0_130")
					(number "T42")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN0_130")
					(number "T43")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYRXP1_130")
					(number "U45")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYRXN1_130")
					(number "U46")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTREFCLK0P_130")
					(number "V38")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTREFCLK0N_130")
					(number "V39")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYRXP0_130")
					(number "W45")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYRXN0_130")
					(number "W46")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_21_1"
				(text "Quads 224, 225"
					(at 7.62 2.54 0)
				)
				(text "Die 1"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "MGTYRXN3_225")
					(number "AJ3")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "MGTYRXP3_225")
					(number "AJ4")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MGTREFCLK1N_225")
					(number "AJ8")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MGTREFCLK1P_225")
					(number "AJ9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "MGTYRXN2_225")
					(number "AK1")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "MGTYRXP2_225")
					(number "AK2")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MGTREFCLK0N_225")
					(number "AL8")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MGTREFCLK0P_225")
					(number "AL9")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MGTYRXN1_225")
					(number "AM1")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MGTYRXP1_225")
					(number "AM2")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "AN8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "AN9")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MGTYRXN0_225")
					(number "AP1")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTYRXP0_225")
					(number "AP2")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "MGTYTXN3_225")
					(number "AP6")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "MGTYTXP3_225")
					(number "AP7")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "MGTYTXN2_225")
					(number "AR4")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "MGTYTXP2_225")
					(number "AR5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "AR8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "AR9")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTYRXN3_224")
					(number "AT1")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXP3_224")
					(number "AT2")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MGTYTXN1_225")
					(number "AT6")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MGTYTXP1_225")
					(number "AT7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MGTYTXN0_225")
					(number "AU4")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "MGTYTXP0_225")
					(number "AU5")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXN2_224")
					(number "AV1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXP2_224")
					(number "AV2")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTYTXN3_224")
					(number "AW4")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTYTXP3_224")
					(number "AW5")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYRXN1_224")
					(number "AY1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYRXP1_224")
					(number "AY2")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYTXN2_224")
					(number "BA4")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYTXP2_224")
					(number "BA5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYRXN0_224")
					(number "BB1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYRXP0_224")
					(number "BB2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYTXN1_224")
					(number "BC4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MGTYTXP1_224")
					(number "BC5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN0_224")
					(number "BE4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP0_224")
					(number "BE5")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_22_1"
				(text "Quads 226, 227"
					(at 7.62 2.54 0)
				)
				(text "Die 1"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "MGTYRXN3_227")
					(number "AA3")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "MGTYRXP3_227")
					(number "AA4")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MGTREFCLK1N_227")
					(number "AA8")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MGTREFCLK1P_227")
					(number "AA9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "MGTYRXN2_227")
					(number "AB1")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "MGTYRXP2_227")
					(number "AB2")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "MGTYTXN2_227")
					(number "AB6")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "MGTYTXP2_227")
					(number "AB7")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MGTYRXN1_227")
					(number "AC3")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MGTYRXP1_227")
					(number "AC4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MGTREFCLK0N_227")
					(number "AC8")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MGTREFCLK0P_227")
					(number "AC9")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MGTYRXN0_227")
					(number "AD1")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTYRXP0_227")
					(number "AD2")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MGTYTXN1_227")
					(number "AD6")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MGTYTXP1_227")
					(number "AD7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTYRXN3_226")
					(number "AE3")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXP3_226")
					(number "AE4")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTREFCLK1N_226")
					(number "AE8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTREFCLK1P_226")
					(number "AE9")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXN2_226")
					(number "AF1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXP2_226")
					(number "AF2")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MGTYTXN0_227")
					(number "AF6")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "MGTYTXP0_227")
					(number "AF7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYRXN1_226")
					(number "AG3")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYRXP1_226")
					(number "AG4")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTREFCLK0N_226")
					(number "AG8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTREFCLK0P_226")
					(number "AG9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYRXN0_226")
					(number "AH1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYRXP0_226")
					(number "AH2")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTYTXN3_226")
					(number "AH6")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTYTXP3_226")
					(number "AH7")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYTXN2_226")
					(number "AK6")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYTXP2_226")
					(number "AK7")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYTXN1_226")
					(number "AM6")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MGTYTXP1_226")
					(number "AM7")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN0_226")
					(number "AN4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP0_226")
					(number "AN5")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "MGTYTXN3_227")
					(number "Y6")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "MGTYTXP3_227")
					(number "Y7")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_23_1"
				(text "Quads 229, 230"
					(at 7.62 2.54 0)
				)
				(text "Die 2"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "MGTYTXN3_230")
					(number "H6")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "MGTYTXP3_230")
					(number "H7")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "MGTYTXN2_230")
					(number "J4")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "MGTYTXP2_230")
					(number "J5")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MGTYTXN1_230")
					(number "K6")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MGTYTXP1_230")
					(number "K7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MGTYTXN0_230")
					(number "L4")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "MGTYTXP0_230")
					(number "L5")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "MGTYRXN3_230")
					(number "M1")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "MGTYRXP3_230")
					(number "M2")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTYTXN3_229")
					(number "M6")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTYTXP3_229")
					(number "M7")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MGTREFCLK1N_230")
					(number "N8")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MGTREFCLK1P_230")
					(number "N9")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "MGTYRXN2_230")
					(number "P1")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "MGTYRXP2_230")
					(number "P2")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYTXN2_229")
					(number "P6")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYTXP2_229")
					(number "P7")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MGTYRXN1_230")
					(number "R3")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MGTYRXP1_230")
					(number "R4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MGTREFCLK0N_230")
					(number "R8")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MGTREFCLK0P_230")
					(number "R9")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MGTYRXN0_230")
					(number "T1")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MGTYRXP0_230")
					(number "T2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYTXN1_229")
					(number "T6")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MGTYTXP1_229")
					(number "T7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTYRXN3_229")
					(number "U3")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXP3_229")
					(number "U4")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTREFCLK1N_229")
					(number "U8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTREFCLK1P_229")
					(number "U9")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXN2_229")
					(number "V1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXP2_229")
					(number "V2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN0_229")
					(number "V6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP0_229")
					(number "V7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYRXN1_229")
					(number "W3")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYRXP1_229")
					(number "W4")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTREFCLK0N_229")
					(number "W8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTREFCLK0P_229")
					(number "W9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYRXN0_229")
					(number "Y1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYRXP0_229")
					(number "Y2")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_24_1"
				(text "Quad 231"
					(at 7.62 2.54 0)
				)
				(text "Die 2"
					(at 26.67 2.54 0)
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MGTYTXN3_231")
					(number "C4")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MGTYTXP3_231")
					(number "C5")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MGTYRXN3_231")
					(number "D1")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MGTYRXP3_231")
					(number "D2")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MGTYTXN2_231")
					(number "E4")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MGTYTXP2_231")
					(number "E5")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MGTYRXN2_231")
					(number "F1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MGTYRXP2_231")
					(number "F2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MGTYTXN1_231")
					(number "F6")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MGTYTXP1_231")
					(number "F7")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTYTXN0_231")
					(number "G4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTYTXP0_231")
					(number "G5")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTYRXN1_231")
					(number "H1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTYRXP1_231")
					(number "H2")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MGTREFCLK1N_231")
					(number "J8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MGTREFCLK1P_231")
					(number "J9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTYRXN0_231")
					(number "K1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "MGTYRXP0_231")
					(number "K2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTREFCLK0N_231")
					(number "L8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTREFCLK0P_231")
					(number "L9")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_25_1"
				(text "MGTxVCC"
					(at 7.62 2.54 0)
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTAVCC_RN")
					(number "AA10")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTAVCC_LN")
					(number "AA36")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTVCCAUX_LN")
					(number "AA38")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "AB9")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LN")
					(number "AB37")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "AC10")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTAVCC_LS")
					(number "AC36")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LN")
					(number "AC39")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTVCCAUX_RS")
					(number "AD8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "AD11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LS")
					(number "AD37")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "MGTAVCC_RS")
					(number "AE10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LS")
					(number "AE36")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTVCCAUX_LS")
					(number "AE38")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "MGTVCCAUX_RS")
					(number "AF9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AF11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LS")
					(number "AF37")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AG10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LS")
					(number "AG37")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "MGTVCCAUX_LS")
					(number "AG39")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AH8")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AJ10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LS")
					(number "AJ38")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AK9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AL10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LS")
					(number "AL39")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AM8")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AN10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AP9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LS")
					(number "AP40")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AR10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RS")
					(number "AT8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "K9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "M8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "P9")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LN")
					(number "P40")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTVCCAUX_RN")
					(number "T8")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LN")
					(number "U38")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "MGTVCCAUX_RN")
					(number "V9")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LN")
					(number "V37")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "W10")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LN")
					(number "W36")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "MGTVCCAUX_LN")
					(number "W39")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_RN")
					(number "Y8")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_LN")
					(number "Y37")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_26_1"
				(text "MGTAVTT"
					(at 7.62 2.54 0)
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 5.08)
					(name "MGTRREF_RN")
					(number "A4")
				)
				(pin passive line
					(at 44.45 -5.08 180)
					(length 5.08)
					(name "MGTAVTTRCAL_RN")
					(number "A5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "MGTAVTT_LN")
					(number "A42")
				)
				(pin power_in line
					(at 44.45 -2.54 180)
					(length 5.08)
					(name "MGTAVTT_RS")
					(number "AA6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "AB40")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AC7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTAVTT_LS")
					(number "AD41")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AE6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AF40")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AG7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AH41")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AH43")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AJ6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AJ42")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AK40")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AL4")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AL7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AL43")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AM5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AM41")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AN6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AN42")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AP4")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AR7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AR43")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AT5")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AU6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AU42")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AV4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "AW43")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "AY5")
				)
				(pin power_in line
					(at 44.45 0 180)
					(length 5.08)
					(name "MGTAVTT_RN")
					(number "B3")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "B5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "B44")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "BA42")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "BB4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "BC43")
				)
				(pin passive line
					(at 44.45 -12.7 180)
					(length 5.08)
					(name "MGTRREF_RS")
					(number "BD2")
				)
				(pin passive line
					(at 44.45 -7.62 180)
					(length 5.08)
					(name "MGTAVTTRCAL_RS")
					(number "BD3")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "BD5")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "BE3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "BE42")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LS")
					(number "BE44")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RS")
					(number "BF4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTAVTTRCAL_LS")
					(number "BF42")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTRREF_LS")
					(number "BF43")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "C43")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "C45")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "D4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "E42")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "F5")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "G7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "G43")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "H4")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "J6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "J42")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "K5")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "L7")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTAVTTRCAL_LN")
					(number "L40")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTRREF_LN")
					(number "L41")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "L43")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "M4")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "N5")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "N6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "N42")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "R7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "R43")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "T41")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "U6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "U42")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "V40")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "V43")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_RN")
					(number "W7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_LN")
					(number "Y41")
				)
			)
			(symbol "XCVU13P-2FHGA2104E_27_1"
				(text "POWER"
					(at 7.62 2.54 0)
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A6")
				)
				(pin power_in line
					(at 26.67 -11.43 180)
					(length 5.08)
					(name "GND")
					(number "A12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCINT")
					(number "AA15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AA25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA26")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCCINT_IO")
					(number "AA27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA28")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "AA29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA30")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AA31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA32")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 5.08)
					(name "VCCAUX")
					(number "AA33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AB26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB27")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AB28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB29")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AB30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB31")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AB32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB33")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AB34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC11")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VCCBRAM")
					(number "AC13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AC25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "AC27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC28")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AC29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC30")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AC31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC32")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AC33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "AD14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AD26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD27")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AD28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD29")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AD30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD31")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AD32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD33")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AD34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AE25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "AE27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE28")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AE29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE30")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AE31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE32")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AE33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF12")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "AF14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AF26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF27")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AF28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF29")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AF30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF31")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AF32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF33")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AF34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "AG13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AG25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "AG27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG28")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AG29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG30")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AG35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH13")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "AH14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AH26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH27")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "AH28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AJ25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "AJ27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "AK26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK27")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "AK28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AR44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AT46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AU44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AV46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW14")
				)
				(pin no_connect line
					(at 21.59 0 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AW21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AW44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AY46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BA44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BB46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BC44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BD46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BE45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "BF44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "U27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U28")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "U29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U39")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V27")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "V28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V41")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V46")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W6")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "W27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W28")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "W29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W37")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W38")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W43")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W44")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y27")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "Y28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y29")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "Y30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y35")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y36")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y40")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y42")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y45")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y46")
				)
			)
			(embedded_fonts no)
		)
)
