(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "XCZU7EV-2FFVC1156I"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 114.3 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "XCZU7EV-2FFVC1156I"
				(at 114.3 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "XCZU7EV-2FFVC1156I"
				(at 114.3 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/2621630.pdf?_gl=1*kdjd1r*_gcl_aw*R0NMLjE3NTc1ODcwNTYuQ2owS0NRanc1b25HQmhEZUFSSXNBRks2UUpiSHRNLThNNFJpYmNoN3BBeDJyd0FOdlEyZkpqdEhSTUM4cUhyOTF6QVBIY1I4NEgzUjRFa2FBalAwRUFMd193Y0I.*_gcl_au*NjQ4NDIyNTQyLjE3NTYzNjQzOTE."
				(at 114.3 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Quad ARM® Cortex®-A53 MPCore with CoreSight, Dual ARM®Cortex-R5 with CoreSight, ARM Mali-400 MP2 SoC Zynq® UltraScale+ MPSoC EV Zynq®UltraScale+ FPGA, 504K+ Logic Cells 533MHz"
				(at 114.3 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "XCZU7EV-2FFVC1156I"
				(at 114.3 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "AMD-Xilinx"
				(at 114.3 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 114.3 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 114.3 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, SMT, FPGA, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "XCZU7EV-2FFVC1156I_1_1"
				(pin bidirectional line
					(at 71.12 -34.29 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_28")
					(number "A18")
				)
				(pin bidirectional line
					(at 71.12 -31.75 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_28")
					(number "A19")
				)
				(pin bidirectional line
					(at 71.12 -44.45 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_28")
					(number "A20")
				)
				(pin bidirectional line
					(at 71.12 -41.91 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_28")
					(number "A21")
				)
				(pin bidirectional line
					(at 71.12 -54.61 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_28")
					(number "A22")
				)
				(pin bidirectional line
					(at 71.12 -52.07 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_28")
					(number "A23")
				)
				(pin bidirectional line
					(at 71.12 -49.53 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_28")
					(number "B18")
				)
				(pin bidirectional line
					(at 71.12 -46.99 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_28")
					(number "B19")
				)
				(pin bidirectional line
					(at 71.12 -59.69 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_28")
					(number "B20")
				)
				(pin bidirectional line
					(at 71.12 -57.15 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_28")
					(number "B21")
				)
				(pin bidirectional line
					(at 71.12 -69.85 180)
					(length 5.08)
					(name "IO_T3U_N12_28")
					(number "B23")
				)
				(pin bidirectional line
					(at 71.12 -39.37 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_28")
					(number "C18")
				)
				(pin bidirectional line
					(at 71.12 -36.83 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_28")
					(number "C19")
				)
				(pin bidirectional line
					(at 71.12 -13.97 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_28")
					(number "C21")
				)
				(pin bidirectional line
					(at 71.12 -11.43 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_28")
					(number "C22")
				)
				(pin bidirectional line
					(at 71.12 -21.59 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_28")
					(number "C23")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_28")
					(number "D19")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_28")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_28")
					(number "D21")
				)
				(pin bidirectional line
					(at 71.12 -24.13 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_28")
					(number "D22")
				)
				(pin bidirectional line
					(at 71.12 -16.51 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_28")
					(number "D24")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_28")
					(number "E19")
				)
				(pin bidirectional line
					(at 71.12 -64.77 180)
					(length 5.08)
					(name "IO_T1U_N12_28")
					(number "E20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_28")
					(number "E21")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_28")
					(number "E22")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_28")
					(number "E23")
				)
				(pin bidirectional line
					(at 71.12 -19.05 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_28")
					(number "E24")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_28")
					(number "F20")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_28")
					(number "F21")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_28")
					(number "F22")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_28")
					(number "F23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_28")
					(number "F24")
				)
				(pin bidirectional line
					(at 71.12 -67.31 180)
					(length 5.08)
					(name "IO_T2U_N12_28")
					(number "F25")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_28")
					(number "G20")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_28")
					(number "G21")
				)
				(pin bidirectional line
					(at 71.12 -8.89 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_28")
					(number "G23")
				)
				(pin bidirectional line
					(at 71.12 -6.35 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_28")
					(number "G24")
				)
				(pin bidirectional line
					(at 71.12 -29.21 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_28")
					(number "G25")
				)
				(pin bidirectional line
					(at 71.12 -26.67 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_28")
					(number "G26")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_28")
					(number "H20")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_28")
					(number "H21")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_28")
					(number "H22")
				)
				(pin bidirectional line
					(at 71.12 -62.23 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_28")
					(number "H23")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_28")
					(number "H24")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_28")
					(number "H26")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_28")
					(number "J21")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_28")
					(number "J22")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_28")
					(number "J24")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_28")
					(number "J25")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_28")
					(number "K22")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_28")
					(number "K23")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_28")
					(number "K24")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_28")
					(number "L21")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_28")
					(number "L22")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_28")
					(number "L23")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_28")
					(number "M23")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_2_1"
				(pin bidirectional line
					(at 71.12 -54.61 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AA14")
				)
				(pin bidirectional line
					(at 71.12 -46.99 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AA15")
				)
				(pin bidirectional line
					(at 71.12 -49.53 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AA16")
				)
				(pin bidirectional line
					(at 71.12 -69.85 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AA17")
				)
				(pin bidirectional line
					(at 71.12 -52.07 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AB14")
				)
				(pin bidirectional line
					(at 71.12 -41.91 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AB15")
				)
				(pin bidirectional line
					(at 71.12 -44.45 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AB16")
				)
				(pin bidirectional line
					(at 71.12 -36.83 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AC16")
				)
				(pin bidirectional line
					(at 71.12 -39.37 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AC17")
				)
				(pin bidirectional line
					(at 71.12 -34.29 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AD15")
				)
				(pin bidirectional line
					(at 71.12 -57.15 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AD16")
				)
				(pin bidirectional line
					(at 71.12 -59.69 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AD17")
				)
				(pin bidirectional line
					(at 71.12 -31.75 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AE15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_64")
					(number "AE16")
				)
				(pin bidirectional line
					(at 71.12 -13.97 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AE17")
				)
				(pin bidirectional line
					(at 71.12 -21.59 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AF15")
				)
				(pin bidirectional line
					(at 71.12 -24.13 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AF16")
				)
				(pin bidirectional line
					(at 71.12 -11.43 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AF17")
				)
				(pin bidirectional line
					(at 71.12 -8.89 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AF18")
				)
				(pin bidirectional line
					(at 71.12 -26.67 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AG14")
				)
				(pin bidirectional line
					(at 71.12 -29.21 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AG15")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_64")
					(number "AG16")
				)
				(pin bidirectional line
					(at 71.12 -6.35 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AG18")
				)
				(pin bidirectional line
					(at 71.12 -19.05 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AH14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "AH15")
				)
				(pin bidirectional line
					(at 71.12 -67.31 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AH16")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AH17")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AH18")
				)
				(pin bidirectional line
					(at 71.12 -16.51 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AJ14")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AJ15")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AJ16")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AJ17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_64")
					(number "AJ18")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AK14")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AK15")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AK17")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AK18")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AL15")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AL16")
				)
				(pin bidirectional line
					(at 71.12 -64.77 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AL17")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AL18")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AM14")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AM15")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AM16")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AM18")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AN13")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AN14")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AN16")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AN17")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AN18")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AP13")
				)
				(pin bidirectional line
					(at 71.12 -62.23 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AP14")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AP15")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AP16")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AP17")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AP18")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_3_1"
				(pin bidirectional line
					(at 78.74 -48.26 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "AA18")
				)
				(pin bidirectional line
					(at 78.74 -58.42 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "AA19")
				)
				(pin bidirectional line
					(at 78.74 -55.88 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "AA20")
				)
				(pin bidirectional line
					(at 78.74 -45.72 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "AB18")
				)
				(pin bidirectional line
					(at 78.74 -38.1 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "AB19")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_65")
					(number "AB20")
				)
				(pin bidirectional line
					(at 78.74 -53.34 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "AC18")
				)
				(pin bidirectional line
					(at 78.74 -35.56 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "AC19")
				)
				(pin bidirectional line
					(at 78.74 -50.8 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "AD19")
				)
				(pin bidirectional line
					(at 78.74 -43.18 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "AD20")
				)
				(pin bidirectional line
					(at 78.74 -33.02 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "AE18")
				)
				(pin bidirectional line
					(at 78.74 -30.48 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "AE19")
				)
				(pin bidirectional line
					(at 78.74 -40.64 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "AE20")
				)
				(pin bidirectional line
					(at 78.74 -68.58 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "AE22")
				)
				(pin bidirectional line
					(at 78.74 -27.94 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "AE23")
				)
				(pin bidirectional line
					(at 78.74 -25.4 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "AE24")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_65")
					(number "AF19")
				)
				(pin bidirectional line
					(at 78.74 -66.04 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "AF20")
				)
				(pin bidirectional line
					(at 78.74 -22.86 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "AF21")
				)
				(pin bidirectional line
					(at 78.74 -20.32 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "AF22")
				)
				(pin bidirectional line
					(at 78.74 -17.78 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "AF23")
				)
				(pin bidirectional line
					(at 78.74 -12.7 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "AG19")
				)
				(pin bidirectional line
					(at 78.74 -10.16 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "AG20")
				)
				(pin bidirectional line
					(at 78.74 -7.62 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "AG21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "AG22")
				)
				(pin bidirectional line
					(at 78.74 -15.24 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "AG23")
				)
				(pin bidirectional line
					(at 78.74 -63.5 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "AH19")
				)
				(pin bidirectional line
					(at 78.74 -5.08 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "AH21")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "AH22")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "AH23")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "AJ19")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "AJ20")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "AJ21")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "AJ22")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "AK19")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "AK20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_65")
					(number "AK21")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "AK22")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "AK23")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "AL20")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "AL21")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "AL22")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "AL23")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "AM19")
				)
				(pin bidirectional line
					(at 78.74 -60.96 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "AM20")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "AM21")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "AM23")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "AN19")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "AN21")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "AN22")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "AN23")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "AP19")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "AP20")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "AP21")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "AP22")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "AP23")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_4_1"
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_66")
					(number "AB12")
				)
				(pin bidirectional line
					(at 69.85 -59.69 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "AB13")
				)
				(pin bidirectional line
					(at 69.85 -49.53 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "AC12")
				)
				(pin bidirectional line
					(at 69.85 -57.15 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "AC13")
				)
				(pin bidirectional line
					(at 69.85 -69.85 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "AC14")
				)
				(pin bidirectional line
					(at 69.85 -46.99 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "AD12")
				)
				(pin bidirectional line
					(at 69.85 -39.37 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "AD14")
				)
				(pin bidirectional line
					(at 69.85 -54.61 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "AE12")
				)
				(pin bidirectional line
					(at 69.85 -44.45 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "AE13")
				)
				(pin bidirectional line
					(at 69.85 -36.83 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "AE14")
				)
				(pin bidirectional line
					(at 69.85 -29.21 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "AF8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_66")
					(number "AF9")
				)
				(pin bidirectional line
					(at 69.85 -31.75 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "AF10")
				)
				(pin bidirectional line
					(at 69.85 -34.29 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "AF11")
				)
				(pin bidirectional line
					(at 69.85 -52.07 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "AF12")
				)
				(pin bidirectional line
					(at 69.85 -41.91 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "AF13")
				)
				(pin bidirectional line
					(at 69.85 -26.67 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "AG8")
				)
				(pin bidirectional line
					(at 69.85 -19.05 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "AG9")
				)
				(pin bidirectional line
					(at 69.85 -21.59 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "AG10")
				)
				(pin bidirectional line
					(at 69.85 -24.13 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "AG11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "AG12")
				)
				(pin bidirectional line
					(at 69.85 -13.97 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "AG13")
				)
				(pin bidirectional line
					(at 69.85 -67.31 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "AH8")
				)
				(pin bidirectional line
					(at 69.85 -16.51 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "AH9")
				)
				(pin bidirectional line
					(at 69.85 -8.89 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "AH11")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "AH12")
				)
				(pin bidirectional line
					(at 69.85 -11.43 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "AH13")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "AJ9")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "AJ10")
				)
				(pin bidirectional line
					(at 69.85 -6.35 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "AJ11")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "AJ12")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "AK8")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "AK9")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "AK10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_66")
					(number "AK11")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "AK12")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "AK13")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "AL8")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "AL10")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "AL11")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "AL12")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "AL13")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "AM8")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "AM9")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "AM10")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "AM11")
				)
				(pin bidirectional line
					(at 69.85 -64.77 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "AM13")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "AN8")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "AN9")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "AN11")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "AN12")
				)
				(pin bidirectional line
					(at 69.85 -62.23 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "AP8")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "AP9")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "AP10")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "AP11")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "AP12")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_5_1"
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_67")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_67")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_67")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_67")
					(number "A15")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_67")
					(number "A16")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_67")
					(number "A17")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_67")
					(number "B13")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_67")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2N_T0L_N3_67")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L2P_T0L_N2_67")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_67")
					(number "C12")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_67")
					(number "C13")
				)
				(pin bidirectional line
					(at 71.12 -62.23 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_67")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_67")
					(number "C16")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_67")
					(number "C17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_67")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_67")
					(number "D14")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_67")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_67")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_67")
					(number "D17")
				)
				(pin bidirectional line
					(at 71.12 -64.77 180)
					(length 5.08)
					(name "IO_T1U_N12_67")
					(number "E13")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_67")
					(number "E14")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_67")
					(number "E15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_67")
					(number "E17")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_67")
					(number "E18")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_67")
					(number "F13")
				)
				(pin bidirectional line
					(at 71.12 -6.35 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_67")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_67")
					(number "F16")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_67")
					(number "F17")
				)
				(pin bidirectional line
					(at 71.12 -21.59 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_67")
					(number "F18")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_67")
					(number "G14")
				)
				(pin bidirectional line
					(at 71.12 -8.89 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_67")
					(number "G15")
				)
				(pin bidirectional line
					(at 71.12 -26.67 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_67")
					(number "G16")
				)
				(pin bidirectional line
					(at 71.12 -24.13 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_67")
					(number "G18")
				)
				(pin bidirectional line
					(at 71.12 -11.43 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_67")
					(number "G19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_67")
					(number "H15")
				)
				(pin bidirectional line
					(at 71.12 -29.21 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_67")
					(number "H16")
				)
				(pin bidirectional line
					(at 71.12 -16.51 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_67")
					(number "H17")
				)
				(pin bidirectional line
					(at 71.12 -19.05 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_67")
					(number "H18")
				)
				(pin bidirectional line
					(at 71.12 -13.97 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_67")
					(number "H19")
				)
				(pin bidirectional line
					(at 71.12 -36.83 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_67")
					(number "J15")
				)
				(pin bidirectional line
					(at 71.12 -39.37 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_67")
					(number "J16")
				)
				(pin bidirectional line
					(at 71.12 -41.91 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_67")
					(number "J17")
				)
				(pin bidirectional line
					(at 71.12 -67.31 180)
					(length 5.08)
					(name "IO_T2U_N12_67")
					(number "J19")
				)
				(pin bidirectional line
					(at 71.12 -69.85 180)
					(length 5.08)
					(name "IO_T3U_N12_67")
					(number "J20")
				)
				(pin bidirectional line
					(at 71.12 -46.99 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_67")
					(number "K15")
				)
				(pin bidirectional line
					(at 71.12 -44.45 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_67")
					(number "K17")
				)
				(pin bidirectional line
					(at 71.12 -52.07 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_67")
					(number "K18")
				)
				(pin bidirectional line
					(at 71.12 -54.61 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_67")
					(number "K19")
				)
				(pin bidirectional line
					(at 71.12 -31.75 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_67")
					(number "K20")
				)
				(pin bidirectional line
					(at 71.12 -49.53 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_67")
					(number "L15")
				)
				(pin bidirectional line
					(at 71.12 -57.15 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_67")
					(number "L16")
				)
				(pin bidirectional line
					(at 71.12 -59.69 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_67")
					(number "L17")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_67")
					(number "L18")
				)
				(pin bidirectional line
					(at 71.12 -34.29 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_67")
					(number "L20")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_6_1"
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_68")
					(number "A6")
				)
				(pin bidirectional line
					(at 72.39 -11.43 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_68")
					(number "A7")
				)
				(pin bidirectional line
					(at 72.39 -13.97 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_68")
					(number "A8")
				)
				(pin bidirectional line
					(at 72.39 -69.85 180)
					(length 5.08)
					(name "IO_T3U_N12_68")
					(number "A9")
				)
				(pin bidirectional line
					(at 72.39 -6.35 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_68")
					(number "A10")
				)
				(pin bidirectional line
					(at 72.39 -16.51 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_68")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_68")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_68")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_68")
					(number "B9")
				)
				(pin bidirectional line
					(at 72.39 -8.89 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_68")
					(number "B10")
				)
				(pin bidirectional line
					(at 72.39 -19.05 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_68")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_68")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_68")
					(number "C7")
				)
				(pin bidirectional line
					(at 72.39 -52.07 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_68")
					(number "C8")
				)
				(pin bidirectional line
					(at 72.39 -54.61 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_68")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_68")
					(number "C11")
				)
				(pin bidirectional line
					(at 72.39 -64.77 180)
					(length 5.08)
					(name "IO_T1U_N12_68")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_68")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_68")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_68")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_68")
					(number "D12")
				)
				(pin bidirectional line
					(at 72.39 -46.99 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_68")
					(number "E7")
				)
				(pin bidirectional line
					(at 72.39 -57.15 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_68")
					(number "E8")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_68")
					(number "E9")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_68")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_68")
					(number "E12")
				)
				(pin bidirectional line
					(at 72.39 -49.53 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_68")
					(number "F7")
				)
				(pin bidirectional line
					(at 72.39 -59.69 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_68")
					(number "F8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_68")
					(number "F9")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_68")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_68")
					(number "F11")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_68")
					(number "F12")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_68")
					(number "G9")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_68")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_68")
					(number "G11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_68")
					(number "G12")
				)
				(pin bidirectional line
					(at 72.39 -67.31 180)
					(length 5.08)
					(name "IO_T2U_N12_68")
					(number "G13")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_68")
					(number "H9")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_68")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_68")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_68")
					(number "H13")
				)
				(pin bidirectional line
					(at 72.39 -62.23 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_68")
					(number "H14")
				)
				(pin bidirectional line
					(at 72.39 -21.59 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_68")
					(number "J10")
				)
				(pin bidirectional line
					(at 72.39 -31.75 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_68")
					(number "J11")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VREF_68")
					(number "J12")
				)
				(pin bidirectional line
					(at 72.39 -36.83 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_68")
					(number "J14")
				)
				(pin bidirectional line
					(at 72.39 -24.13 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_68")
					(number "K10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_68")
					(number "K11")
				)
				(pin bidirectional line
					(at 72.39 -34.29 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_68")
					(number "K12")
				)
				(pin bidirectional line
					(at 72.39 -41.91 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_68")
					(number "K13")
				)
				(pin bidirectional line
					(at 72.39 -39.37 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_68")
					(number "K14")
				)
				(pin bidirectional line
					(at 72.39 -26.67 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_68")
					(number "L11")
				)
				(pin bidirectional line
					(at 72.39 -29.21 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_68")
					(number "L12")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_68")
					(number "L13")
				)
				(pin bidirectional line
					(at 72.39 -44.45 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_68")
					(number "L14")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_68")
					(number "M13")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_7_1"
				(pin bidirectional line
					(at 52.07 -19.05 180)
					(length 5.08)
					(name "IO_L10N_AD2N_87")
					(number "G6")
				)
				(pin bidirectional line
					(at 52.07 -24.13 180)
					(length 5.08)
					(name "IO_L11N_AD1N_87")
					(number "G7")
				)
				(pin bidirectional line
					(at 52.07 -29.21 180)
					(length 5.08)
					(name "IO_L12N_AD0N_87")
					(number "G8")
				)
				(pin bidirectional line
					(at 52.07 -21.59 180)
					(length 5.08)
					(name "IO_L10P_AD2P_87")
					(number "H6")
				)
				(pin bidirectional line
					(at 52.07 -26.67 180)
					(length 5.08)
					(name "IO_L11P_AD1P_87")
					(number "H7")
				)
				(pin bidirectional line
					(at 52.07 -31.75 180)
					(length 5.08)
					(name "IO_L12P_AD0P_87")
					(number "H8")
				)
				(pin bidirectional line
					(at 52.07 -13.97 180)
					(length 5.08)
					(name "IO_L9N_AD3N_87")
					(number "J6")
				)
				(pin bidirectional line
					(at 52.07 -16.51 180)
					(length 5.08)
					(name "IO_L9P_AD3P_87")
					(number "J7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_87")
					(number "J8")
				)
				(pin bidirectional line
					(at 52.07 -8.89 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_87")
					(number "J9")
				)
				(pin bidirectional line
					(at 52.07 -3.81 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_87")
					(number "K8")
				)
				(pin bidirectional line
					(at 52.07 -11.43 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_87")
					(number "K9")
				)
				(pin bidirectional line
					(at 52.07 -6.35 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_87")
					(number "L8")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_87")
					(number "L10")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_87")
					(number "M8")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_87")
					(number "M9")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_87")
					(number "M10")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L4N_AD8N_87")
					(number "M11")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L3N_AD9N_87")
					(number "M12")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L2N_AD10N_87")
					(number "N8")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2P_AD10P_87")
					(number "N9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_87")
					(number "N10")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4P_AD8P_87")
					(number "N11")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_L1N_AD11N_87")
					(number "N12")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3P_AD9P_87")
					(number "N13")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1P_AD11P_87")
					(number "P12")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_8_1"
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "IO_L3N_AD13N_88")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "IO_L3P_AD13P_88")
					(number "A3")
				)
				(pin bidirectional line
					(at 48.26 -19.05 180)
					(length 5.08)
					(name "IO_L10N_AD10N_88")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "IO_L2N_AD14N_88")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "IO_L6N_HDGC_88")
					(number "B3")
				)
				(pin bidirectional line
					(at 48.26 -3.81 180)
					(length 5.08)
					(name "IO_L7N_HDGC_88")
					(number "B4")
				)
				(pin bidirectional line
					(at 48.26 -21.59 180)
					(length 5.08)
					(name "IO_L10P_AD10P_88")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "IO_L2P_AD14P_88")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "IO_L5N_HDGC_88")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "IO_L6P_HDGC_88")
					(number "C3")
				)
				(pin bidirectional line
					(at 48.26 -6.35 180)
					(length 5.08)
					(name "IO_L7P_HDGC_88")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "IO_L1N_AD15N_88")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "IO_L5P_HDGC_88")
					(number "D2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_88")
					(number "D3")
				)
				(pin bidirectional line
					(at 48.26 -8.89 180)
					(length 5.08)
					(name "IO_L8N_HDGC_88")
					(number "D4")
				)
				(pin bidirectional line
					(at 48.26 -24.13 180)
					(length 5.08)
					(name "IO_L11N_AD9N_88")
					(number "D5")
				)
				(pin bidirectional line
					(at 48.26 -26.67 180)
					(length 5.08)
					(name "IO_L11P_AD9P_88")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "IO_L1P_AD15P_88")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "IO_L4N_AD12N_88")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "IO_L4P_AD12P_88")
					(number "E3")
				)
				(pin bidirectional line
					(at 48.26 -11.43 180)
					(length 5.08)
					(name "IO_L8P_HDGC_88")
					(number "E4")
				)
				(pin bidirectional line
					(at 48.26 -29.21 180)
					(length 5.08)
					(name "IO_L12N_AD8N_88")
					(number "E5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_88")
					(number "E6")
				)
				(pin bidirectional line
					(at 48.26 -13.97 180)
					(length 5.08)
					(name "IO_L9N_AD11N_88")
					(number "F4")
				)
				(pin bidirectional line
					(at 48.26 -16.51 180)
					(length 5.08)
					(name "IO_L9P_AD11P_88")
					(number "F5")
				)
				(pin bidirectional line
					(at 48.26 -31.75 180)
					(length 5.08)
					(name "IO_L12P_AD8P_88")
					(number "F6")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_9_1"
				(pin bidirectional clock
					(at 49.53 -24.13 180)
					(length 5.08)
					(name "MGTREFCLK1N_223")
					(number "AC9")
				)
				(pin bidirectional clock
					(at 49.53 -21.59 180)
					(length 5.08)
					(name "MGTREFCLK1P_223")
					(number "AC10")
				)
				(pin bidirectional clock
					(at 0 -24.13 0)
					(length 5.08)
					(name "MGTREFCLK0N_223")
					(number "AD7")
				)
				(pin bidirectional clock
					(at 0 -21.59 0)
					(length 5.08)
					(name "MGTREFCLK0P_223")
					(number "AD8")
				)
				(pin output line
					(at 49.53 -17.78 180)
					(length 5.08)
					(name "MGTHTXN3_223")
					(number "AJ5")
				)
				(pin output line
					(at 49.53 -15.24 180)
					(length 5.08)
					(name "MGTHTXP3_223")
					(number "AJ6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTHRXN3_223")
					(number "AK3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTHRXP3_223")
					(number "AK4")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTHRXN2_223")
					(number "AL1")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTHRXP2_223")
					(number "AL2")
				)
				(pin output line
					(at 49.53 -12.7 180)
					(length 5.08)
					(name "MGTHTXN2_223")
					(number "AL5")
				)
				(pin output line
					(at 49.53 -10.16 180)
					(length 5.08)
					(name "MGTHTXP2_223")
					(number "AL6")
				)
				(pin output line
					(at 49.53 -7.62 180)
					(length 5.08)
					(name "MGTHTXN1_223")
					(number "AM3")
				)
				(pin output line
					(at 49.53 -5.08 180)
					(length 5.08)
					(name "MGTHTXP1_223")
					(number "AM4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTHRXN1_223")
					(number "AN1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTHRXP1_223")
					(number "AN2")
				)
				(pin output line
					(at 49.53 -2.54 180)
					(length 5.08)
					(name "MGTHTXN0_223")
					(number "AN5")
				)
				(pin output line
					(at 49.53 0 180)
					(length 5.08)
					(name "MGTHTXP0_223")
					(number "AN6")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTHRXN0_223")
					(number "AP3")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "MGTHRXP0_223")
					(number "AP4")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_10_1"
				(pin bidirectional clock
					(at 49.53 -24.13 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "AA9")
				)
				(pin bidirectional clock
					(at 49.53 -21.59 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "AA10")
				)
				(pin bidirectional clock
					(at 0 -24.13 0)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "AB7")
				)
				(pin bidirectional clock
					(at 0 -21.59 0)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "AB8")
				)
				(pin output line
					(at 49.53 -17.78 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "AD3")
				)
				(pin output line
					(at 49.53 -15.24 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "AD4")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "AE1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "AE2")
				)
				(pin output line
					(at 49.53 -12.7 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "AE5")
				)
				(pin output line
					(at 49.53 -10.16 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "AE6")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "AF3")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "AF4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "AG1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "AG2")
				)
				(pin output line
					(at 49.53 -7.62 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "AG5")
				)
				(pin output line
					(at 49.53 -5.08 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "AG6")
				)
				(pin output line
					(at 49.53 -2.54 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "AH3")
				)
				(pin output line
					(at 49.53 0 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "AH4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "AJ1")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "AJ2")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_11_1"
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTHRXN2_225")
					(number "AA1")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTHRXP2_225")
					(number "AA2")
				)
				(pin output line
					(at 49.53 -7.62 180)
					(length 5.08)
					(name "MGTHTXN1_225")
					(number "AA5")
				)
				(pin output line
					(at 49.53 -5.08 180)
					(length 5.08)
					(name "MGTHTXP1_225")
					(number "AA6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTHRXN1_225")
					(number "AB3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTHRXP1_225")
					(number "AB4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTHRXN0_225")
					(number "AC1")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "MGTHRXP0_225")
					(number "AC2")
				)
				(pin output line
					(at 49.53 -2.54 180)
					(length 5.08)
					(name "MGTHTXN0_225")
					(number "AC5")
				)
				(pin output line
					(at 49.53 0 180)
					(length 5.08)
					(name "MGTHTXP0_225")
					(number "AC6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTHRXN3_225")
					(number "W1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTHRXP3_225")
					(number "W2")
				)
				(pin output line
					(at 49.53 -17.78 180)
					(length 5.08)
					(name "MGTHTXN3_225")
					(number "W5")
				)
				(pin output line
					(at 49.53 -15.24 180)
					(length 5.08)
					(name "MGTHTXP3_225")
					(number "W6")
				)
				(pin bidirectional clock
					(at 49.53 -24.13 180)
					(length 5.08)
					(name "MGTREFCLK1N_225")
					(number "W9")
				)
				(pin bidirectional clock
					(at 49.53 -21.59 180)
					(length 5.08)
					(name "MGTREFCLK1P_225")
					(number "W10")
				)
				(pin output line
					(at 49.53 -12.7 180)
					(length 5.08)
					(name "MGTHTXN2_225")
					(number "Y3")
				)
				(pin output line
					(at 49.53 -10.16 180)
					(length 5.08)
					(name "MGTHTXP2_225")
					(number "Y4")
				)
				(pin bidirectional clock
					(at 0 -24.13 0)
					(length 5.08)
					(name "MGTREFCLK0N_225")
					(number "Y7")
				)
				(pin bidirectional clock
					(at 0 -21.59 0)
					(length 5.08)
					(name "MGTREFCLK0P_225")
					(number "Y8")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_12_1"
				(pin output line
					(at 49.53 -17.78 180)
					(length 5.08)
					(name "MGTHTXN3_226")
					(number "N5")
				)
				(pin output line
					(at 49.53 -15.24 180)
					(length 5.08)
					(name "MGTHTXP3_226")
					(number "N6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTHRXN3_226")
					(number "P3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTHRXP3_226")
					(number "P4")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTHRXN2_226")
					(number "R1")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTHRXP2_226")
					(number "R2")
				)
				(pin output line
					(at 49.53 -12.7 180)
					(length 5.08)
					(name "MGTHTXN2_226")
					(number "R5")
				)
				(pin output line
					(at 49.53 -10.16 180)
					(length 5.08)
					(name "MGTHTXP2_226")
					(number "R6")
				)
				(pin output line
					(at 49.53 -7.62 180)
					(length 5.08)
					(name "MGTHTXN1_226")
					(number "T3")
				)
				(pin output line
					(at 49.53 -5.08 180)
					(length 5.08)
					(name "MGTHTXP1_226")
					(number "T4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTHRXN1_226")
					(number "U1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTHRXP1_226")
					(number "U2")
				)
				(pin output line
					(at 49.53 -2.54 180)
					(length 5.08)
					(name "MGTHTXN0_226")
					(number "U5")
				)
				(pin output line
					(at 49.53 0 180)
					(length 5.08)
					(name "MGTHTXP0_226")
					(number "U6")
				)
				(pin bidirectional clock
					(at 49.53 -24.13 180)
					(length 5.08)
					(name "MGTREFCLK1N_226")
					(number "U9")
				)
				(pin bidirectional clock
					(at 49.53 -21.59 180)
					(length 5.08)
					(name "MGTREFCLK1P_226")
					(number "U10")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTHRXN0_226")
					(number "V3")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "MGTHRXP0_226")
					(number "V4")
				)
				(pin bidirectional clock
					(at 0 -24.13 0)
					(length 5.08)
					(name "MGTREFCLK0N_226")
					(number "V7")
				)
				(pin bidirectional clock
					(at 0 -21.59 0)
					(length 5.08)
					(name "MGTREFCLK0P_226")
					(number "V8")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_13_1"
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MGTHRXN3_227")
					(number "G1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTHRXP3_227")
					(number "G2")
				)
				(pin output line
					(at 49.53 -17.78 180)
					(length 5.08)
					(name "MGTHTXN3_227")
					(number "H3")
				)
				(pin output line
					(at 49.53 -15.24 180)
					(length 5.08)
					(name "MGTHTXP3_227")
					(number "H4")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTHRXN2_227")
					(number "J1")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MGTHRXP2_227")
					(number "J2")
				)
				(pin output line
					(at 49.53 -12.7 180)
					(length 5.08)
					(name "MGTHTXN2_227")
					(number "K3")
				)
				(pin output line
					(at 49.53 -10.16 180)
					(length 5.08)
					(name "MGTHTXP2_227")
					(number "K4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MGTHRXN1_227")
					(number "L1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTHRXP1_227")
					(number "L2")
				)
				(pin output line
					(at 49.53 -7.62 180)
					(length 5.08)
					(name "MGTHTXN1_227")
					(number "L5")
				)
				(pin output line
					(at 49.53 -5.08 180)
					(length 5.08)
					(name "MGTHTXP1_227")
					(number "L6")
				)
				(pin output line
					(at 49.53 -2.54 180)
					(length 5.08)
					(name "MGTHTXN0_227")
					(number "M3")
				)
				(pin output line
					(at 49.53 0 180)
					(length 5.08)
					(name "MGTHTXP0_227")
					(number "M4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTHRXN0_227")
					(number "N1")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "MGTHRXP0_227")
					(number "N2")
				)
				(pin bidirectional clock
					(at 49.53 -24.13 180)
					(length 5.08)
					(name "MGTREFCLK1N_227")
					(number "R9")
				)
				(pin bidirectional clock
					(at 49.53 -21.59 180)
					(length 5.08)
					(name "MGTREFCLK1P_227")
					(number "R10")
				)
				(pin bidirectional clock
					(at 0 -24.13 0)
					(length 5.08)
					(name "MGTREFCLK0N_227")
					(number "T7")
				)
				(pin bidirectional clock
					(at 0 -21.59 0)
					(length 5.08)
					(name "MGTREFCLK0P_227")
					(number "T8")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_14_1"
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "PS_MIO0")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "PS_MIO4")
					(number "A25")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PS_MIO6")
					(number "A26")
				)
				(pin bidirectional line
					(at 34.29 -8.89 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "A27")
				)
				(pin bidirectional line
					(at 34.29 -13.97 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "A28")
				)
				(pin power_in line
					(at 34.29 -39.37 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "AA24")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCC_PSADC")
					(number "AA25")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PS_MIO2")
					(number "B24")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "PS_MIO7")
					(number "B25")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "PS_MIO11")
					(number "B26")
				)
				(pin bidirectional line
					(at 34.29 -21.59 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "B28")
				)
				(pin bidirectional line
					(at 34.29 -31.75 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "B29")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "PS_MIO1")
					(number "C24")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "C25")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "PS_MIO9")
					(number "C26")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "PS_MIO12")
					(number "C27")
				)
				(pin bidirectional line
					(at 34.29 -26.67 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "C28")
				)
				(pin bidirectional line
					(at 34.29 -16.51 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "C29")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PS_MIO5")
					(number "D25")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "PS_MIO8")
					(number "D26")
				)
				(pin bidirectional line
					(at 34.29 -6.35 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "D27")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSIO0_500")
					(number "D28")
				)
				(pin bidirectional line
					(at 34.29 -36.83 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "D29")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PS_MIO3")
					(number "E25")
				)
				(pin bidirectional line
					(at 34.29 -11.43 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "E27")
				)
				(pin bidirectional line
					(at 34.29 -34.29 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "E28")
				)
				(pin bidirectional line
					(at 34.29 -24.13 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "E29")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "PS_MIO10")
					(number "F26")
				)
				(pin bidirectional line
					(at 34.29 -19.05 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "F27")
				)
				(pin bidirectional line
					(at 34.29 -29.21 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "F28")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_15_1"
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "PS_MIO26")
					(number "A29")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "PS_MIO27")
					(number "A30")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "PS_MIO28")
					(number "A31")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PS_MIO29")
					(number "A32")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PS_MIO30")
					(number "A33")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "PS_MIO31")
					(number "B30")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PS_MIO32")
					(number "B31")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "B32")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PS_MIO33")
					(number "B33")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "PS_MIO34")
					(number "B34")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "PS_MIO35")
					(number "C31")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "PS_MIO36")
					(number "C32")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "PS_MIO37")
					(number "C33")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "PS_MIO38")
					(number "C34")
				)
				(pin bidirectional line
					(at 34.29 -3.81 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "D30")
				)
				(pin bidirectional line
					(at 34.29 -6.35 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "D31")
				)
				(pin bidirectional line
					(at 34.29 -8.89 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "D32")
				)
				(pin bidirectional line
					(at 34.29 -11.43 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "D34")
				)
				(pin bidirectional line
					(at 34.29 -13.97 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "E30")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSIO1_501")
					(number "E31")
				)
				(pin bidirectional line
					(at 34.29 -16.51 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "E32")
				)
				(pin bidirectional line
					(at 34.29 -19.05 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "E33")
				)
				(pin bidirectional line
					(at 34.29 -21.59 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "E34")
				)
				(pin bidirectional line
					(at 34.29 -24.13 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "F30")
				)
				(pin bidirectional line
					(at 34.29 -26.67 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "F31")
				)
				(pin bidirectional line
					(at 34.29 -29.21 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "F32")
				)
				(pin bidirectional line
					(at 34.29 -31.75 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "F33")
				)
				(pin bidirectional line
					(at 34.29 -34.29 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "F34")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_16_1"
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "PS_MIO52")
					(number "G29")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "PS_MIO53")
					(number "G30")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "PS_MIO54")
					(number "G31")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PS_MIO55")
					(number "G33")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PS_MIO56")
					(number "G34")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "PS_MIO57")
					(number "H29")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "H30")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PS_MIO58")
					(number "H31")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PS_MIO59")
					(number "H32")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "PS_MIO60")
					(number "H33")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "PS_MIO61")
					(number "H34")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "PS_MIO62")
					(number "J29")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "PS_MIO63")
					(number "J30")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "PS_MIO64")
					(number "J31")
				)
				(pin bidirectional line
					(at 34.29 -3.81 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "J32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSIO2_502")
					(number "J33")
				)
				(pin bidirectional line
					(at 34.29 -6.35 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "J34")
				)
				(pin bidirectional line
					(at 34.29 -8.89 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "K28")
				)
				(pin bidirectional line
					(at 34.29 -11.43 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "K29")
				)
				(pin bidirectional line
					(at 34.29 -13.97 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "K30")
				)
				(pin bidirectional line
					(at 34.29 -16.51 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "K31")
				)
				(pin bidirectional line
					(at 34.29 -19.05 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "K32")
				)
				(pin bidirectional line
					(at 34.29 -21.59 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "K33")
				)
				(pin bidirectional line
					(at 34.29 -24.13 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "K34")
				)
				(pin bidirectional line
					(at 34.29 -26.67 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "L29")
				)
				(pin bidirectional line
					(at 34.29 -29.21 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "L30")
				)
				(pin bidirectional line
					(at 34.29 -31.75 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "L33")
				)
				(pin bidirectional line
					(at 34.29 -34.29 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "L34")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_17_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "G27")
				)
				(pin output line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "G28")
				)
				(pin bidirectional line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "H27")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "H28")
				)
				(pin bidirectional line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "J26")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "J27")
				)
				(pin bidirectional line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "K25")
				)
				(pin bidirectional line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "K26")
				)
				(pin input clock
					(at 0 -16.51 0)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "K27")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PS_PADO")
					(number "L25")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 5.08)
					(name "~{PS_POR}")
					(number "M24")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PS_PADI")
					(number "M25")
				)
				(pin output line
					(at 45.72 0 180)
					(length 5.08)
					(name "PS_DONE")
					(number "N24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSIO3_503")
					(number "N25")
				)
				(pin bidirectional line
					(at 45.72 -8.89 180)
					(length 5.08)
					(name "~{PS_INIT}")
					(number "P24")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 5.08)
					(name "~{PS_SRST}")
					(number "P25")
				)
				(pin input clock
					(at 0 -12.7 0)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R24")
				)
				(pin output line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "R25")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 5.08)
					(name "~{PS_PROG}")
					(number "T24")
				)
				(pin output line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "T25")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_18_1"
				(pin output line
					(at 48.26 -74.93 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "AA26")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "~{PS_DDR_ALERT}")
					(number "AB26")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "AC26")
				)
				(pin output line
					(at 48.26 -46.99 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "AC32")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "~{PS_DDR_RAM_RST}")
					(number "AD26")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "AD27")
				)
				(pin output line
					(at 48.26 -41.91 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "AD29")
				)
				(pin output line
					(at 48.26 0 180)
					(length 5.08)
					(name "~{PS_DDR_ACT}")
					(number "AE25")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AE26")
				)
				(pin output line
					(at 48.26 -6.35 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "AE27")
				)
				(pin output line
					(at 48.26 -8.89 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "AE28")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSDDR_504")
					(number "AE31")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AF26")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "AF27")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AF28")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AF30")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AF31")
				)
				(pin output line
					(at 48.26 -52.07 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "AF34")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSDDR_504")
					(number "AG27")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AG28")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AG29")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AG30")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AG31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSDDR_504")
					(number "AG32")
				)
				(pin output line
					(at 48.26 -36.83 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AH24")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AH31")
				)
				(pin output line
					(at 48.26 -21.59 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "AH32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSDDR_504")
					(number "AJ28")
				)
				(pin output line
					(at 48.26 -39.37 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AJ29")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AJ30")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AJ31")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "AJ32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSDDR_504")
					(number "AJ33")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "AK30")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "AK32")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AK33")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCO_PSDDR_504")
					(number "AL29")
				)
				(pin output clock
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "AL30")
				)
				(pin output clock
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "AL31")
				)
				(pin output clock
					(at 48.26 -64.77 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "AL32")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "AL33")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AL34")
				)
				(pin output line
					(at 48.26 -34.29 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AM29")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AM33")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "AM34")
				)
				(pin output line
					(at 48.26 -31.75 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AN24")
				)
				(pin output clock
					(at 48.26 -62.23 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "AN32")
				)
				(pin output line
					(at 48.26 -19.05 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "AN33")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "AN34")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "AP32")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "AP33")
				)
				(pin output line
					(at 48.26 -44.45 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "Y29")
				)
				(pin output line
					(at 48.26 -49.53 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "Y32")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_19_1"
				(pin bidirectional line
					(at 46.99 -12.7 180)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "AA27")
				)
				(pin bidirectional line
					(at 46.99 -15.24 180)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "AA28")
				)
				(pin bidirectional line
					(at 46.99 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "AA30")
				)
				(pin bidirectional line
					(at 46.99 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "AA31")
				)
				(pin bidirectional line
					(at 46.99 -30.48 180)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "AA32")
				)
				(pin bidirectional line
					(at 46.99 -33.02 180)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "AA33")
				)
				(pin bidirectional line
					(at 46.99 -35.56 180)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "AA34")
				)
				(pin bidirectional line
					(at 46.99 -17.78 180)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "AB28")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "AB29")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "AB30")
				)
				(pin bidirectional line
					(at 46.99 -43.18 180)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "AB31")
				)
				(pin bidirectional line
					(at 46.99 -97.79 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "AB33")
				)
				(pin bidirectional line
					(at 46.99 -100.33 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "AB34")
				)
				(pin bidirectional line
					(at 46.99 -10.16 180)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "AC27")
				)
				(pin bidirectional line
					(at 46.99 -5.08 180)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "AC28")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "AC29")
				)
				(pin bidirectional line
					(at 46.99 0 180)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "AC31")
				)
				(pin bidirectional line
					(at 46.99 -48.26 180)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "AC33")
				)
				(pin bidirectional line
					(at 46.99 -45.72 180)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "AC34")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "AD30")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "AD31")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "AD32")
				)
				(pin bidirectional line
					(at 46.99 -40.64 180)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "AD34")
				)
				(pin bidirectional line
					(at 46.99 -7.62 180)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "AE29")
				)
				(pin bidirectional line
					(at 46.99 -2.54 180)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "AE30")
				)
				(pin bidirectional line
					(at 46.99 -73.66 180)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "AE32")
				)
				(pin bidirectional line
					(at 46.99 -78.74 180)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "AE33")
				)
				(pin bidirectional line
					(at 46.99 -38.1 180)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "AE34")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AF25")
				)
				(pin bidirectional line
					(at 46.99 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "AF32")
				)
				(pin bidirectional line
					(at 46.99 -81.28 180)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "AF33")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG24")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AG25")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AG26")
				)
				(pin bidirectional line
					(at 46.99 -107.95 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "AG33")
				)
				(pin bidirectional line
					(at 46.99 -110.49 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "AG34")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AH26")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH27")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH28")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AH29")
				)
				(pin bidirectional line
					(at 46.99 -76.2 180)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "AH33")
				)
				(pin bidirectional line
					(at 46.99 -83.82 180)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "AH34")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AJ24")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AJ25")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AJ26")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AJ27")
				)
				(pin bidirectional line
					(at 46.99 -86.36 180)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "AJ34")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AK24")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AK25")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AK27")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AK28")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AK29")
				)
				(pin bidirectional line
					(at 46.99 -88.9 180)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "AK34")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AL25")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AL26")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AL27")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AL28")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AM24")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AM25")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AM26")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AM28")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AM30")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AM31")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AN26")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AN27")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AN28")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AN29")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AN31")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AP24")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AP25")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AP26")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AP27")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AP28")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AP29")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AP30")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AP31")
				)
				(pin bidirectional line
					(at 46.99 -27.94 180)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "V27")
				)
				(pin bidirectional line
					(at 46.99 -20.32 180)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "W27")
				)
				(pin bidirectional line
					(at 46.99 -25.4 180)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "W28")
				)
				(pin bidirectional line
					(at 46.99 -22.86 180)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "W29")
				)
				(pin bidirectional line
					(at 46.99 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "W30")
				)
				(pin bidirectional line
					(at 46.99 -102.87 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "W31")
				)
				(pin bidirectional line
					(at 46.99 -105.41 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "W32")
				)
				(pin bidirectional line
					(at 46.99 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "W33")
				)
				(pin bidirectional line
					(at 46.99 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "W34")
				)
				(pin bidirectional line
					(at 46.99 -92.71 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "Y27")
				)
				(pin bidirectional line
					(at 46.99 -95.25 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "Y28")
				)
				(pin bidirectional line
					(at 46.99 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "Y30")
				)
				(pin bidirectional line
					(at 46.99 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "Y33")
				)
				(pin bidirectional line
					(at 46.99 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "Y34")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_20_1"
				(pin input clock
					(at 57.15 -25.4 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "M27")
				)
				(pin input clock
					(at 57.15 -27.94 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "M28")
				)
				(pin input clock
					(at 57.15 -30.48 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "M31")
				)
				(pin input clock
					(at 57.15 -33.02 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "M32")
				)
				(pin output line
					(at 57.15 -17.78 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "N29")
				)
				(pin output line
					(at 57.15 -20.32 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "N30")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "N33")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "N34")
				)
				(pin input clock
					(at 0 -30.48 0)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "P27")
				)
				(pin input clock
					(at 0 -33.02 0)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "P28")
				)
				(pin output line
					(at 57.15 -12.7 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "P31")
				)
				(pin output line
					(at 57.15 -15.24 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "P32")
				)
				(pin output line
					(at 57.15 -7.62 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "R29")
				)
				(pin output line
					(at 57.15 -10.16 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "R30")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "R33")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "R34")
				)
				(pin input clock
					(at 0 -25.4 0)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "T27")
				)
				(pin input clock
					(at 0 -27.94 0)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "T28")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "T31")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "T32")
				)
				(pin output line
					(at 57.15 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "U29")
				)
				(pin output line
					(at 57.15 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "U30")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "U31")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "U33")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "U34")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_21_1"
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "AA12")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "~{PUDC}")
					(number "AA13")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCCINT_VCU")
					(number "AD21")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_VCU")
					(number "AD22")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_VCU")
					(number "AD23")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_VCU")
					(number "AD24")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GNDADC")
					(number "R17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCADC")
					(number "R18")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "VREFN")
					(number "T17")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "VP")
					(number "T18")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VN")
					(number "U17")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VREFP")
					(number "U18")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "DXN")
					(number "V17")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DXP")
					(number "V18")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_22_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "AA8")
				)
				(pin power_in line
					(at 44.45 -15.24 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "AA22")
				)
				(pin power_in line
					(at 44.45 -10.16 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA23")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "AB6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "AB10")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP")
					(number "AB21")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP")
					(number "AB22")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP")
					(number "AB23")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP")
					(number "AB24")
				)
				(pin power_in line
					(at 44.45 -12.7 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AB25")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "AC8")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP")
					(number "AC21")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP")
					(number "AC22")
				)
				(pin passive line
					(at 44.45 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP_DDR")
					(number "AC24")
				)
				(pin passive line
					(at 44.45 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTFP_DDR")
					(number "AC25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AD6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "AD9")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MGTRREF_R")
					(number "AD10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AF6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AH6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AK6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AM6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "AP6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "M6")
				)
				(pin power_in line
					(at 44.45 -2.54 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "N27")
				)
				(pin power_in line
					(at 44.45 0 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "N31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "P6")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "PS_MGTRAVTT")
					(number "P29")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "R8")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "PS_MGTRAVCC")
					(number "R27")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "T6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "T10")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 5.08)
					(hide yes)
					(name "PS_MGTRAVTT")
					(number "T29")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "U8")
				)
				(pin power_in line
					(at 44.45 -7.62 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U25")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "V6")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "V10")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTLP")
					(number "V22")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "V24")
				)
				(pin passive line
					(at 44.45 -7.62 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSDDR_PLL")
					(number "V25")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVCC_R")
					(number "W8")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTLP")
					(number "W21")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTLP")
					(number "W22")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSPLL")
					(number "W24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSAUX")
					(number "W25")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSAUX")
					(number "W26")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "MGTAVTT_R")
					(number "Y6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "MGTVCCAUX_R")
					(number "Y10")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTLP")
					(number "Y21")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCC_PSINTLP")
					(number "Y22")
				)
				(pin power_in line
					(at 44.45 -5.08 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y23")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSPLL")
					(number "Y24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VCC_PSAUX")
					(number "Y25")
				)
			)
			(symbol "XCZU7EV-2FFVC1156I_23_1"
				(text "POWER"
					(at 7.62 2.54 0)
				)
				(pin power_in line
					(at 26.67 -11.43 180)
					(length 5.08)
					(name "GND")
					(number "A1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF29")
				)
				(pin power_in line
					(at 26.67 -11.43 180)
					(length 5.08)
					(name "GND")
					(number "AG3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AN30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AP34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H25")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at 26.67 -11.43 180)
					(length 5.08)
					(name "GND")
					(number "K7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCINT")
					(number "M15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "M21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "N20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N21")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "N22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P8")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P10")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCCINT_IO")
					(number "P13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "P21")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P22")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 5.08)
					(name "VCCAUX")
					(number "P23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R11")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VCCBRAM")
					(number "R12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "R14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "R16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "R20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R21")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "R22")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "R23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "T12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "T13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "T21")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "T22")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "U13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "U20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U21")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX_IO")
					(number "U22")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "U23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U24")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U27")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U28")
				)
				(pin power_in line
					(at 26.67 -11.43 180)
					(length 5.08)
					(name "GND")
					(number "U32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "V12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "V13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "V21")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "V23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V28")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V29")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V30")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V31")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V32")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V33")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V34")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W3")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W4")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W7")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCBRAM")
					(number "W12")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W14")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W16")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W18")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "W20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W23")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y1")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y2")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y5")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y9")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y11")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT_IO")
					(number "Y13")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y15")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y17")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCCINT")
					(number "Y19")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y20")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y26")
				)
				(pin passive line
					(at 26.67 -11.43 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y31")
				)
			)
			(embedded_fonts no)
		)
)
