(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF52805-CAXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF52805-CAXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf52:BGA-28_6x6_2.482x2.464mm"
				(at 1.27 -38.1 0)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/nRF52805_PS_v1.4/resource/nRF52805_PS_v1.4.pdf"
				(at 0 -40.64 0)
			)
			(property "Description" "2.4GHz Bluetooth 5.4 SoC, 192KB Flash, 24KB RAM, Cortex-M4, ADC, SPI, UART, TWI, QDEC, WLCSP-36"
				(at 2.54 -35.56 0)
			)
			(property "ki_keywords" "ble bluetooth-low-energy arm cortex-m4 soc microcontroller two-layer wireless 2mbps csa2 wlcsp nrf52-series"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?28*6x6*2.482x2.464mm*"
				(at 0 0 0)
			)
			(symbol "nRF52805-CAXX_1_0"
				(pin bidirectional line
					(at -22.86 10.16 0)
					(length 2.54)
					(name "P0.00")
					(number "D6")
					(alternate "XL1" input line)
				)
				(pin bidirectional line
					(at -22.86 5.08 0)
					(length 2.54)
					(name "P0.01")
					(number "D5")
					(alternate "XL2" input line)
				)
				(pin bidirectional line
					(at -22.86 -2.54 0)
					(length 2.54)
					(name "P0.04")
					(number "F5")
					(alternate "AIN2" input line)
				)
				(pin bidirectional line
					(at -22.86 -5.08 0)
					(length 2.54)
					(name "P0.05")
					(number "F6")
					(alternate "AIN3" input line)
				)
				(pin bidirectional line
					(at -22.86 -7.62 0)
					(length 2.54)
					(name "P0.12")
					(number "G5")
				)
				(pin bidirectional line
					(at -22.86 -10.16 0)
					(length 2.54)
					(name "P0.14")
					(number "F4")
				)
				(pin bidirectional line
					(at -22.86 -12.7 0)
					(length 2.54)
					(name "P0.16")
					(number "G4")
				)
				(pin bidirectional line
					(at -22.86 -15.24 0)
					(length 2.54)
					(name "P0.18")
					(number "G3")
				)
				(pin bidirectional line
					(at -22.86 -17.78 0)
					(length 2.54)
					(name "P0.20")
					(number "F2")
				)
				(pin power_in line
					(at 0 33.02 270)
					(length 2.54)
					(name "VDD")
					(number "A6")
				)
				(pin power_in line
					(at 0 33.02 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "G6")
				)
				(pin power_in line
					(at 0 -33.02 90)
					(length 2.54)
					(name "VSS")
					(number "B3")
				)
				(pin passive line
					(at 0 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "B4")
				)
				(pin passive line
					(at 0 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "VSS_PA")
					(number "C1")
				)
				(pin passive line
					(at 0 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D3")
				)
				(pin passive line
					(at 0 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 0 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E3")
				)
				(pin passive line
					(at 0 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin power_out line
					(at 2.54 33.02 270)
					(length 2.54)
					(name "DCC")
					(number "A5")
				)
				(pin passive line
					(at 22.86 22.86 180)
					(length 2.54)
					(name "DEC1")
					(number "B6")
				)
				(pin passive line
					(at 22.86 20.32 180)
					(length 2.54)
					(name "DEC2")
					(number "A3")
				)
				(pin passive line
					(at 22.86 17.78 180)
					(length 2.54)
					(name "DEC4")
					(number "A4")
				)
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "ANT")
					(number "E1")
				)
				(pin input line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "~{RESET}")
					(number "G2")
					(alternate "P0.21" bidirectional line)
				)
				(pin input line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "SWDCLK")
					(number "G1")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "SWDIO")
					(number "F1")
				)
			)
			(symbol "nRF52805-CAXX_1_1"
				(pin input line
					(at -22.86 22.86 0)
					(length 2.54)
					(name "XC1")
					(number "A1")
				)
				(pin input line
					(at -22.86 17.78 0)
					(length 2.54)
					(name "XC2")
					(number "A2")
				)
			)
			(embedded_fonts no)
		)
)
