(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF52820-CFXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF52820-CFXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf52:BGA-44_7x7_2.531x2.531mm"
				(at 0 -68.58 0)
			)
			(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf52820/attach/nRF52820_PS_v1.5.pdf?_LANG=enus"
				(at 0 -73.66 0)
			)
			(property "Description" "2.4GHz Bluetooth 5.4 USB SoC, 256KB Flash, 32KB RAM, Cortex-M4, Comparator, UART, SPI, TWI, QDEC, CSP-"
				(at 0 -71.12 0)
			)
			(property "ki_keywords" "ble bluetooth-low-energy bluetooth-mesh thread zigbee arm microcontroller wireless 2mbps usb2 direction-finding mesh-networking csp nrf52-series"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?44*7x7*2.531x2.531mm*"
				(at 0 0 0)
			)
			(symbol "nRF52820-CFXX_0_0"
				(pin bidirectional line
					(at -25.4 45.72 0)
					(length 2.54)
					(name "D+")
					(number "G5")
				)
				(pin bidirectional line
					(at -25.4 43.18 0)
					(length 2.54)
					(name "D-")
					(number "G4")
				)
				(pin input line
					(at -25.4 33.02 0)
					(length 2.54)
					(name "XC1")
					(number "A1")
				)
				(pin input line
					(at -25.4 27.94 0)
					(length 2.54)
					(name "XC2")
					(number "A2")
				)
				(pin bidirectional line
					(at -25.4 -10.16 0)
					(length 2.54)
					(name "P0.06")
					(number "E6")
				)
				(pin bidirectional line
					(at -25.4 -12.7 0)
					(length 2.54)
					(name "P0.07")
					(number "F6")
				)
				(pin bidirectional line
					(at -25.4 -15.24 0)
					(length 2.54)
					(name "P0.08")
					(number "B3")
				)
				(pin bidirectional line
					(at -25.4 -17.78 0)
					(length 2.54)
					(name "P0.14")
					(number "F4")
				)
				(pin bidirectional line
					(at -25.4 -20.32 0)
					(length 2.54)
					(name "P0.15")
					(number "F3")
				)
				(pin bidirectional line
					(at -25.4 -22.86 0)
					(length 2.54)
					(name "P0.16")
					(number "E3")
				)
				(pin bidirectional line
					(at -25.4 -25.4 0)
					(length 2.54)
					(name "P0.17")
					(number "E2")
				)
				(pin bidirectional line
					(at -25.4 -27.94 0)
					(length 2.54)
					(name "P0.20")
					(number "F2")
				)
				(pin bidirectional line
					(at -25.4 -30.48 0)
					(length 2.54)
					(name "P0.28")
					(number "C5")
				)
				(pin bidirectional line
					(at -25.4 -33.02 0)
					(length 2.54)
					(name "P0.29")
					(number "C4")
				)
				(pin bidirectional line
					(at -25.4 -35.56 0)
					(length 2.54)
					(name "P0.30")
					(number "B4")
				)
				(pin power_in line
					(at -5.08 58.42 270)
					(length 2.54)
					(name "VBUS")
					(number "G7")
				)
				(pin passive line
					(at 0 58.42 270)
					(length 2.54)
					(name "VDD")
					(number "E7")
				)
				(pin power_in line
					(at 0 -58.42 90)
					(length 2.54)
					(name "VSS")
					(number "D3")
				)
				(pin power_out line
					(at 2.54 58.42 270)
					(length 2.54)
					(name "DCC")
					(number "A6")
				)
				(pin power_in line
					(at 7.62 58.42 270)
					(length 2.54)
					(name "VDDH")
					(number "F7")
				)
				(pin passive line
					(at 25.4 35.56 180)
					(length 2.54)
					(name "DECUSB")
					(number "G6")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "ANT")
					(number "E1")
				)
				(pin input line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "SWDCLK")
					(number "G2")
				)
				(pin bidirectional line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "SWDIO")
					(number "G1")
				)
			)
			(symbol "nRF52820-CFXX_1_0"
				(pin bidirectional line
					(at -25.4 17.78 0)
					(length 2.54)
					(name "P0.00")
					(number "C7")
					(alternate "XL1" input line)
				)
				(pin bidirectional line
					(at -25.4 12.7 0)
					(length 2.54)
					(name "P0.01")
					(number "D7")
					(alternate "XL2" input line)
				)
				(pin bidirectional line
					(at -25.4 0 0)
					(length 2.54)
					(name "P0.02")
					(number "B6")
					(alternate "AIN0" input line)
				)
				(pin bidirectional line
					(at -25.4 -2.54 0)
					(length 2.54)
					(name "P0.03")
					(number "B5")
					(alternate "AIN1" input line)
				)
				(pin bidirectional line
					(at -25.4 -5.08 0)
					(length 2.54)
					(name "P0.04")
					(number "C6")
					(alternate "AIN2" input line)
				)
				(pin bidirectional line
					(at -25.4 -7.62 0)
					(length 2.54)
					(name "P0.05")
					(number "D6")
					(alternate "AIN3" input line)
				)
				(pin passive line
					(at 0 58.42 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "A3")
				)
				(pin passive line
					(at 0 58.42 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "B7")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "A4")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "VSS_PA")
					(number "C1")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 25.4 45.72 180)
					(length 2.54)
					(name "DEC1")
					(number "A7")
				)
				(pin passive line
					(at 25.4 43.18 180)
					(length 2.54)
					(name "DEC4")
					(number "A5")
				)
				(pin passive line
					(at 25.4 40.64 180)
					(length 2.54)
					(name "DEC5")
					(number "F1")
				)
				(pin passive line
					(at 25.4 38.1 180)
					(length 2.54)
					(name "DEC6")
					(number "C2")
				)
				(pin input line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "~{RESET}")
					(number "G3")
					(alternate "P0.18" bidirectional line)
				)
			)
			(symbol "nRF52820-CFXX_1_1")
			(embedded_fonts no)
		)
)
