(footprint "BGA-51_7x8_2.956x3.226mm"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Nordic BGA-51_7x8_2.956x3.226mm, 2.956x3.226mm, 50 Ball, 7x8 Layout, 0.4mm Pitch, generated with kicad-footprint-generator ipc_bga_generator.py, https://docs.nordicsemi.com/bundle/nRF52832_PS_v1.9/resource/nRF52832_PS_v1.9.pdf")
	(tags "BGA 50 0.4")
	(property "Reference" "REF**"
		(at 0 -2.613 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-51_7x8_2.956x3.226mm"
		(at 0 2.613 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1.2 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -0.8 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -0.4 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 0 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 0.4 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at 0.8 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 1.2 -1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -0.8 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -0.4 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 0 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 0.4 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at 0.8 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 1.2 -1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -0.8 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -0.4 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 0 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 0.4 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at 0.8 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at 1.2 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -1.2 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -0.8 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -0.4 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at 0.8 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at 1.2 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -1.2 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -0.8 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -0.4 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at 0.8 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at 1.2 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -1.2 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -0.8 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -0.4 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at 0 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 0.4 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 0.8 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 1.2 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -1.2 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -0.8 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -0.4 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at 0 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at 0.4 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at 0.8 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 1.2 1)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -1.2 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -0.8 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -0.4 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at 0 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at 0.4 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at 0.8 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 1.2 1.4)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "nordic_nrf52832_cixx.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
