(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF52832-CIXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF52832-CIXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf52:BGA-51_7x8_2.956x3.226mm"
				(at 0 -73.66 0)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/nRF52832_PS_v1.9/resource/nRF52832_PS_v1.9.pdf"
				(at 0 -78.74 0)
			)
			(property "Description" "2.4GHz Bluetooth 5.4 NFC SoC, 64MHz Cortex-M4 FPU, PDM, I2S, CSP-51"
				(at 0 -76.2 0)
			)
			(property "ki_keywords" "ble bluetooth-low-energy bluetooth-mesh arm microcontroller wireless 2mbps ant nfc-a audio mesh-networking floating-point nrf52-series csp"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?51*7x8*2.956x3.226mm*"
				(at 0 0 0)
			)
			(symbol "nRF52832-CIXX_0_0"
				(pin input line
					(at -30.48 45.72 0)
					(length 2.54)
					(name "XC1")
					(number "B2")
				)
				(pin input line
					(at -30.48 40.64 0)
					(length 2.54)
					(name "XC2")
					(number "A1")
				)
				(pin bidirectional line
					(at -30.48 -7.62 0)
					(length 2.54)
					(name "P0.06")
					(number "F7")
				)
				(pin bidirectional line
					(at -30.48 -10.16 0)
					(length 2.54)
					(name "P0.07")
					(number "F6")
				)
				(pin bidirectional line
					(at -30.48 -12.7 0)
					(length 2.54)
					(name "P0.08")
					(number "G7")
				)
				(pin bidirectional line
					(at -30.48 -15.24 0)
					(length 2.54)
					(name "P0.11")
					(number "F4")
				)
				(pin bidirectional line
					(at -30.48 -17.78 0)
					(length 2.54)
					(name "P0.12")
					(number "H6")
				)
				(pin bidirectional line
					(at -30.48 -20.32 0)
					(length 2.54)
					(name "P0.13")
					(number "G4")
				)
				(pin bidirectional line
					(at -30.48 -22.86 0)
					(length 2.54)
					(name "P0.17")
					(number "G3")
				)
				(pin bidirectional line
					(at -30.48 -25.4 0)
					(length 2.54)
					(name "P0.19")
					(number "F3")
				)
				(pin bidirectional line
					(at -30.48 -27.94 0)
					(length 2.54)
					(name "P0.22")
					(number "F2")
				)
				(pin bidirectional line
					(at -30.48 -30.48 0)
					(length 2.54)
					(name "P0.23")
					(number "E2")
				)
				(pin bidirectional line
					(at -30.48 -33.02 0)
					(length 2.54)
					(name "P0.24")
					(number "E1")
				)
				(pin bidirectional line
					(at -30.48 -35.56 0)
					(length 2.54)
					(name "P0.25")
					(number "B3")
				)
				(pin bidirectional line
					(at -30.48 -38.1 0)
					(length 2.54)
					(name "P0.26")
					(number "D3")
				)
				(pin bidirectional line
					(at -30.48 -40.64 0)
					(length 2.54)
					(name "P0.27")
					(number "B4")
				)
				(pin power_in line
					(at 0 63.5 270)
					(length 2.54)
					(name "VDD")
					(number "A7")
				)
				(pin power_in line
					(at 0 -63.5 90)
					(length 2.54)
					(name "VSS")
					(number "C4")
				)
				(pin power_out line
					(at 2.54 63.5 270)
					(length 2.54)
					(name "DCC")
					(number "B6")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 2.54)
					(name "ANT")
					(number "D1")
				)
				(pin input line
					(at 30.48 -48.26 180)
					(length 2.54)
					(name "SWDCLK")
					(number "F1")
				)
				(pin bidirectional line
					(at 30.48 -50.8 180)
					(length 2.54)
					(name "SWDIO")
					(number "G1")
				)
			)
			(symbol "nRF52832-CIXX_1_0"
				(pin bidirectional line
					(at -30.48 33.02 0)
					(length 2.54)
					(name "P0.00")
					(number "D7")
					(alternate "XL1" input line)
				)
				(pin bidirectional line
					(at -30.48 27.94 0)
					(length 2.54)
					(name "P0.01")
					(number "C7")
					(alternate "XL2" input line)
				)
				(pin bidirectional line
					(at -30.48 17.78 0)
					(length 2.54)
					(name "P0.09")
					(number "G6")
					(alternate "NFC1" input line)
				)
				(pin bidirectional line
					(at -30.48 12.7 0)
					(length 2.54)
					(name "P0.10")
					(number "G5")
					(alternate "NFC2" input line)
				)
				(pin bidirectional line
					(at -30.48 2.54 0)
					(length 2.54)
					(name "P0.02")
					(number "C6")
					(alternate "AIN0" input line)
				)
				(pin bidirectional line
					(at -30.48 0 0)
					(length 2.54)
					(name "P0.03")
					(number "D6")
					(alternate "AIN1" input line)
				)
				(pin bidirectional line
					(at -30.48 -2.54 0)
					(length 2.54)
					(name "P0.04")
					(number "E6")
					(alternate "AIN2" input line)
				)
				(pin bidirectional line
					(at -30.48 -5.08 0)
					(length 2.54)
					(name "P0.05")
					(number "E7")
					(alternate "AIN3" input line)
				)
				(pin bidirectional line
					(at -30.48 -43.18 0)
					(length 2.54)
					(name "P0.28")
					(number "A3")
					(alternate "AIN4" input line)
				)
				(pin bidirectional line
					(at -30.48 -45.72 0)
					(length 2.54)
					(name "P0.29")
					(number "A4")
					(alternate "AIN5" input line)
				)
				(pin bidirectional line
					(at -30.48 -48.26 0)
					(length 2.54)
					(name "P0.30")
					(number "A5")
					(alternate "AIN6" input line)
				)
				(pin bidirectional line
					(at -30.48 -50.8 0)
					(length 2.54)
					(name "P0.31")
					(number "B5")
					(alternate "AIN7" input line)
				)
				(pin no_connect line
					(at -27.94 -53.34 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C3")
				)
				(pin passive line
					(at 0 63.5 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "H7")
				)
				(pin passive line
					(at 0 -63.5 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "C5")
				)
				(pin passive line
					(at 0 -63.5 90)
					(length 2.54)
					(hide yes)
					(name "VSS_PA")
					(number "D2")
				)
				(pin passive line
					(at 0 -63.5 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E3")
				)
				(pin passive line
					(at 0 -63.5 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 30.48 45.72 180)
					(length 2.54)
					(name "DEC1")
					(number "B7")
				)
				(pin passive line
					(at 30.48 43.18 180)
					(length 2.54)
					(name "DEC2")
					(number "A2")
				)
				(pin passive line
					(at 30.48 40.64 180)
					(length 2.54)
					(name "DEC3")
					(number "C2")
				)
				(pin passive line
					(at 30.48 38.1 180)
					(length 2.54)
					(name "DEC4")
					(number "A6")
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "P0.18")
					(number "H2")
					(alternate "TRACEDATA[0]" output line)
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "P0.16")
					(number "H3")
					(alternate "TRACEDATA[1]" output line)
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "P0.15")
					(number "H4")
					(alternate "TRACEDATA[2]" output line)
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "P0.14")
					(number "H5")
					(alternate "TRACEDATA[3]" output line)
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "P0.20")
					(number "G2")
					(alternate "TRACECLK" input line)
				)
				(pin input line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "~{RESET}")
					(number "H1")
					(alternate "P0.21" bidirectional line)
				)
			)
			(symbol "nRF52832-CIXX_1_1")
			(embedded_fonts no)
		)
)
