(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF52833-CJXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF52833-CJXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf52:BGA-76_9x9_3.175x3.175mm"
				(at 0 -93.98 0)
			)
			(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf52833/attach/nRF52833_PS_v1.7.pdf?_LANG=enus"
				(at 0 -99.06 0)
			)
			(property "Description" "2.4GHz Bluetooth 5.4 USB NFC SoC, 512KB Flash, 128KB RAM, 105°C Cortex-M4 FPU, ADC, SPI, UART, TWI, PWM, I2S, PDM, CSP-76"
				(at 0 -96.52 0)
			)
			(property "ki_keywords" "ble bluetooth-low-energy bluetooth-mesh thread zigbee arm microcontroller wireless 2mbps direction-finding mesh-networking floating-point nfc-a usb2 industrial high-temp nrf52-series csp"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?76*9x9*3.175x3.175mm*"
				(at 0 0 0)
			)
			(symbol "nRF52833-CJXX_0_0"
				(pin bidirectional line
					(at -35.56 71.12 0)
					(length 2.54)
					(name "D+")
					(number "J7")
				)
				(pin bidirectional line
					(at -35.56 68.58 0)
					(length 2.54)
					(name "D-")
					(number "H7")
				)
				(pin input line
					(at -35.56 58.42 0)
					(length 2.54)
					(name "XC1")
					(number "A1")
				)
				(pin input line
					(at -35.56 53.34 0)
					(length 2.54)
					(name "XC2")
					(number "A2")
				)
				(pin bidirectional line
					(at -35.56 -2.54 0)
					(length 2.54)
					(name "P0.06")
					(number "E9")
				)
				(pin bidirectional line
					(at -35.56 -5.08 0)
					(length 2.54)
					(name "P0.08")
					(number "E7")
				)
				(pin bidirectional line
					(at -35.56 -7.62 0)
					(length 2.54)
					(name "P0.13")
					(number "F7")
				)
				(pin bidirectional line
					(at -35.56 -10.16 0)
					(length 2.54)
					(name "P0.14")
					(number "J6")
				)
				(pin bidirectional line
					(at -35.56 -12.7 0)
					(length 2.54)
					(name "P0.15")
					(number "H5")
				)
				(pin bidirectional line
					(at -35.56 -15.24 0)
					(length 2.54)
					(name "P0.16")
					(number "G6")
				)
				(pin bidirectional line
					(at -35.56 -17.78 0)
					(length 2.54)
					(name "P0.17")
					(number "J5")
				)
				(pin bidirectional line
					(at -35.56 -20.32 0)
					(length 2.54)
					(name "P0.19")
					(number "C5")
				)
				(pin bidirectional line
					(at -35.56 -22.86 0)
					(length 2.54)
					(name "P0.20")
					(number "G5")
				)
				(pin bidirectional line
					(at -35.56 -25.4 0)
					(length 2.54)
					(name "P0.21")
					(number "G4")
				)
				(pin bidirectional line
					(at -35.56 -27.94 0)
					(length 2.54)
					(name "P0.22")
					(number "J3")
				)
				(pin bidirectional line
					(at -35.56 -30.48 0)
					(length 2.54)
					(name "P0.23")
					(number "D7")
				)
				(pin bidirectional line
					(at -35.56 -33.02 0)
					(length 2.54)
					(name "P0.24")
					(number "G3")
				)
				(pin bidirectional line
					(at -35.56 -35.56 0)
					(length 2.54)
					(name "P0.25")
					(number "A3")
				)
				(pin bidirectional line
					(at -35.56 -38.1 0)
					(length 2.54)
					(name "P0.26")
					(number "C9")
				)
				(pin bidirectional line
					(at -35.56 -40.64 0)
					(length 2.54)
					(name "P0.27")
					(number "C8")
				)
				(pin bidirectional line
					(at -35.56 -53.34 0)
					(length 2.54)
					(name "P1.01")
					(number "F3")
				)
				(pin bidirectional line
					(at -35.56 -55.88 0)
					(length 2.54)
					(name "P1.02")
					(number "H1")
				)
				(pin bidirectional line
					(at -35.56 -58.42 0)
					(length 2.54)
					(name "P1.03")
					(number "B4")
				)
				(pin bidirectional line
					(at -35.56 -60.96 0)
					(length 2.54)
					(name "P1.04")
					(number "G2")
				)
				(pin bidirectional line
					(at -35.56 -63.5 0)
					(length 2.54)
					(name "P1.05")
					(number "C4")
				)
				(pin bidirectional line
					(at -35.56 -66.04 0)
					(length 2.54)
					(name "P1.06")
					(number "E3")
				)
				(pin bidirectional line
					(at -35.56 -68.58 0)
					(length 2.54)
					(name "P1.07")
					(number "G1")
				)
				(pin bidirectional line
					(at -35.56 -71.12 0)
					(length 2.54)
					(name "P1.08")
					(number "F9")
				)
				(pin passive line
					(at 0 83.82 270)
					(length 2.54)
					(name "VDD")
					(number "J4")
				)
				(pin power_in line
					(at 0 -83.82 90)
					(length 2.54)
					(name "VSS")
					(number "D6")
				)
				(pin power_out line
					(at 2.54 83.82 270)
					(length 2.54)
					(name "DCC")
					(number "A8")
				)
				(pin power_in line
					(at 7.62 83.82 270)
					(length 2.54)
					(name "VDDH")
					(number "H9")
				)
				(pin passive line
					(at 35.56 60.96 180)
					(length 2.54)
					(name "DECUSB")
					(number "J8")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 2.54)
					(name "ANT")
					(number "E1")
				)
				(pin input line
					(at 35.56 -68.58 180)
					(length 2.54)
					(name "SWDCLK")
					(number "H2")
				)
				(pin bidirectional line
					(at 35.56 -71.12 180)
					(length 2.54)
					(name "SWDIO")
					(number "J2")
				)
			)
			(symbol "nRF52833-CJXX_1_0"
				(pin bidirectional line
					(at -35.56 43.18 0)
					(length 2.54)
					(name "P0.00")
					(number "B8")
					(alternate "XL1" input line)
				)
				(pin bidirectional line
					(at -35.56 38.1 0)
					(length 2.54)
					(name "P0.01")
					(number "B7")
					(alternate "XL2" input line)
				)
				(pin bidirectional line
					(at -35.56 22.86 0)
					(length 2.54)
					(name "P0.09")
					(number "F2")
					(alternate "NFC1" input line)
				)
				(pin bidirectional line
					(at -35.56 17.78 0)
					(length 2.54)
					(name "P0.10")
					(number "E2")
					(alternate "NFC2" input line)
				)
				(pin bidirectional line
					(at -35.56 7.62 0)
					(length 2.54)
					(name "P0.02")
					(number "C6")
					(alternate "AIN0" input line)
				)
				(pin bidirectional line
					(at -35.56 5.08 0)
					(length 2.54)
					(name "P0.03")
					(number "A4")
					(alternate "AIN1" input line)
				)
				(pin bidirectional line
					(at -35.56 2.54 0)
					(length 2.54)
					(name "P0.04")
					(number "D8")
					(alternate "AIN2" input line)
				)
				(pin bidirectional line
					(at -35.56 0 0)
					(length 2.54)
					(name "P0.05")
					(number "D9")
					(alternate "AIN3" input line)
				)
				(pin bidirectional line
					(at -35.56 -43.18 0)
					(length 2.54)
					(name "P0.28")
					(number "C7")
					(alternate "AIN4" input line)
				)
				(pin bidirectional line
					(at -35.56 -45.72 0)
					(length 2.54)
					(name "P0.29")
					(number "A5")
					(alternate "AIN5" input line)
				)
				(pin bidirectional line
					(at -35.56 -48.26 0)
					(length 2.54)
					(name "P0.30")
					(number "B5")
					(alternate "AIN6" input line)
				)
				(pin bidirectional line
					(at -35.56 -50.8 0)
					(length 2.54)
					(name "P0.31")
					(number "B6")
					(alternate "AIN7" input line)
				)
				(pin power_in line
					(at -5.08 83.82 270)
					(length 2.54)
					(name "VBUS")
					(number "H8")
				)
				(pin passive line
					(at 0 83.82 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "A9")
				)
				(pin passive line
					(at 0 83.82 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "B3")
				)
				(pin passive line
					(at 0 83.82 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "G9")
				)
				(pin passive line
					(at 0 83.82 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "J1")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "A7")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS_PA")
					(number "C1")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D3")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "F4")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "F6")
				)
				(pin passive line
					(at 0 -83.82 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "J9")
				)
				(pin passive line
					(at 35.56 71.12 180)
					(length 2.54)
					(name "DEC1")
					(number "B9")
				)
				(pin passive line
					(at 35.56 68.58 180)
					(length 2.54)
					(name "DEC4")
					(number "A6")
				)
				(pin passive line
					(at 35.56 66.04 180)
					(length 2.54)
					(name "DEC5")
					(number "F1")
					(alternate "NC" no_connect line)
				)
				(pin passive line
					(at 35.56 63.5 180)
					(length 2.54)
					(name "DEC6")
					(number "C2")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 2.54)
					(name "P1.00")
					(number "H3")
					(alternate "TRACEDATA[0]" output line)
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 2.54)
					(name "P0.12")
					(number "H6")
					(alternate "TRACEDATA[1]" output line)
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 2.54)
					(name "P0.11")
					(number "G8")
					(alternate "TRACEDATA[2]" output line)
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 2.54)
					(name "P1.09")
					(number "F8")
					(alternate "TRACEDATA[3]" output line)
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 2.54)
					(name "P0.07")
					(number "E8")
					(alternate "TRACECLK" input line)
				)
				(pin input line
					(at 35.56 -63.5 180)
					(length 2.54)
					(name "~{RESET}")
					(number "H4")
					(alternate "P0.18" bidirectional line)
				)
			)
			(symbol "nRF52833-CJXX_1_1")
			(embedded_fonts no)
		)
)
