(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF52840-CKXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF52840-CKXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf52:BGA-94_10x10_3.544x3.607mm"
				(at 0 -99.06 0)
			)
			(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf52840/attach/nRF52840_PS_v1.11.pdf?_LANG=enus"
				(at 0 -101.6 0)
			)
			(property "Description" "2.4GHz Bluetooth 5.4 USB NFC SoC, 64MHz Cortex-M4 FPU, CryptoCell, PDM, I2S, QSPI, CSP-94"
				(at 0 -104.14 0)
			)
			(property "ki_keywords" "ble bluetooth-low-energy bluetooth-mesh thread zigbee arm microcontroller wireless 2mbps mesh-networking 802.15.4 ant trustzone floating-point nfc-a usb2 csp nrf52-series"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?94*10x10*3.544x3.607mm*"
				(at 0 0 0)
			)
			(symbol "nRF52840-CKXX_0_0"
				(pin bidirectional line
					(at -34.29 76.2 0)
					(length 3.81)
					(name "D+")
					(number "K8")
				)
				(pin bidirectional line
					(at -34.29 73.66 0)
					(length 3.81)
					(name "D-")
					(number "J8")
				)
				(pin input line
					(at -34.29 63.5 0)
					(length 3.81)
					(name "XC1")
					(number "A1")
				)
				(pin input line
					(at -34.29 58.42 0)
					(length 3.81)
					(name "XC2")
					(number "A2")
				)
				(pin bidirectional line
					(at -34.29 7.62 0)
					(length 3.81)
					(name "P0.06")
					(number "E9")
				)
				(pin bidirectional line
					(at -34.29 5.08 0)
					(length 3.81)
					(name "P0.08")
					(number "E10")
				)
				(pin bidirectional line
					(at -34.29 2.54 0)
					(length 3.81)
					(name "P0.13")
					(number "H7")
				)
				(pin bidirectional line
					(at -34.29 0 0)
					(length 3.81)
					(name "P0.14")
					(number "J7")
				)
				(pin bidirectional line
					(at -34.29 -2.54 0)
					(length 3.81)
					(name "P0.15")
					(number "K7")
				)
				(pin bidirectional line
					(at -34.29 -5.08 0)
					(length 3.81)
					(name "P0.16")
					(number "H6")
				)
				(pin bidirectional line
					(at -34.29 -7.62 0)
					(length 3.81)
					(name "P0.17")
					(number "J6")
				)
				(pin bidirectional line
					(at -34.29 -10.16 0)
					(length 3.81)
					(name "P0.19")
					(number "K4")
				)
				(pin bidirectional line
					(at -34.29 -12.7 0)
					(length 3.81)
					(name "P0.20")
					(number "J5")
				)
				(pin bidirectional line
					(at -34.29 -15.24 0)
					(length 3.81)
					(name "P0.21")
					(number "J4")
				)
				(pin bidirectional line
					(at -34.29 -17.78 0)
					(length 3.81)
					(name "P0.22")
					(number "K3")
				)
				(pin bidirectional line
					(at -34.29 -20.32 0)
					(length 3.81)
					(name "P0.23")
					(number "H5")
				)
				(pin bidirectional line
					(at -34.29 -22.86 0)
					(length 3.81)
					(name "P0.24")
					(number "H4")
				)
				(pin bidirectional line
					(at -34.29 -25.4 0)
					(length 3.81)
					(name "P0.25")
					(number "K2")
				)
				(pin bidirectional line
					(at -34.29 -27.94 0)
					(length 3.81)
					(name "P0.26")
					(number "C9")
				)
				(pin bidirectional line
					(at -34.29 -30.48 0)
					(length 3.81)
					(name "P0.27")
					(number "D9")
				)
				(pin bidirectional line
					(at -34.29 -43.18 0)
					(length 3.81)
					(name "P1.01")
					(number "J1")
				)
				(pin bidirectional line
					(at -34.29 -45.72 0)
					(length 3.81)
					(name "P1.02")
					(number "G3")
				)
				(pin bidirectional line
					(at -34.29 -48.26 0)
					(length 3.81)
					(name "P1.03")
					(number "F3")
				)
				(pin bidirectional line
					(at -34.29 -50.8 0)
					(length 3.81)
					(name "P1.04")
					(number "H1")
				)
				(pin bidirectional line
					(at -34.29 -53.34 0)
					(length 3.81)
					(name "P1.05")
					(number "G2")
				)
				(pin bidirectional line
					(at -34.29 -55.88 0)
					(length 3.81)
					(name "P1.06")
					(number "E3")
				)
				(pin bidirectional line
					(at -34.29 -58.42 0)
					(length 3.81)
					(name "P1.07")
					(number "G1")
				)
				(pin bidirectional line
					(at -34.29 -60.96 0)
					(length 3.81)
					(name "P1.08")
					(number "G9")
				)
				(pin bidirectional line
					(at -34.29 -63.5 0)
					(length 3.81)
					(name "P1.10")
					(number "B4")
				)
				(pin bidirectional line
					(at -34.29 -66.04 0)
					(length 3.81)
					(name "P1.11")
					(number "A3")
				)
				(pin bidirectional line
					(at -34.29 -68.58 0)
					(length 3.81)
					(name "P1.12")
					(number "C5")
				)
				(pin bidirectional line
					(at -34.29 -71.12 0)
					(length 3.81)
					(name "P1.13")
					(number "A4")
				)
				(pin bidirectional line
					(at -34.29 -73.66 0)
					(length 3.81)
					(name "P1.14")
					(number "B5")
				)
				(pin bidirectional line
					(at -34.29 -76.2 0)
					(length 3.81)
					(name "P1.15")
					(number "C6")
				)
				(pin power_in line
					(at -7.62 87.63 270)
					(length 3.81)
					(name "VBUS")
					(number "J9")
				)
				(pin passive line
					(at -2.54 87.63 270)
					(length 3.81)
					(name "VDD")
					(number "K1")
				)
				(pin power_out line
					(at 0 87.63 270)
					(length 3.81)
					(name "DCC")
					(number "A9")
				)
				(pin power_in line
					(at 0 -87.63 90)
					(length 3.81)
					(name "VSS")
					(number "K10")
				)
				(pin power_in line
					(at 5.08 87.63 270)
					(length 3.81)
					(name "VDDH")
					(number "J10")
				)
				(pin power_out line
					(at 7.62 87.63 270)
					(length 3.81)
					(name "DCCH")
					(number "H9")
				)
				(pin passive line
					(at 34.29 66.04 180)
					(length 3.81)
					(name "DECUSB")
					(number "K9")
				)
				(pin bidirectional line
					(at 34.29 0 180)
					(length 3.81)
					(name "ANT")
					(number "E1")
				)
				(pin input line
					(at 34.29 -73.66 180)
					(length 3.81)
					(name "SWDCLK")
					(number "H2")
				)
				(pin bidirectional line
					(at 34.29 -76.2 180)
					(length 3.81)
					(name "SWDIO")
					(number "J2")
				)
			)
			(symbol "nRF52840-CKXX_1_0"
				(pin bidirectional line
					(at -34.29 48.26 0)
					(length 3.81)
					(name "P0.00")
					(number "B9")
					(alternate "XL1" input line)
				)
				(pin bidirectional line
					(at -34.29 43.18 0)
					(length 3.81)
					(name "P0.01")
					(number "B10")
					(alternate "XL2" input line)
				)
				(pin bidirectional line
					(at -34.29 33.02 0)
					(length 3.81)
					(name "P0.09")
					(number "F1")
					(alternate "NFC1" input line)
				)
				(pin bidirectional line
					(at -34.29 27.94 0)
					(length 3.81)
					(name "P0.10")
					(number "E2")
					(alternate "NFC2" input line)
				)
				(pin bidirectional line
					(at -34.29 17.78 0)
					(length 3.81)
					(name "P0.02")
					(number "B6")
					(alternate "AIN0" input line)
				)
				(pin bidirectional line
					(at -34.29 15.24 0)
					(length 3.81)
					(name "P0.03")
					(number "A5")
					(alternate "AIN1" input line)
				)
				(pin bidirectional line
					(at -34.29 12.7 0)
					(length 3.81)
					(name "P0.04")
					(number "C10")
					(alternate "AIN2" input line)
				)
				(pin bidirectional line
					(at -34.29 10.16 0)
					(length 3.81)
					(name "P0.05")
					(number "D10")
					(alternate "AIN3" input line)
				)
				(pin bidirectional line
					(at -34.29 -33.02 0)
					(length 3.81)
					(name "P0.28")
					(number "A6")
					(alternate "AIN4" input line)
				)
				(pin bidirectional line
					(at -34.29 -35.56 0)
					(length 3.81)
					(name "P0.29")
					(number "C7")
					(alternate "AIN5" input line)
				)
				(pin bidirectional line
					(at -34.29 -38.1 0)
					(length 3.81)
					(name "P0.30")
					(number "A7")
					(alternate "AIN6" input line)
				)
				(pin bidirectional line
					(at -34.29 -40.64 0)
					(length 3.81)
					(name "P0.31")
					(number "C8")
					(alternate "AIN7" input line)
				)
				(pin passive line
					(at -2.54 87.63 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "B3")
				)
				(pin passive line
					(at -2.54 87.63 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "B8")
				)
				(pin passive line
					(at -2.54 87.63 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "H10")
				)
				(pin passive line
					(at -2.54 87.63 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "K5")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B7")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS_PA")
					(number "C1")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C4")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D3")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D6")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D7")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D8")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E7")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E8")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F4")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F6")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F7")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G4")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G6")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G7")
				)
				(pin passive line
					(at 0 -87.63 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 34.29 76.2 180)
					(length 3.81)
					(name "DEC1")
					(number "A10")
				)
				(pin passive line
					(at 34.29 73.66 180)
					(length 3.81)
					(name "DEC4")
					(number "A8")
				)
				(pin passive line
					(at 34.29 71.12 180)
					(length 3.81)
					(name "DEC5/NC")
					(number "F2")
				)
				(pin passive line
					(at 34.29 68.58 180)
					(length 3.81)
					(name "DEC6")
					(number "C2")
				)
				(pin bidirectional line
					(at 34.29 -48.26 180)
					(length 3.81)
					(name "P1.00")
					(number "J3")
					(alternate "TRACEDATA[0]" output line)
				)
				(pin bidirectional line
					(at 34.29 -50.8 180)
					(length 3.81)
					(name "P0.12")
					(number "G10")
					(alternate "TRACEDATA[1]" output line)
				)
				(pin bidirectional line
					(at 34.29 -53.34 180)
					(length 3.81)
					(name "P0.11")
					(number "H8")
					(alternate "TRACEDATA[2]" output line)
				)
				(pin bidirectional line
					(at 34.29 -55.88 180)
					(length 3.81)
					(name "P1.09")
					(number "F10")
					(alternate "TRACEDATA[3]" output line)
				)
				(pin bidirectional line
					(at 34.29 -58.42 180)
					(length 3.81)
					(name "P0.07")
					(number "F9")
					(alternate "TRACECLK" input line)
				)
				(pin input line
					(at 34.29 -68.58 180)
					(length 3.81)
					(name "~{RESET}")
					(number "K6")
					(alternate "P0.18" bidirectional line)
				)
			)
			(symbol "nRF52840-CKXX_1_1")
			(embedded_fonts no)
		)
)
