(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF5340-CLXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF5340-CLXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf53:BGA-132_12x11_4.39x3.994mm"
				(at 2.54 -20.32 0)
			)
			(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf5340/attach/nRF5340_PS_v1.5.pdf"
				(at 2.54 -20.32 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?132*12x11*4.39x3.994mm*"
				(at 0 0 0)
			)
			(symbol "nRF5340-CLXX_1_0"
				(pin bidirectional line
					(at -30.48 58.42 0)
					(length 5.08)
					(name "XC1")
					(number "A1")
				)
				(pin bidirectional line
					(at -30.48 53.34 0)
					(length 5.08)
					(name "XC2")
					(number "A2")
				)
				(pin bidirectional line
					(at -30.48 43.18 0)
					(length 5.08)
					(name "P0.00/XL1")
					(number "F11")
				)
				(pin bidirectional line
					(at -30.48 38.1 0)
					(length 5.08)
					(name "P0.01/XL2")
					(number "F12")
				)
				(pin bidirectional line
					(at -30.48 25.4 0)
					(length 5.08)
					(name "D+")
					(number "A12")
				)
				(pin bidirectional line
					(at -30.48 22.86 0)
					(length 5.08)
					(name "D-")
					(number "A11")
				)
				(pin bidirectional line
					(at -30.48 15.24 0)
					(length 5.08)
					(name "P0.02/NFC1")
					(number "G11")
				)
				(pin bidirectional line
					(at -30.48 12.7 0)
					(length 5.08)
					(name "P0.03/NFC2")
					(number "H12")
				)
				(pin bidirectional line
					(at -30.48 5.08 0)
					(length 5.08)
					(name "P0.04/AIN0")
					(number "G10")
				)
				(pin bidirectional line
					(at -30.48 2.54 0)
					(length 5.08)
					(name "P0.05/AIN1")
					(number "F10")
				)
				(pin bidirectional line
					(at -30.48 0 0)
					(length 5.08)
					(name "P0.06/AIN2")
					(number "H10")
				)
				(pin bidirectional line
					(at -30.48 -2.54 0)
					(length 5.08)
					(name "P0.07/AIN3")
					(number "J10")
				)
				(pin bidirectional line
					(at -30.48 -5.08 0)
					(length 5.08)
					(name "P0.25/AIN4")
					(number "L1")
				)
				(pin bidirectional line
					(at -30.48 -7.62 0)
					(length 5.08)
					(name "P0.26/AIN5")
					(number "J2")
				)
				(pin bidirectional line
					(at -30.48 -10.16 0)
					(length 5.08)
					(name "P0.27/AIN6")
					(number "H1")
				)
				(pin bidirectional line
					(at -30.48 -12.7 0)
					(length 5.08)
					(name "P0.28/AIN7")
					(number "E3")
				)
				(pin bidirectional line
					(at -30.48 -20.32 0)
					(length 5.08)
					(name "P1.02/TWI")
					(number "J11")
				)
				(pin bidirectional line
					(at -30.48 -22.86 0)
					(length 5.08)
					(name "P1.03/TWI")
					(number "K12")
				)
				(pin bidirectional line
					(at -30.48 -30.48 0)
					(length 5.08)
					(name "P0.13/IO0")
					(number "K10")
				)
				(pin bidirectional line
					(at -30.48 -33.02 0)
					(length 5.08)
					(name "P0.14/IO1")
					(number "K9")
				)
				(pin bidirectional line
					(at -30.48 -35.56 0)
					(length 5.08)
					(name "P0.15/IO2")
					(number "L9")
				)
				(pin bidirectional line
					(at -30.48 -38.1 0)
					(length 5.08)
					(name "P0.16/IO3")
					(number "K8")
				)
				(pin bidirectional line
					(at -30.48 -40.64 0)
					(length 5.08)
					(name "P0.17/SCK")
					(number "L7")
				)
				(pin bidirectional line
					(at -30.48 -43.18 0)
					(length 5.08)
					(name "P0.18/~{CS}")
					(number "K7")
				)
				(pin bidirectional line
					(at -30.48 -50.8 0)
					(length 5.08)
					(name "P0.09/TRACEDATA2/MOSI")
					(number "J9")
				)
				(pin bidirectional line
					(at -30.48 -53.34 0)
					(length 5.08)
					(name "P0.10/TRACEDATA1/MISO")
					(number "J8")
				)
				(pin bidirectional line
					(at -30.48 -55.88 0)
					(length 5.08)
					(name "P0.08/TRACEDATA3/SCK")
					(number "L12")
				)
				(pin bidirectional line
					(at -30.48 -58.42 0)
					(length 5.08)
					(name "P0.11/TRACEDATA0/~{CS}")
					(number "J7")
				)
				(pin bidirectional line
					(at -30.48 -60.96 0)
					(length 5.08)
					(name "P0.12/TRACECLK/DCX")
					(number "J6")
				)
				(pin bidirectional line
					(at 30.48 58.42 180)
					(length 5.08)
					(name "P0.19")
					(number "J5")
				)
				(pin bidirectional line
					(at 30.48 55.88 180)
					(length 5.08)
					(name "P0.20")
					(number "K5")
				)
				(pin bidirectional line
					(at 30.48 53.34 180)
					(length 5.08)
					(name "P0.21")
					(number "J4")
				)
				(pin bidirectional line
					(at 30.48 50.8 180)
					(length 5.08)
					(name "P0.22")
					(number "K4")
				)
				(pin bidirectional line
					(at 30.48 48.26 180)
					(length 5.08)
					(name "P0.23")
					(number "H3")
				)
				(pin bidirectional line
					(at 30.48 45.72 180)
					(length 5.08)
					(name "P0.24")
					(number "K2")
				)
				(pin bidirectional line
					(at 30.48 43.18 180)
					(length 5.08)
					(name "P0.29")
					(number "E2")
				)
				(pin bidirectional line
					(at 30.48 40.64 180)
					(length 5.08)
					(name "P0.30")
					(number "C4")
				)
				(pin bidirectional line
					(at 30.48 38.1 180)
					(length 5.08)
					(name "P0.31")
					(number "C5")
				)
				(pin bidirectional line
					(at 30.48 35.56 180)
					(length 5.08)
					(name "P1.00")
					(number "D10")
				)
				(pin bidirectional line
					(at 30.48 33.02 180)
					(length 5.08)
					(name "P1.01")
					(number "E10")
				)
				(pin bidirectional line
					(at 30.48 30.48 180)
					(length 5.08)
					(name "P1.04")
					(number "K3")
				)
				(pin bidirectional line
					(at 30.48 27.94 180)
					(length 5.08)
					(name "P1.05")
					(number "L3")
				)
				(pin bidirectional line
					(at 30.48 25.4 180)
					(length 5.08)
					(name "P1.06")
					(number "J3")
				)
				(pin bidirectional line
					(at 30.48 22.86 180)
					(length 5.08)
					(name "P1.07")
					(number "G3")
				)
				(pin bidirectional line
					(at 30.48 20.32 180)
					(length 5.08)
					(name "P1.08")
					(number "F3")
				)
				(pin bidirectional line
					(at 30.48 17.78 180)
					(length 5.08)
					(name "P1.09")
					(number "H2")
				)
				(pin bidirectional line
					(at 30.48 15.24 180)
					(length 5.08)
					(name "P1.10")
					(number "E4")
				)
				(pin bidirectional line
					(at 30.48 12.7 180)
					(length 5.08)
					(name "P1.11")
					(number "C6")
				)
				(pin bidirectional line
					(at 30.48 10.16 180)
					(length 5.08)
					(name "P1.12")
					(number "C7")
				)
				(pin bidirectional line
					(at 30.48 7.62 180)
					(length 5.08)
					(name "P1.13")
					(number "C8")
				)
				(pin bidirectional line
					(at 30.48 5.08 180)
					(length 5.08)
					(name "P1.14")
					(number "C9")
				)
				(pin bidirectional line
					(at 30.48 2.54 180)
					(length 5.08)
					(name "P1.15")
					(number "C10")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 5.08)
					(name "ANT")
					(number "D1")
				)
				(pin input line
					(at 30.48 -17.78 180)
					(length 5.08)
					(name "~{RESET}")
					(number "G2")
				)
				(pin input line
					(at 30.48 -22.86 180)
					(length 5.08)
					(name "SWDCLK")
					(number "F2")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 5.08)
					(name "SWDIO")
					(number "F1")
				)
			)
			(symbol "nRF5340-CLXX_1_1"
				(text "nRF5340-CLXX\nI/O"
					(at 0 -5.08 0)
				)
			)
			(symbol "nRF5340-CLXX_2_0"
				(pin passive line
					(at -22.86 7.62 0)
					(length 5.08)
					(name "DCC")
					(number "B6")
				)
				(pin passive line
					(at -22.86 2.54 0)
					(length 5.08)
					(name "DECR")
					(number "B4")
				)
				(pin passive line
					(at -22.86 0 0)
					(length 5.08)
					(name "DECRF")
					(number "B1")
				)
				(pin passive line
					(at -22.86 -5.08 0)
					(length 5.08)
					(name "DCCD")
					(number "A9")
				)
				(pin passive line
					(at -22.86 -10.16 0)
					(length 5.08)
					(name "DECD")
					(number "A7")
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "B10")
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "B7")
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "D2")
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "E11")
				)
				(pin power_in line
					(at -2.54 20.32 270)
					(length 5.08)
					(name "VDD")
					(number "H11")
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "K1")
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "L11")
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "L5")
				)
				(pin power_in line
					(at 0 20.32 270)
					(length 5.08)
					(name "VDDH")
					(number "B12")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A5")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B2")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B9")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C2")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D12")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E7")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E8")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F6")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F7")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "G5")
				)
				(pin power_in line
					(at 0 -20.32 90)
					(length 5.08)
					(name "VSS")
					(number "G6")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G7")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "K11")
				)
				(pin passive line
					(at 0 -20.32 90)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "K6")
				)
				(pin power_in line
					(at 2.54 20.32 270)
					(length 5.08)
					(name "VBUS")
					(number "B11")
				)
				(pin passive line
					(at 22.86 7.62 180)
					(length 5.08)
					(name "DECA")
					(number "B8")
				)
				(pin passive line
					(at 22.86 5.08 180)
					(length 5.08)
					(name "DECN")
					(number "B5")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 5.08)
					(name "DCCH")
					(number "D11")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 5.08)
					(name "DECUSB")
					(number "C11")
				)
			)
			(symbol "nRF5340-CLXX_2_1"
				(text "nRF5340-CLXX\nPWR"
					(at 0 -5.08 0)
				)
				(pin passive line
					(at -2.54 20.32 270)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "A3")
				)
			)
			(embedded_fonts no)
		)
)
