(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF54L15-QGXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace yes)
			)
			(property "Value" "nRF54L15-QGXX"
				(at 0 -2.54 0)
				(show_name no)
				(do_not_autoplace yes)
			)
			(property "Footprint" "nordic-lib-kicad-nrf54l:QFN-52-1EP_6x6mm_P0.4mm_EP4.7x4.7mm_ThermalVias"
				(at 0 -68.58 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf54L15"
				(at 0 -71.12 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "nRF54L Dual Core Multiprotocol BLE SoC"
				(at 0 -66.04 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "BLE SoC nRF QFN48"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "QFN*52*1EP*6x6mm*P0.4mm*EP4.7x4.7mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "nRF54L15-QGXX_1_0"
				(pin bidirectional line
					(at -27.94 43.18 0)
					(length 2.54)
					(name "P1.00")
					(number "1")
					(alternate "XL1" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 38.1 0)
					(length 2.54)
					(name "P1.01")
					(number "2")
					(alternate "XL2" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 10.16 0)
					(length 2.54)
					(name "P1.02")
					(number "3")
					(alternate "NFC1" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 7.62 0)
					(length 2.54)
					(name "P1.03")
					(number "4")
					(alternate "NFC2" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 5.08 0)
					(length 2.54)
					(name "P1.04")
					(number "5")
					(alternate "AIN0" input line)
					(alternate "ASO[0]" output line)
				)
				(pin bidirectional line
					(at -27.94 -25.4 0)
					(length 2.54)
					(name "P1.16")
					(number "6")
				)
				(pin bidirectional line
					(at -27.94 2.54 0)
					(length 2.54)
					(name "P1.05")
					(number "7")
					(alternate "AIN1" bidirectional line)
					(alternate "ASI[0]" input line)
				)
				(pin bidirectional line
					(at -27.94 0 0)
					(length 2.54)
					(name "P1.06")
					(number "8")
					(alternate "AIN2" input line)
					(alternate "ASO[1]" output line)
				)
				(pin bidirectional line
					(at -27.94 -2.54 0)
					(length 2.54)
					(name "P1.07")
					(number "9")
					(alternate "AIN3" input line)
					(alternate "ASI[1]" input line)
				)
				(pin bidirectional line
					(at -27.94 -5.08 0)
					(length 2.54)
					(name "P1.08")
					(number "10")
					(alternate "EXTREF" input line)
					(alternate "GRTCHFOUT" output line)
					(alternate "TAMPC.EXT" bidirectional line)
				)
				(pin power_in line
					(at 0 63.5 270)
					(length 2.54)
					(name "VDD")
					(number "11")
				)
				(pin bidirectional line
					(at -27.94 -30.48 0)
					(length 2.54)
					(name "P2.00")
					(number "12")
					(alternate "QSPI_D3" bidirectional line)
					(alternate "SPIM_DCX" output line)
					(alternate "UARTE_RXD" input line)
				)
				(pin bidirectional line
					(at -27.94 -33.02 0)
					(length 2.54)
					(name "P2.01")
					(number "13")
					(alternate "QSPI_SCK" output line)
					(alternate "SPIM_SCK" output line)
					(alternate "SPIS_SCK" output line)
				)
				(pin bidirectional line
					(at -27.94 -35.56 0)
					(length 2.54)
					(name "P2.02")
					(number "14")
					(alternate "QSPI_D0" bidirectional line)
					(alternate "SPIM_MOSI" output line)
					(alternate "SPIS_MISO" output line)
					(alternate "SWO" output line)
					(alternate "UARTE_TXD" output line)
				)
				(pin bidirectional line
					(at -27.94 -38.1 0)
					(length 2.54)
					(name "P2.03")
					(number "15")
					(alternate "QSPI_D2" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 -40.64 0)
					(length 2.54)
					(name "P2.04")
					(number "16")
					(alternate "QSPI_D1" bidirectional line)
					(alternate "SPIM_MISO" input line)
					(alternate "SPIS_MOSI" input line)
					(alternate "UARTE_CTS" input line)
				)
				(pin bidirectional line
					(at -27.94 -43.18 0)
					(length 2.54)
					(name "P2.05")
					(number "17")
					(alternate "QSPI_CS" output line)
					(alternate "SPIM_CS" output line)
					(alternate "UARTE_RTS" output line)
				)
				(pin bidirectional line
					(at -27.94 -45.72 0)
					(length 2.54)
					(name "P2.06")
					(number "18")
					(alternate "SPIM_SCK" output line)
					(alternate "SPIS_SCK" input line)
					(alternate "TRACE_CLK" input line)
				)
				(pin bidirectional line
					(at -27.94 -48.26 0)
					(length 2.54)
					(name "P2.07")
					(number "19")
					(alternate "SPIM_DCX" output line)
					(alternate "SWO" output line)
					(alternate "TRACEDATA[0]" output line)
					(alternate "UARTE_RXD" input line)
				)
				(pin bidirectional line
					(at -27.94 -50.8 0)
					(length 2.54)
					(name "P2.08")
					(number "20")
					(alternate "SPIM_MOSI" output line)
					(alternate "SPIS_MISO" input line)
					(alternate "TRACEDATA[1]" output line)
					(alternate "UARTE_TXD" output line)
				)
				(pin bidirectional line
					(at -27.94 -53.34 0)
					(length 2.54)
					(name "P2.09")
					(number "21")
					(alternate "SPIM_MISO" input line)
					(alternate "SPIS_MOSI" input line)
					(alternate "TRACEDATA[2]" output line)
					(alternate "UARTE_CTS" input line)
				)
				(pin bidirectional line
					(at -27.94 -55.88 0)
					(length 2.54)
					(name "P2.10")
					(number "22")
					(alternate "SPIM_CS" output line)
					(alternate "TRACEDATA[3]" output line)
					(alternate "UARTE_RTS" output line)
				)
				(pin passive line
					(at 0 63.5 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "23")
				)
				(pin bidirectional line
					(at -27.94 15.24 0)
					(length 2.54)
					(name "P0.06")
					(number "24")
					(alternate "GRTCLFCLKOUT" output line)
				)
				(pin bidirectional line
					(at -27.94 30.48 0)
					(length 2.54)
					(name "P0.00")
					(number "25")
				)
				(pin bidirectional line
					(at -27.94 27.94 0)
					(length 2.54)
					(name "P0.01")
					(number "26")
				)
				(pin bidirectional line
					(at 27.94 -55.88 180)
					(length 2.54)
					(name "SWDIO")
					(number "27")
				)
				(pin input line
					(at 27.94 -53.34 180)
					(length 2.54)
					(name "SWDCLK")
					(number "28")
				)
				(pin bidirectional line
					(at -27.94 25.4 0)
					(length 2.54)
					(name "P0.02")
					(number "29")
				)
				(pin bidirectional line
					(at -27.94 22.86 0)
					(length 2.54)
					(name "P0.03")
					(number "30")
					(alternate "GRTCPWM" output line)
				)
				(pin bidirectional line
					(at -27.94 20.32 0)
					(length 2.54)
					(name "P0.04")
					(number "31")
					(alternate "GRTCLFCLKOUT" output line)
				)
				(pin bidirectional line
					(at -27.94 17.78 0)
					(length 2.54)
					(name "P0.05")
					(number "32")
					(alternate "GRTCLFCLKOUT" output line)
				)
				(pin input line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "~{RESET}")
					(number "33")
				)
				(pin output line
					(at 27.94 0 180)
					(length 2.54)
					(name "ANT")
					(number "34")
				)
				(pin passive line
					(at 0 -63.5 90)
					(length 2.54)
					(hide yes)
					(name "VSS_PA")
					(number "35")
				)
				(pin passive line
					(at 27.94 53.34 180)
					(length 2.54)
					(name "DECRF")
					(number "36")
				)
				(pin bidirectional line
					(at -27.94 55.88 0)
					(length 2.54)
					(name "XC1")
					(number "37")
				)
				(pin bidirectional line
					(at -27.94 50.8 0)
					(length 2.54)
					(name "XC2")
					(number "38")
				)
				(pin passive line
					(at 0 63.5 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "39")
				)
				(pin bidirectional line
					(at -27.94 -7.62 0)
					(length 2.54)
					(name "P1.09")
					(number "40")
					(alternate "ASO[2]" output line)
				)
				(pin bidirectional line
					(at -27.94 -10.16 0)
					(length 2.54)
					(name "P1.10")
					(number "41")
					(alternate "ASI[2]" input line)
				)
				(pin bidirectional line
					(at -27.94 -12.7 0)
					(length 2.54)
					(name "P1.11")
					(number "42")
					(alternate "AIN4" input line)
					(alternate "ASO[3]" output line)
				)
				(pin bidirectional line
					(at -27.94 -15.24 0)
					(length 2.54)
					(name "P1.12")
					(number "43")
					(alternate "AIN5" input line)
					(alternate "ASI[3]" input line)
				)
				(pin bidirectional line
					(at -27.94 -17.78 0)
					(length 2.54)
					(name "P1.13")
					(number "44")
					(alternate "AIN6" input line)
				)
				(pin bidirectional line
					(at -27.94 -20.32 0)
					(length 2.54)
					(name "P1.14")
					(number "45")
					(alternate "AIN7" input line)
				)
				(pin bidirectional line
					(at -27.94 -22.86 0)
					(length 2.54)
					(name "P1.15")
					(number "46")
				)
				(pin passive line
					(at 27.94 55.88 180)
					(length 2.54)
					(name "DECA")
					(number "47")
				)
				(pin power_in line
					(at 0 -63.5 90)
					(length 2.54)
					(name "VSS")
					(number "48")
				)
				(pin passive line
					(at 27.94 50.8 180)
					(length 2.54)
					(name "DECD")
					(number "49")
				)
				(pin power_out line
					(at 27.94 45.72 180)
					(length 2.54)
					(name "DCC")
					(number "50")
				)
				(pin passive line
					(at 0 63.5 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "51")
				)
				(pin passive line
					(at 0 63.5 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "52")
				)
				(pin passive line
					(at 0 -63.5 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "53")
				)
			)
			(symbol "nRF54L15-QGXX_1_1"
				(text "CLK"
					(at -15.24 22.86 0)
				)
				(text "CLK"
					(at -15.24 20.32 0)
				)
				(text "CLK"
					(at -15.24 7.62 0)
				)
				(text "CLK"
					(at -15.24 5.08 0)
				)
				(text "CLK"
					(at -15.24 -5.08 0)
				)
				(text "CLK"
					(at -15.24 -12.7 0)
				)
				(text "CLK"
					(at -15.24 -15.24 0)
				)
				(text "CLK"
					(at -15.24 -33.02 0)
				)
				(text "CLK"
					(at -15.24 -45.72 0)
				)
			)
			(embedded_fonts no)
		)
)
