(footprint "Nordic_FCCSP-98_3.67x3.85mm_Layout10x10_P0.35mm_Offcenter"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Nordic FCCSP-98, 3.67x3.85mm, 98 Ball, 10x10 Layout, 0.35mm Pitch, generated with kicad-footprint-generator ipc_bga_generator.py, https://docs-be.nordicsemi.com/bundle/ps_nrf54LM20A/page/pdf/nRF54LM20A_Preliminary_Datasheet_v0.7.pdf")
	(tags "CSP 98 0.35")
	(property "Reference" "REF**"
		(at 0 -2.925 0)
		(layer "F.SilkS")
	)
	(property "Value" "Nordic_FCCSP-98_3.67x3.85mm_Layout10x10_P0.35mm_Offcenter"
		(at 0 2.925 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1.575 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -1.225 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -0.875 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -0.525 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -0.175 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at 0.175 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 0.525 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 0.875 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 1.225 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at 1.575 -1.665)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -1.575 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -1.225 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -0.875 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -0.525 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -0.175 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at 0.175 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 0.525 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 0.875 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 1.225 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 1.575 -1.315)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -1.575 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -1.225 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -0.875 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -0.525 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -0.175 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at 0.175 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at 0.525 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 0.875 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at 1.225 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at 1.575 -0.965)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -1.575 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -1.225 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -0.525 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -0.175 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at 0.175 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at 0.525 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 0.875 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 1.225 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at 1.575 -0.615)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -1.575 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -0.875 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -0.525 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -0.175 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at 0.175 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at 0.525 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 0.875 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 1.225 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at 1.575 -0.265)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -1.575 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -1.225 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -0.875 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -0.525 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -0.175 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 0.175 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 0.525 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 0.875 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 1.225 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at 1.575 0.085)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -1.575 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -1.225 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -0.875 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -0.525 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at -0.175 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at 0.175 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 0.525 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 0.875 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 1.225 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at 1.575 0.435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -1.575 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -1.225 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -0.875 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -0.525 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -0.175 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at 0.175 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 0.525 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 0.875 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 1.225 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at 1.575 0.785)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -1.575 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -1.225 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -0.875 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -0.525 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -0.175 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at 0.175 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at 0.525 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 0.875 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 1.225 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at 1.575 1.135)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -1.575 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -1.225 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -0.875 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -0.525 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -0.175 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K6" smd circle
		(at 0.175 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at 0.525 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 0.875 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 1.225 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at 1.575 1.485)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "nordic_nrf54lm20a_paxx.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
