(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF54LM20A-PAXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 0 1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "nRF54LM20A-PAXX"
				(at 0 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "nordic-lib-kicad-nrf54l:Nordic_FCCSP-98_3.67x3.85mm_Layout10x10_P0.35mm_Offcenter"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf54LM20A/page/pdf/nRF54LM20A_Preliminary_Datasheet_v0.7.pdf"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_fp_filters" "Nordic?FCCSP?98*3.67x3.85mm*P0.35mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "nRF54LM20A-PAXX_1_0"
				(pin power_in line
					(at 0 -34.29 90)
					(length 3.81)
					(name "VSS")
					(number "A1")
				)
				(pin input line
					(at -19.05 15.24 0)
					(length 3.81)
					(name "XC1")
					(number "A2")
				)
				(pin power_in line
					(at 0 34.29 270)
					(length 3.81)
					(name "VDD")
					(number "A3")
				)
				(pin passive line
					(at 0 34.29 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "A4")
				)
				(pin passive line
					(at 19.05 25.4 180)
					(length 3.81)
					(name "DCC")
					(number "A5")
				)
				(pin passive line
					(at 19.05 20.32 180)
					(length 3.81)
					(name "DECD")
					(number "A6")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "A7")
				)
				(pin passive line
					(at 19.05 15.24 180)
					(length 3.81)
					(name "DECA")
					(number "A8")
				)
				(pin passive line
					(at 0 34.29 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "A9")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "A10")
				)
				(pin output line
					(at -19.05 10.16 0)
					(length 3.81)
					(name "XC2")
					(number "B1")
				)
				(pin passive line
					(at 19.05 7.62 180)
					(length 3.81)
					(name "DECRF")
					(number "C1")
				)
				(pin bidirectional line
					(at -19.05 2.54 0)
					(length 3.81)
					(name "P1.20")
					(number "C6")
					(alternate "XL1" input line)
				)
				(pin bidirectional line
					(at -19.05 -2.54 0)
					(length 3.81)
					(name "P1.21")
					(number "C7")
					(alternate "XL2" output line)
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D1")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D2")
				)
				(pin passive line
					(at 19.05 -10.16 180)
					(length 3.81)
					(name "ANT")
					(number "E1")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F1")
				)
				(pin input line
					(at 19.05 -17.78 180)
					(length 3.81)
					(name "~{RESET}")
					(number "F2")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F6")
				)
				(pin input line
					(at 19.05 -22.86 180)
					(length 3.81)
					(name "SWDCLK")
					(number "G1")
				)
				(pin bidirectional line
					(at 19.05 -25.4 180)
					(length 3.81)
					(name "SWDIO")
					(number "G2")
				)
				(pin passive line
					(at 0 34.29 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "G10")
				)
				(pin passive line
					(at 0 34.29 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "H1")
				)
				(pin bidirectional line
					(at -19.05 -20.32 0)
					(length 3.81)
					(name "TXRTUNE")
					(number "J5")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K1")
				)
				(pin bidirectional line
					(at -19.05 -15.24 0)
					(length 3.81)
					(name "D-")
					(number "K4")
				)
				(pin bidirectional line
					(at -19.05 -12.7 0)
					(length 3.81)
					(name "D+")
					(number "K5")
				)
				(pin passive line
					(at -19.05 -25.4 0)
					(length 3.81)
					(name "DECUSB")
					(number "K6")
				)
				(pin power_in line
					(at -19.05 25.4 0)
					(length 3.81)
					(name "VBUS")
					(number "K7")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K10")
				)
			)
			(symbol "nRF54LM20A-PAXX_1_1")
			(symbol "nRF54LM20A-PAXX_2_0"
				(pin bidirectional line
					(at 19.05 -11.43 180)
					(length 3.81)
					(name "P0.09")
					(number "E3")
				)
				(pin bidirectional line
					(at 19.05 -8.89 180)
					(length 3.81)
					(name "P0.08")
					(number "F3")
				)
				(pin bidirectional line
					(at 19.05 -6.35 180)
					(length 3.81)
					(name "P0.07")
					(number "G3")
				)
				(pin bidirectional line
					(at 19.05 -3.81 180)
					(length 3.81)
					(name "P0.06")
					(number "H2")
				)
				(pin bidirectional line
					(at 19.05 -1.27 180)
					(length 3.81)
					(name "P0.05")
					(number "H3")
				)
				(pin bidirectional line
					(at 19.05 1.27 180)
					(length 3.81)
					(name "P0.04")
					(number "J1")
				)
				(pin bidirectional line
					(at 19.05 3.81 180)
					(length 3.81)
					(name "P0.03")
					(number "J2")
				)
				(pin bidirectional line
					(at 19.05 6.35 180)
					(length 3.81)
					(name "P0.02")
					(number "J3")
				)
				(pin bidirectional line
					(at 19.05 8.89 180)
					(length 3.81)
					(name "P0.01")
					(number "K2")
				)
				(pin bidirectional line
					(at 19.05 11.43 180)
					(length 3.81)
					(name "P0.00")
					(number "K3")
				)
			)
			(symbol "nRF54LM20A-PAXX_2_1")
			(symbol "nRF54LM20A-PAXX_3_0"
				(pin bidirectional line
					(at 19.05 -1.27 180)
					(length 3.81)
					(name "P1.15")
					(number "B2")
				)
				(pin bidirectional line
					(at 19.05 -3.81 180)
					(length 3.81)
					(name "P1.16")
					(number "B3")
				)
				(pin bidirectional line
					(at 19.05 -6.35 180)
					(length 3.81)
					(name "P1.17")
					(number "B4")
				)
				(pin bidirectional line
					(at 19.05 -8.89 180)
					(length 3.81)
					(name "P1.18")
					(number "B5")
				)
				(pin bidirectional line
					(at 19.05 -11.43 180)
					(length 3.81)
					(name "P1.19")
					(number "B6")
				)
				(pin bidirectional line
					(at 19.05 -16.51 180)
					(length 3.81)
					(name "P1.23")
					(number "B7")
				)
				(pin bidirectional line
					(at 19.05 -24.13 180)
					(length 3.81)
					(name "P1.26")
					(number "B8")
				)
				(pin bidirectional line
					(at 19.05 1.27 180)
					(length 3.81)
					(name "P1.14")
					(number "C2")
				)
				(pin bidirectional line
					(at 19.05 3.81 180)
					(length 3.81)
					(name "P1.13")
					(number "C3")
				)
				(pin bidirectional line
					(at 19.05 6.35 180)
					(length 3.81)
					(name "P1.12")
					(number "C4")
				)
				(pin bidirectional line
					(at 19.05 8.89 180)
					(length 3.81)
					(name "P1.11")
					(number "C5")
				)
				(pin bidirectional line
					(at 19.05 -26.67 180)
					(length 3.81)
					(name "P1.27")
					(number "C8")
				)
				(pin bidirectional line
					(at 19.05 11.43 180)
					(length 3.81)
					(name "P1.10")
					(number "D5")
				)
				(pin bidirectional line
					(at 19.05 -13.97 180)
					(length 3.81)
					(name "P1.22")
					(number "D6")
				)
				(pin bidirectional line
					(at 19.05 -19.05 180)
					(length 3.81)
					(name "P1.24")
					(number "D7")
				)
				(pin bidirectional line
					(at 19.05 -29.21 180)
					(length 3.81)
					(name "P1.28")
					(number "D8")
				)
				(pin bidirectional line
					(at 19.05 -21.59 180)
					(length 3.81)
					(name "P1.25")
					(number "E7")
				)
				(pin bidirectional line
					(at 19.05 13.97 180)
					(length 3.81)
					(name "P1.09")
					(number "E8")
				)
				(pin bidirectional line
					(at 19.05 16.51 180)
					(length 3.81)
					(name "P1.08")
					(number "F8")
				)
				(pin bidirectional line
					(at 19.05 19.05 180)
					(length 3.81)
					(name "P1.07")
					(number "G8")
				)
				(pin bidirectional line
					(at 19.05 24.13 180)
					(length 3.81)
					(name "P1.05")
					(number "H8")
				)
				(pin bidirectional line
					(at 19.05 29.21 180)
					(length 3.81)
					(name "P1.03")
					(number "H9")
				)
				(pin bidirectional line
					(at 19.05 -31.75 180)
					(length 3.81)
					(name "P1.29")
					(number "H10")
				)
				(pin bidirectional line
					(at 19.05 34.29 180)
					(length 3.81)
					(name "P1.01")
					(number "J6")
				)
				(pin bidirectional line
					(at 19.05 31.75 180)
					(length 3.81)
					(name "P1.02")
					(number "J7")
				)
				(pin bidirectional line
					(at 19.05 21.59 180)
					(length 3.81)
					(name "P1.06")
					(number "J8")
				)
				(pin bidirectional line
					(at 19.05 26.67 180)
					(length 3.81)
					(name "P1.04")
					(number "J9")
				)
				(pin bidirectional line
					(at 19.05 -34.29 180)
					(length 3.81)
					(name "P1.30")
					(number "J10")
				)
				(pin bidirectional line
					(at 19.05 36.83 180)
					(length 3.81)
					(name "P1.00")
					(number "K8")
				)
				(pin bidirectional line
					(at 19.05 -36.83 180)
					(length 3.81)
					(name "P1.31")
					(number "K9")
				)
			)
			(symbol "nRF54LM20A-PAXX_3_1")
			(symbol "nRF54LM20A-PAXX_4_0"
				(pin bidirectional line
					(at 19.05 -2.54 180)
					(length 3.81)
					(name "P2.06")
					(number "B9")
				)
				(pin bidirectional line
					(at 19.05 12.7 180)
					(length 3.81)
					(name "P2.00")
					(number "B10")
				)
				(pin bidirectional line
					(at 19.05 -5.08 180)
					(length 3.81)
					(name "P2.07")
					(number "C9")
				)
				(pin bidirectional line
					(at 19.05 10.16 180)
					(length 3.81)
					(name "P2.01")
					(number "C10")
				)
				(pin bidirectional line
					(at 19.05 -7.62 180)
					(length 3.81)
					(name "P2.08")
					(number "D9")
				)
				(pin bidirectional line
					(at 19.05 7.62 180)
					(length 3.81)
					(name "P2.02")
					(number "D10")
				)
				(pin bidirectional line
					(at 19.05 -10.16 180)
					(length 3.81)
					(name "P2.09")
					(number "E9")
				)
				(pin bidirectional line
					(at 19.05 5.08 180)
					(length 3.81)
					(name "P2.03")
					(number "E10")
				)
				(pin bidirectional line
					(at 19.05 -12.7 180)
					(length 3.81)
					(name "P2.10")
					(number "F9")
				)
				(pin bidirectional line
					(at 19.05 2.54 180)
					(length 3.81)
					(name "P2.04")
					(number "F10")
				)
				(pin bidirectional line
					(at 19.05 0 180)
					(length 3.81)
					(name "P2.05")
					(number "G9")
				)
			)
			(symbol "nRF54LM20A-PAXX_4_1")
			(symbol "nRF54LM20A-PAXX_5_0"
				(pin bidirectional line
					(at 19.05 -15.24 180)
					(length 3.81)
					(name "P3.12")
					(number "D4")
				)
				(pin bidirectional line
					(at 19.05 -12.7 180)
					(length 3.81)
					(name "P3.11")
					(number "E4")
				)
				(pin bidirectional line
					(at 19.05 -10.16 180)
					(length 3.81)
					(name "P3.10")
					(number "F4")
				)
				(pin bidirectional line
					(at 19.05 -7.62 180)
					(length 3.81)
					(name "P3.09")
					(number "F7")
				)
				(pin bidirectional line
					(at 19.05 -5.08 180)
					(length 3.81)
					(name "P3.08")
					(number "G4")
				)
				(pin bidirectional line
					(at 19.05 -2.54 180)
					(length 3.81)
					(name "P3.07")
					(number "G5")
				)
				(pin bidirectional line
					(at 19.05 0 180)
					(length 3.81)
					(name "P3.06")
					(number "G6")
				)
				(pin bidirectional line
					(at 19.05 2.54 180)
					(length 3.81)
					(name "P3.05")
					(number "G7")
				)
				(pin bidirectional line
					(at 19.05 7.62 180)
					(length 3.81)
					(name "P3.03")
					(number "H4")
				)
				(pin bidirectional line
					(at 19.05 10.16 180)
					(length 3.81)
					(name "P3.02")
					(number "H5")
				)
				(pin bidirectional line
					(at 19.05 12.7 180)
					(length 3.81)
					(name "P3.01")
					(number "H6")
				)
				(pin bidirectional line
					(at 19.05 15.24 180)
					(length 3.81)
					(name "P3.00")
					(number "H7")
				)
				(pin bidirectional line
					(at 19.05 5.08 180)
					(length 3.81)
					(name "P3.04")
					(number "J4")
				)
			)
			(symbol "nRF54LM20A-PAXX_5_1")
			(embedded_fonts no)
		)
)
