(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF54LM20A-QGXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at -12.7 35.56 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "nRF54LM20A-QGXX"
				(at -13.97 33.02 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "nordic-lib-kicad-nrf54l:QFN-52-1EP_6x6mm_P0.4mm_EP4.7x4.7mm_ThermalVias"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf54LM20A/page/pdf/nRF54LM20A_Preliminary_Datasheet_v0.7.pdf"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_fp_filters" "QFN*52*1EP*6x6mm*P0.4mm*EP4.7x4.7mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "nRF54LM20A-QGXX_1_0"
				(pin power_in line
					(at 0 34.29 270)
					(length 3.81)
					(name "VDD")
					(number "6")
				)
				(pin power_in line
					(at -19.05 25.4 0)
					(length 3.81)
					(name "VBUS")
					(number "17")
				)
				(pin passive line
					(at -19.05 -25.4 0)
					(length 3.81)
					(name "DECUSB")
					(number "18")
				)
				(pin bidirectional line
					(at -19.05 -12.7 0)
					(length 3.81)
					(name "D+")
					(number "19")
				)
				(pin bidirectional line
					(at -19.05 -15.24 0)
					(length 3.81)
					(name "D-")
					(number "20")
				)
				(pin bidirectional line
					(at -19.05 -20.32 0)
					(length 3.81)
					(name "TXRTUNE")
					(number "21")
				)
				(pin input line
					(at 19.05 -22.86 180)
					(length 3.81)
					(name "SWDCLK")
					(number "31")
				)
				(pin bidirectional line
					(at 19.05 -25.4 180)
					(length 3.81)
					(name "SWDIO")
					(number "32")
				)
				(pin input line
					(at 19.05 -17.78 180)
					(length 3.81)
					(name "~{RESET}")
					(number "33")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 3.81)
					(name "ANT")
					(number "34")
				)
				(pin power_in line
					(at 0 -34.29 90)
					(length 3.81)
					(name "VSS")
					(number "35")
				)
				(pin passive line
					(at 19.05 12.7 180)
					(length 3.81)
					(name "DECRF")
					(number "36")
				)
				(pin input line
					(at -19.05 15.24 0)
					(length 3.81)
					(name "XC1")
					(number "37")
				)
				(pin output line
					(at -19.05 10.16 0)
					(length 3.81)
					(name "XC2")
					(number "38")
				)
				(pin passive line
					(at 0 34.29 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "42")
				)
				(pin passive line
					(at 19.05 25.4 180)
					(length 3.81)
					(name "DCC")
					(number "43")
				)
				(pin passive line
					(at 19.05 20.32 180)
					(length 3.81)
					(name "DECD")
					(number "44")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "45")
				)
				(pin passive line
					(at 19.05 15.24 180)
					(length 3.81)
					(name "DECA")
					(number "46")
				)
				(pin bidirectional line
					(at -19.05 2.54 0)
					(length 3.81)
					(name "P1.20")
					(number "48")
					(alternate "XL1" input line)
				)
				(pin bidirectional line
					(at -19.05 -2.54 0)
					(length 3.81)
					(name "P1.21")
					(number "49")
					(alternate "XL2" output line)
				)
				(pin passive line
					(at 0 34.29 270)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "51")
				)
				(pin passive line
					(at 0 -34.29 90)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "53")
				)
			)
			(symbol "nRF54LM20A-QGXX_1_1")
			(symbol "nRF54LM20A-QGXX_2_0"
				(pin bidirectional line
					(at 19.05 6.35 180)
					(length 3.81)
					(name "P0.03")
					(number "25")
				)
				(pin bidirectional line
					(at 19.05 3.81 180)
					(length 3.81)
					(name "P0.04")
					(number "26")
				)
				(pin bidirectional line
					(at 19.05 1.27 180)
					(length 3.81)
					(name "P0.06")
					(number "27")
				)
				(pin bidirectional line
					(at 19.05 -1.27 180)
					(length 3.81)
					(name "P0.07")
					(number "28")
				)
				(pin bidirectional line
					(at 19.05 -3.81 180)
					(length 3.81)
					(name "P0.08")
					(number "29")
				)
				(pin bidirectional line
					(at 19.05 -6.35 180)
					(length 3.81)
					(name "P0.09")
					(number "30")
				)
			)
			(symbol "nRF54LM20A-QGXX_2_1")
			(symbol "nRF54LM20A-QGXX_3_0"
				(pin bidirectional line
					(at 19.05 -16.51 180)
					(length 3.81)
					(name "P1.29")
					(number "7")
				)
				(pin bidirectional line
					(at 19.05 -19.05 180)
					(length 3.81)
					(name "P1.30")
					(number "8")
				)
				(pin bidirectional line
					(at 19.05 -21.59 180)
					(length 3.81)
					(name "P1.31")
					(number "9")
				)
				(pin bidirectional line
					(at 19.05 21.59 180)
					(length 3.81)
					(name "P1.00")
					(number "10")
				)
				(pin bidirectional line
					(at 19.05 19.05 180)
					(length 3.81)
					(name "P1.01")
					(number "11")
				)
				(pin bidirectional line
					(at 19.05 16.51 180)
					(length 3.81)
					(name "P1.02")
					(number "12")
				)
				(pin bidirectional line
					(at 19.05 13.97 180)
					(length 3.81)
					(name "P1.03")
					(number "13")
				)
				(pin bidirectional line
					(at 19.05 11.43 180)
					(length 3.81)
					(name "P1.04")
					(number "14")
				)
				(pin bidirectional line
					(at 19.05 8.89 180)
					(length 3.81)
					(name "P1.05")
					(number "15")
				)
				(pin bidirectional line
					(at 19.05 6.35 180)
					(length 3.81)
					(name "P1.06")
					(number "16")
				)
				(pin bidirectional line
					(at 19.05 3.81 180)
					(length 3.81)
					(name "P1.07")
					(number "22")
				)
				(pin bidirectional line
					(at 19.05 1.27 180)
					(length 3.81)
					(name "P1.08")
					(number "23")
				)
				(pin bidirectional line
					(at 19.05 -1.27 180)
					(length 3.81)
					(name "P1.09")
					(number "24")
				)
				(pin bidirectional line
					(at 19.05 -3.81 180)
					(length 3.81)
					(name "P1.15")
					(number "39")
				)
				(pin bidirectional line
					(at 19.05 -6.35 180)
					(length 3.81)
					(name "P1.16")
					(number "40")
				)
				(pin bidirectional line
					(at 19.05 -8.89 180)
					(length 3.81)
					(name "P1.18")
					(number "41")
				)
				(pin bidirectional line
					(at 19.05 -11.43 180)
					(length 3.81)
					(name "P1.19")
					(number "47")
				)
				(pin bidirectional line
					(at 19.05 -13.97 180)
					(length 3.81)
					(name "P1.24")
					(number "50")
				)
			)
			(symbol "nRF54LM20A-QGXX_3_1")
			(symbol "nRF54LM20A-QGXX_4_0"
				(pin bidirectional line
					(at 19.05 3.81 180)
					(length 3.81)
					(name "P2.01")
					(number "1")
				)
				(pin bidirectional line
					(at 19.05 1.27 180)
					(length 3.81)
					(name "P2.02")
					(number "2")
				)
				(pin bidirectional line
					(at 19.05 -1.27 180)
					(length 3.81)
					(name "P2.03")
					(number "3")
				)
				(pin bidirectional line
					(at 19.05 -3.81 180)
					(length 3.81)
					(name "P2.04")
					(number "4")
				)
				(pin bidirectional line
					(at 19.05 -6.35 180)
					(length 3.81)
					(name "P2.05")
					(number "5")
				)
				(pin bidirectional line
					(at 19.05 6.35 180)
					(length 3.81)
					(name "P2.00")
					(number "52")
				)
			)
			(symbol "nRF54LM20A-QGXX_4_1")
			(embedded_fonts no)
		)
)
