(footprint "Nordic_CSP-29_1.9268x2.2893mm_Layout5x6_P0.35mm_Offcenter"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Nordic CSP-29, 1.9268x2.2893mm, 29 Ball, 5x6 Layout, 0.35mm Pitch, generated with kicad-footprint-generator ipc_bga_generator.py, https://docs.nordicsemi.com/bundle/ps_nrf54LV10/page/keyfeatures_html5.html")
	(tags "CSP 29 0.35")
	(property "Reference" "REF**"
		(at 0 -2.14465 0)
		(layer "F.SilkS")
	)
	(property "Value" "Nordic_CSP-29_1.9268x2.2893mm_Layout5x6_P0.35mm_Offcenter"
		(at 0 2.14465 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.6765 -0.8565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -0.3265 -0.8565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at 0.0235 -0.8565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 0.3735 -0.8565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 0.7235 -0.8565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -0.6765 -0.5065)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at 0.0235 -0.5065)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 0.3735 -0.5065)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 0.7235 -0.5065)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.6765 -0.1565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -0.3265 -0.1565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at 0.0235 -0.1565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 0.3735 -0.1565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 0.7235 -0.1565)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -0.6765 0.1935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -0.3265 0.1935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at 0.0235 0.1935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at 0.3735 0.1935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at 0.7235 0.1935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -0.6765 0.5435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -0.3265 0.5435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at 0.0235 0.5435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at 0.3735 0.5435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at 0.7235 0.5435)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -0.6765 0.8935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -0.3265 0.8935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at 0.0235 0.8935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at 0.3735 0.8935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 0.7235 0.8935)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "nordic_nrf54lv10a_caaa.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
