(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF54LV10A-CAAA"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "nRF54LV10A-CAAA"
				(at 0 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "nordic-lib-kicad-nrf54l:Nordic_CSP-29_1.9268x2.2893mm_Layout5x6_P0.35mm_Offcenter"
				(at 0 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf54LV10/page/keyfeatures_html5.html"
				(at 0 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "nRF54LV Ultra-low power Bluetooth 5.4 SoC, 1.5V-3.6V, CSP29"
				(at 0 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "BLE Bluetooth SoC nRF nRF54 ultra-low-power WLCSP"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "*CSP?29*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "nRF54LV10A-CAAA_1_0"
				(pin passive line
					(at 17.78 27.94 180)
					(length 2.54)
					(name "DECRF")
					(number "A1")
				)
				(pin bidirectional line
					(at -17.78 33.02 0)
					(length 2.54)
					(name "XC1")
					(number "A2")
				)
				(pin bidirectional line
					(at -17.78 27.94 0)
					(length 2.54)
					(name "XC2")
					(number "A3")
				)
				(pin bidirectional line
					(at -17.78 -17.78 0)
					(length 2.54)
					(name "P1.03")
					(number "A4")
					(alternate "AIN3" input line)
				)
				(pin bidirectional line
					(at -17.78 -27.94 0)
					(length 2.54)
					(name "P1.10")
					(number "A5")
					(alternate "AIN5" input line)
					(alternate "ASO[1]" output line)
					(alternate "TRACECLK" output line)
				)
				(pin bidirectional line
					(at 17.78 0 180)
					(length 2.54)
					(name "ANT")
					(number "B1")
				)
				(pin bidirectional line
					(at -17.78 -25.4 0)
					(length 2.54)
					(name "P1.09")
					(number "B3")
				)
				(pin bidirectional line
					(at -17.78 -20.32 0)
					(length 2.54)
					(name "P1.05")
					(number "B4")
					(alternate "ASO[0]" output line)
					(alternate "EXTREF" input line)
				)
				(pin bidirectional line
					(at -17.78 20.32 0)
					(length 2.54)
					(name "P1.13")
					(number "B5")
					(alternate "TRACEDATA[2]" output line)
					(alternate "XL1" bidirectional line)
				)
				(pin power_in line
					(at 0 -40.64 90)
					(length 2.54)
					(name "VSS")
					(number "C1")
				)
				(pin input line
					(at 17.78 -25.4 180)
					(length 2.54)
					(name "~{RESET}")
					(number "C2")
				)
				(pin bidirectional line
					(at -17.78 -12.7 0)
					(length 2.54)
					(name "P1.01")
					(number "C3")
					(alternate "AIN1" input line)
				)
				(pin bidirectional line
					(at -17.78 -22.86 0)
					(length 2.54)
					(name "P1.07")
					(number "C4")
					(alternate "AIN4" input line)
					(alternate "ASI[0]" input line)
				)
				(pin bidirectional line
					(at -17.78 15.24 0)
					(length 2.54)
					(name "P1.14")
					(number "C5")
					(alternate "TRACEDATA[3]" output line)
					(alternate "XL2" bidirectional line)
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "D1")
				)
				(pin input line
					(at 17.78 -30.48 180)
					(length 2.54)
					(name "SWDCLK")
					(number "D2")
				)
				(pin bidirectional line
					(at -17.78 -15.24 0)
					(length 2.54)
					(name "P1.02")
					(number "D3")
					(alternate "AIN2" input line)
				)
				(pin bidirectional line
					(at -17.78 -30.48 0)
					(length 2.54)
					(name "P1.11")
					(number "D4")
					(alternate "AIN6" input line)
					(alternate "ASI[1]" input line)
					(alternate "SWO" output line)
					(alternate "TRACEDATA[0]" output line)
				)
				(pin passive line
					(at 17.78 33.02 180)
					(length 2.54)
					(name "DECA")
					(number "D5")
				)
				(pin passive line
					(at 17.78 30.48 180)
					(length 2.54)
					(name "DECB")
					(number "E1")
				)
				(pin bidirectional line
					(at 17.78 -33.02 180)
					(length 2.54)
					(name "SWDIO")
					(number "E2")
				)
				(pin bidirectional line
					(at -17.78 -10.16 0)
					(length 2.54)
					(name "P1.00")
					(number "E3")
					(alternate "AIN0" input line)
				)
				(pin bidirectional line
					(at -17.78 -33.02 0)
					(length 2.54)
					(name "P1.12")
					(number "E4")
					(alternate "AIN7" input line)
					(alternate "TRACEDATA[1]" output line)
				)
				(pin passive line
					(at 17.78 25.4 180)
					(length 2.54)
					(name "DECD")
					(number "E5")
				)
				(pin passive line
					(at 17.78 12.7 180)
					(length 2.54)
					(name "CFLYH")
					(number "F1")
				)
				(pin passive line
					(at 17.78 7.62 180)
					(length 2.54)
					(name "CFLYL")
					(number "F2")
				)
				(pin power_in line
					(at 0 40.64 270)
					(length 2.54)
					(name "VDDL")
					(number "F3")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "F4")
				)
				(pin power_out line
					(at 17.78 20.32 180)
					(length 2.54)
					(name "DCC")
					(number "F5")
				)
			)
			(embedded_fonts no)
		)
)
