(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF7002-CEXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF7002-CEXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf7:BGA-90_10x9_3.7495x3.385mm"
				(at 0 -50.8 0)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf7002/page/keyfeatures_html5.html"
				(at 0 -53.34 0)
			)
			(property "Description" "2.4/5GHz Wi-Fi 6 Companion IC, SSID scanning, Matter support, CSP-90"
				(at 0 -55.88 0)
			)
			(property "ki_keywords" "wifi6 802.11ax matter companion-ic locationing ssid-scan low-power coexistence csp"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?90*10x9*3.7495x3.385mm*"
				(at 0 0 0)
			)
			(symbol "nRF7002-CEXX_0_0"
				(pin output line
					(at -38.1 -25.4 0)
					(length 5.08)
					(name "COEX_GRANT")
					(number "A11")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "A13")
				)
				(pin output line
					(at -38.1 -30.48 0)
					(length 5.08)
					(name "SW_CTRL0")
					(number "A16")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "A18")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "A20")
				)
				(pin bidirectional line
					(at -38.1 -10.16 0)
					(length 5.08)
					(name "QSPI_DATA2")
					(number "A3")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "A7")
				)
				(pin bidirectional line
					(at -38.1 -33.02 0)
					(length 5.08)
					(name "SW_CTRL1")
					(number "A9")
				)
				(pin output line
					(at -38.1 -27.94 0)
					(length 5.08)
					(name "HOST_IRQ")
					(number "B10")
				)
				(pin power_in line
					(at -2.54 40.64 270)
					(length 5.08)
					(name "IOVDD")
					(number "B12")
				)
				(pin no_connect line
					(at 22.86 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "B15")
				)
				(pin power_in line
					(at 2.54 40.64 270)
					(length 5.08)
					(name "OTPVDD")
					(number "B17")
				)
				(pin no_connect line
					(at 25.4 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "B19")
				)
				(pin bidirectional line
					(at -38.1 -12.7 0)
					(length 5.08)
					(name "QSPI_DATA3")
					(number "B6")
				)
				(pin bidirectional line
					(at -38.1 -20.32 0)
					(length 5.08)
					(name "COEX_STATUS0")
					(number "B8")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "C11")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "C13")
				)
				(pin no_connect line
					(at 27.94 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "C16")
				)
				(pin no_connect line
					(at 7.62 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "C18")
				)
				(pin no_connect line
					(at 10.16 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "C20")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "C7")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "C9")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D1")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D11")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D13")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D16")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D20")
				)
				(pin power_in line
					(at 5.08 40.64 270)
					(length 5.08)
					(name "PWRIOVDD")
					(number "D3")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D7")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "D9")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "E13")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "E3")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "E9")
				)
				(pin passive line
					(at 38.1 -30.48 180)
					(length 5.08)
					(name "DIGVDD")
					(number "F1")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "F13")
				)
				(pin passive line
					(at 38.1 -22.86 180)
					(length 5.08)
					(name "PWRBUCKVDD")
					(number "F3")
				)
				(pin power_in line
					(at 38.1 -7.62 180)
					(length 5.08)
					(name "BUCKVBATS")
					(number "F5")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "F9")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "H20")
				)
				(pin passive line
					(at 38.1 -17.78 180)
					(length 5.08)
					(name "XOLDO")
					(number "J11")
				)
				(pin input line
					(at -38.1 -17.78 0)
					(length 5.08)
					(name "BUCKEN")
					(number "J5")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "J7")
				)
				(pin passive line
					(at 38.1 -33.02 180)
					(length 5.08)
					(name "AFELDO")
					(number "J9")
				)
				(pin passive line
					(at 38.1 -25.4 180)
					(length 5.08)
					(name "RFVDD")
					(number "K13")
				)
				(pin passive line
					(at 38.1 -15.24 180)
					(length 5.08)
					(name "SXLDO")
					(number "K16")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "K20")
				)
				(pin power_out line
					(at 38.1 15.24 180)
					(length 5.08)
					(name "BUCKOUT")
					(number "K3")
				)
				(pin no_connect line
					(at 12.7 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "K5")
				)
				(pin no_connect line
					(at 15.24 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "K7")
				)
				(pin power_in line
					(at 38.1 -5.08 180)
					(length 5.08)
					(name "BUCKVBAT")
					(number "L1")
				)
				(pin passive line
					(at 38.1 -20.32 180)
					(length 5.08)
					(name "RFBUCKVDD")
					(number "L13")
				)
				(pin power_in line
					(at -12.7 40.64 270)
					(length 5.08)
					(name "VBAT")
					(number "L16")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "L18")
				)
				(pin power_out line
					(at 38.1 7.62 180)
					(length 5.08)
					(name "PALDO")
					(number "L20")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "L3")
				)
				(pin no_connect line
					(at 17.78 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "L5")
				)
				(pin no_connect line
					(at 20.32 -35.56 90)
					(length 5.08) hide
					(name "NC")
					(number "L7")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "GND")
					(number "L9")
				)
			)
			(symbol "nRF7002-CEXX_1_0"
				(pin power_in line
					(at 0 -40.64 90)
					(length 5.08)
					(name "VSS")
					(number "A1")
				)
				(pin bidirectional line
					(at -38.1 -22.86 0)
					(length 5.08)
					(name "COEX_REQ")
					(number "A5")
				)
				(pin bidirectional line
					(at -38.1 -5.08 0)
					(length 5.08)
					(name "QSPI_DATA0")
					(number "B2")
					(alternate "SPI_MOSI" bidirectional line)
				)
				(pin bidirectional line
					(at -38.1 -7.62 0)
					(length 5.08)
					(name "QSPI_DATA1")
					(number "B4")
					(alternate "SPI_MISO" bidirectional line)
				)
				(pin input line
					(at -38.1 0 0)
					(length 5.08)
					(name "QSPI_CLK")
					(number "C1")
					(alternate "SPI_CLK" input line)
				)
				(pin input line
					(at -38.1 -2.54 0)
					(length 5.08)
					(name "~{QSPI_SS}")
					(number "C3")
					(alternate "~{SPI_SS}" input line)
				)
				(pin bidirectional line
					(at 38.1 22.86 180)
					(length 5.08)
					(name "TXRF1")
					(number "D18")
				)
				(pin power_in line
					(at 38.1 2.54 180)
					(length 5.08)
					(name "PAVDD1")
					(number "E16")
				)
				(pin bidirectional line
					(at 38.1 27.94 180)
					(length 5.08)
					(name "TXRF0")
					(number "G16")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "BUCKVSSS")
					(number "J1")
				)
				(pin power_in line
					(at 38.1 5.08 180)
					(length 5.08)
					(name "PAVDD0")
					(number "J14")
				)
				(pin passive line
					(at 38.1 -27.94 180)
					(length 5.08)
					(name "BUCKVMID")
					(number "J3")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 5.08) hide
					(name "BUCKVSS")
					(number "K1")
				)
				(pin input line
					(at -38.1 20.32 0)
					(length 5.08)
					(name "XOP")
					(number "K11")
				)
				(pin power_in line
					(at 38.1 -2.54 180)
					(length 5.08)
					(name "AFEVBAT")
					(number "K9")
				)
				(pin output line
					(at -38.1 15.24 0)
					(length 5.08)
					(name "XON")
					(number "L11")
				)
			)
			(symbol "nRF7002-CEXX_1_1")
		)
)
