(footprint "LGA_9151_12.1x11.1mm"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Nordic nRF9151 SiP, 12.1x11.1mm, 113 Pad, generated with kicad-footprint-generator ipc_bga_generator.py, https://docs.nordicsemi.com/bundle/ps_nrf9151/page/nRF9151_html5_keyfeatures.html")
	(tags "LGA 113")
	(property "Reference" "REF**"
		(at 0 -6.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "LGA_9151_12.1x11.1mm"
		(at 0 6.55 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -5.5 -5)
		(size 0.7 0.7)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "2" smd roundrect
		(at -5.625 -4.25037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "3" smd roundrect
		(at -5.625 -3.75037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "4" smd roundrect
		(at -5.625 -3.25037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "5" smd roundrect
		(at -5.625 -2.75037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "6" smd roundrect
		(at -5.625 -2.25037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "7" smd roundrect
		(at -5.625 -1.75037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "8" smd roundrect
		(at -5.625 -1.25037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "9" smd roundrect
		(at -5.625 -0.75037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "10" smd roundrect
		(at -5.625 -0.25037)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "11" smd roundrect
		(at -5.625 0.24963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "12" smd roundrect
		(at -5.625 0.74963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "13" smd roundrect
		(at -5.625 1.24963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "14" smd roundrect
		(at -5.625 1.74963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "15" smd roundrect
		(at -5.625 2.24963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "16" smd roundrect
		(at -5.625 2.74963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "17" smd roundrect
		(at -5.625 3.24963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "18" smd roundrect
		(at -5.625 3.74963)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "19" smd roundrect
		(at -5.625 4.24999)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "20" smd roundrect
		(at -5.5 5)
		(size 0.7 0.7)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "21" smd roundrect
		(at -4.75 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "22" smd roundrect
		(at -4.25 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "23" smd roundrect
		(at -3.74997 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "24" smd roundrect
		(at -3.24997 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "25" smd roundrect
		(at -2.74997 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "26" smd roundrect
		(at -2.24997 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "27" smd roundrect
		(at -1.74997 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "28" smd roundrect
		(at -1.25 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "29" smd roundrect
		(at -0.75 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "30" smd roundrect
		(at -0.25 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "31" smd roundrect
		(at 0.25 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "32" smd roundrect
		(at 0.75 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "33" smd roundrect
		(at 1.25002 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "34" smd roundrect
		(at 1.75003 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "35" smd roundrect
		(at 2.25003 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "36" smd roundrect
		(at 2.75003 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "37" smd roundrect
		(at 3.25003 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "38" smd roundrect
		(at 3.75002 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "39" smd roundrect
		(at 4.25003 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "40" smd roundrect
		(at 4.75003 5.125 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "41" smd roundrect
		(at 5.5 5)
		(size 0.7 0.7)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "42" smd roundrect
		(at 5.625 4.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "43" smd roundrect
		(at 5.625 3.75)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "44" smd roundrect
		(at 5.625 3.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "45" smd roundrect
		(at 5.625 2.75)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "46" smd roundrect
		(at 5.625 2.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "47" smd roundrect
		(at 5.625 1.75)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "48" smd roundrect
		(at 5.625 1.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "49" smd roundrect
		(at 5.625 0.75)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "50" smd roundrect
		(at 5.625 0.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "51" smd roundrect
		(at 5.625 -0.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "52" smd roundrect
		(at 5.625 -0.75001)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "53" smd roundrect
		(at 5.625 -1.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "54" smd roundrect
		(at 5.625 -1.75)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "55" smd roundrect
		(at 5.625 -2.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "56" smd roundrect
		(at 5.625 -2.75)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "57" smd roundrect
		(at 5.625 -3.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "58" smd roundrect
		(at 5.625 -3.75)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "59" smd roundrect
		(at 5.625 -4.25)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "60" smd roundrect
		(at 5.5 -5)
		(size 0.7 0.7)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "61" smd roundrect
		(at 4.75 -5.12501 90)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "62" smd roundrect
		(at 4.25 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "63" smd roundrect
		(at 3.74997 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "64" smd roundrect
		(at 3.24997 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "65" smd roundrect
		(at 2.74997 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "66" smd roundrect
		(at 2.24997 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "67" smd roundrect
		(at 1.74998 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "68" smd roundrect
		(at 1.24997 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "69" smd roundrect
		(at 0.75 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "70" smd roundrect
		(at 0.25 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "71" smd roundrect
		(at -0.25 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "72" smd roundrect
		(at -0.75 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "73" smd roundrect
		(at -1.25 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "74" smd roundrect
		(at -1.75 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "75" smd roundrect
		(at -2.25 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "76" smd roundrect
		(at -2.75 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "77" smd roundrect
		(at -3.25 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "78" smd roundrect
		(at -3.75 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "79" smd roundrect
		(at -4.25 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "80" smd roundrect
		(at -4.75 -5.12501 270)
		(size 0.45 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "81" smd roundrect
		(at -4.1 -3.40001 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "82" smd roundrect
		(at -4.1 -2.85 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "83" smd roundrect
		(at -4.1 -2.30001 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "84" smd roundrect
		(at -4.1 -0.55 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "85" smd roundrect
		(at -4.1 0 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "86" smd roundrect
		(at -4.1 0.54999 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "87" smd roundrect
		(at -4.1 2.3 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "88" smd roundrect
		(at -4.1 2.84999 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "89" smd roundrect
		(at -4.1 3.4 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "90" smd roundrect
		(at -0.55 2.15 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "91" smd roundrect
		(at 0 2.15 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "92" smd roundrect
		(at 0.55 2.15 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "93" smd roundrect
		(at 4.1 3.4 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "94" smd roundrect
		(at 4.1 2.84999 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "95" smd roundrect
		(at 4.1 2.3 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "96" smd roundrect
		(at 4.1 0.54999 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "97" smd roundrect
		(at 4.1 0 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "98" smd roundrect
		(at 4.1 -0.55 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "99" smd roundrect
		(at 4.1 -2.30001 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "100" smd roundrect
		(at 4.1 -2.85 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "101" smd roundrect
		(at 4.1 -3.40001 90)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "102" smd roundrect
		(at 0.55 -2.15001 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "103" smd roundrect
		(at 0 -2.15001 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "104" smd roundrect
		(at -0.55 -2.15001 270)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "105" smd roundrect
		(at -2.85 -2.85)
		(size 1.6 1.6)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "106" smd roundrect
		(at -2.85 0)
		(size 1.6 1.6)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "107" smd roundrect
		(at -2.85 2.84999)
		(size 1.6 1.6)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "108" smd roundrect
		(at 0 3.57499)
		(size 1.6 1.95)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "109" smd roundrect
		(at 2.85 2.84999)
		(size 1.6 1.6)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "110" smd roundrect
		(at 2.85 0)
		(size 1.6 1.6)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "111" smd roundrect
		(at 2.85 -2.85)
		(size 1.6 1.6)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "112" smd roundrect
		(at 0 -3.57501)
		(size 1.6 1.95)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "113" smd roundrect
		(at 0 0)
		(size 1.6 1.6)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(embedded_fonts no)
	(model "nordic_nrf9151_laxx.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
