(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF9160-SIXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nRF9160-SIXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf9:LGA_9160_16.0x10.5mm"
				(at 0 -83.82 0)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf9160/page/nRF9160_html5_keyfeatures.html"
				(at 0 -86.36 0)
			)
			(property "Description" "LTE-M/NB-IoT SiP, 1MB Flash, 256KB RAM, Cortex-M33, GNSS, ADC, SPI, I2C, I2S, UART, PDM, PWM, LGA-100"
				(at 0 -88.9 0)
			)
			(property "ki_keywords" "cellular iot lte-m nb-iot gnss trustzone cryptocell arm microcontroller wireless secure-boot esim psa-certified fota nrf91-series lga"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LGA?9160*16.0x10.5m*"
				(at 0 0 0)
			)
			(symbol "nRF9160-SIXX_0_0"
				(pin input line
					(at -33.02 58.42 0)
					(length 5.08)
					(name "ENABLE")
					(number "101")
				)
				(pin bidirectional line
					(at -33.02 50.8 0)
					(length 5.08)
					(name "P0.00")
					(number "95")
				)
				(pin bidirectional line
					(at -33.02 48.26 0)
					(length 5.08)
					(name "P0.01")
					(number "96")
				)
				(pin bidirectional line
					(at -33.02 45.72 0)
					(length 5.08)
					(name "P0.02")
					(number "97")
				)
				(pin bidirectional line
					(at -33.02 43.18 0)
					(length 5.08)
					(name "P0.03")
					(number "99")
				)
				(pin bidirectional line
					(at -33.02 40.64 0)
					(length 5.08)
					(name "P0.04")
					(number "100")
				)
				(pin bidirectional line
					(at -33.02 38.1 0)
					(length 5.08)
					(name "P0.05")
					(number "2")
				)
				(pin bidirectional line
					(at -33.02 35.56 0)
					(length 5.08)
					(name "P0.06")
					(number "3")
				)
				(pin bidirectional line
					(at -33.02 33.02 0)
					(length 5.08)
					(name "P0.07")
					(number "4")
				)
				(pin bidirectional line
					(at -33.02 30.48 0)
					(length 5.08)
					(name "P0.08")
					(number "15")
				)
				(pin bidirectional line
					(at -33.02 27.94 0)
					(length 5.08)
					(name "P0.09")
					(number "16")
				)
				(pin bidirectional line
					(at -33.02 25.4 0)
					(length 5.08)
					(name "P0.10")
					(number "18")
				)
				(pin bidirectional line
					(at -33.02 22.86 0)
					(length 5.08)
					(name "P0.11")
					(number "19")
				)
				(pin bidirectional line
					(at -33.02 20.32 0)
					(length 5.08)
					(name "P0.12")
					(number "20")
				)
				(pin bidirectional line
					(at -33.02 17.78 0)
					(length 5.08)
					(name "P0.13/AIN0")
					(number "23")
				)
				(pin bidirectional line
					(at -33.02 15.24 0)
					(length 5.08)
					(name "P0.14/AIN1")
					(number "24")
				)
				(pin bidirectional line
					(at -33.02 12.7 0)
					(length 5.08)
					(name "P0.15/AIN2")
					(number "25")
				)
				(pin bidirectional line
					(at -33.02 10.16 0)
					(length 5.08)
					(name "P0.16/AIN3")
					(number "26")
				)
				(pin bidirectional line
					(at -33.02 7.62 0)
					(length 5.08)
					(name "P0.17/AIN4")
					(number "28")
				)
				(pin bidirectional line
					(at -33.02 5.08 0)
					(length 5.08)
					(name "P0.18/AIN5")
					(number "29")
				)
				(pin bidirectional line
					(at -33.02 2.54 0)
					(length 5.08)
					(name "P0.19/AIN6")
					(number "30")
				)
				(pin bidirectional line
					(at -33.02 0 0)
					(length 5.08)
					(name "P0.20/AIN7")
					(number "35")
				)
				(pin bidirectional line
					(at -33.02 -2.54 0)
					(length 5.08)
					(name "P0.26")
					(number "83")
				)
				(pin bidirectional line
					(at -33.02 -5.08 0)
					(length 5.08)
					(name "P0.27")
					(number "84")
				)
				(pin bidirectional line
					(at -33.02 -7.62 0)
					(length 5.08)
					(name "P0.28")
					(number "86")
				)
				(pin bidirectional line
					(at -33.02 -10.16 0)
					(length 5.08)
					(name "P0.29")
					(number "87")
				)
				(pin bidirectional line
					(at -33.02 -12.7 0)
					(length 5.08)
					(name "P0.30")
					(number "88")
				)
				(pin bidirectional line
					(at -33.02 -15.24 0)
					(length 5.08)
					(name "P0.31")
					(number "89")
				)
				(pin bidirectional line
					(at -33.02 -25.4 0)
					(length 5.08)
					(name "MAGPIO0")
					(number "55")
				)
				(pin bidirectional line
					(at -33.02 -27.94 0)
					(length 5.08)
					(name "MAGPIO1")
					(number "54")
				)
				(pin bidirectional line
					(at -33.02 -30.48 0)
					(length 5.08)
					(name "MAGPIO2")
					(number "53")
				)
				(pin bidirectional line
					(at -33.02 -40.64 0)
					(length 5.08)
					(name "SIM_CLK")
					(number "46")
				)
				(pin bidirectional line
					(at -33.02 -43.18 0)
					(length 5.08)
					(name "SIM_IO")
					(number "48")
				)
				(pin bidirectional line
					(at -33.02 -45.72 0)
					(length 5.08)
					(name "SIM_RST")
					(number "43")
				)
				(pin bidirectional line
					(at -33.02 -48.26 0)
					(length 5.08)
					(name "SIM_DET")
					(number "45")
				)
				(pin bidirectional line
					(at -33.02 -55.88 0)
					(length 5.08)
					(name "COEX0")
					(number "93")
				)
				(pin bidirectional line
					(at -33.02 -58.42 0)
					(length 5.08)
					(name "COEX1")
					(number "92")
				)
				(pin bidirectional line
					(at -33.02 -60.96 0)
					(length 5.08)
					(name "COEX2")
					(number "91")
				)
				(pin power_in line
					(at -5.08 73.66 270)
					(length 5.08)
					(name "VDD1")
					(number "102")
				)
				(pin power_in line
					(at -2.54 73.66 270)
					(length 5.08)
					(name "VDD2")
					(number "22")
				)
				(pin power_in line
					(at 0 73.66 270)
					(length 5.08)
					(name "VDD_GPIO")
					(number "12")
				)
				(pin power_in line
					(at 0 -73.66 90)
					(length 5.08)
					(name "VSS")
					(number "103")
				)
				(pin power_in line
					(at 5.08 73.66 270)
					(length 5.08)
					(name "SIM_1V8")
					(number "49")
				)
				(pin bidirectional line
					(at 33.02 38.1 180)
					(length 5.08)
					(name "ANT")
					(number "61")
				)
				(pin bidirectional line
					(at 33.02 35.56 180)
					(length 5.08)
					(name "AUX")
					(number "64")
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 5.08)
					(name "P0.21/TRACECLK")
					(number "37")
				)
				(pin bidirectional line
					(at 33.02 -7.62 180)
					(length 5.08)
					(name "P0.22/TRACEDATA0")
					(number "38")
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 5.08)
					(name "P0.23/TRACEDATA1")
					(number "39")
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 5.08)
					(name "P0.24/TRACEDATA2")
					(number "40")
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 5.08)
					(name "P0.25/TRACEDATA3")
					(number "42")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 5.08)
					(name "SCLK")
					(number "58")
				)
				(pin bidirectional line
					(at 33.02 -33.02 180)
					(length 5.08)
					(name "SDATA")
					(number "59")
				)
				(pin bidirectional line
					(at 33.02 -45.72 180)
					(length 5.08)
					(name "SWDCLK")
					(number "33")
				)
				(pin bidirectional line
					(at 33.02 -48.26 180)
					(length 5.08)
					(name "SWDIO")
					(number "34")
				)
			)
			(symbol "nRF9160-SIXX_1_0"
				(pin no_connect line
					(at -27.94 -50.8 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "115")
				)
				(pin no_connect line
					(at -27.94 -53.34 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "125")
				)
				(pin no_connect line
					(at -25.4 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "117")
				)
				(pin no_connect line
					(at -22.86 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "114")
				)
				(pin no_connect line
					(at -20.32 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "106")
				)
				(pin no_connect line
					(at -17.78 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "118")
				)
				(pin no_connect line
					(at -15.24 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "107")
				)
				(pin no_connect line
					(at -12.7 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "108")
				)
				(pin no_connect line
					(at -10.16 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "127")
				)
				(pin no_connect line
					(at -7.62 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "70")
				)
				(pin no_connect line
					(at -5.08 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "119")
				)
				(pin no_connect line
					(at -2.54 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "71")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "1")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "11")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "14")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "17")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "21")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "27")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "31")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "36")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "41")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "44")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "47")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "5")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "50")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "52")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "56")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "6")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "60")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "62")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "63")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "65")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "66")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "68")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "69")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "7")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "72")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "74")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "75")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "76")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "77")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "78")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "79")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "8")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "80")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "81")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "82")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "85")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "9")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "90")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "94")
				)
				(pin passive line
					(at 0 -73.66 90)
					(length 5.08)
					(hide yes)
					(name "GND_Shield")
					(number "98")
				)
				(pin no_connect line
					(at 2.54 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "104")
				)
				(pin no_connect line
					(at 5.08 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "122")
				)
				(pin no_connect line
					(at 7.62 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "111")
				)
				(pin no_connect line
					(at 10.16 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "51")
				)
				(pin no_connect line
					(at 12.7 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "73")
				)
				(pin no_connect line
					(at 15.24 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "110")
				)
				(pin no_connect line
					(at 17.78 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "121")
				)
				(pin no_connect line
					(at 20.32 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin no_connect line
					(at 22.86 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "109")
				)
				(pin no_connect line
					(at 25.4 -68.58 90)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "120")
				)
				(pin no_connect line
					(at 27.94 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "112")
				)
				(pin no_connect line
					(at 27.94 -35.56 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "123")
				)
				(pin no_connect line
					(at 27.94 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "124")
				)
				(pin no_connect line
					(at 27.94 -50.8 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "113")
				)
				(pin no_connect line
					(at 27.94 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "105")
				)
				(pin no_connect line
					(at 27.94 -55.88 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "126")
				)
				(pin no_connect line
					(at 27.94 -66.04 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "116")
				)
				(pin passive line
					(at 33.02 58.42 180)
					(length 5.08)
					(name "DEC0")
					(number "13")
				)
				(pin input line
					(at 33.02 15.24 180)
					(length 5.08)
					(name "GPS")
					(number "67")
				)
				(pin power_in line
					(at 33.02 -27.94 180)
					(length 5.08)
					(name "VIO")
					(number "57")
				)
				(pin input line
					(at 33.02 -40.64 180)
					(length 5.08)
					(name "~{RESET}")
					(number "32")
				)
			)
			(symbol "nRF9160-SIXX_1_1")
			(embedded_fonts no)
		)
)
