(footprint "LGA_9161_16.0x10.5mm"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Nordic nRF9161 SiP, 16.0x10.5mm, 159 Pad, generated with kicad-footprint-generator ipc_bga_generator.py, https://docs.nordicsemi.com/bundle/ps_nrf9161/page/nRF9161_html5_keyfeatures.html")
	(tags "LGA 159")
	(solder_paste_ratio -0.15)
	(property "Reference" "REF**"
		(at 0 -6.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "LGA_9161_16.0x10.5mm"
		(at 0 6.25 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -7.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -7.75 -4.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -7.75 -4)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -7.75 -3.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -7.75 -3)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -7.75 -2.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -7.75 -2)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -7.75 -1.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -7.75 -1)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -7.75 -0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -7.75 0)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -7.75 0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -7.75 1)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -7.75 1.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -7.75 2)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -7.75 2.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -7.75 3)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -7.75 3.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -7.75 4)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -7.75 4.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -7.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -7.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -6.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -6.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -5.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -5.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -4.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -4.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -3.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -3.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -2.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -2.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at -1.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at -1.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at -0.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -0.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 0.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 0.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 1.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 1.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 2.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 2.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 3.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 3.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 4.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 4.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 5.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 5.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 6.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at 6.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at 7.25 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at 7.75 5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at 7.75 4.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at 7.75 4)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at 7.75 3.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at 7.75 3)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at 7.75 2.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at 7.75 2)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at 7.75 1.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at 7.75 1)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at 7.75 0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at 7.75 0)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at 7.75 -0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at 7.75 -1)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at 7.75 -1.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at 7.75 -2)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at 7.75 -2.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at 7.75 -3)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "69" smd roundrect
		(at 7.75 -3.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "70" smd roundrect
		(at 7.75 -4)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "71" smd roundrect
		(at 7.75 -4.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "72" smd roundrect
		(at 7.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "73" smd roundrect
		(at 7.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "74" smd roundrect
		(at 6.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "75" smd roundrect
		(at 6.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "76" smd roundrect
		(at 5.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "77" smd roundrect
		(at 5.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "78" smd roundrect
		(at 4.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "79" smd roundrect
		(at 4.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "80" smd roundrect
		(at 3.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "81" smd roundrect
		(at 3.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "82" smd roundrect
		(at 2.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "83" smd roundrect
		(at 2.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "84" smd roundrect
		(at 1.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "85" smd roundrect
		(at 1.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "86" smd roundrect
		(at 0.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "87" smd roundrect
		(at 0.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "88" smd roundrect
		(at -0.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "89" smd roundrect
		(at -0.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "90" smd roundrect
		(at -1.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "91" smd roundrect
		(at -1.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "92" smd roundrect
		(at -2.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "93" smd roundrect
		(at -2.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "94" smd roundrect
		(at -3.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "95" smd roundrect
		(at -3.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "96" smd roundrect
		(at -4.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "97" smd roundrect
		(at -4.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "98" smd roundrect
		(at -5.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "99" smd roundrect
		(at -5.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "100" smd roundrect
		(at -6.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "101" smd roundrect
		(at -6.75 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "102" smd roundrect
		(at -7.25 -5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -6 -3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -6 -1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -6 0)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -6 1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -6 3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -4 -3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -4 -1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -4 0)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -4 1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -4 3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -2 -3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -2 -1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -2 0)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -2 1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -2 3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 0 -3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 0 -1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 0 0)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 0 1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 0 3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 2 -3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 2 -1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 2 0)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 2 1.6)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 2 3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 4 -3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 4 0)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 4 3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 5 -1.6)
		(size 1.6 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 5 1.6)
		(size 1.6 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 6 -3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 6 0)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 6 3.2)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "104" smd roundrect
		(at -5.75 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "105" smd roundrect
		(at -5.25 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "106" smd roundrect
		(at -4.75 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "107" smd roundrect
		(at -4.25 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "108" smd roundrect
		(at -1.75 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "109" smd roundrect
		(at -1.25 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "110" smd roundrect
		(at -0.75 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "111" smd roundrect
		(at -0.25 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "112" smd roundrect
		(at 3.25 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "113" smd roundrect
		(at 3.75 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "114" smd roundrect
		(at 4.25 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "115" smd roundrect
		(at 4.75 4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "116" smd roundrect
		(at 4.75 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "117" smd roundrect
		(at 4.25 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "118" smd roundrect
		(at 3.75 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "119" smd roundrect
		(at 3.25 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "120" smd roundrect
		(at -0.25 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "121" smd roundrect
		(at -0.75 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "122" smd roundrect
		(at -1.25 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "123" smd roundrect
		(at -1.75 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "124" smd roundrect
		(at -4.25 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "125" smd roundrect
		(at -4.75 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "126" smd roundrect
		(at -5.25 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "127" smd roundrect
		(at -5.75 -4.35)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "nordic_nrf9161_sixx.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
