(kicad_symbol_lib (version 20231120) (generator "partreel-gen-mcu")
  (symbol "stm32g431rbtx" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -33.02 31.12 0))
    (property "Value" "STM32G431RBTX" (at 0 -12.15 0))
    (symbol "stm32g431rbtx_1_1"
      (pin power_in line (at -33.02 19.05 0) (length 5.08)
        (name "VBAT")
        (number "1"))
      (pin bidirectional line (at -33.02 16.51 0) (length 5.08)
        (name "PC13")
        (number "2"))
      (pin bidirectional line (at -33.02 13.97 0) (length 5.08)
        (name "PC14-OSC32_IN")
        (number "3"))
      (pin bidirectional line (at -33.02 11.43 0) (length 5.08)
        (name "PC15-OSC32_OUT")
        (number "4"))
      (pin bidirectional line (at -33.02 8.89 0) (length 5.08)
        (name "PF0-OSC_IN")
        (number "5"))
      (pin bidirectional line (at -33.02 6.35 0) (length 5.08)
        (name "PF1-OSC_OUT")
        (number "6"))
      (pin bidirectional line (at -33.02 3.81 0) (length 5.08)
        (name "PG10-NRST")
        (number "7"))
      (pin bidirectional line (at -33.02 1.27 0) (length 5.08)
        (name "PC0")
        (number "8"))
      (pin bidirectional line (at -33.02 -1.27 0) (length 5.08)
        (name "PC1")
        (number "9"))
      (pin bidirectional line (at -33.02 -3.81 0) (length 5.08)
        (name "PC2")
        (number "10"))
      (pin bidirectional line (at -33.02 -6.35 0) (length 5.08)
        (name "PC3")
        (number "11"))
      (pin bidirectional line (at -33.02 -8.89 0) (length 5.08)
        (name "PA0")
        (number "12"))
      (pin bidirectional line (at -33.02 -11.43 0) (length 5.08)
        (name "PA1")
        (number "13"))
      (pin bidirectional line (at -33.02 -13.97 0) (length 5.08)
        (name "PA2")
        (number "14"))
      (pin power_in line (at -33.02 -16.51 0) (length 5.08)
        (name "VSS")
        (number "15"))
      (pin power_in line (at -33.02 -19.05 0) (length 5.08)
        (name "VDD")
        (number "16"))
      (pin bidirectional line (at -19.05 -33.02 90) (length 5.08)
        (name "PA3")
        (number "17"))
      (pin bidirectional line (at -16.51 -33.02 90) (length 5.08)
        (name "PA4")
        (number "18"))
      (pin bidirectional line (at -13.97 -33.02 90) (length 5.08)
        (name "PA5")
        (number "19"))
      (pin bidirectional line (at -11.43 -33.02 90) (length 5.08)
        (name "PA6")
        (number "20"))
      (pin bidirectional line (at -8.89 -33.02 90) (length 5.08)
        (name "PA7")
        (number "21"))
      (pin bidirectional line (at -6.35 -33.02 90) (length 5.08)
        (name "PC4")
        (number "22"))
      (pin bidirectional line (at -3.81 -33.02 90) (length 5.08)
        (name "PC5")
        (number "23"))
      (pin bidirectional line (at -1.27 -33.02 90) (length 5.08)
        (name "PB0")
        (number "24"))
      (pin bidirectional line (at 1.27 -33.02 90) (length 5.08)
        (name "PB1")
        (number "25"))
      (pin bidirectional line (at 3.81 -33.02 90) (length 5.08)
        (name "PB2")
        (number "26"))
      (pin power_in line (at 6.35 -33.02 90) (length 5.08)
        (name "VSSA")
        (number "27"))
      (pin power_in line (at 8.89 -33.02 90) (length 5.08)
        (name "VREF+")
        (number "28"))
      (pin power_in line (at 11.43 -33.02 90) (length 5.08)
        (name "VDDA")
        (number "29"))
      (pin bidirectional line (at 13.97 -33.02 90) (length 5.08)
        (name "PB10")
        (number "30"))
      (pin power_in line (at 16.51 -33.02 90) (length 5.08)
        (name "VSS")
        (number "31"))
      (pin power_in line (at 19.05 -33.02 90) (length 5.08)
        (name "VDD")
        (number "32"))
      (pin bidirectional line (at 33.02 -19.05 180) (length 5.08)
        (name "PB11")
        (number "33"))
      (pin bidirectional line (at 33.02 -16.51 180) (length 5.08)
        (name "PB12")
        (number "34"))
      (pin bidirectional line (at 33.02 -13.97 180) (length 5.08)
        (name "PB13")
        (number "35"))
      (pin bidirectional line (at 33.02 -11.43 180) (length 5.08)
        (name "PB14")
        (number "36"))
      (pin bidirectional line (at 33.02 -8.89 180) (length 5.08)
        (name "PB15")
        (number "37"))
      (pin bidirectional line (at 33.02 -6.35 180) (length 5.08)
        (name "PC6")
        (number "38"))
      (pin bidirectional line (at 33.02 -3.81 180) (length 5.08)
        (name "PC7")
        (number "39"))
      (pin bidirectional line (at 33.02 -1.27 180) (length 5.08)
        (name "PC8")
        (number "40"))
      (pin bidirectional line (at 33.02 1.27 180) (length 5.08)
        (name "PC9")
        (number "41"))
      (pin bidirectional line (at 33.02 3.81 180) (length 5.08)
        (name "PA8")
        (number "42"))
      (pin bidirectional line (at 33.02 6.35 180) (length 5.08)
        (name "PA9")
        (number "43"))
      (pin bidirectional line (at 33.02 8.89 180) (length 5.08)
        (name "PA10")
        (number "44"))
      (pin bidirectional line (at 33.02 11.43 180) (length 5.08)
        (name "PA11")
        (number "45"))
      (pin bidirectional line (at 33.02 13.97 180) (length 5.08)
        (name "PA12")
        (number "46"))
      (pin power_in line (at 33.02 16.51 180) (length 5.08)
        (name "VSS")
        (number "47"))
      (pin power_in line (at 33.02 19.05 180) (length 5.08)
        (name "VDD")
        (number "48"))
      (pin bidirectional line (at 19.05 33.02 270) (length 5.08)
        (name "PA13")
        (number "49"))
      (pin bidirectional line (at 16.51 33.02 270) (length 5.08)
        (name "PA14")
        (number "50"))
      (pin bidirectional line (at 13.97 33.02 270) (length 5.08)
        (name "PA15")
        (number "51"))
      (pin bidirectional line (at 11.43 33.02 270) (length 5.08)
        (name "PC10")
        (number "52"))
      (pin bidirectional line (at 8.89 33.02 270) (length 5.08)
        (name "PC11")
        (number "53"))
      (pin bidirectional line (at 6.35 33.02 270) (length 5.08)
        (name "PC12")
        (number "54"))
      (pin bidirectional line (at 3.81 33.02 270) (length 5.08)
        (name "PD2")
        (number "55"))
      (pin bidirectional line (at 1.27 33.02 270) (length 5.08)
        (name "PB3")
        (number "56"))
      (pin bidirectional line (at -1.27 33.02 270) (length 5.08)
        (name "PB4")
        (number "57"))
      (pin bidirectional line (at -3.81 33.02 270) (length 5.08)
        (name "PB5")
        (number "58"))
      (pin bidirectional line (at -6.35 33.02 270) (length 5.08)
        (name "PB6")
        (number "59"))
      (pin bidirectional line (at -8.89 33.02 270) (length 5.08)
        (name "PB7")
        (number "60"))
      (pin bidirectional line (at -11.43 33.02 270) (length 5.08)
        (name "PB8-BOOT0")
        (number "61"))
      (pin bidirectional line (at -13.97 33.02 270) (length 5.08)
        (name "PB9")
        (number "62"))
      (pin power_in line (at -16.51 33.02 270) (length 5.08)
        (name "VSS")
        (number "63"))
      (pin power_in line (at -19.05 33.02 270) (length 5.08)
        (name "VDD")
        (number "64"))
    )))