(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_Module_ESP8266_2491"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_Module_ESP8266_2491"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_Module_ESP8266_2491"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Adafruit%20PDFs/2491_Web.pdf"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "WiFi Development Tools - 802.11 ESP8266 SMT Module - ESP-12F"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "2491"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Adafruit"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, SMT, TRANSCEIVER, MODULE, WIFI, BLUETOOTH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_Module_ESP8266_2491_1_1"
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "RST")
					(number "1")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "ADC")
					(number "2")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "IO16")
					(number "4")
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "IO14")
					(number "5")
				)
				(pin bidirectional line
					(at 15.24 -15.24 180)
					(length 2.54)
					(name "IO12")
					(number "6")
				)
				(pin bidirectional line
					(at 15.24 -12.7 180)
					(length 2.54)
					(name "IO13")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 15.24 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 2.54)
					(name "IO15")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "IO2")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "IO0")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "IO4")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "IO5")
					(number "14")
				)
				(pin output line
					(at 15.24 0 180)
					(length 2.54)
					(name "RXD0")
					(number "15")
				)
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "TXD0")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
