(footprint "Antenna_ANT-LTE-CER-T"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 8 3.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Antenna_ANT-LTE-CER-T"
		(at -18.6 3.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "KEEPOUT AREA"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at -20.25 6.311 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -20.25 7.511 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -20.25 8.711 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 4.9 2.25)
		(size 1.2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.975 2.25)
		(size 1.65 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 6.825 2.25)
		(size 1.65 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP1" smd rect
		(at -18 0)
		(size 4 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP2" smd rect
		(at 18 0)
		(size 4 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "KEEPOUT")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 22.5 9) (xy 7.75 9) (xy 7.75 1.25) (xy 2 1.25) (xy 2 9) (xy -22.5 9) (xy -22.5 -4) (xy 22.5 -4)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_ant_lte_cer_t.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
