(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_ATWINC1500-MR210PB"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_ATWINC1500-MR210PB"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_ATWINC1500-MR210PB"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://4donline.ihs.com/images/VipMasterIC/IC/MCHP/MCHP-S-A0001584156/MCHP-S-A0001584156-1.pdf?hkey=6D3A4C79FDBF58556ACFDE234799DDF0"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF Transceiver Module, 16/64-QAM, (D)(B)(Q)PSK, OFDM, 72.2Mbps, 2.472GHz, 18.5dBm, 3V to 4.2V, SPI"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ATWINC1500-MR210PB"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_ATWINC1500-MR210PB_1_1"
				(pin bidirectional line
					(at 26.67 -22.86 180)
					(length 2.54)
					(name "GPIO_6")
					(number "1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "I2C_SCL")
					(number "2")
				)
				(pin bidirectional line
					(at 26.67 0 180)
					(length 2.54)
					(name "I2C_SDA")
					(number "3")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RESET_N")
					(number "4")
				)
				(pin no_connect line
					(at 24.13 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 24.13 -29.21 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 24.13 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 24.13 -26.67 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SPI_CFG")
					(number "10")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "WAKE")
					(number "11")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GND")
					(number "12")
				)
				(pin output line
					(at 26.67 -2.54 180)
					(length 2.54)
					(name "IRQN")
					(number "13")
				)
				(pin output line
					(at 26.67 -7.62 180)
					(length 2.54)
					(name "UART_TXD")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SPI_RXD")
					(number "15")
				)
				(pin bidirectional line
					(at 26.67 -5.08 180)
					(length 2.54)
					(name "SPI_SSN")
					(number "16")
				)
				(pin bidirectional line
					(at 26.67 -10.16 180)
					(length 2.54)
					(name "SPI_TXD")
					(number "17")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SPI_SCK")
					(number "18")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "UART_RXD")
					(number "19")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VBATT")
					(number "20")
				)
				(pin bidirectional line
					(at 26.67 -12.7 180)
					(length 2.54)
					(name "GPIO_1/RTC")
					(number "21")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "CHIP_EN")
					(number "22")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDIO")
					(number "23")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "1P3V_TP")
					(number "24")
				)
				(pin bidirectional line
					(at 26.67 -15.24 180)
					(length 2.54)
					(name "GPIO_3")
					(number "25")
				)
				(pin bidirectional line
					(at 26.67 -17.78 180)
					(length 2.54)
					(name "GPIO_4")
					(number "26")
				)
				(pin bidirectional line
					(at 26.67 -20.32 180)
					(length 2.54)
					(name "GPIO_5")
					(number "27")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PADDLE_GND")
					(number "29")
				)
			)
			(embedded_fonts no)
		)
)
