(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_Bluetooth_AW-CM389NF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 64.77 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_Bluetooth_AW-CM389NF"
				(at 64.77 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_Bluetooth_AW-CM389NF"
				(at 64.77 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.azurewave.com/img/wireless-modules/AW-CM389NF_DS_0B_A_STD.pdf"
				(at 64.77 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "WLAN+BTCombo Module IEEE 802.11a/b/g/n/ac Bluetooth v4.0(BLE)"
				(at 64.77 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "AzureWave Technologies"
				(at 64.77 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AW-CM389NF"
				(at 64.77 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 64.77 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 64.77 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_Bluetooth_AW-CM389NF_1_1"
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "TMS")
					(number "1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "TCK")
					(number "2")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "TDI")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "3.3V")
					(number "4")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "3.3V")
					(number "5")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(name "GND")
					(number "6")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TDO")
					(number "7")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "CONFIG_HOST[0]")
					(number "8")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "CONFIG_HOST[1]")
					(number "9")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "CONFIG_HOST[2]")
					(number "10")
				)
				(pin passive line
					(at 35.56 -17.78 180)
					(length 3.81)
					(name "GPIO[1]")
					(number "11")
					(alternate "LTE_SOUT" passive line)
				)
				(pin passive line
					(at 35.56 -20.32 180)
					(length 3.81)
					(name "GPIO[2]")
					(number "12")
					(alternate "LTE_SIN" passive line)
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "CONFIG_HOST[3]")
					(number "13")
				)
				(pin passive line
					(at 35.56 -40.64 180)
					(length 3.81)
					(name "GPIO[10]")
					(number "14")
				)
				(pin no_connect line
					(at 31.75 -64.77 180)
					(length 3.81)
					(hide yes)
					(name "NC_1")
					(number "15")
				)
				(pin no_connect line
					(at 31.75 -66.04 180)
					(length 3.81)
					(hide yes)
					(name "NC_2")
					(number "16")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "17")
				)
				(pin no_connect line
					(at 31.75 -67.31 180)
					(length 3.81)
					(hide yes)
					(name "NC_3")
					(number "18")
				)
				(pin no_connect line
					(at 31.75 -68.58 180)
					(length 3.81)
					(hide yes)
					(name "NC_4")
					(number "19")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "20")
				)
				(pin no_connect line
					(at 31.75 -69.85 180)
					(length 3.81)
					(hide yes)
					(name "NC_5")
					(number "21")
				)
				(pin no_connect line
					(at 31.75 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "NC_6")
					(number "22")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin no_connect line
					(at 31.75 -72.39 180)
					(length 3.81)
					(hide yes)
					(name "NC_7")
					(number "24")
				)
				(pin no_connect line
					(at 31.75 -73.66 180)
					(length 3.81)
					(hide yes)
					(name "NC_8")
					(number "25")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "SLP_CLK")
					(number "27")
				)
				(pin passive line
					(at 35.56 -48.26 180)
					(length 3.81)
					(name "GPIO[13]")
					(number "28")
					(alternate "BT_IRQ(O)" passive line)
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PCIE_WAKEN")
					(number "29")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PCIE_CLKREQN")
					(number "30")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 3.81)
					(name "GPIO[12]")
					(number "31")
					(alternate "PCIE_PERSTN" passive line)
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "32")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PCIE_RCLK_N")
					(number "33")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PCIE_RCLK_P")
					(number "34")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "35")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PCIE_TX_N")
					(number "36")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PCIE_TX_P")
					(number "37")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "38")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PCIE_RX_N")
					(number "39")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PCIE_RX_P")
					(number "40")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin passive line
					(at 35.56 -15.24 180)
					(length 3.81)
					(name "GPIO[0]")
					(number "42")
					(alternate "CLK_REQ" passive line)
				)
				(pin passive line
					(at 35.56 -43.18 180)
					(length 3.81)
					(name "GPIO[11]")
					(number "43")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VIO_SD")
					(number "44")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PDN")
					(number "45")
				)
				(pin passive line
					(at 35.56 -22.86 180)
					(length 3.81)
					(name "GPIO[3]")
					(number "46")
					(alternate "WLAN_IRQ(O)" passive line)
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "SD_DAT[3]")
					(number "47")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "SD_DAT[2]")
					(number "48")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "SD_DAT[1]")
					(number "49")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "SD_DAT[0]")
					(number "50")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "SD_CMD")
					(number "51")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "SD_CLK")
					(number "52")
				)
				(pin no_connect line
					(at 31.75 -74.93 180)
					(length 3.81)
					(hide yes)
					(name "NC_9")
					(number "53")
				)
				(pin passive line
					(at 35.56 -30.48 180)
					(length 3.81)
					(name "GPIO[6]")
					(number "54")
				)
				(pin passive line
					(at 35.56 -25.4 180)
					(length 3.81)
					(name "GPIO[4]")
					(number "55")
				)
				(pin passive line
					(at 35.56 -27.94 180)
					(length 3.81)
					(name "GPIO[5]")
					(number "56")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 3.81)
					(name "GPIO[7]")
					(number "57")
				)
				(pin passive line
					(at 35.56 -60.96 180)
					(length 3.81)
					(name "GPIO[22]")
					(number "58")
					(alternate "PCM_SYNC" passive line)
				)
				(pin passive line
					(at 35.56 -53.34 180)
					(length 3.81)
					(name "GPIO[19]")
					(number "59")
					(alternate "PCM_IN" passive line)
				)
				(pin passive line
					(at 35.56 -55.88 180)
					(length 3.81)
					(name "GPIO[20]")
					(number "60")
					(alternate "PCM_OUT" passive line)
				)
				(pin passive line
					(at 35.56 -58.42 180)
					(length 3.81)
					(name "GPIO[21]")
					(number "61")
					(alternate "PCM_CLK" passive line)
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "62")
				)
				(pin passive line
					(at 35.56 -50.8 180)
					(length 3.81)
					(name "GPIO[14]")
					(number "63")
				)
				(pin passive line
					(at 35.56 -35.56 180)
					(length 3.81)
					(name "GPIO[8]")
					(number "64")
					(alternate "WLAN_LED" passive line)
				)
				(pin passive line
					(at 35.56 -38.1 180)
					(length 3.81)
					(name "GPIO[9]")
					(number "65")
					(alternate "BT_LED" passive line)
				)
				(pin no_connect line
					(at 31.75 -76.2 180)
					(length 3.81)
					(hide yes)
					(name "NC_10")
					(number "66")
				)
				(pin no_connect line
					(at 31.75 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "NC_11")
					(number "67")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "68")
				)
				(pin passive line
					(at 35.56 -7.62 180)
					(length 3.81)
					(name "USB_DN")
					(number "69")
				)
				(pin passive line
					(at 35.56 -10.16 180)
					(length 3.81)
					(name "USB_DP")
					(number "70")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "71")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 3.81)
					(name "3V3_USB")
					(number "72")
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 3.81)
					(name "VIO")
					(number "73")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "74")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "75")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "76")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "77")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "78")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "79")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "80")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "81")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "82")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "83")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "84")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "85")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "86")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "87")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "88")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "89")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "90")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "91")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "92")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "93")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "94")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "95")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "96")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G2")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G4")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G9")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G10")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G12")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G13")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G14")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G15")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G16")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G17")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G18")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G19")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G20")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G21")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G22")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G23")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G24")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G25")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G26")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G27")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G28")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G29")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G30")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G31")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G32")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G33")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G34")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G35")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G36")
				)
			)
			(embedded_fonts no)
		)
)
