(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_BC118_1103394"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 58.42 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_BC118_1103394"
				(at 58.42 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_BC118_1103394"
				(at 58.42 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/BlueCreation%20PDFs/BC118_DS.pdf"
				(at 58.42 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver module"
				(at 58.42 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BC118_1103394"
				(at 58.42 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Sierra Wireless"
				(at 58.42 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 58.42 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_BC118_1103394_1_1"
				(pin power_in line
					(at 31.75 -25.4 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "AIO_2")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "AIO_1")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "AIO_0")
					(number "5")
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 2.54)
					(name "UART_TX")
					(number "6")
				)
				(pin bidirectional line
					(at 31.75 -2.54 180)
					(length 2.54)
					(name "UART_RX")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PIO_3")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PIO_4")
					(number "9")
				)
				(pin bidirectional line
					(at 31.75 -5.08 180)
					(length 2.54)
					(name "PIO_5/SPI_CLK")
					(number "10")
				)
				(pin bidirectional line
					(at 31.75 -7.62 180)
					(length 2.54)
					(name "PIO_6/SPI_CSB")
					(number "11")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at 31.75 -10.16 180)
					(length 2.54)
					(name "PIO_6/SPI_MOSI")
					(number "14")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "15")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_PADS")
					(number "17")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PIO_8")
					(number "19")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SPI_PCM#")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PIO_2")
					(number "21")
				)
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 2.54)
					(name "I2C_SCL")
					(number "22")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "24")
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "I2C_SDA")
					(number "25")
				)
				(pin bidirectional line
					(at 31.75 -17.78 180)
					(length 2.54)
					(name "PIO_9")
					(number "26")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VBAT")
					(number "27")
				)
				(pin bidirectional line
					(at 31.75 -20.32 180)
					(length 2.54)
					(name "PIO_10")
					(number "28")
				)
				(pin bidirectional line
					(at 31.75 -22.86 180)
					(length 2.54)
					(name "PIO_11")
					(number "29")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "WAKE")
					(number "30")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "31")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "32")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "34")
				)
				(pin passive line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "35")
				)
			)
			(embedded_fonts no)
		)
)
