(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_BC127-1103383"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_BC127-1103383"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_BC127-1103383"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/2282/BC127_-HD_-EXT_TechSpec_4-9-17.pdf"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver module"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BC127-1103383"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Sierra Wireless"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_BC127-1103383_1_1"
				(pin power_in line
					(at 29.21 -55.88 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 29.21 -45.72 180)
					(length 2.54)
					(name "PIO_6")
					(number "5")
				)
				(pin bidirectional line
					(at 29.21 -43.18 180)
					(length 2.54)
					(name "PIO_7")
					(number "6")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "CAP_SENSE_1")
					(number "7")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CAP_SENSE_4")
					(number "8")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "CAP_SENSE_3")
					(number "9")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CAP_SENSE_2")
					(number "10")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 2.54)
					(name "AIO_1")
					(number "12")
				)
				(pin output line
					(at 29.21 -5.08 180)
					(length 2.54)
					(name "SPKR_LN")
					(number "13")
				)
				(pin output line
					(at 29.21 -2.54 180)
					(length 2.54)
					(name "SPKR_LP")
					(number "14")
				)
				(pin output line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "SPKR_RN")
					(number "15")
				)
				(pin output line
					(at 29.21 -7.62 180)
					(length 2.54)
					(name "SPKR_RP")
					(number "16")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "MIC_BIAS_A")
					(number "17")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "MIC_RN")
					(number "18")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "MIC_RP")
					(number "19")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "MIC_LN")
					(number "20")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "MIC_LP")
					(number "21")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PIO_0")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PIO_1")
					(number "24")
				)
				(pin bidirectional line
					(at 29.21 -48.26 180)
					(length 2.54)
					(name "PIO_5")
					(number "25")
				)
				(pin bidirectional line
					(at 29.21 -50.8 180)
					(length 2.54)
					(name "PIO_4")
					(number "26")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "VREGEN")
					(number "28")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "CHG_EXT")
					(number "29")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCHG")
					(number "30")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "VBAT_SENSE")
					(number "31")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VBAT")
					(number "32")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD_PADS")
					(number "33")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "3.3_VSB")
					(number "34")
				)
				(pin bidirectional line
					(at 29.21 -15.24 180)
					(length 2.54)
					(name "USB_N")
					(number "35")
				)
				(pin bidirectional line
					(at 29.21 -12.7 180)
					(length 2.54)
					(name "USB_P")
					(number "36")
				)
				(pin output line
					(at 29.21 -17.78 180)
					(length 2.54)
					(name "LED_0")
					(number "37")
				)
				(pin output line
					(at 29.21 -20.32 180)
					(length 2.54)
					(name "LED_1")
					(number "38")
				)
				(pin output line
					(at 29.21 -22.86 180)
					(length 2.54)
					(name "LED_2")
					(number "39")
				)
				(pin bidirectional line
					(at 29.21 -25.4 180)
					(length 2.54)
					(name "UART_CTS")
					(number "40")
				)
				(pin bidirectional line
					(at 29.21 -27.94 180)
					(length 2.54)
					(name "UART_TX")
					(number "41")
				)
				(pin bidirectional line
					(at 29.21 -30.48 180)
					(length 2.54)
					(name "UART_RX")
					(number "42")
				)
				(pin bidirectional line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "UART_RTS")
					(number "43")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "RST#")
					(number "44")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "SPI_PCM#")
					(number "45")
				)
				(pin bidirectional line
					(at 29.21 -35.56 180)
					(length 2.54)
					(name "PCM_SYNC")
					(number "46")
				)
				(pin bidirectional line
					(at 29.21 -38.1 180)
					(length 2.54)
					(name "PCM_CLK")
					(number "47")
				)
				(pin output line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "PCM_OUT")
					(number "48")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PCM_IN")
					(number "49")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "PIO_2")
					(number "50")
				)
				(pin bidirectional line
					(at 29.21 -53.34 180)
					(length 2.54)
					(name "PIO_3")
					(number "51")
				)
			)
			(embedded_fonts no)
		)
)
