(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_BL600-SA"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_BL600-SA"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_BL600-SA"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://assets.lairdtech.com/home/brandworld/files/Product%20Brief%20-%20Bx600%20Breakout%20Boards%20and%20DVK-BL600.pdf"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "smartBASIC Single Mode BLE Module with Internal Antenna"
				(at 50.8 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Laird"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BL600-SA"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_BL600-SA_1_1"
				(pin power_in line
					(at 24.13 -41.91 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SIO_1/AN")
					(number "2")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SIO_2/AIN")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "SIO_3/AIN")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "SIO_4/AIN")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "SIO_5/AIN")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SIO_6/AIN")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "SIO_7")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "10")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 2.54)
					(name "SIO_8")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "SIO_9")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 2.54)
					(name "SIO_10")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "SIO_11")
					(number "15")
				)
				(pin bidirectional line
					(at 24.13 0 180)
					(length 2.54)
					(name "SIO_12")
					(number "16")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "17")
				)
				(pin bidirectional line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "SIO_13")
					(number "18")
				)
				(pin bidirectional line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "SIO_14")
					(number "19")
				)
				(pin bidirectional line
					(at 24.13 -7.62 180)
					(length 2.54)
					(name "SIO_15")
					(number "20")
				)
				(pin bidirectional line
					(at 24.13 -10.16 180)
					(length 2.54)
					(name "SIO_16")
					(number "21")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "nRESET")
					(number "22")
				)
				(pin no_connect line
					(at 2.54 -36.83 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "23")
				)
				(pin bidirectional line
					(at 24.13 -12.7 180)
					(length 2.54)
					(name "SIO_17")
					(number "24")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 2.54)
					(name "SIO_18")
					(number "25")
				)
				(pin bidirectional line
					(at 24.13 -17.78 180)
					(length 2.54)
					(name "SIO_19")
					(number "26")
				)
				(pin no_connect line
					(at 2.54 -39.37 0)
					(length 2.54)
					(hide yes)
					(name "SIO_20/NC")
					(number "27")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "29")
				)
				(pin no_connect line
					(at 2.54 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "31")
				)
				(pin bidirectional line
					(at 24.13 -20.32 180)
					(length 2.54)
					(name "SIO_21")
					(number "32")
				)
				(pin bidirectional line
					(at 24.13 -22.86 180)
					(length 2.54)
					(name "SIO_22")
					(number "33")
				)
				(pin bidirectional line
					(at 24.13 -25.4 180)
					(length 2.54)
					(name "SIO_23")
					(number "34")
				)
				(pin bidirectional line
					(at 24.13 -27.94 180)
					(length 2.54)
					(name "SIO_24")
					(number "35")
				)
				(pin bidirectional line
					(at 24.13 -30.48 180)
					(length 2.54)
					(name "SIO_25")
					(number "36")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "37")
				)
				(pin no_connect line
					(at 2.54 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "SIO_26/NC")
					(number "38")
				)
				(pin no_connect line
					(at 2.54 -41.91 0)
					(length 2.54)
					(hide yes)
					(name "SIO_27/NC")
					(number "39")
				)
				(pin bidirectional line
					(at 24.13 -33.02 180)
					(length 2.54)
					(name "SIO_28")
					(number "40")
				)
				(pin bidirectional line
					(at 24.13 -35.56 180)
					(length 2.54)
					(name "SIO_29")
					(number "41")
				)
				(pin bidirectional line
					(at 24.13 -38.1 180)
					(length 2.54)
					(name "SIO_30")
					(number "42")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SIO_0")
					(number "44")
				)
			)
			(embedded_fonts no)
		)
)
