(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_BLE112-A-V1"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_BLE112-A-V1"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_BLE112-A-V1"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.silabs.com/documents/login/data-sheets/BLE112-DataSheet.pdf"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Class 2 Bluetooth® Low Energy Module with Integrated Chip Antenna and Software Version 1.0"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BLE112-A-V1"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Silicon Labs"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_BLE112-A-V1_1_1"
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVDD")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "3")
				)
				(pin bidirectional line
					(at 20.32 0 180)
					(length 2.54)
					(name "P2_2")
					(number "4")
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "P2_1")
					(number "5")
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "P2_0")
					(number "6")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "P1_7")
					(number "7")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "P1_6")
					(number "8")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD_USB")
					(number "9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "10")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "USB+")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "USB-")
					(number "12")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "P1_5")
					(number "13")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "P1_4")
					(number "14")
				)
				(pin bidirectional line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "P1_3")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "P1_2")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -27.94 180)
					(length 2.54)
					(name "P1_1")
					(number "17")
				)
				(pin bidirectional line
					(at 20.32 -30.48 180)
					(length 2.54)
					(name "P1_0")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "P0_7")
					(number "19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "DVDD")
					(number "20")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "P0_6")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "P0_5")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "P0_4")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "P0_3")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "P0_2")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "P0_1")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "P0_0")
					(number "28")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RESET")
					(number "29")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "30")
				)
			)
			(embedded_fonts no)
		)
)
