(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_BMD-300-A-R"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_BMD-300-A-R"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_BMD-300-A-R"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/1025/BMD_300_DataSheet_UBX_19033350-3180233.pdf"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver module"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BMD-300-A-R"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Rigado"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_BMD-300-A-R_1_1"
				(pin power_in line
					(at 21.59 -43.18 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "P0.25")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "P0.26")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "P0.27")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "P0.28")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "P0.29")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "P0.30")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "P0.31")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "P0.00")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "P0.01")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "P0.02")
					(number "15")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "17")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "P0.03")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PO.04")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PO.05")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PO.06")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PO.07")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PO.08")
					(number "24")
				)
				(pin bidirectional line
					(at 21.59 0 180)
					(length 2.54)
					(name "PO.09")
					(number "25")
				)
				(pin bidirectional line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "PO.10")
					(number "26")
				)
				(pin bidirectional line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "PO.11")
					(number "27")
				)
				(pin bidirectional line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "PO.12")
					(number "28")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "29")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "30")
				)
				(pin bidirectional line
					(at 21.59 -10.16 180)
					(length 2.54)
					(name "PO.13")
					(number "31")
				)
				(pin bidirectional line
					(at 21.59 -12.7 180)
					(length 2.54)
					(name "PO.14")
					(number "32")
				)
				(pin bidirectional line
					(at 21.59 -15.24 180)
					(length 2.54)
					(name "PO.15")
					(number "33")
				)
				(pin bidirectional line
					(at 21.59 -17.78 180)
					(length 2.54)
					(name "PO.16")
					(number "34")
				)
				(pin bidirectional line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "PO.17")
					(number "35")
				)
				(pin bidirectional line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "PO.18")
					(number "36")
				)
				(pin bidirectional line
					(at 21.59 -25.4 180)
					(length 2.54)
					(name "PO.19")
					(number "37")
				)
				(pin bidirectional line
					(at 21.59 -27.94 180)
					(length 2.54)
					(name "PO.20")
					(number "38")
				)
				(pin bidirectional line
					(at 21.59 -30.48 180)
					(length 2.54)
					(name "PO.21")
					(number "39")
				)
				(pin bidirectional line
					(at 21.59 -33.02 180)
					(length 2.54)
					(name "PO.22")
					(number "40")
				)
				(pin bidirectional line
					(at 21.59 -35.56 180)
					(length 2.54)
					(name "PO.23")
					(number "41")
				)
				(pin bidirectional line
					(at 21.59 -38.1 180)
					(length 2.54)
					(name "PO.24")
					(number "42")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SWCLK")
					(number "43")
				)
				(pin bidirectional line
					(at 21.59 -40.64 180)
					(length 2.54)
					(name "SWDIO")
					(number "44")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "46")
				)
				(pin passive line
					(at 21.59 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "47")
				)
			)
			(embedded_fonts no)
		)
)
