(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_CYBLE-022001-00"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_CYBLE-022001-00"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_CYBLE-022001-00"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.cypress.com/file/140791/download"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PSoC® Module, Bluetooth® v4.1 Low Energy Communication, 2.4GHz, Single Mode"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CYBLE-022001-00"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Cypress Semiconductor"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_CYBLE-022001-00_1_1"
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "P4.1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "P5.1")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "P5.0")
					(number "4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDR")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "P1.6")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "P0.7")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "P0.4")
					(number "8")
				)
				(pin bidirectional line
					(at 17.78 0 180)
					(length 2.54)
					(name "P0.5")
					(number "9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "10")
				)
				(pin bidirectional line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "P0.6")
					(number "11")
				)
				(pin bidirectional line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "P1.7")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "13")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "XRES")
					(number "14")
				)
				(pin bidirectional line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "P3.5")
					(number "15")
				)
				(pin bidirectional line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "P3.4")
					(number "16")
				)
				(pin bidirectional line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "P3.7")
					(number "17")
				)
				(pin bidirectional line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "P1.4")
					(number "18")
				)
				(pin bidirectional line
					(at 17.78 -17.78 180)
					(length 2.54)
					(name "P1.5")
					(number "19")
				)
				(pin bidirectional line
					(at 17.78 -20.32 180)
					(length 2.54)
					(name "P3.6")
					(number "20")
				)
				(pin bidirectional line
					(at 17.78 -22.86 180)
					(length 2.54)
					(name "P4.0")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
