(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RF_Location_DWM1000"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RF_Location_DWM1000"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RF_Location_DWM1000"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/412/DWM1000_Data_Sheet-1950396.pdf"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver module"
				(at 45.72 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DWM1000"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "DecaWave"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RF_Location_DWM1000_1_1"
				(pin output line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "EXTON")
					(number "1")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "WAKEUP")
					(number "2")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "RSTn")
					(number "3")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "GPIO7")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDAON")
					(number "5")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD3V3")
					(number "6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD3V3")
					(number "7")
				)
				(pin passive line
					(at 25.4 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "GPIO6")
					(number "9")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "GPIO5")
					(number "10")
				)
				(pin bidirectional line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "GPIO4")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GPIO3")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GPIO2")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GPIO1")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GPIO0")
					(number "15")
				)
				(pin power_in line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "16")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SPICSn")
					(number "17")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SPIMOSI")
					(number "18")
				)
				(pin output line
					(at 25.4 0 180)
					(length 2.54)
					(name "SPIMISO")
					(number "19")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SPICLK")
					(number "20")
				)
				(pin passive line
					(at 25.4 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "IRQ/GPIO8")
					(number "22")
				)
				(pin passive line
					(at 25.4 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin passive line
					(at 25.4 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
