(footprint "WiFi_Bluetooth_Module_LBEE5PK2AE"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "WiFi_Bluetooth_Module_LBEE5PK2AE"
		(at 0 5.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -4.25 6.3 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.25 7.5 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.25 8.7 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.3 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "2" smd roundrect
		(at -2.7 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "3" smd roundrect
		(at -2.1 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "4" smd roundrect
		(at -1.5 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "5" smd roundrect
		(at -0.9 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "6" smd roundrect
		(at -0.3 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "7" smd roundrect
		(at 0.3 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "8" smd roundrect
		(at 0.9 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "9" smd roundrect
		(at 1.5 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "10" smd roundrect
		(at 2.1 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "11" smd roundrect
		(at 2.7 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "12" smd roundrect
		(at 3.3 3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "13" smd roundrect
		(at 3.475 2.7 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "14" smd roundrect
		(at 3.475 2.1 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "15" smd roundrect
		(at 3.475 1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "16" smd roundrect
		(at 3.475 0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "17" smd roundrect
		(at 3.475 0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "18" smd roundrect
		(at 3.475 -0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "19" smd roundrect
		(at 3.475 -0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "20" smd roundrect
		(at 3.475 -1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "21" smd roundrect
		(at 3.475 -2.1 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "22" smd roundrect
		(at 3.475 -2.7 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "23" smd roundrect
		(at 3.3 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "24" smd roundrect
		(at 2.7 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "25" smd roundrect
		(at 2.1 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "26" smd roundrect
		(at 1.5 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "27" smd roundrect
		(at 0.9 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "28" smd roundrect
		(at 0.3 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "29" smd roundrect
		(at -0.3 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "30" smd roundrect
		(at -0.9 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "31" smd roundrect
		(at -1.5 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "32" smd roundrect
		(at -2.1 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "33" smd roundrect
		(at -2.7 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "34" smd roundrect
		(at -3.3 -3.375 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "35" smd roundrect
		(at -3.475 -2.7 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "36" smd roundrect
		(at -3.475 -2.1 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "37" smd roundrect
		(at -3.475 -1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "38" smd roundrect
		(at -3.475 -0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "39" smd roundrect
		(at -3.475 -0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "40" smd roundrect
		(at -3.475 0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "41" smd roundrect
		(at -3.475 0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "42" smd roundrect
		(at -3.475 1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "43" smd roundrect
		(at -3.475 2.1 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "44" smd roundrect
		(at -3.475 2.7 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "45" smd roundrect
		(at -1.5 2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "46" smd roundrect
		(at -0.9 2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "47" smd roundrect
		(at -0.3 2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "48" smd roundrect
		(at 0.3 2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "49" smd roundrect
		(at 0.9 2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "50" smd roundrect
		(at 1.5 2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "51" smd roundrect
		(at 2.275 1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "52" smd roundrect
		(at 2.275 0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "53" smd roundrect
		(at 2.275 0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "54" smd roundrect
		(at 2.275 -0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "55" smd roundrect
		(at 2.275 -0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "56" smd roundrect
		(at 2.275 -1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "57" smd roundrect
		(at 1.5 -2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "58" smd roundrect
		(at 0.9 -2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "59" smd roundrect
		(at 0.3 -2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "60" smd roundrect
		(at -0.3 -2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "61" smd roundrect
		(at -0.9 -2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "62" smd roundrect
		(at -1.5 -2.175 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "63" smd roundrect
		(at -2.275 -1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "64" smd roundrect
		(at -2.275 -0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "65" smd roundrect
		(at -2.275 -0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "66" smd roundrect
		(at -2.275 0.3 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "67" smd roundrect
		(at -2.275 0.9 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "68" smd roundrect
		(at -2.275 1.5 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "69" smd roundrect
		(at -1 1 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "70" smd roundrect
		(at 0 1 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "71" smd roundrect
		(at 1 1 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "72" smd roundrect
		(at 1 0 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "73" smd roundrect
		(at 1 -1 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "74" smd roundrect
		(at 0 -1 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "75" smd roundrect
		(at -1 -1 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "76" smd roundrect
		(at -1 0 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(pad "77" smd roundrect
		(at 0 0 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.18)
	)
	(embedded_fonts no)
	(model "antmicro_lbee5pk2ae.glb"
		(offset
			(xyz 0 0 0.04)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
