(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_Bluetooth_LBEE5PK2AE"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_Bluetooth_LBEE5PK2AE"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_Bluetooth_LBEE5PK2AE"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.murata.com/products/productdata/8816428220446/type2ae.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "WiFi and Bluetooth Module"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Murata"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LBEE5PK2AE"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "MODULE, WIFI, BLUETOOTH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_Bluetooth_LBEE5PK2AE_1_1"
				(pin power_in line
					(at 38.1 -67.31 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_out line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SR_VLX")
					(number "2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VBAT")
					(number "3")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "WL_REG_EN")
					(number "4")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "LPO_IN")
					(number "5")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "BT_PCM_IN")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "BT_PCM_CLK")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "BT_PCM_SYNC")
					(number "8")
				)
				(pin output line
					(at 0 -39.37 0)
					(length 2.54)
					(name "BT_PCM_OUT")
					(number "9")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 2.54)
					(name "BT_UART_TXD")
					(number "10")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "BT_UART_CTS_N")
					(number "11")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "BT_UART_RXD")
					(number "12")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 2.54)
					(name "BT_UART_RTS_N")
					(number "13")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "16")
				)
				(pin bidirectional line
					(at 38.1 -31.75 180)
					(length 2.54)
					(name "BT_HOST_WAKE")
					(number "17")
				)
				(pin bidirectional line
					(at 38.1 -34.29 180)
					(length 2.54)
					(name "BT_GPIO_2")
					(number "18")
				)
				(pin bidirectional line
					(at 38.1 -36.83 180)
					(length 2.54)
					(name "BT_GPIO_3")
					(number "19")
				)
				(pin bidirectional line
					(at 38.1 -39.37 180)
					(length 2.54)
					(name "BT_GPIO_5")
					(number "20")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin bidirectional line
					(at 38.1 0 180)
					(length 2.54)
					(name "WL_ANT")
					(number "22")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "24")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RF_SW_CTRL_5")
					(number "25")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RF_SW_CTRL_0")
					(number "26")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 2.54)
					(name "SDIO_CMD")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 2.54)
					(name "SDIO_DATA_1")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 2.54)
					(name "SDIO_DATA_0")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 2.54)
					(name "SDIO_DATA_3")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 2.54)
					(name "SDIO_DATA_2")
					(number "32")
				)
				(pin input line
					(at 0 -67.31 0)
					(length 2.54)
					(name "SDIO_CLK")
					(number "33")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "34")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "42")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VIN_LDO")
					(number "43")
				)
				(pin bidirectional line
					(at 38.1 -41.91 180)
					(length 2.54)
					(name "GPIO_1")
					(number "45")
				)
				(pin bidirectional line
					(at 38.1 -48.26 180)
					(length 2.54)
					(name "USB2_DM")
					(number "46")
				)
				(pin bidirectional line
					(at 38.1 -45.72 180)
					(length 2.54)
					(name "USB2_DP")
					(number "47")
				)
				(pin output line
					(at 38.1 -50.8 180)
					(length 2.54)
					(name "USB2_MONCDR")
					(number "48")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "USB2_AVDD33")
					(number "49")
				)
				(pin bidirectional line
					(at 38.1 -53.34 180)
					(length 2.54)
					(name "USB2_RREF")
					(number "50")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "BT_DEV_WAKE")
					(number "51")
				)
				(pin output line
					(at 38.1 -10.16 180)
					(length 2.54)
					(name "WL_HOST_WAKE")
					(number "52")
				)
				(pin input line
					(at 38.1 -15.24 180)
					(length 2.54)
					(name "JTAG_SEL")
					(number "53")
				)
				(pin input line
					(at 38.1 -59.69 180)
					(length 2.54)
					(name "STRAP_1")
					(number "54")
				)
				(pin input line
					(at 38.1 -62.23 180)
					(length 2.54)
					(name "STRAP_2")
					(number "55")
				)
				(pin input line
					(at 38.1 -57.15 180)
					(length 2.54)
					(name "STRAP_0")
					(number "56")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "57")
				)
				(pin bidirectional line
					(at 38.1 -17.78 180)
					(length 2.54)
					(name "TRST_L")
					(number "63")
				)
				(pin bidirectional line
					(at 38.1 -20.32 180)
					(length 2.54)
					(name "JTAG_TDI")
					(number "64")
				)
				(pin bidirectional line
					(at 38.1 -22.86 180)
					(length 2.54)
					(name "JTAG_TDO")
					(number "65")
				)
				(pin bidirectional line
					(at 38.1 -25.4 180)
					(length 2.54)
					(name "JTAG_TCK/SWCLK")
					(number "66")
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 2.54)
					(name "JTAG_TMS/SWDIO")
					(number "67")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "BT_REG_EN")
					(number "68")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "69")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "70")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "71")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "72")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "73")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "74")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "75")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "76")
				)
				(pin passive line
					(at 38.1 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "77")
				)
			)
			(symbol "WiFi_Bluetooth_LBEE5PK2AE_2_1"
				(pin no_connect line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin no_connect line
					(at 0 -1.27 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at 0 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "39")
				)
				(pin no_connect line
					(at 11.43 0 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "40")
				)
				(pin no_connect line
					(at 11.43 -1.27 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "44")
				)
				(pin no_connect line
					(at 11.43 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "58")
				)
				(pin no_connect line
					(at 11.43 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "59")
				)
				(pin no_connect line
					(at 11.43 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "60")
				)
				(pin no_connect line
					(at 11.43 -6.35 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "61")
				)
				(pin no_connect line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "62")
				)
			)
			(embedded_fonts no)
		)
)
