(footprint "BGA-108_16x11.9x3.51mm_Layout9x11_P1.27mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -8.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-108_16x11.9x3.51mm_Layout9x11_P1.27mm"
		(at 0 9.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -7.62 12.16 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -7.62 13.36 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -7.62 14.56 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -5.08 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A2" smd circle
		(at -3.81 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A3" smd circle
		(at -2.54 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A4" smd circle
		(at -1.27 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A5" smd circle
		(at 0 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A6" smd circle
		(at 1.27 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A7" smd circle
		(at 2.54 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A8" smd circle
		(at 3.81 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A9" smd circle
		(at 5.08 -6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B1" smd circle
		(at -5.08 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B2" smd circle
		(at -3.81 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B3" smd circle
		(at -2.54 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B4" smd circle
		(at -1.27 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B5" smd circle
		(at 0 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B6" smd circle
		(at 1.27 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B7" smd circle
		(at 2.54 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B8" smd circle
		(at 3.81 -5.715 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "B9" smd circle
		(at 5.08 -5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C1" smd circle
		(at -5.08 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C2" smd circle
		(at -3.81 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C3" smd circle
		(at -2.54 -4.445 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "C4" smd circle
		(at -1.27 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C5" smd circle
		(at 0 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C6" smd circle
		(at 1.27 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C7" smd circle
		(at 2.54 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C8" smd circle
		(at 3.81 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C9" smd circle
		(at 5.08 -4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D1" smd circle
		(at -5.08 -3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D2" smd circle
		(at -3.81 -3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D3" smd circle
		(at -2.54 -3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D4" smd circle
		(at -1.27 -3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D5" smd circle
		(at 0 -3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D6" smd circle
		(at 1.27 -3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D7" smd circle
		(at 2.54 -3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D8" smd circle
		(at 3.81 -3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D9" smd circle
		(at 5.08 -3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "E1" smd circle
		(at -5.08 -1.905 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "E2" smd circle
		(at -3.81 -1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E3" smd circle
		(at -2.54 -1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E4" smd circle
		(at -1.27 -1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E5" smd circle
		(at 0 -1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E6" smd circle
		(at 1.27 -1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E7" smd circle
		(at 2.54 -1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E8" smd circle
		(at 3.81 -1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E9" smd circle
		(at 5.08 -1.905 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F1" smd circle
		(at -5.08 -0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F2" smd circle
		(at -3.81 -0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F3" smd circle
		(at -2.54 -0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F4" smd circle
		(at -1.27 -0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F5" smd circle
		(at 0 -0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F6" smd circle
		(at 1.27 -0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F7" smd circle
		(at 2.54 -0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F8" smd circle
		(at 3.81 -0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F9" smd circle
		(at 5.08 -0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G1" smd circle
		(at -5.08 0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G2" smd circle
		(at -3.81 0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G3" smd circle
		(at -2.54 0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G4" smd circle
		(at -1.27 0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G5" smd circle
		(at 0 0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G6" smd circle
		(at 1.27 0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G7" smd circle
		(at 2.54 0.635 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G8" smd circle
		(at 3.81 0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G9" smd circle
		(at 5.08 0.635 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "H1" smd circle
		(at -5.08 1.905 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "H2" smd circle
		(at -3.81 1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H3" smd circle
		(at -2.54 1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H4" smd circle
		(at -1.27 1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H5" smd circle
		(at 0 1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H6" smd circle
		(at 1.27 1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H7" smd circle
		(at 2.54 1.905 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H8" smd circle
		(at 3.81 1.905 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "H9" smd circle
		(at 5.08 1.905 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J1" smd circle
		(at -5.08 3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J2" smd circle
		(at -3.81 3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J3" smd circle
		(at -2.54 3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J4" smd circle
		(at -1.27 3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J5" smd circle
		(at 0 3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J6" smd circle
		(at 1.27 3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J7" smd circle
		(at 2.54 3.175 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J8" smd circle
		(at 3.81 3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J9" smd circle
		(at 5.08 3.175 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K1" smd circle
		(at -5.08 4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K2" smd circle
		(at -3.81 4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K3" smd circle
		(at -2.54 4.445 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "K4" smd circle
		(at -1.27 4.445 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "K5" smd circle
		(at 0 4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K6" smd circle
		(at 1.27 4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K7" smd circle
		(at 2.54 4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K8" smd circle
		(at 3.81 4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K9" smd circle
		(at 5.08 4.445 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L1" smd circle
		(at -5.08 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L2" smd circle
		(at -3.81 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L3" smd circle
		(at -2.54 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L4" smd circle
		(at -1.27 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L5" smd circle
		(at 0 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L6" smd circle
		(at 1.27 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L7" smd circle
		(at 2.54 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L8" smd circle
		(at 3.81 5.715 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "L9" smd circle
		(at 5.08 5.715 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M1" smd circle
		(at -5.08 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M2" smd circle
		(at -3.81 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M3" smd circle
		(at -2.54 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M4" smd circle
		(at -1.27 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M5" smd circle
		(at 0 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M6" smd circle
		(at 1.27 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M7" smd circle
		(at 2.54 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M8" smd circle
		(at 3.81 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M9" smd circle
		(at 5.08 6.985 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(embedded_fonts no)
	(model "antmicro_ltm4675ey_pbf.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
