(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LTM4675"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LTM4675"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LTM4675"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltm4675.pdf"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Module, Regulator, Vin 4.5V-17V , Vout 0.5V - 5.5V, Iout 2x9A|1x18A"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LTM4675EY#PBF"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "REGULATOR, IC, POWER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LTM4675_1_1"
				(pin passive line
					(at 26.67 -27.94 180)
					(length 2.54)
					(name "TSNS0")
					(number "C3")
				)
				(pin passive line
					(at 26.67 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "TSNS0")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SDA")
					(number "D4")
				)
				(pin bidirectional line
					(at 26.67 -12.7 180)
					(length 2.54)
					(name "~{GPIO0}")
					(number "E2")
				)
				(pin input line
					(at 26.67 -17.78 180)
					(length 2.54)
					(name "~{ALERT}")
					(number "E3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCL")
					(number "E4")
				)
				(pin bidirectional line
					(at 26.67 -8.89 180)
					(length 2.54)
					(name "SYNC")
					(number "E5")
				)
				(pin bidirectional line
					(at 26.67 -15.24 180)
					(length 2.54)
					(name "~{GPIO1}")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "RUN0")
					(number "F3")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "RUN1")
					(number "F4")
				)
				(pin power_in line
					(at 26.67 -33.02 180)
					(length 2.54)
					(name "SGND")
					(number "F5")
				)
				(pin passive line
					(at 26.67 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "SGND")
					(number "F6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "INTVCC")
					(number "F7")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SVIN")
					(number "F9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ASEL")
					(number "G2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VOUT0CFG")
					(number "G3")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "VOUT1CFG")
					(number "G4")
				)
				(pin passive line
					(at 26.67 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "SGND")
					(number "G5")
				)
				(pin passive line
					(at 26.67 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "SGND")
					(number "G6")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "INTVCC")
					(number "G7")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "FSWPHCFG")
					(number "H2")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "VTRIM0CFG")
					(number "H3")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "VTRIM1CFG")
					(number "H4")
				)
				(pin bidirectional line
					(at 26.67 -6.35 180)
					(length 2.54)
					(name "SHARE_CLK")
					(number "H5")
				)
				(pin passive line
					(at 26.67 -21.59 180)
					(length 2.54)
					(name "TSNS1A")
					(number "J3")
				)
				(pin output line
					(at 26.67 -2.54 180)
					(length 2.54)
					(name "VDD25")
					(number "J4")
				)
				(pin output line
					(at 26.67 0 180)
					(length 2.54)
					(name "VDD33")
					(number "J5")
				)
				(pin passive line
					(at 26.67 -24.13 180)
					(length 2.54)
					(name "TSNS1B")
					(number "K3")
				)
				(pin passive line
					(at 26.67 -30.48 180)
					(length 2.54)
					(name "WP")
					(number "K4")
				)
			)
			(symbol "LTM4675_2_1"
				(pin power_out line
					(at 26.67 0 180)
					(length 2.54)
					(name "VOUT0")
					(number "A1")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GND")
					(number "A2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A8")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "VIN0")
					(number "A9")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 2.54)
					(hide yes)
					(name "VOUT0")
					(number "B1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 2.54)
					(name "SW0")
					(number "B8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN0")
					(number "B9")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 2.54)
					(hide yes)
					(name "VOUT0")
					(number "C1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN0")
					(number "C9")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 2.54)
					(hide yes)
					(name "VOUT0")
					(number "D1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "D2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "COMP0B")
					(number "D6")
				)
				(pin input line
					(at 26.67 -8.89 180)
					(length 2.54)
					(name "VOSNS0+")
					(number "D7")
				)
				(pin passive line
					(at 26.67 -19.05 180)
					(length 2.54)
					(name "VORB0+")
					(number "D8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN0")
					(number "D9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "COMP0A")
					(number "E6")
				)
				(pin input line
					(at 26.67 -11.43 180)
					(length 2.54)
					(name "VOSNS0-")
					(number "E7")
				)
				(pin passive line
					(at 26.67 -21.59 180)
					(length 2.54)
					(name "VORB0-")
					(number "E8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "F1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "G9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "H1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "COMP1A")
					(number "H6")
				)
				(pin input line
					(at 26.67 -15.24 180)
					(length 2.54)
					(name "VOSNS1")
					(number "H7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "H9")
				)
				(pin power_out line
					(at 26.67 -2.54 180)
					(length 2.54)
					(name "VOUT1")
					(number "J1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "J2")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "COMP1B")
					(number "J6")
				)
				(pin passive line
					(at 26.67 -25.4 180)
					(length 2.54)
					(name "VORB1")
					(number "J7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "J8")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VIN1")
					(number "J9")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VOUT1")
					(number "K1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VIN1")
					(number "K9")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VOUT1")
					(number "L1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L7")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SW1")
					(number "L8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VIN1")
					(number "L9")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VOUT1")
					(number "M1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VIN1")
					(number "M9")
				)
			)
			(embedded_fonts no)
		)
)
