(footprint "BGA-144_16x16x5mm_Layout12x12_P1.27mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -8.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-144_16x16x5mm_Layout12x12_P1.27mm"
		(at 0 9.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -8.4 12.16 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.4 13.36 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -8.4 14.56 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -7 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A2" smd circle
		(at -5.73 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A3" smd circle
		(at -4.46 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A4" smd circle
		(at -3.19 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A5" smd circle
		(at -1.92 -7 270)
		(size 0.737 0.737)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.051)
		(solder_paste_margin -0.064)
	)
	(pad "A6" smd circle
		(at -0.65 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A7" smd circle
		(at 0.62 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A8" smd circle
		(at 1.89 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A9" smd circle
		(at 3.16 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A10" smd circle
		(at 4.43 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A11" smd circle
		(at 5.7 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "A12" smd circle
		(at 6.97 -7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B1" smd circle
		(at -7 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B2" smd circle
		(at -5.73 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B3" smd circle
		(at -4.46 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B4" smd circle
		(at -3.19 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B5" smd circle
		(at -1.92 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B6" smd circle
		(at -0.65 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B7" smd circle
		(at 0.62 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B8" smd circle
		(at 1.89 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B9" smd circle
		(at 3.16 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B10" smd circle
		(at 4.43 -5.73 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "B11" smd circle
		(at 5.7 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "B12" smd circle
		(at 6.97 -5.73 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C1" smd circle
		(at -7 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C2" smd circle
		(at -5.73 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C3" smd circle
		(at -4.46 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C4" smd circle
		(at -3.19 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C5" smd circle
		(at -1.92 -4.46 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "C6" smd circle
		(at -0.65 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C7" smd circle
		(at 0.62 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C8" smd circle
		(at 1.89 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C9" smd circle
		(at 3.16 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C10" smd circle
		(at 4.43 -4.46 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "C11" smd circle
		(at 5.7 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "C12" smd circle
		(at 6.97 -4.46 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D1" smd circle
		(at -7 -3.19 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D2" smd circle
		(at -5.73 -3.19 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D3" smd circle
		(at -4.46 -3.19 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D4" smd circle
		(at -3.19 -3.19 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D5" smd circle
		(at -1.92 -3.19 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D6" smd circle
		(at -0.65 -3.19 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D7" smd circle
		(at 0.62 -3.19 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D8" smd circle
		(at 1.89 -3.19 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D9" smd circle
		(at 3.16 -3.19 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D10" smd circle
		(at 4.43 -3.19 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "D11" smd circle
		(at 5.7 -3.19 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "D12" smd circle
		(at 6.97 -3.19 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "E1" smd circle
		(at -7 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E2" smd circle
		(at -5.73 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E3" smd circle
		(at -4.46 -1.92 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "E4" smd circle
		(at -3.19 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E5" smd circle
		(at -1.92 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E6" smd circle
		(at -0.65 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E7" smd circle
		(at 0.62 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E8" smd circle
		(at 1.89 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E9" smd circle
		(at 3.16 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E10" smd circle
		(at 4.43 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E11" smd circle
		(at 5.7 -1.92 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "E12" smd circle
		(at 6.97 -1.92 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F1" smd circle
		(at -7 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F2" smd circle
		(at -5.73 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F3" smd circle
		(at -4.46 -0.65 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F4" smd circle
		(at -3.19 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F5" smd circle
		(at -1.92 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F6" smd circle
		(at -0.65 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F7" smd circle
		(at 0.62 -0.65 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F8" smd circle
		(at 1.89 -0.65 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F9" smd circle
		(at 3.16 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F10" smd circle
		(at 4.43 -0.65 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "F11" smd circle
		(at 5.7 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "F12" smd circle
		(at 6.97 -0.65 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G1" smd circle
		(at -7 0.62 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G2" smd circle
		(at -5.73 0.62 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G3" smd circle
		(at -4.46 0.62 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G4" smd circle
		(at -3.19 0.62 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G5" smd circle
		(at -1.92 0.62 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G6" smd circle
		(at -0.65 0.62 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G7" smd circle
		(at 0.62 0.62 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G8" smd circle
		(at 1.89 0.62 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G9" smd circle
		(at 3.16 0.62 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "G10" smd circle
		(at 4.43 0.62 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G11" smd circle
		(at 5.7 0.62 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "G12" smd circle
		(at 6.97 0.62 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "H1" smd circle
		(at -7 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H2" smd circle
		(at -5.73 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H3" smd circle
		(at -4.46 1.89 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "H4" smd circle
		(at -3.19 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H5" smd circle
		(at -1.92 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H6" smd circle
		(at -0.65 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H7" smd circle
		(at 0.62 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H8" smd circle
		(at 1.89 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H9" smd circle
		(at 3.16 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H10" smd circle
		(at 4.43 1.89 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "H11" smd circle
		(at 5.7 1.89 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "H12" smd circle
		(at 6.97 1.89 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J1" smd circle
		(at -7 3.16 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J2" smd circle
		(at -5.73 3.16 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J3" smd circle
		(at -4.46 3.16 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J4" smd circle
		(at -3.19 3.16 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J5" smd circle
		(at -1.92 3.16 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J6" smd circle
		(at -0.65 3.16 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J7" smd circle
		(at 0.62 3.16 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J8" smd circle
		(at 1.89 3.16 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J9" smd circle
		(at 3.16 3.16 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "J10" smd circle
		(at 4.43 3.16 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J11" smd circle
		(at 5.7 3.16 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "J12" smd circle
		(at 6.97 3.16 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K1" smd circle
		(at -7 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K2" smd circle
		(at -5.73 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K3" smd circle
		(at -4.46 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K4" smd circle
		(at -3.19 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K5" smd circle
		(at -1.92 4.43 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "K6" smd circle
		(at -0.65 4.43 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "K7" smd circle
		(at 0.62 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K8" smd circle
		(at 1.89 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K9" smd circle
		(at 3.16 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K10" smd circle
		(at 4.43 4.43 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "K11" smd circle
		(at 5.7 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "K12" smd circle
		(at 6.97 4.43 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L1" smd circle
		(at -7 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L2" smd circle
		(at -5.73 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L3" smd circle
		(at -4.46 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L4" smd circle
		(at -3.19 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L5" smd circle
		(at -1.92 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L6" smd circle
		(at -0.65 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L7" smd circle
		(at 0.62 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L8" smd circle
		(at 1.89 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L9" smd circle
		(at 3.16 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L10" smd circle
		(at 4.43 5.7 270)
		(size 0.635 0.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
		(solder_paste_margin -0.0127)
	)
	(pad "L11" smd circle
		(at 5.7 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "L12" smd circle
		(at 6.97 5.7 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M1" smd circle
		(at -7 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M2" smd circle
		(at -5.73 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M3" smd circle
		(at -4.46 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M4" smd circle
		(at -3.19 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M5" smd circle
		(at -1.92 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M6" smd circle
		(at -0.65 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M7" smd circle
		(at 0.62 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M8" smd circle
		(at 1.89 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M9" smd circle
		(at 3.16 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M10" smd circle
		(at 4.43 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M11" smd circle
		(at 5.7 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(pad "M12" smd circle
		(at 6.97 6.97 270)
		(size 0.7366 0.7366)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.0508)
		(solder_paste_margin -0.0635)
	)
	(embedded_fonts no)
	(model "antmicro_ltm4677ey_pbf.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
