(footprint "BGA-330_15x22x7.8_Layout15x22_P1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -11.8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-330_15x22x7.8_Layout15x22_P1mm"
		(at 0 12.3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -35.153 14 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -35.153 15.2 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -35.153 16.4 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -7 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A2" smd circle
		(at -6 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A3" smd circle
		(at -5 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A4" smd circle
		(at -4 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A5" smd circle
		(at -3 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A6" smd circle
		(at -2 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A7" smd circle
		(at -1 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A8" smd circle
		(at 0 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A9" smd circle
		(at 1 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A10" smd circle
		(at 2 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A11" smd circle
		(at 3 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A12" smd circle
		(at 4 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A13" smd circle
		(at 5 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A14" smd circle
		(at 6 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "A15" smd circle
		(at 7 -10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA1" smd circle
		(at -7 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA2" smd circle
		(at -6 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA3" smd circle
		(at -5 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA4" smd circle
		(at -4 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA5" smd circle
		(at -3 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA6" smd circle
		(at -2 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA7" smd circle
		(at -1 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA8" smd circle
		(at 0 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA9" smd circle
		(at 1 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA10" smd circle
		(at 2 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA11" smd circle
		(at 3 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA12" smd circle
		(at 4 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA13" smd circle
		(at 5 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA14" smd circle
		(at 6 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AA15" smd circle
		(at 7 9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB1" smd circle
		(at -7 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB2" smd circle
		(at -6 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB3" smd circle
		(at -5 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB4" smd circle
		(at -4 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB5" smd circle
		(at -3 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB6" smd circle
		(at -2 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB7" smd circle
		(at -1 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB8" smd circle
		(at 0 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB9" smd circle
		(at 1 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB10" smd circle
		(at 2 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB11" smd circle
		(at 3 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB12" smd circle
		(at 4 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB13" smd circle
		(at 5 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB14" smd circle
		(at 6 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "AB15" smd circle
		(at 7 10.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B1" smd circle
		(at -7 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B2" smd circle
		(at -6 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B3" smd circle
		(at -5 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B4" smd circle
		(at -4 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B5" smd circle
		(at -3 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B6" smd circle
		(at -2 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B7" smd circle
		(at -1 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B8" smd circle
		(at 0 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B9" smd circle
		(at 1 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B10" smd circle
		(at 2 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B11" smd circle
		(at 3 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B12" smd circle
		(at 4 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B13" smd circle
		(at 5 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B14" smd circle
		(at 6 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "B15" smd circle
		(at 7 -9.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C1" smd circle
		(at -7 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C2" smd circle
		(at -6 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C3" smd circle
		(at -5 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C4" smd circle
		(at -4 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C5" smd circle
		(at -3 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C6" smd circle
		(at -2 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C7" smd circle
		(at -1 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C8" smd circle
		(at 0 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C9" smd circle
		(at 1 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C10" smd circle
		(at 2 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C11" smd circle
		(at 3 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C12" smd circle
		(at 4 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C13" smd circle
		(at 5 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C14" smd circle
		(at 6 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "C15" smd circle
		(at 7 -8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D1" smd circle
		(at -7 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D2" smd circle
		(at -6 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D3" smd circle
		(at -5 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D4" smd circle
		(at -4 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D5" smd circle
		(at -3 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D6" smd circle
		(at -2 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D7" smd circle
		(at -1 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D8" smd circle
		(at 0 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D9" smd circle
		(at 1 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D10" smd circle
		(at 2 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D11" smd circle
		(at 3 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D12" smd circle
		(at 4 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D13" smd circle
		(at 5 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D14" smd circle
		(at 6 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "D15" smd circle
		(at 7 -7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E1" smd circle
		(at -7 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E2" smd circle
		(at -6 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E3" smd circle
		(at -5 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E4" smd circle
		(at -4 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E5" smd circle
		(at -3 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E6" smd circle
		(at -2 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E7" smd circle
		(at -1 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E8" smd circle
		(at 0 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E9" smd circle
		(at 1 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E10" smd circle
		(at 2 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E11" smd circle
		(at 3 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E12" smd circle
		(at 4 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E13" smd circle
		(at 5 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E14" smd circle
		(at 6 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "E15" smd circle
		(at 7 -6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F1" smd circle
		(at -7 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F2" smd circle
		(at -6 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F3" smd circle
		(at -5 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F4" smd circle
		(at -4 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F5" smd circle
		(at -3 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F6" smd circle
		(at -2 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F7" smd circle
		(at -1 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F8" smd circle
		(at 0 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F9" smd circle
		(at 1 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F10" smd circle
		(at 2 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F11" smd circle
		(at 3 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F12" smd circle
		(at 4 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F13" smd circle
		(at 5 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F14" smd circle
		(at 6 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "F15" smd circle
		(at 7 -5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G1" smd circle
		(at -7 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G2" smd circle
		(at -6 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G3" smd circle
		(at -5 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G4" smd circle
		(at -4 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G5" smd circle
		(at -3 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G6" smd circle
		(at -2 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G7" smd circle
		(at -1 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G8" smd circle
		(at 0 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G9" smd circle
		(at 1 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G10" smd circle
		(at 2 -4.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "G11" smd circle
		(at 3 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G12" smd circle
		(at 4 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G13" smd circle
		(at 5 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "G14" smd circle
		(at 6 -4.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "G15" smd circle
		(at 7 -4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H1" smd circle
		(at -7 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H2" smd circle
		(at -6 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H3" smd circle
		(at -5 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H4" smd circle
		(at -4 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H5" smd circle
		(at -3 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H6" smd circle
		(at -2 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H7" smd circle
		(at -1 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H8" smd circle
		(at 0 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "H9" smd circle
		(at 1 -3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "H10" smd circle
		(at 2 -3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "H11" smd circle
		(at 3 -3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "H12" smd circle
		(at 4 -3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "H13" smd circle
		(at 5 -3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "H14" smd circle
		(at 6 -3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "H15" smd circle
		(at 7 -3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J1" smd circle
		(at -7 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J2" smd circle
		(at -6 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J3" smd circle
		(at -5 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J4" smd circle
		(at -4 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J5" smd circle
		(at -3 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J6" smd circle
		(at -2 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J7" smd circle
		(at -1 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "J8" smd circle
		(at 0 -2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "J9" smd circle
		(at 1 -2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "J10" smd circle
		(at 2 -2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "J11" smd circle
		(at 3 -2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "J12" smd circle
		(at 4 -2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "J13" smd circle
		(at 5 -2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "J14" smd circle
		(at 6 -2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "J15" smd circle
		(at 7 -2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K1" smd circle
		(at -7 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K2" smd circle
		(at -6 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K3" smd circle
		(at -5 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K4" smd circle
		(at -4 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K5" smd circle
		(at -3 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K6" smd circle
		(at -2 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K7" smd circle
		(at -1 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K8" smd circle
		(at 0 -1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "K9" smd circle
		(at 1 -1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "K10" smd circle
		(at 2 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K11" smd circle
		(at 3 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "K12" smd circle
		(at 4 -1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "K13" smd circle
		(at 5 -1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "K14" smd circle
		(at 6 -1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "K15" smd circle
		(at 7 -1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L1" smd circle
		(at -7 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L2" smd circle
		(at -6 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L3" smd circle
		(at -5 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L4" smd circle
		(at -4 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L5" smd circle
		(at -3 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L6" smd circle
		(at -2 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L7" smd circle
		(at -1 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L8" smd circle
		(at 0 -0.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "L9" smd circle
		(at 1 -0.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "L10" smd circle
		(at 2 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L11" smd circle
		(at 3 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L12" smd circle
		(at 4 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L13" smd circle
		(at 5 -0.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "L14" smd circle
		(at 6 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "L15" smd circle
		(at 7 -0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M1" smd circle
		(at -7 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M2" smd circle
		(at -6 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M3" smd circle
		(at -5 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M4" smd circle
		(at -4 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M5" smd circle
		(at -3 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M6" smd circle
		(at -2 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M7" smd circle
		(at -1 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M8" smd circle
		(at 0 0.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "M9" smd circle
		(at 1 0.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "M10" smd circle
		(at 2 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M11" smd circle
		(at 3 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M12" smd circle
		(at 4 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M13" smd circle
		(at 5 0.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "M14" smd circle
		(at 6 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "M15" smd circle
		(at 7 0.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N1" smd circle
		(at -7 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N2" smd circle
		(at -6 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N3" smd circle
		(at -5 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N4" smd circle
		(at -4 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N5" smd circle
		(at -3 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N6" smd circle
		(at -2 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N7" smd circle
		(at -1 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N8" smd circle
		(at 0 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N9" smd circle
		(at 1 1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "N10" smd circle
		(at 2 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N11" smd circle
		(at 3 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N12" smd circle
		(at 4 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "N13" smd circle
		(at 5 1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "N14" smd circle
		(at 6 1.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "N15" smd circle
		(at 7 1.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P1" smd circle
		(at -7 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P2" smd circle
		(at -6 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P3" smd circle
		(at -5 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P4" smd circle
		(at -4 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P5" smd circle
		(at -3 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P6" smd circle
		(at -2 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P7" smd circle
		(at -1 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P8" smd circle
		(at 0 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P9" smd circle
		(at 1 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P10" smd circle
		(at 2 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P11" smd circle
		(at 3 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P12" smd circle
		(at 4 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "P13" smd circle
		(at 5 2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "P14" smd circle
		(at 6 2.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "P15" smd circle
		(at 7 2.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R1" smd circle
		(at -7 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R2" smd circle
		(at -6 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R3" smd circle
		(at -5 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R4" smd circle
		(at -4 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R5" smd circle
		(at -3 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R6" smd circle
		(at -2 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R7" smd circle
		(at -1 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R8" smd circle
		(at 0 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R9" smd circle
		(at 1 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R10" smd circle
		(at 2 3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "R11" smd circle
		(at 3 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R12" smd circle
		(at 4 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "R13" smd circle
		(at 5 3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "R14" smd circle
		(at 6 3.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "R15" smd circle
		(at 7 3.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T1" smd circle
		(at -7 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T2" smd circle
		(at -6 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T3" smd circle
		(at -5 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T4" smd circle
		(at -4 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T5" smd circle
		(at -3 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T6" smd circle
		(at -2 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T7" smd circle
		(at -1 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T8" smd circle
		(at 0 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T9" smd circle
		(at 1 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T10" smd circle
		(at 2 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T11" smd circle
		(at 3 4.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "T12" smd circle
		(at 4 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T13" smd circle
		(at 5 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "T14" smd circle
		(at 6 4.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "T15" smd circle
		(at 7 4.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U1" smd circle
		(at -7 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U2" smd circle
		(at -6 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U3" smd circle
		(at -5 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U4" smd circle
		(at -4 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U5" smd circle
		(at -3 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U6" smd circle
		(at -2 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U7" smd circle
		(at -1 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U8" smd circle
		(at 0 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U9" smd circle
		(at 1 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U10" smd circle
		(at 2 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U11" smd circle
		(at 3 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U12" smd circle
		(at 4 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U13" smd circle
		(at 5 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U14" smd circle
		(at 6 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "U15" smd circle
		(at 7 5.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V1" smd circle
		(at -7 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V2" smd circle
		(at -6 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V3" smd circle
		(at -5 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V4" smd circle
		(at -4 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V5" smd circle
		(at -3 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V6" smd circle
		(at -2 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V7" smd circle
		(at -1 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V8" smd circle
		(at 0 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V9" smd circle
		(at 1 6.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "V10" smd circle
		(at 2 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V11" smd circle
		(at 3 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V12" smd circle
		(at 4 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V13" smd circle
		(at 5 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V14" smd circle
		(at 6 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "V15" smd circle
		(at 7 6.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W1" smd circle
		(at -7 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W2" smd circle
		(at -6 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W3" smd circle
		(at -5 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W4" smd circle
		(at -4 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W5" smd circle
		(at -3 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W6" smd circle
		(at -2 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W7" smd circle
		(at -1 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W8" smd circle
		(at 0 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W9" smd circle
		(at 1 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W10" smd circle
		(at 2 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W11" smd circle
		(at 3 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W12" smd circle
		(at 4 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W13" smd circle
		(at 5 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W14" smd circle
		(at 6 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "W15" smd circle
		(at 7 7.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y1" smd circle
		(at -7 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y2" smd circle
		(at -6 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y3" smd circle
		(at -5 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y4" smd circle
		(at -4 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y5" smd circle
		(at -3 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y6" smd circle
		(at -2 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y7" smd circle
		(at -1 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y8" smd circle
		(at 0 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y9" smd circle
		(at 1 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y10" smd circle
		(at 2 8.5 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.06)
		(solder_paste_margin -0.01)
	)
	(pad "Y11" smd circle
		(at 3 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y12" smd circle
		(at 4 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y13" smd circle
		(at 5 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y14" smd circle
		(at 6 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(pad "Y15" smd circle
		(at 7 8.5 270)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.06)
	)
	(embedded_fonts no)
	(model "antmicro_ltm4700ey_pbf.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
