(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LTM4700"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LTM4700"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LTM4700"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltm4700.pdf"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dual Power Module, Vin 4.5V-16V , Vout 0.5V-1.8V, Iout 2x50A | 1x100A"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LTM4700EY#PBF"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, REGULATOR, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LTM4700_1_1"
				(pin output line
					(at 31.75 -2.54 180)
					(length 5.08)
					(name "VDD25")
					(number "G10")
				)
				(pin passive line
					(at 31.75 -35.56 180)
					(length 5.08)
					(name "TSNS1B")
					(number "G14")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VTRIM1CFG")
					(number "H9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(name "VOUT1CFG")
					(number "H10")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "ASEL")
					(number "H11")
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 5.08)
					(name "~{FAULT1}")
					(number "H12")
				)
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 5.08)
					(name "~{FAULT0}")
					(number "H13")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "SDA")
					(number "H14")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(name "WP")
					(number "J8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VTRIM0CFG")
					(number "J9")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(name "VOUT0CFG")
					(number "J10")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "FSWPH_CFG")
					(number "J11")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "RUN0")
					(number "J12")
				)
				(pin output line
					(at 31.75 -17.78 180)
					(length 5.08)
					(name "~{ALERT}")
					(number "J13")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 5.08)
					(name "SCL")
					(number "J14")
				)
				(pin bidirectional line
					(at 31.75 -6.35 180)
					(length 5.08)
					(name "SHARE_CLK")
					(number "K8")
				)
				(pin output line
					(at 31.75 0 180)
					(length 5.08)
					(name "VDD33")
					(number "K9")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "RUN1")
					(number "K12")
				)
				(pin passive line
					(at 31.75 -27.94 180)
					(length 5.08)
					(name "TSNS0A")
					(number "K13")
				)
				(pin bidirectional line
					(at 31.75 -8.89 180)
					(length 5.08)
					(name "SYNC")
					(number "K14")
				)
				(pin power_in line
					(at 31.75 -40.64 180)
					(length 5.08)
					(name "SGND")
					(number "L10")
				)
				(pin passive line
					(at 31.75 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "SGND")
					(number "L11")
				)
				(pin passive line
					(at 31.75 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "SGND")
					(number "L12")
				)
				(pin passive line
					(at 31.75 -33.02 180)
					(length 5.08)
					(name "TSNS1A")
					(number "L13")
				)
				(pin passive line
					(at 31.75 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "SGND")
					(number "M10")
				)
				(pin passive line
					(at 31.75 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "SGND")
					(number "M11")
				)
				(pin passive line
					(at 31.75 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "SGND")
					(number "M12")
				)
				(pin output line
					(at 31.75 -24.13 180)
					(length 5.08)
					(name "PGOOD1")
					(number "N9")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "INTVCC")
					(number "R10")
				)
				(pin output line
					(at 31.75 -21.59 180)
					(length 5.08)
					(name "PGOOD0")
					(number "R14")
				)
				(pin passive line
					(at 31.75 -30.48 180)
					(length 5.08)
					(name "TSNS0B")
					(number "T14")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "SVIN")
					(number "V9")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "RUNP")
					(number "Y10")
				)
			)
			(symbol "LTM4700_2_1"
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(name "SW0")
					(number "AA1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "AA2")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "VIN0")
					(number "AA6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "AA7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "AA8")
				)
				(pin power_out line
					(at 29.21 0 180)
					(length 5.08)
					(name "VOUT0")
					(number "AA12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "AA13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "AA14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "AA15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "AB1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "AB2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "AB6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "AB7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "AB8")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "AB12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "AB13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "AB14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "AB15")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(name "COMP0B")
					(number "M13")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "N1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "N2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "N6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "N7")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(name "COMP0A")
					(number "N13")
				)
				(pin input line
					(at 29.21 -7.62 180)
					(length 5.08)
					(name "VOSNSO-")
					(number "N14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "N15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "P1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "P2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "P6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "P7")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "IIN-")
					(number "P13")
				)
				(pin input line
					(at 29.21 -5.08 180)
					(length 5.08)
					(name "VOSNSO+")
					(number "P14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "P15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "R1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "R2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "R6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "R7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "R8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "IIN+")
					(number "R13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "R15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "T1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "T2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "T6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "T7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "T8")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "T15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "U1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "U2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "U6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "U7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "U8")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "U12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "U13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "U14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "U15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "V1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "V2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "V6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "V7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "V8")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "V12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "V13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "V14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "V15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "W1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "W2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "W6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "W7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "W8")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "W12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "W13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "W14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "W15")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "Y1")
				)
				(pin passive line
					(at 29.21 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "SW0")
					(number "Y2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "Y6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "Y7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN0")
					(number "Y8")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "Y12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "Y13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "Y14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT0")
					(number "Y15")
				)
			)
			(symbol "LTM4700_3_1"
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SW1")
					(number "A1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "A2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "VIN1")
					(number "A6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "A7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "A8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A9")
				)
				(pin power_in line
					(at 29.21 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "A10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A11")
				)
				(pin power_out line
					(at 29.21 0 180)
					(length 5.08)
					(name "VOUT1")
					(number "A12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "A13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "A14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "A15")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB11")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "B1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "B2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "B6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "B7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "B8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "B12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "B13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "B14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "B15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "C1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "C2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "C6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "C7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "C8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "C11")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "C12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "C13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "C14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "C15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "D1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "D2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "D6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "D7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "D8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D11")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "D12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "D13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "D14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "D15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "E1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "E2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "E6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "E7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "E8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "E12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "E13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "E14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "E15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "F1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "F2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "F6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "F7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "F8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "F12")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "F13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "F14")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "F15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "G1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "G2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "G6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "G7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "G8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G12")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G13")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "G15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "H1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "H2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "H6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "H7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "H8")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "H15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "J1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "J2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "J6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "J7")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "J15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "K1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "SW1")
					(number "K2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "K6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VIN1")
					(number "K7")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "VOUT1")
					(number "K15")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L1")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L6")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L7")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 5.08)
					(name "COMP1A")
					(number "L8")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 5.08)
					(name "COMP1B")
					(number "L9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L14")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L15")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M1")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M2")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M6")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M7")
				)
				(pin input line
					(at 29.21 -6.35 180)
					(length 5.08)
					(name "VOSNS1-")
					(number "M8")
				)
				(pin input line
					(at 29.21 -3.81 180)
					(length 5.08)
					(name "VOSNS1+")
					(number "M9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M14")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M15")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N12")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P8")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P12")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R12")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T10")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "VBIAS")
					(number "T11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T12")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T13")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W10")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W11")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y3")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y4")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y5")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y9")
				)
				(pin passive line
					(at 29.21 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y11")
				)
			)
			(embedded_fonts no)
		)
)
